#
# \brief  Test for the TCP terminal
# \author Norman Feske
# \date   2011-09-08
#

#
# TODO: Add support for Linux via user-level networking (using the
#       tun/tap proxy driver at os/src/drivers/nic/linux)
#
if {[have_spec linux]} {
	puts "Run script does not support Linux."; exit 0 }

create_boot_directory

import_from_depot [depot_user]/src/[base_src] \
                  [depot_user]/pkg/[drivers_nic_pkg] \
                  [depot_user]/src/init \
                  [depot_user]/src/libc \
                  [depot_user]/src/nic_router \
                  [depot_user]/src/vfs \
                  [depot_user]/src/vfs_lwip \
                  [depot_user]/src/vfs_pipe

build { server/tcp_terminal test/terminal_echo }

install_config {
<config verbose="yes">
	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<default caps="100"/>
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Timer"/> </provides>
	</start>
	<start name="drivers" caps="1000" managing_system="yes">
		<resource name="RAM" quantum="32M"/>
		<binary name="init"/>
		<route>
			<service name="ROM" label="config"> <parent label="drivers.config"/> </service>
			<service name="Timer"> <child name="timer"/> </service>
			<service name="Uplink"> <child name="nic_router"/> </service>
			<any-service> <parent/> </any-service>
		</route>
	</start>
	<start name="nic_router" caps="200">
		<resource name="RAM" quantum="10M"/>
		<provides>
			<service name="Nic"/>
			<service name="Uplink"/>
		</provides>
		<config verbose_domain_state="yes">

			<policy label_prefix="tcp_terminal" domain="downlink"/>
			<policy label_prefix="drivers"      domain="uplink"/>

			<domain name="uplink">

				<nat domain="downlink"
				     tcp-ports="16384"
				     udp-ports="16384"
				     icmp-ids="16384"/>

				<tcp-forward port="8888" domain="downlink" to="10.0.3.2"/>

			</domain>

			<domain name="downlink" interface="10.0.3.1/24">

				<dhcp-server ip_first="10.0.3.2" ip_last="10.0.3.2">
					<dns-server ip="8.8.8.8"/>
					<dns-server ip="1.1.1.1"/>
				</dhcp-server>

				<tcp dst="0.0.0.0/0"><permit-any domain="uplink" /></tcp>
				<udp dst="0.0.0.0/0"><permit-any domain="uplink" /></udp>
				<icmp dst="0.0.0.0/0" domain="uplink"/>

			</domain>

		</config>
	</start>
	<start name="tcp_terminal" caps="200">
		<resource name="RAM" quantum="8M"/>
		<provides> <service name="Terminal"/> </provides>
		<config>
			<policy label_prefix="test-terminal_echo" port="8888"/>
			<vfs>
				<dir name="dev"> <log/> </dir>
				<dir name="socket"> <lwip dhcp="yes"/> </dir>
				<dir name="pipe"> <pipe/> </dir>
			</vfs>
			<libc stdout="/dev/log" socket="/socket" pipe="/pipe"/>
		</config>
		<route>
			<service name="Nic"> <child name="nic_router"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>
	<start name="test-terminal_echo">
		<resource name="RAM" quantum="1M"/>
	</start>
</config>
}

build_boot_image { tcp_terminal test-terminal_echo }


# qemu config

append qemu_args " -nographic "
append_qemu_nic_args "hostfwd=tcp::5555-:8888"

run_genode_until forever

#
# Now, connect via 'telnet localhost 5555'
#

# vi: set ft=tcl :
