set use_net 0
set use_ps2 1
set use_usb 0
set use_serial 1
set use_top 1

set use_vbox5_nova 0

# use_gui starts two VMs
set use_gui 0

set build_components {
	drivers/framebuffer
	server/report_rom
}

append build_components virtualbox5

set virtualbox_binary "virtualbox5"

if {$use_vbox5_nova} {
	set virtualbox_binary "virtualbox5-nova"
}

create_boot_directory

import_from_depot [depot_user]/src/[base_src] \
                  [depot_user]/src/init \
                  [depot_user]/src/nitpicker \
                  [depot_user]/src/vfs_pipe \
                  [depot_user]/src/jpeg

source ${genode_dir}/repos/base/run/platform_drv.inc
# override defaults of platform_drv.inc
proc platform_drv_priority {} { return { priority="-1"} }

lappend_if [expr $use_top]    build_components app/top
lappend_if [expr $use_ps2]    build_components drivers/ps2
lappend_if [expr $use_usb]    build_components drivers/usb
lappend_if [expr $use_serial] build_components server/log_terminal
lappend_if [have_spec x86]    build_components drivers/rtc

lappend_if [expr $use_net]    build_components drivers/nic
lappend_if [expr $use_net]    build_components server/nic_router

append_platform_drv_build_components

build $build_components

set config {
<config prio_levels="4">
	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
		<service name="VM"/>}

append_if [expr $use_top] config {
		<service name="TRACE"/>}

append config {
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<default caps="100"/>
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Timer"/></provides>
	</start>}

append_if [expr $use_top] config {
	<start name="top">
		<resource name="RAM" quantum="2M"/>
		<config period_ms="15000"/>
	</start>}

append_platform_drv_config

append_if [expr $use_ps2] config {
	<start name="ps2_drv" priority="-1">
		<resource name="RAM" quantum="2M"/>
		<config/>
	</start>}

append_if [expr $use_usb] config {
	<start name="usb_drv" priority="-1" caps="120">
		<resource name="RAM" quantum="12M"/>}

append_if [expr $use_usb] config {
		<config uhci="yes" ehci="yes" xhci="yes">
			<hid/>
		</config>
	</start>}

append_if [have_board pc] config {
	<start name="fb_drv" priority="-1" caps="150">
		<binary name="vesa_fb_drv"/>
		<resource name="RAM" quantum="12M"/>}
append_if [expr [have_board pc] && [have_include power_on/qemu]] config {
		<config width="1280" height="1024" buffered="yes"/>}
append_if [have_board pc] config {
	</start>}

append_if [have_board linux] config {
	<start name="fb_sdl" priority="-1" ld="no">
		<resource name="RAM" quantum="4M"/>
	</start>}

append_if [have_spec x86] config {
	<start name="rtc_drv" priority="-1">
		<resource name="RAM" quantum="1M"/>
		<provides>
			<service name="Rtc"/>
		</provides>
	</start>}

append_if [expr $use_net] config {
	<start name="nic_drv" priority="-1">
		<binary name="ipxe_nic_drv"/>
		<resource name="RAM" quantum="8M"/>
		<config mode="uplink_client"/>
		<route>
			<service name="Uplink"> <child name="nic_router"/> </service>
			<any-service> <parent/> <any-child /> </any-service>
		</route>
	</start>

	<start name="nic_router" caps="120">
		<resource name="RAM" quantum="5M"/>
		<provides>
			<service name="Nic"/>
			<service name="Uplink"/>
		</provides>
		<config verbose_domain_state="yes">

			<policy label_prefix="vbox"    domain="downlink"/>
			<policy label_prefix="nic_drv" domain="uplink"/>

			<domain name="uplink">

				<nat domain="downlink"
				     tcp-ports="16384"
				     udp-ports="16384"
				     icmp-ids="16384"/>

			</domain>

			<domain name="downlink" interface="10.0.3.1/24" verbose_packets="no">

				<dhcp-server ip_first="10.0.3.100" ip_last="10.0.3.200">
					<dns-server ip="8.8.8.8"/>
					<dns-server ip="1.1.1.1"/>
				</dhcp-server>

				<tcp dst="0.0.0.0/0"><permit-any domain="uplink" /></tcp>
				<udp dst="0.0.0.0/0"><permit-any domain="uplink" /></udp>
				<icmp dst="0.0.0.0/0" domain="uplink"/>

			</domain>

		</config>
	</start> }

append_if [expr $use_serial] config {
	<start name="log_terminal" priority="-1">
		<resource name="RAM" quantum="2M"/>
		<provides>
			<service name="Terminal"/>
		</provides>
	</start>
}

append config {
	<start name="report_rom" priority="-1">
		<resource name="RAM" quantum="2M"/>
		<provides> <service name="Report"/> <service name="ROM"/> </provides>
		<config>
			<policy label="pointer -> hover" report="nitpicker -> hover"/>
			<policy label="pointer -> xray"  report="nitpicker -> xray"/>
		</config>
	</start>

	<start name="nitpicker" priority="-1">
		<resource name="RAM" quantum="4M"/>
		<provides>
			<service name="Gui"/> <service name="Capture"/> <service name="Event"/>
		</provides>
		<route>
			<service name="Report"> <child name="report_rom" /> </service>}

append config {
			<any-service> <parent/> <any-child /> </any-service>
		</route>
		<config>
			<capture/> <event/>

			<report focus="yes" hover="yes" xray="yes" />

			<domain name="pointer"  layer="1" content="client" label="no" origin="pointer" />
			<domain name=""         layer="2" content="client" focus="click" hover="always" />

			<policy label_prefix="pointer" domain="pointer"/>
			<default-policy domain=""/>
		</config>
	</start>

	<start name="pointer" priority="-1">
		<resource name="RAM" quantum="2M"/>
		<provides><service name="Report"/></provides>
		<config shapes="yes"/>
		<route>
			<service name="Gui"> <child name="nitpicker"/>  </service>
			<service name="ROM" label="hover"> <child name="report_rom"/> </service>
			<service name="ROM" label="xray"> <child name="report_rom"/> </service>
			<any-service> <parent/> </any-service>
		</route>
	</start>}

append_if [expr $use_gui] config {
	<start name="vbox2" priority="-2" caps="1200">
		<binary name="} $virtualbox_binary {"/>
		<resource name="RAM" quantum="448M"/>
		<config vbox_file="test.vbox" vm_name="TestVM">
			<libc stdout="/dev/log" stderr="/dev/log" pipe="/pipe" rtc="/dev/rtc"/>
			<vfs>
				<dir name="dev">
					<log/> <rtc/>
				</dir>
				<dir name="pipe"> <pipe/> </dir>
				<rom name="test.vbox" />
				<rom name="test.iso" />
			</vfs>
		</config>
		<route>
			<service name="Nic"> <child name="nic_router"/> </service>
			<service name="Report" label="shape"> <child name="pointer" label="gui_fb2 -> shape"/> </service>
			<service name="Report"> <child name="report_rom"/> </service>
			<any-service> <parent /> <any-child /> </any-service>
		</route>
	</start>}

append config {
	<start name="vbox1" priority="-2" caps="1200">
		<binary name="} $virtualbox_binary {"/>
		<resource name="RAM" quantum="448M"/>
		<config vbox_file="test.vbox" vm_name="TestVM">
			<libc stdout="/dev/log" stderr="/dev/log" pipe="/pipe" rtc="/dev/rtc"/>
			<vfs>
				<dir name="dev">
					<log/> <rtc/>
				</dir>
				<dir name="pipe"> <pipe/> </dir>}

append_if [expr $use_serial] config {
				<dir name="dev"> <terminal/> </dir>}

append config {
				<rom name="test.vbox" />
				<rom name="test.iso" />
			</vfs>
		</config>
		<route>
			<service name="Nic"> <child name="nic_router"/> </service>
			<service name="Report" label="shape"> <child name="pointer" label="gui_fb1 -> shape"/> </service>
			<service name="Report"> <child name="report_rom"/> </service>
			<any-service> <parent /> <any-child /> </any-service>
		</route>
	</start>
</config>
}

install_config $config

exec cp ${genode_dir}/repos/ports/run/test.vbox bin/.

set boot_modules { test.iso test.vbox }

append boot_modules $virtualbox_binary

# platform-specific modules
lappend_if [expr         $use_usb] boot_modules usb_drv
lappend_if [expr         $use_ps2] boot_modules ps2_drv
lappend_if [have_board pc] boot_modules vesa_fb_drv
lappend_if [have_board linux] boot_modules fb_sdl
lappend_if [have_spec         x86] boot_modules rtc_drv
lappend_if [expr         $use_top] boot_modules top
lappend_if [expr         $use_gui] boot_modules report_rom

append boot_modules {
	libc.lib.so vfs.lib.so libm.lib.so
	libiconv.lib.so stdcxx.lib.so
	qemu-usb.lib.so
}

append_if [expr $use_net]          boot_modules { ipxe_nic_drv }
append_if [expr $use_net]          boot_modules { nic_router }
append_if [expr $use_serial]       boot_modules { log_terminal }

append_platform_drv_boot_modules

build_boot_image $boot_modules

if {[have_include "power_on/qemu"]} {
	if {[expr $use_gui]} {
		append qemu_args " -m 2048 "
	} else {
		append qemu_args " -m 1024 "
	}

	append qemu_args " -cpu phenom "
	if {[expr $use_usb]} {
		append qemu_args " -usbdevice mouse -usbdevice keyboard"
	}
}

run_genode_until forever
