#!/bin/bash
# Boot from a local disk installation

BOARD_NAME=${CONFIG_BOARD_NAME:-${CONFIG_BOARD}} 
MAIN_MENU_TITLE="${BOARD_NAME} | $CONFIG_BRAND_NAME Basic Boot Menu"
export BG_COLOR_MAIN_MENU=""

. /etc/functions
. /etc/gui_functions
. /tmp/config

# skip_to_menu is set if the user selects "continue to the main menu" from any
# error, so we will indeed go to the main menu even if other errors occur.  It's
# reset when we reach the main menu so the user can retry from the main menu and
# # see errors again.
skip_to_menu="false"

mount_boot()
{
  TRACE "Under /bin/gui-init:mount_boot"
  # Mount local disk if it is not already mounted
  while ! grep -q /boot /proc/mounts ; do
    # try to mount if CONFIG_BOOT_DEV exists
    if [ -e "$CONFIG_BOOT_DEV" ]; then
      mount -o ro $CONFIG_BOOT_DEV /boot 
      [[ $? -eq 0 ]] && continue
    fi

    # CONFIG_BOOT_DEV doesn't exist or couldn't be mounted, so give user options
    BG_COLOR_MAIN_MENU=$BG_COLOR_ERROR
    whiptail $BG_COLOR_ERROR --title "ERROR: No Bootable OS Found!" \
        --menu "    No bootable OS was found on the default boot device $CONFIG_BOOT_DEV.
    How would you like to proceed?" 0 80 4 \
        'b' ' Select a new boot device' \
        'u' ' Boot from USB' \
        'm' ' Continue to the main menu' \
        'x' ' Exit to recovery shell' \
        2>/tmp/whiptail || recovery "GUI menu failed"

    option=$(cat /tmp/whiptail)
    case "$option" in 
      b )
        config-gui.sh boot_device_select
        if [ $? -eq 0 ]; then
          # update CONFIG_BOOT_DEV
          . /tmp/config
          BG_COLOR_MAIN_MENU=""
        fi
        ;;
      u )
        exec /bin/usb-init
        ;;
      m )
        skip_to_menu="true"
        break
        ;;
      * )
        recovery "User requested recovery shell"
        ;;
    esac
  done
}

prompt_auto_default_boot()
{
  TRACE "Under /bin/gui-init:prompt_auto_default_boot"
  echo -e "\n\n"
  if pause_automatic_boot; then
    echo -e "\n\nAttempting default boot...\n\n"
    attempt_default_boot
  fi
}

show_main_menu()
{
  TRACE "Under /bin/gui-init:show_main_menu"
  date=`date "+%Y-%m-%d %H:%M:%S %Z"`
  whiptail $BG_COLOR_MAIN_MENU --title "$MAIN_MENU_TITLE" \
    --menu "$date" 0 80 10 \
    'd' ' Default boot' \
    'o' ' Options -->' \
    's' ' System Info' \
    'p' ' Power Off' \
    2>/tmp/whiptail || recovery "GUI menu failed"

  option=$(cat /tmp/whiptail)
  case "$option" in 
    d )
      attempt_default_boot
      ;;
    o )
      show_options_menu
      ;;
    s )
      show_system_info
      ;;
    p )
      poweroff
      ;;
  esac
}

show_options_menu()
{
  TRACE "Under /bin/gui-init:show_options_menu"
  whiptail $BG_COLOR_MAIN_MENU --title "$CONFIG_BRAND_NAME Basic Options" \
    --menu "" 0 80 10 \
    'b' ' Boot Options -->' \
    'c' ' Change configuration settings -->' \
    'f' ' Flash/Update the BIOS -->' \
    'x' ' Exit to recovery shell' \
    'r' ' <-- Return to main menu' \
    2>/tmp/whiptail || recovery "GUI menu failed"

  option=$(cat /tmp/whiptail)
  case "$option" in 
    b )
      show_boot_options_menu
      ;;
    c )
      config-gui.sh
      ;;
    f )
      flash-gui.sh
      ;;
    x )
      recovery "User requested recovery shell"
      ;;
    r )
      ;;
  esac
}

show_boot_options_menu()
{
  TRACE "Under /bin/gui-init:show_boot_options_menu"
  whiptail $BG_COLOR_MAIN_MENU --title "Boot Options" \
    --menu "Select A Boot Option" 0 80 10 \
    'm' ' Show OS boot menu' \
    'u' ' USB boot' \
    'r' ' <-- Return to main menu' \
    2>/tmp/whiptail || recovery "GUI menu failed"

  option=$(cat /tmp/whiptail)
  case "$option" in 
    m )
      # select a kernel from the menu
      select_os_boot_option
      ;;
    u )
      exec /bin/usb-init
      ;;
    r )
      ;;
  esac
}

select_os_boot_option()
{
  TRACE "Under /bin/gui-init:select_os_boot_option"
  mount_boot
  kexec-select-boot -m -b /boot -c "grub.cfg" -g -i
}

attempt_default_boot()
{
  TRACE "Under /bin/gui-init:attempt_default_boot"
  mount_boot

  DEFAULT_FILE=`find /boot/kexec_default.*.txt 2>/dev/null | head -1`
  # Basic by default boots automatically to the first menu option.  This allows
  # kernel updates to work in Basic by default without prompting to select a
  # new default boot option.
  if [ "$CONFIG_BASIC_NO_AUTOMATIC_DEFAULT" != "y" ]; then
    basic-autoboot.sh
  elif [ -r "$DEFAULT_FILE" ]; then
    kexec-select-boot -b /boot -c "grub.cfg" -g -i -s \
    || recovery "Failed default boot"
  elif (whiptail $BG_COLOR_WARNING --title 'No Default Boot Option Configured' \
        --yesno "There is no default boot option configured yet.\nWould you like to load a menu of boot options?\nOtherwise you will return to the main menu." 0 80) then
    kexec-select-boot -m -b /boot -c "grub.cfg" -g -i
  fi
}

# gui-init-basic start
TRACE "Under /bin/gui-init, start"

# USB automatic boot (if configured) occurs before mounting /boot, this should
# work even if no OS is installed
if [ "$CONFIG_BASIC_USB_AUTOBOOT" = "y" ] && usb-autoboot.sh; then
  # USB autoboot was offered and interrupted.  Don't offer the default boot,
  # go to the menu.
  skip_to_menu=true
fi

if ! detect_boot_device ; then
  # can't determine /boot device or no OS installed, 
  # so fall back to interactive selection
  mount_boot
fi

if [ "$skip_to_menu" != "true" -a -n "$CONFIG_AUTO_BOOT_TIMEOUT" ]; then
  prompt_auto_default_boot
fi

while true; do
  TRACE "Under gui-init:while true loop"
  skip_to_menu="false"
  show_main_menu
done

recovery "Something failed during boot"
