From 30367636930864f71b2bd462adedcf8484313864 Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Sun, 23 Oct 2022 16:47:06 +0200
Subject: [PATCH 02/29] usb: fotg210: Collect pieces of dual mode controller

The Faraday FOTG210 is a dual-mode OTG USB controller that can
act as host, peripheral or both. To be able to probe from one
hardware description and to follow the pattern of other dual-
mode controllers such as MUSB or MTU3 we need to collect the
two, currently completely separate drivers in the same
directory.

After this, users need to select the main symbol USB_FOTG210
and then each respective subdriver. We pave the road to
compile both drivers into the same kernel and select the
one we want to use at probe() time, and possibly add OTG
support in the end.

This patch doesn't do much more than create the new symbol
and collect the drivers in one place. We also add a comment
for the section of dual-mode controllers in the Kconfig
file so people can see what these selections are about.

Also add myself as maintainer as there has been little
response on my patches to these drivers.

Cc: Fabian Vogt <fabian@ritter-vogt.de>
Cc: Yuan-Hsin Chen <yhchen@faraday-tech.com>
Cc: Felipe Balbi <balbi@kernel.org>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
Link: https://lore.kernel.org/r/20221023144708.3596563-1-linus.walleij@linaro.org
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
--- a/drivers/usb/Kconfig
+++ b/drivers/usb/Kconfig
@@ -111,8 +111,12 @@ source "drivers/usb/usbip/Kconfig"
 
 endif
 
+comment "USB dual-mode controller drivers"
+
 source "drivers/usb/cdns3/Kconfig"
 
+source "drivers/usb/fotg210/Kconfig"
+
 source "drivers/usb/mtu3/Kconfig"
 
 source "drivers/usb/musb/Kconfig"
--- a/drivers/usb/Makefile
+++ b/drivers/usb/Makefile
@@ -17,6 +17,8 @@ obj-$(CONFIG_USB_CDNS_SUPPORT)	+= cdns3/
 obj-$(CONFIG_USB_CDNS3)		+= cdns3/
 obj-$(CONFIG_USB_CDNSP_PCI)	+= cdns3/
 
+obj-$(CONFIG_USB_FOTG210)	+= fotg210/
+
 obj-$(CONFIG_USB_MON)		+= mon/
 obj-$(CONFIG_USB_MTU3)		+= mtu3/
 
--- /dev/null
+++ b/drivers/usb/fotg210/Kconfig
@@ -0,0 +1,36 @@
+# SPDX-License-Identifier: GPL-2.0
+
+config USB_FOTG210
+	tristate "Faraday FOTG210 USB2 Dual Role controller"
+	depends on USB || USB_GADGET
+	depends on HAS_DMA && HAS_IOMEM
+	default ARCH_GEMINI
+	help
+	  Faraday FOTG210 is a dual-mode USB controller that can act
+	  in both host controller and peripheral controller mode.
+
+if USB_FOTG210
+
+config USB_FOTG210_HCD
+	tristate "Faraday FOTG210 USB Host Controller support"
+	depends on USB
+	help
+	  Faraday FOTG210 is an OTG controller which can be configured as
+	  an USB2.0 host. It is designed to meet USB2.0 EHCI specification
+	  with minor modification.
+
+	  To compile this driver as a module, choose M here: the
+	  module will be called fotg210-hcd.
+
+config USB_FOTG210_UDC
+	depends on USB_GADGET
+	tristate "Faraday FOTG210 USB Peripheral Controller support"
+	help
+	   Faraday USB2.0 OTG controller which can be configured as
+	   high speed or full speed USB device. This driver suppports
+	   Bulk Transfer so far.
+
+	   Say "y" to link the driver statically, or "m" to build a
+	   dynamically linked module called "fotg210-udc".
+
+endif
--- /dev/null
+++ b/drivers/usb/fotg210/Makefile
@@ -0,0 +1,3 @@
+# SPDX-License-Identifier: GPL-2.0
+obj-$(CONFIG_USB_FOTG210_HCD)	+= fotg210-hcd.o
+obj-$(CONFIG_USB_FOTG210_UDC)	+= fotg210-udc.o
--- a/drivers/usb/host/fotg210-hcd.c
+++ /dev/null
@@ -1,5724 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0+
-/* Faraday FOTG210 EHCI-like driver
- *
- * Copyright (c) 2013 Faraday Technology Corporation
- *
- * Author: Yuan-Hsin Chen <yhchen@faraday-tech.com>
- *	   Feng-Hsin Chiang <john453@faraday-tech.com>
- *	   Po-Yu Chuang <ratbert.chuang@gmail.com>
- *
- * Most of code borrowed from the Linux-3.7 EHCI driver
- */
-#include <linux/module.h>
-#include <linux/of.h>
-#include <linux/device.h>
-#include <linux/dmapool.h>
-#include <linux/kernel.h>
-#include <linux/delay.h>
-#include <linux/ioport.h>
-#include <linux/sched.h>
-#include <linux/vmalloc.h>
-#include <linux/errno.h>
-#include <linux/init.h>
-#include <linux/hrtimer.h>
-#include <linux/list.h>
-#include <linux/interrupt.h>
-#include <linux/usb.h>
-#include <linux/usb/hcd.h>
-#include <linux/moduleparam.h>
-#include <linux/dma-mapping.h>
-#include <linux/debugfs.h>
-#include <linux/slab.h>
-#include <linux/uaccess.h>
-#include <linux/platform_device.h>
-#include <linux/io.h>
-#include <linux/iopoll.h>
-#include <linux/clk.h>
-
-#include <asm/byteorder.h>
-#include <asm/irq.h>
-#include <asm/unaligned.h>
-
-#define DRIVER_AUTHOR "Yuan-Hsin Chen"
-#define DRIVER_DESC "FOTG210 Host Controller (EHCI) Driver"
-static const char hcd_name[] = "fotg210_hcd";
-
-#undef FOTG210_URB_TRACE
-#define FOTG210_STATS
-
-/* magic numbers that can affect system performance */
-#define FOTG210_TUNE_CERR	3 /* 0-3 qtd retries; 0 == don't stop */
-#define FOTG210_TUNE_RL_HS	4 /* nak throttle; see 4.9 */
-#define FOTG210_TUNE_RL_TT	0
-#define FOTG210_TUNE_MULT_HS	1 /* 1-3 transactions/uframe; 4.10.3 */
-#define FOTG210_TUNE_MULT_TT	1
-
-/* Some drivers think it's safe to schedule isochronous transfers more than 256
- * ms into the future (partly as a result of an old bug in the scheduling
- * code).  In an attempt to avoid trouble, we will use a minimum scheduling
- * length of 512 frames instead of 256.
- */
-#define FOTG210_TUNE_FLS 1 /* (medium) 512-frame schedule */
-
-/* Initial IRQ latency:  faster than hw default */
-static int log2_irq_thresh; /* 0 to 6 */
-module_param(log2_irq_thresh, int, S_IRUGO);
-MODULE_PARM_DESC(log2_irq_thresh, "log2 IRQ latency, 1-64 microframes");
-
-/* initial park setting:  slower than hw default */
-static unsigned park;
-module_param(park, uint, S_IRUGO);
-MODULE_PARM_DESC(park, "park setting; 1-3 back-to-back async packets");
-
-/* for link power management(LPM) feature */
-static unsigned int hird;
-module_param(hird, int, S_IRUGO);
-MODULE_PARM_DESC(hird, "host initiated resume duration, +1 for each 75us");
-
-#define INTR_MASK (STS_IAA | STS_FATAL | STS_PCD | STS_ERR | STS_INT)
-
-#include "fotg210.h"
-
-#define fotg210_dbg(fotg210, fmt, args...) \
-	dev_dbg(fotg210_to_hcd(fotg210)->self.controller, fmt, ## args)
-#define fotg210_err(fotg210, fmt, args...) \
-	dev_err(fotg210_to_hcd(fotg210)->self.controller, fmt, ## args)
-#define fotg210_info(fotg210, fmt, args...) \
-	dev_info(fotg210_to_hcd(fotg210)->self.controller, fmt, ## args)
-#define fotg210_warn(fotg210, fmt, args...) \
-	dev_warn(fotg210_to_hcd(fotg210)->self.controller, fmt, ## args)
-
-/* check the values in the HCSPARAMS register (host controller _Structural_
- * parameters) see EHCI spec, Table 2-4 for each value
- */
-static void dbg_hcs_params(struct fotg210_hcd *fotg210, char *label)
-{
-	u32 params = fotg210_readl(fotg210, &fotg210->caps->hcs_params);
-
-	fotg210_dbg(fotg210, "%s hcs_params 0x%x ports=%d\n", label, params,
-			HCS_N_PORTS(params));
-}
-
-/* check the values in the HCCPARAMS register (host controller _Capability_
- * parameters) see EHCI Spec, Table 2-5 for each value
- */
-static void dbg_hcc_params(struct fotg210_hcd *fotg210, char *label)
-{
-	u32 params = fotg210_readl(fotg210, &fotg210->caps->hcc_params);
-
-	fotg210_dbg(fotg210, "%s hcc_params %04x uframes %s%s\n", label,
-			params,
-			HCC_PGM_FRAMELISTLEN(params) ? "256/512/1024" : "1024",
-			HCC_CANPARK(params) ? " park" : "");
-}
-
-static void __maybe_unused
-dbg_qtd(const char *label, struct fotg210_hcd *fotg210, struct fotg210_qtd *qtd)
-{
-	fotg210_dbg(fotg210, "%s td %p n%08x %08x t%08x p0=%08x\n", label, qtd,
-			hc32_to_cpup(fotg210, &qtd->hw_next),
-			hc32_to_cpup(fotg210, &qtd->hw_alt_next),
-			hc32_to_cpup(fotg210, &qtd->hw_token),
-			hc32_to_cpup(fotg210, &qtd->hw_buf[0]));
-	if (qtd->hw_buf[1])
-		fotg210_dbg(fotg210, "  p1=%08x p2=%08x p3=%08x p4=%08x\n",
-				hc32_to_cpup(fotg210, &qtd->hw_buf[1]),
-				hc32_to_cpup(fotg210, &qtd->hw_buf[2]),
-				hc32_to_cpup(fotg210, &qtd->hw_buf[3]),
-				hc32_to_cpup(fotg210, &qtd->hw_buf[4]));
-}
-
-static void __maybe_unused
-dbg_qh(const char *label, struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
-{
-	struct fotg210_qh_hw *hw = qh->hw;
-
-	fotg210_dbg(fotg210, "%s qh %p n%08x info %x %x qtd %x\n", label, qh,
-			hw->hw_next, hw->hw_info1, hw->hw_info2,
-			hw->hw_current);
-
-	dbg_qtd("overlay", fotg210, (struct fotg210_qtd *) &hw->hw_qtd_next);
-}
-
-static void __maybe_unused
-dbg_itd(const char *label, struct fotg210_hcd *fotg210, struct fotg210_itd *itd)
-{
-	fotg210_dbg(fotg210, "%s[%d] itd %p, next %08x, urb %p\n", label,
-			itd->frame, itd, hc32_to_cpu(fotg210, itd->hw_next),
-			itd->urb);
-
-	fotg210_dbg(fotg210,
-			"  trans: %08x %08x %08x %08x %08x %08x %08x %08x\n",
-			hc32_to_cpu(fotg210, itd->hw_transaction[0]),
-			hc32_to_cpu(fotg210, itd->hw_transaction[1]),
-			hc32_to_cpu(fotg210, itd->hw_transaction[2]),
-			hc32_to_cpu(fotg210, itd->hw_transaction[3]),
-			hc32_to_cpu(fotg210, itd->hw_transaction[4]),
-			hc32_to_cpu(fotg210, itd->hw_transaction[5]),
-			hc32_to_cpu(fotg210, itd->hw_transaction[6]),
-			hc32_to_cpu(fotg210, itd->hw_transaction[7]));
-
-	fotg210_dbg(fotg210,
-			"  buf:   %08x %08x %08x %08x %08x %08x %08x\n",
-			hc32_to_cpu(fotg210, itd->hw_bufp[0]),
-			hc32_to_cpu(fotg210, itd->hw_bufp[1]),
-			hc32_to_cpu(fotg210, itd->hw_bufp[2]),
-			hc32_to_cpu(fotg210, itd->hw_bufp[3]),
-			hc32_to_cpu(fotg210, itd->hw_bufp[4]),
-			hc32_to_cpu(fotg210, itd->hw_bufp[5]),
-			hc32_to_cpu(fotg210, itd->hw_bufp[6]));
-
-	fotg210_dbg(fotg210, "  index: %d %d %d %d %d %d %d %d\n",
-			itd->index[0], itd->index[1], itd->index[2],
-			itd->index[3], itd->index[4], itd->index[5],
-			itd->index[6], itd->index[7]);
-}
-
-static int __maybe_unused
-dbg_status_buf(char *buf, unsigned len, const char *label, u32 status)
-{
-	return scnprintf(buf, len, "%s%sstatus %04x%s%s%s%s%s%s%s%s%s%s",
-			label, label[0] ? " " : "", status,
-			(status & STS_ASS) ? " Async" : "",
-			(status & STS_PSS) ? " Periodic" : "",
-			(status & STS_RECL) ? " Recl" : "",
-			(status & STS_HALT) ? " Halt" : "",
-			(status & STS_IAA) ? " IAA" : "",
-			(status & STS_FATAL) ? " FATAL" : "",
-			(status & STS_FLR) ? " FLR" : "",
-			(status & STS_PCD) ? " PCD" : "",
-			(status & STS_ERR) ? " ERR" : "",
-			(status & STS_INT) ? " INT" : "");
-}
-
-static int __maybe_unused
-dbg_intr_buf(char *buf, unsigned len, const char *label, u32 enable)
-{
-	return scnprintf(buf, len, "%s%sintrenable %02x%s%s%s%s%s%s",
-			label, label[0] ? " " : "", enable,
-			(enable & STS_IAA) ? " IAA" : "",
-			(enable & STS_FATAL) ? " FATAL" : "",
-			(enable & STS_FLR) ? " FLR" : "",
-			(enable & STS_PCD) ? " PCD" : "",
-			(enable & STS_ERR) ? " ERR" : "",
-			(enable & STS_INT) ? " INT" : "");
-}
-
-static const char *const fls_strings[] = { "1024", "512", "256", "??" };
-
-static int dbg_command_buf(char *buf, unsigned len, const char *label,
-		u32 command)
-{
-	return scnprintf(buf, len,
-			"%s%scommand %07x %s=%d ithresh=%d%s%s%s period=%s%s %s",
-			label, label[0] ? " " : "", command,
-			(command & CMD_PARK) ? " park" : "(park)",
-			CMD_PARK_CNT(command),
-			(command >> 16) & 0x3f,
-			(command & CMD_IAAD) ? " IAAD" : "",
-			(command & CMD_ASE) ? " Async" : "",
-			(command & CMD_PSE) ? " Periodic" : "",
-			fls_strings[(command >> 2) & 0x3],
-			(command & CMD_RESET) ? " Reset" : "",
-			(command & CMD_RUN) ? "RUN" : "HALT");
-}
-
-static char *dbg_port_buf(char *buf, unsigned len, const char *label, int port,
-		u32 status)
-{
-	char *sig;
-
-	/* signaling state */
-	switch (status & (3 << 10)) {
-	case 0 << 10:
-		sig = "se0";
-		break;
-	case 1 << 10:
-		sig = "k";
-		break; /* low speed */
-	case 2 << 10:
-		sig = "j";
-		break;
-	default:
-		sig = "?";
-		break;
-	}
-
-	scnprintf(buf, len, "%s%sport:%d status %06x %d sig=%s%s%s%s%s%s%s%s",
-			label, label[0] ? " " : "", port, status,
-			status >> 25, /*device address */
-			sig,
-			(status & PORT_RESET) ? " RESET" : "",
-			(status & PORT_SUSPEND) ? " SUSPEND" : "",
-			(status & PORT_RESUME) ? " RESUME" : "",
-			(status & PORT_PEC) ? " PEC" : "",
-			(status & PORT_PE) ? " PE" : "",
-			(status & PORT_CSC) ? " CSC" : "",
-			(status & PORT_CONNECT) ? " CONNECT" : "");
-
-	return buf;
-}
-
-/* functions have the "wrong" filename when they're output... */
-#define dbg_status(fotg210, label, status) {			\
-	char _buf[80];						\
-	dbg_status_buf(_buf, sizeof(_buf), label, status);	\
-	fotg210_dbg(fotg210, "%s\n", _buf);			\
-}
-
-#define dbg_cmd(fotg210, label, command) {			\
-	char _buf[80];						\
-	dbg_command_buf(_buf, sizeof(_buf), label, command);	\
-	fotg210_dbg(fotg210, "%s\n", _buf);			\
-}
-
-#define dbg_port(fotg210, label, port, status) {			       \
-	char _buf[80];							       \
-	fotg210_dbg(fotg210, "%s\n",					       \
-			dbg_port_buf(_buf, sizeof(_buf), label, port, status));\
-}
-
-/* troubleshooting help: expose state in debugfs */
-static int debug_async_open(struct inode *, struct file *);
-static int debug_periodic_open(struct inode *, struct file *);
-static int debug_registers_open(struct inode *, struct file *);
-static int debug_async_open(struct inode *, struct file *);
-
-static ssize_t debug_output(struct file*, char __user*, size_t, loff_t*);
-static int debug_close(struct inode *, struct file *);
-
-static const struct file_operations debug_async_fops = {
-	.owner		= THIS_MODULE,
-	.open		= debug_async_open,
-	.read		= debug_output,
-	.release	= debug_close,
-	.llseek		= default_llseek,
-};
-static const struct file_operations debug_periodic_fops = {
-	.owner		= THIS_MODULE,
-	.open		= debug_periodic_open,
-	.read		= debug_output,
-	.release	= debug_close,
-	.llseek		= default_llseek,
-};
-static const struct file_operations debug_registers_fops = {
-	.owner		= THIS_MODULE,
-	.open		= debug_registers_open,
-	.read		= debug_output,
-	.release	= debug_close,
-	.llseek		= default_llseek,
-};
-
-static struct dentry *fotg210_debug_root;
-
-struct debug_buffer {
-	ssize_t (*fill_func)(struct debug_buffer *);	/* fill method */
-	struct usb_bus *bus;
-	struct mutex mutex;	/* protect filling of buffer */
-	size_t count;		/* number of characters filled into buffer */
-	char *output_buf;
-	size_t alloc_size;
-};
-
-static inline char speed_char(u32 scratch)
-{
-	switch (scratch & (3 << 12)) {
-	case QH_FULL_SPEED:
-		return 'f';
-
-	case QH_LOW_SPEED:
-		return 'l';
-
-	case QH_HIGH_SPEED:
-		return 'h';
-
-	default:
-		return '?';
-	}
-}
-
-static inline char token_mark(struct fotg210_hcd *fotg210, __hc32 token)
-{
-	__u32 v = hc32_to_cpu(fotg210, token);
-
-	if (v & QTD_STS_ACTIVE)
-		return '*';
-	if (v & QTD_STS_HALT)
-		return '-';
-	if (!IS_SHORT_READ(v))
-		return ' ';
-	/* tries to advance through hw_alt_next */
-	return '/';
-}
-
-static void qh_lines(struct fotg210_hcd *fotg210, struct fotg210_qh *qh,
-		char **nextp, unsigned *sizep)
-{
-	u32 scratch;
-	u32 hw_curr;
-	struct fotg210_qtd *td;
-	unsigned temp;
-	unsigned size = *sizep;
-	char *next = *nextp;
-	char mark;
-	__le32 list_end = FOTG210_LIST_END(fotg210);
-	struct fotg210_qh_hw *hw = qh->hw;
-
-	if (hw->hw_qtd_next == list_end) /* NEC does this */
-		mark = '@';
-	else
-		mark = token_mark(fotg210, hw->hw_token);
-	if (mark == '/') { /* qh_alt_next controls qh advance? */
-		if ((hw->hw_alt_next & QTD_MASK(fotg210)) ==
-		    fotg210->async->hw->hw_alt_next)
-			mark = '#'; /* blocked */
-		else if (hw->hw_alt_next == list_end)
-			mark = '.'; /* use hw_qtd_next */
-		/* else alt_next points to some other qtd */
-	}
-	scratch = hc32_to_cpup(fotg210, &hw->hw_info1);
-	hw_curr = (mark == '*') ? hc32_to_cpup(fotg210, &hw->hw_current) : 0;
-	temp = scnprintf(next, size,
-			"qh/%p dev%d %cs ep%d %08x %08x(%08x%c %s nak%d)",
-			qh, scratch & 0x007f,
-			speed_char(scratch),
-			(scratch >> 8) & 0x000f,
-			scratch, hc32_to_cpup(fotg210, &hw->hw_info2),
-			hc32_to_cpup(fotg210, &hw->hw_token), mark,
-			(cpu_to_hc32(fotg210, QTD_TOGGLE) & hw->hw_token)
-				? "data1" : "data0",
-			(hc32_to_cpup(fotg210, &hw->hw_alt_next) >> 1) & 0x0f);
-	size -= temp;
-	next += temp;
-
-	/* hc may be modifying the list as we read it ... */
-	list_for_each_entry(td, &qh->qtd_list, qtd_list) {
-		scratch = hc32_to_cpup(fotg210, &td->hw_token);
-		mark = ' ';
-		if (hw_curr == td->qtd_dma)
-			mark = '*';
-		else if (hw->hw_qtd_next == cpu_to_hc32(fotg210, td->qtd_dma))
-			mark = '+';
-		else if (QTD_LENGTH(scratch)) {
-			if (td->hw_alt_next == fotg210->async->hw->hw_alt_next)
-				mark = '#';
-			else if (td->hw_alt_next != list_end)
-				mark = '/';
-		}
-		temp = snprintf(next, size,
-				"\n\t%p%c%s len=%d %08x urb %p",
-				td, mark, ({ char *tmp;
-				switch ((scratch>>8)&0x03) {
-				case 0:
-					tmp = "out";
-					break;
-				case 1:
-					tmp = "in";
-					break;
-				case 2:
-					tmp = "setup";
-					break;
-				default:
-					tmp = "?";
-					break;
-				 } tmp; }),
-				(scratch >> 16) & 0x7fff,
-				scratch,
-				td->urb);
-		if (size < temp)
-			temp = size;
-		size -= temp;
-		next += temp;
-	}
-
-	temp = snprintf(next, size, "\n");
-	if (size < temp)
-		temp = size;
-
-	size -= temp;
-	next += temp;
-
-	*sizep = size;
-	*nextp = next;
-}
-
-static ssize_t fill_async_buffer(struct debug_buffer *buf)
-{
-	struct usb_hcd *hcd;
-	struct fotg210_hcd *fotg210;
-	unsigned long flags;
-	unsigned temp, size;
-	char *next;
-	struct fotg210_qh *qh;
-
-	hcd = bus_to_hcd(buf->bus);
-	fotg210 = hcd_to_fotg210(hcd);
-	next = buf->output_buf;
-	size = buf->alloc_size;
-
-	*next = 0;
-
-	/* dumps a snapshot of the async schedule.
-	 * usually empty except for long-term bulk reads, or head.
-	 * one QH per line, and TDs we know about
-	 */
-	spin_lock_irqsave(&fotg210->lock, flags);
-	for (qh = fotg210->async->qh_next.qh; size > 0 && qh;
-			qh = qh->qh_next.qh)
-		qh_lines(fotg210, qh, &next, &size);
-	if (fotg210->async_unlink && size > 0) {
-		temp = scnprintf(next, size, "\nunlink =\n");
-		size -= temp;
-		next += temp;
-
-		for (qh = fotg210->async_unlink; size > 0 && qh;
-				qh = qh->unlink_next)
-			qh_lines(fotg210, qh, &next, &size);
-	}
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-
-	return strlen(buf->output_buf);
-}
-
-/* count tds, get ep direction */
-static unsigned output_buf_tds_dir(char *buf, struct fotg210_hcd *fotg210,
-		struct fotg210_qh_hw *hw, struct fotg210_qh *qh, unsigned size)
-{
-	u32 scratch = hc32_to_cpup(fotg210, &hw->hw_info1);
-	struct fotg210_qtd *qtd;
-	char *type = "";
-	unsigned temp = 0;
-
-	/* count tds, get ep direction */
-	list_for_each_entry(qtd, &qh->qtd_list, qtd_list) {
-		temp++;
-		switch ((hc32_to_cpu(fotg210, qtd->hw_token) >> 8) & 0x03) {
-		case 0:
-			type = "out";
-			continue;
-		case 1:
-			type = "in";
-			continue;
-		}
-	}
-
-	return scnprintf(buf, size, "(%c%d ep%d%s [%d/%d] q%d p%d)",
-			speed_char(scratch), scratch & 0x007f,
-			(scratch >> 8) & 0x000f, type, qh->usecs,
-			qh->c_usecs, temp, (scratch >> 16) & 0x7ff);
-}
-
-#define DBG_SCHED_LIMIT 64
-static ssize_t fill_periodic_buffer(struct debug_buffer *buf)
-{
-	struct usb_hcd *hcd;
-	struct fotg210_hcd *fotg210;
-	unsigned long flags;
-	union fotg210_shadow p, *seen;
-	unsigned temp, size, seen_count;
-	char *next;
-	unsigned i;
-	__hc32 tag;
-
-	seen = kmalloc_array(DBG_SCHED_LIMIT, sizeof(*seen), GFP_ATOMIC);
-	if (!seen)
-		return 0;
-
-	seen_count = 0;
-
-	hcd = bus_to_hcd(buf->bus);
-	fotg210 = hcd_to_fotg210(hcd);
-	next = buf->output_buf;
-	size = buf->alloc_size;
-
-	temp = scnprintf(next, size, "size = %d\n", fotg210->periodic_size);
-	size -= temp;
-	next += temp;
-
-	/* dump a snapshot of the periodic schedule.
-	 * iso changes, interrupt usually doesn't.
-	 */
-	spin_lock_irqsave(&fotg210->lock, flags);
-	for (i = 0; i < fotg210->periodic_size; i++) {
-		p = fotg210->pshadow[i];
-		if (likely(!p.ptr))
-			continue;
-
-		tag = Q_NEXT_TYPE(fotg210, fotg210->periodic[i]);
-
-		temp = scnprintf(next, size, "%4d: ", i);
-		size -= temp;
-		next += temp;
-
-		do {
-			struct fotg210_qh_hw *hw;
-
-			switch (hc32_to_cpu(fotg210, tag)) {
-			case Q_TYPE_QH:
-				hw = p.qh->hw;
-				temp = scnprintf(next, size, " qh%d-%04x/%p",
-						p.qh->period,
-						hc32_to_cpup(fotg210,
-							&hw->hw_info2)
-							/* uframe masks */
-							& (QH_CMASK | QH_SMASK),
-						p.qh);
-				size -= temp;
-				next += temp;
-				/* don't repeat what follows this qh */
-				for (temp = 0; temp < seen_count; temp++) {
-					if (seen[temp].ptr != p.ptr)
-						continue;
-					if (p.qh->qh_next.ptr) {
-						temp = scnprintf(next, size,
-								" ...");
-						size -= temp;
-						next += temp;
-					}
-					break;
-				}
-				/* show more info the first time around */
-				if (temp == seen_count) {
-					temp = output_buf_tds_dir(next,
-							fotg210, hw,
-							p.qh, size);
-
-					if (seen_count < DBG_SCHED_LIMIT)
-						seen[seen_count++].qh = p.qh;
-				} else
-					temp = 0;
-				tag = Q_NEXT_TYPE(fotg210, hw->hw_next);
-				p = p.qh->qh_next;
-				break;
-			case Q_TYPE_FSTN:
-				temp = scnprintf(next, size,
-						" fstn-%8x/%p",
-						p.fstn->hw_prev, p.fstn);
-				tag = Q_NEXT_TYPE(fotg210, p.fstn->hw_next);
-				p = p.fstn->fstn_next;
-				break;
-			case Q_TYPE_ITD:
-				temp = scnprintf(next, size,
-						" itd/%p", p.itd);
-				tag = Q_NEXT_TYPE(fotg210, p.itd->hw_next);
-				p = p.itd->itd_next;
-				break;
-			}
-			size -= temp;
-			next += temp;
-		} while (p.ptr);
-
-		temp = scnprintf(next, size, "\n");
-		size -= temp;
-		next += temp;
-	}
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-	kfree(seen);
-
-	return buf->alloc_size - size;
-}
-#undef DBG_SCHED_LIMIT
-
-static const char *rh_state_string(struct fotg210_hcd *fotg210)
-{
-	switch (fotg210->rh_state) {
-	case FOTG210_RH_HALTED:
-		return "halted";
-	case FOTG210_RH_SUSPENDED:
-		return "suspended";
-	case FOTG210_RH_RUNNING:
-		return "running";
-	case FOTG210_RH_STOPPING:
-		return "stopping";
-	}
-	return "?";
-}
-
-static ssize_t fill_registers_buffer(struct debug_buffer *buf)
-{
-	struct usb_hcd *hcd;
-	struct fotg210_hcd *fotg210;
-	unsigned long flags;
-	unsigned temp, size, i;
-	char *next, scratch[80];
-	static const char fmt[] = "%*s\n";
-	static const char label[] = "";
-
-	hcd = bus_to_hcd(buf->bus);
-	fotg210 = hcd_to_fotg210(hcd);
-	next = buf->output_buf;
-	size = buf->alloc_size;
-
-	spin_lock_irqsave(&fotg210->lock, flags);
-
-	if (!HCD_HW_ACCESSIBLE(hcd)) {
-		size = scnprintf(next, size,
-				"bus %s, device %s\n"
-				"%s\n"
-				"SUSPENDED(no register access)\n",
-				hcd->self.controller->bus->name,
-				dev_name(hcd->self.controller),
-				hcd->product_desc);
-		goto done;
-	}
-
-	/* Capability Registers */
-	i = HC_VERSION(fotg210, fotg210_readl(fotg210,
-			&fotg210->caps->hc_capbase));
-	temp = scnprintf(next, size,
-			"bus %s, device %s\n"
-			"%s\n"
-			"EHCI %x.%02x, rh state %s\n",
-			hcd->self.controller->bus->name,
-			dev_name(hcd->self.controller),
-			hcd->product_desc,
-			i >> 8, i & 0x0ff, rh_state_string(fotg210));
-	size -= temp;
-	next += temp;
-
-	/* FIXME interpret both types of params */
-	i = fotg210_readl(fotg210, &fotg210->caps->hcs_params);
-	temp = scnprintf(next, size, "structural params 0x%08x\n", i);
-	size -= temp;
-	next += temp;
-
-	i = fotg210_readl(fotg210, &fotg210->caps->hcc_params);
-	temp = scnprintf(next, size, "capability params 0x%08x\n", i);
-	size -= temp;
-	next += temp;
-
-	/* Operational Registers */
-	temp = dbg_status_buf(scratch, sizeof(scratch), label,
-			fotg210_readl(fotg210, &fotg210->regs->status));
-	temp = scnprintf(next, size, fmt, temp, scratch);
-	size -= temp;
-	next += temp;
-
-	temp = dbg_command_buf(scratch, sizeof(scratch), label,
-			fotg210_readl(fotg210, &fotg210->regs->command));
-	temp = scnprintf(next, size, fmt, temp, scratch);
-	size -= temp;
-	next += temp;
-
-	temp = dbg_intr_buf(scratch, sizeof(scratch), label,
-			fotg210_readl(fotg210, &fotg210->regs->intr_enable));
-	temp = scnprintf(next, size, fmt, temp, scratch);
-	size -= temp;
-	next += temp;
-
-	temp = scnprintf(next, size, "uframe %04x\n",
-			fotg210_read_frame_index(fotg210));
-	size -= temp;
-	next += temp;
-
-	if (fotg210->async_unlink) {
-		temp = scnprintf(next, size, "async unlink qh %p\n",
-				fotg210->async_unlink);
-		size -= temp;
-		next += temp;
-	}
-
-#ifdef FOTG210_STATS
-	temp = scnprintf(next, size,
-			"irq normal %ld err %ld iaa %ld(lost %ld)\n",
-			fotg210->stats.normal, fotg210->stats.error,
-			fotg210->stats.iaa, fotg210->stats.lost_iaa);
-	size -= temp;
-	next += temp;
-
-	temp = scnprintf(next, size, "complete %ld unlink %ld\n",
-			fotg210->stats.complete, fotg210->stats.unlink);
-	size -= temp;
-	next += temp;
-#endif
-
-done:
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-
-	return buf->alloc_size - size;
-}
-
-static struct debug_buffer
-*alloc_buffer(struct usb_bus *bus, ssize_t (*fill_func)(struct debug_buffer *))
-{
-	struct debug_buffer *buf;
-
-	buf = kzalloc(sizeof(struct debug_buffer), GFP_KERNEL);
-
-	if (buf) {
-		buf->bus = bus;
-		buf->fill_func = fill_func;
-		mutex_init(&buf->mutex);
-		buf->alloc_size = PAGE_SIZE;
-	}
-
-	return buf;
-}
-
-static int fill_buffer(struct debug_buffer *buf)
-{
-	int ret = 0;
-
-	if (!buf->output_buf)
-		buf->output_buf = vmalloc(buf->alloc_size);
-
-	if (!buf->output_buf) {
-		ret = -ENOMEM;
-		goto out;
-	}
-
-	ret = buf->fill_func(buf);
-
-	if (ret >= 0) {
-		buf->count = ret;
-		ret = 0;
-	}
-
-out:
-	return ret;
-}
-
-static ssize_t debug_output(struct file *file, char __user *user_buf,
-		size_t len, loff_t *offset)
-{
-	struct debug_buffer *buf = file->private_data;
-	int ret = 0;
-
-	mutex_lock(&buf->mutex);
-	if (buf->count == 0) {
-		ret = fill_buffer(buf);
-		if (ret != 0) {
-			mutex_unlock(&buf->mutex);
-			goto out;
-		}
-	}
-	mutex_unlock(&buf->mutex);
-
-	ret = simple_read_from_buffer(user_buf, len, offset,
-			buf->output_buf, buf->count);
-
-out:
-	return ret;
-
-}
-
-static int debug_close(struct inode *inode, struct file *file)
-{
-	struct debug_buffer *buf = file->private_data;
-
-	if (buf) {
-		vfree(buf->output_buf);
-		kfree(buf);
-	}
-
-	return 0;
-}
-static int debug_async_open(struct inode *inode, struct file *file)
-{
-	file->private_data = alloc_buffer(inode->i_private, fill_async_buffer);
-
-	return file->private_data ? 0 : -ENOMEM;
-}
-
-static int debug_periodic_open(struct inode *inode, struct file *file)
-{
-	struct debug_buffer *buf;
-
-	buf = alloc_buffer(inode->i_private, fill_periodic_buffer);
-	if (!buf)
-		return -ENOMEM;
-
-	buf->alloc_size = (sizeof(void *) == 4 ? 6 : 8)*PAGE_SIZE;
-	file->private_data = buf;
-	return 0;
-}
-
-static int debug_registers_open(struct inode *inode, struct file *file)
-{
-	file->private_data = alloc_buffer(inode->i_private,
-			fill_registers_buffer);
-
-	return file->private_data ? 0 : -ENOMEM;
-}
-
-static inline void create_debug_files(struct fotg210_hcd *fotg210)
-{
-	struct usb_bus *bus = &fotg210_to_hcd(fotg210)->self;
-	struct dentry *root;
-
-	root = debugfs_create_dir(bus->bus_name, fotg210_debug_root);
-
-	debugfs_create_file("async", S_IRUGO, root, bus, &debug_async_fops);
-	debugfs_create_file("periodic", S_IRUGO, root, bus,
-			    &debug_periodic_fops);
-	debugfs_create_file("registers", S_IRUGO, root, bus,
-			    &debug_registers_fops);
-}
-
-static inline void remove_debug_files(struct fotg210_hcd *fotg210)
-{
-	struct usb_bus *bus = &fotg210_to_hcd(fotg210)->self;
-
-	debugfs_lookup_and_remove(bus->bus_name, fotg210_debug_root);
-}
-
-/* handshake - spin reading hc until handshake completes or fails
- * @ptr: address of hc register to be read
- * @mask: bits to look at in result of read
- * @done: value of those bits when handshake succeeds
- * @usec: timeout in microseconds
- *
- * Returns negative errno, or zero on success
- *
- * Success happens when the "mask" bits have the specified value (hardware
- * handshake done).  There are two failure modes:  "usec" have passed (major
- * hardware flakeout), or the register reads as all-ones (hardware removed).
- *
- * That last failure should_only happen in cases like physical cardbus eject
- * before driver shutdown. But it also seems to be caused by bugs in cardbus
- * bridge shutdown:  shutting down the bridge before the devices using it.
- */
-static int handshake(struct fotg210_hcd *fotg210, void __iomem *ptr,
-		u32 mask, u32 done, int usec)
-{
-	u32 result;
-	int ret;
-
-	ret = readl_poll_timeout_atomic(ptr, result,
-					((result & mask) == done ||
-					 result == U32_MAX), 1, usec);
-	if (result == U32_MAX)		/* card removed */
-		return -ENODEV;
-
-	return ret;
-}
-
-/* Force HC to halt state from unknown (EHCI spec section 2.3).
- * Must be called with interrupts enabled and the lock not held.
- */
-static int fotg210_halt(struct fotg210_hcd *fotg210)
-{
-	u32 temp;
-
-	spin_lock_irq(&fotg210->lock);
-
-	/* disable any irqs left enabled by previous code */
-	fotg210_writel(fotg210, 0, &fotg210->regs->intr_enable);
-
-	/*
-	 * This routine gets called during probe before fotg210->command
-	 * has been initialized, so we can't rely on its value.
-	 */
-	fotg210->command &= ~CMD_RUN;
-	temp = fotg210_readl(fotg210, &fotg210->regs->command);
-	temp &= ~(CMD_RUN | CMD_IAAD);
-	fotg210_writel(fotg210, temp, &fotg210->regs->command);
-
-	spin_unlock_irq(&fotg210->lock);
-	synchronize_irq(fotg210_to_hcd(fotg210)->irq);
-
-	return handshake(fotg210, &fotg210->regs->status,
-			STS_HALT, STS_HALT, 16 * 125);
-}
-
-/* Reset a non-running (STS_HALT == 1) controller.
- * Must be called with interrupts enabled and the lock not held.
- */
-static int fotg210_reset(struct fotg210_hcd *fotg210)
-{
-	int retval;
-	u32 command = fotg210_readl(fotg210, &fotg210->regs->command);
-
-	/* If the EHCI debug controller is active, special care must be
-	 * taken before and after a host controller reset
-	 */
-	if (fotg210->debug && !dbgp_reset_prep(fotg210_to_hcd(fotg210)))
-		fotg210->debug = NULL;
-
-	command |= CMD_RESET;
-	dbg_cmd(fotg210, "reset", command);
-	fotg210_writel(fotg210, command, &fotg210->regs->command);
-	fotg210->rh_state = FOTG210_RH_HALTED;
-	fotg210->next_statechange = jiffies;
-	retval = handshake(fotg210, &fotg210->regs->command,
-			CMD_RESET, 0, 250 * 1000);
-
-	if (retval)
-		return retval;
-
-	if (fotg210->debug)
-		dbgp_external_startup(fotg210_to_hcd(fotg210));
-
-	fotg210->port_c_suspend = fotg210->suspended_ports =
-			fotg210->resuming_ports = 0;
-	return retval;
-}
-
-/* Idle the controller (turn off the schedules).
- * Must be called with interrupts enabled and the lock not held.
- */
-static void fotg210_quiesce(struct fotg210_hcd *fotg210)
-{
-	u32 temp;
-
-	if (fotg210->rh_state != FOTG210_RH_RUNNING)
-		return;
-
-	/* wait for any schedule enables/disables to take effect */
-	temp = (fotg210->command << 10) & (STS_ASS | STS_PSS);
-	handshake(fotg210, &fotg210->regs->status, STS_ASS | STS_PSS, temp,
-			16 * 125);
-
-	/* then disable anything that's still active */
-	spin_lock_irq(&fotg210->lock);
-	fotg210->command &= ~(CMD_ASE | CMD_PSE);
-	fotg210_writel(fotg210, fotg210->command, &fotg210->regs->command);
-	spin_unlock_irq(&fotg210->lock);
-
-	/* hardware can take 16 microframes to turn off ... */
-	handshake(fotg210, &fotg210->regs->status, STS_ASS | STS_PSS, 0,
-			16 * 125);
-}
-
-static void end_unlink_async(struct fotg210_hcd *fotg210);
-static void unlink_empty_async(struct fotg210_hcd *fotg210);
-static void fotg210_work(struct fotg210_hcd *fotg210);
-static void start_unlink_intr(struct fotg210_hcd *fotg210,
-			      struct fotg210_qh *qh);
-static void end_unlink_intr(struct fotg210_hcd *fotg210, struct fotg210_qh *qh);
-
-/* Set a bit in the USBCMD register */
-static void fotg210_set_command_bit(struct fotg210_hcd *fotg210, u32 bit)
-{
-	fotg210->command |= bit;
-	fotg210_writel(fotg210, fotg210->command, &fotg210->regs->command);
-
-	/* unblock posted write */
-	fotg210_readl(fotg210, &fotg210->regs->command);
-}
-
-/* Clear a bit in the USBCMD register */
-static void fotg210_clear_command_bit(struct fotg210_hcd *fotg210, u32 bit)
-{
-	fotg210->command &= ~bit;
-	fotg210_writel(fotg210, fotg210->command, &fotg210->regs->command);
-
-	/* unblock posted write */
-	fotg210_readl(fotg210, &fotg210->regs->command);
-}
-
-/* EHCI timer support...  Now using hrtimers.
- *
- * Lots of different events are triggered from fotg210->hrtimer.  Whenever
- * the timer routine runs, it checks each possible event; events that are
- * currently enabled and whose expiration time has passed get handled.
- * The set of enabled events is stored as a collection of bitflags in
- * fotg210->enabled_hrtimer_events, and they are numbered in order of
- * increasing delay values (ranging between 1 ms and 100 ms).
- *
- * Rather than implementing a sorted list or tree of all pending events,
- * we keep track only of the lowest-numbered pending event, in
- * fotg210->next_hrtimer_event.  Whenever fotg210->hrtimer gets restarted, its
- * expiration time is set to the timeout value for this event.
- *
- * As a result, events might not get handled right away; the actual delay
- * could be anywhere up to twice the requested delay.  This doesn't
- * matter, because none of the events are especially time-critical.  The
- * ones that matter most all have a delay of 1 ms, so they will be
- * handled after 2 ms at most, which is okay.  In addition to this, we
- * allow for an expiration range of 1 ms.
- */
-
-/* Delay lengths for the hrtimer event types.
- * Keep this list sorted by delay length, in the same order as
- * the event types indexed by enum fotg210_hrtimer_event in fotg210.h.
- */
-static unsigned event_delays_ns[] = {
-	1 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_POLL_ASS */
-	1 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_POLL_PSS */
-	1 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_POLL_DEAD */
-	1125 * NSEC_PER_USEC,	/* FOTG210_HRTIMER_UNLINK_INTR */
-	2 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_FREE_ITDS */
-	6 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_ASYNC_UNLINKS */
-	10 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_IAA_WATCHDOG */
-	10 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_DISABLE_PERIODIC */
-	15 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_DISABLE_ASYNC */
-	100 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_IO_WATCHDOG */
-};
-
-/* Enable a pending hrtimer event */
-static void fotg210_enable_event(struct fotg210_hcd *fotg210, unsigned event,
-		bool resched)
-{
-	ktime_t *timeout = &fotg210->hr_timeouts[event];
-
-	if (resched)
-		*timeout = ktime_add(ktime_get(), event_delays_ns[event]);
-	fotg210->enabled_hrtimer_events |= (1 << event);
-
-	/* Track only the lowest-numbered pending event */
-	if (event < fotg210->next_hrtimer_event) {
-		fotg210->next_hrtimer_event = event;
-		hrtimer_start_range_ns(&fotg210->hrtimer, *timeout,
-				NSEC_PER_MSEC, HRTIMER_MODE_ABS);
-	}
-}
-
-
-/* Poll the STS_ASS status bit; see when it agrees with CMD_ASE */
-static void fotg210_poll_ASS(struct fotg210_hcd *fotg210)
-{
-	unsigned actual, want;
-
-	/* Don't enable anything if the controller isn't running (e.g., died) */
-	if (fotg210->rh_state != FOTG210_RH_RUNNING)
-		return;
-
-	want = (fotg210->command & CMD_ASE) ? STS_ASS : 0;
-	actual = fotg210_readl(fotg210, &fotg210->regs->status) & STS_ASS;
-
-	if (want != actual) {
-
-		/* Poll again later, but give up after about 20 ms */
-		if (fotg210->ASS_poll_count++ < 20) {
-			fotg210_enable_event(fotg210, FOTG210_HRTIMER_POLL_ASS,
-					true);
-			return;
-		}
-		fotg210_dbg(fotg210, "Waited too long for the async schedule status (%x/%x), giving up\n",
-				want, actual);
-	}
-	fotg210->ASS_poll_count = 0;
-
-	/* The status is up-to-date; restart or stop the schedule as needed */
-	if (want == 0) {	/* Stopped */
-		if (fotg210->async_count > 0)
-			fotg210_set_command_bit(fotg210, CMD_ASE);
-
-	} else {		/* Running */
-		if (fotg210->async_count == 0) {
-
-			/* Turn off the schedule after a while */
-			fotg210_enable_event(fotg210,
-					FOTG210_HRTIMER_DISABLE_ASYNC,
-					true);
-		}
-	}
-}
-
-/* Turn off the async schedule after a brief delay */
-static void fotg210_disable_ASE(struct fotg210_hcd *fotg210)
-{
-	fotg210_clear_command_bit(fotg210, CMD_ASE);
-}
-
-
-/* Poll the STS_PSS status bit; see when it agrees with CMD_PSE */
-static void fotg210_poll_PSS(struct fotg210_hcd *fotg210)
-{
-	unsigned actual, want;
-
-	/* Don't do anything if the controller isn't running (e.g., died) */
-	if (fotg210->rh_state != FOTG210_RH_RUNNING)
-		return;
-
-	want = (fotg210->command & CMD_PSE) ? STS_PSS : 0;
-	actual = fotg210_readl(fotg210, &fotg210->regs->status) & STS_PSS;
-
-	if (want != actual) {
-
-		/* Poll again later, but give up after about 20 ms */
-		if (fotg210->PSS_poll_count++ < 20) {
-			fotg210_enable_event(fotg210, FOTG210_HRTIMER_POLL_PSS,
-					true);
-			return;
-		}
-		fotg210_dbg(fotg210, "Waited too long for the periodic schedule status (%x/%x), giving up\n",
-				want, actual);
-	}
-	fotg210->PSS_poll_count = 0;
-
-	/* The status is up-to-date; restart or stop the schedule as needed */
-	if (want == 0) {	/* Stopped */
-		if (fotg210->periodic_count > 0)
-			fotg210_set_command_bit(fotg210, CMD_PSE);
-
-	} else {		/* Running */
-		if (fotg210->periodic_count == 0) {
-
-			/* Turn off the schedule after a while */
-			fotg210_enable_event(fotg210,
-					FOTG210_HRTIMER_DISABLE_PERIODIC,
-					true);
-		}
-	}
-}
-
-/* Turn off the periodic schedule after a brief delay */
-static void fotg210_disable_PSE(struct fotg210_hcd *fotg210)
-{
-	fotg210_clear_command_bit(fotg210, CMD_PSE);
-}
-
-
-/* Poll the STS_HALT status bit; see when a dead controller stops */
-static void fotg210_handle_controller_death(struct fotg210_hcd *fotg210)
-{
-	if (!(fotg210_readl(fotg210, &fotg210->regs->status) & STS_HALT)) {
-
-		/* Give up after a few milliseconds */
-		if (fotg210->died_poll_count++ < 5) {
-			/* Try again later */
-			fotg210_enable_event(fotg210,
-					FOTG210_HRTIMER_POLL_DEAD, true);
-			return;
-		}
-		fotg210_warn(fotg210, "Waited too long for the controller to stop, giving up\n");
-	}
-
-	/* Clean up the mess */
-	fotg210->rh_state = FOTG210_RH_HALTED;
-	fotg210_writel(fotg210, 0, &fotg210->regs->intr_enable);
-	fotg210_work(fotg210);
-	end_unlink_async(fotg210);
-
-	/* Not in process context, so don't try to reset the controller */
-}
-
-
-/* Handle unlinked interrupt QHs once they are gone from the hardware */
-static void fotg210_handle_intr_unlinks(struct fotg210_hcd *fotg210)
-{
-	bool stopped = (fotg210->rh_state < FOTG210_RH_RUNNING);
-
-	/*
-	 * Process all the QHs on the intr_unlink list that were added
-	 * before the current unlink cycle began.  The list is in
-	 * temporal order, so stop when we reach the first entry in the
-	 * current cycle.  But if the root hub isn't running then
-	 * process all the QHs on the list.
-	 */
-	fotg210->intr_unlinking = true;
-	while (fotg210->intr_unlink) {
-		struct fotg210_qh *qh = fotg210->intr_unlink;
-
-		if (!stopped && qh->unlink_cycle == fotg210->intr_unlink_cycle)
-			break;
-		fotg210->intr_unlink = qh->unlink_next;
-		qh->unlink_next = NULL;
-		end_unlink_intr(fotg210, qh);
-	}
-
-	/* Handle remaining entries later */
-	if (fotg210->intr_unlink) {
-		fotg210_enable_event(fotg210, FOTG210_HRTIMER_UNLINK_INTR,
-				true);
-		++fotg210->intr_unlink_cycle;
-	}
-	fotg210->intr_unlinking = false;
-}
-
-
-/* Start another free-iTDs/siTDs cycle */
-static void start_free_itds(struct fotg210_hcd *fotg210)
-{
-	if (!(fotg210->enabled_hrtimer_events &
-			BIT(FOTG210_HRTIMER_FREE_ITDS))) {
-		fotg210->last_itd_to_free = list_entry(
-				fotg210->cached_itd_list.prev,
-				struct fotg210_itd, itd_list);
-		fotg210_enable_event(fotg210, FOTG210_HRTIMER_FREE_ITDS, true);
-	}
-}
-
-/* Wait for controller to stop using old iTDs and siTDs */
-static void end_free_itds(struct fotg210_hcd *fotg210)
-{
-	struct fotg210_itd *itd, *n;
-
-	if (fotg210->rh_state < FOTG210_RH_RUNNING)
-		fotg210->last_itd_to_free = NULL;
-
-	list_for_each_entry_safe(itd, n, &fotg210->cached_itd_list, itd_list) {
-		list_del(&itd->itd_list);
-		dma_pool_free(fotg210->itd_pool, itd, itd->itd_dma);
-		if (itd == fotg210->last_itd_to_free)
-			break;
-	}
-
-	if (!list_empty(&fotg210->cached_itd_list))
-		start_free_itds(fotg210);
-}
-
-
-/* Handle lost (or very late) IAA interrupts */
-static void fotg210_iaa_watchdog(struct fotg210_hcd *fotg210)
-{
-	if (fotg210->rh_state != FOTG210_RH_RUNNING)
-		return;
-
-	/*
-	 * Lost IAA irqs wedge things badly; seen first with a vt8235.
-	 * So we need this watchdog, but must protect it against both
-	 * (a) SMP races against real IAA firing and retriggering, and
-	 * (b) clean HC shutdown, when IAA watchdog was pending.
-	 */
-	if (fotg210->async_iaa) {
-		u32 cmd, status;
-
-		/* If we get here, IAA is *REALLY* late.  It's barely
-		 * conceivable that the system is so busy that CMD_IAAD
-		 * is still legitimately set, so let's be sure it's
-		 * clear before we read STS_IAA.  (The HC should clear
-		 * CMD_IAAD when it sets STS_IAA.)
-		 */
-		cmd = fotg210_readl(fotg210, &fotg210->regs->command);
-
-		/*
-		 * If IAA is set here it either legitimately triggered
-		 * after the watchdog timer expired (_way_ late, so we'll
-		 * still count it as lost) ... or a silicon erratum:
-		 * - VIA seems to set IAA without triggering the IRQ;
-		 * - IAAD potentially cleared without setting IAA.
-		 */
-		status = fotg210_readl(fotg210, &fotg210->regs->status);
-		if ((status & STS_IAA) || !(cmd & CMD_IAAD)) {
-			INCR(fotg210->stats.lost_iaa);
-			fotg210_writel(fotg210, STS_IAA,
-					&fotg210->regs->status);
-		}
-
-		fotg210_dbg(fotg210, "IAA watchdog: status %x cmd %x\n",
-				status, cmd);
-		end_unlink_async(fotg210);
-	}
-}
-
-
-/* Enable the I/O watchdog, if appropriate */
-static void turn_on_io_watchdog(struct fotg210_hcd *fotg210)
-{
-	/* Not needed if the controller isn't running or it's already enabled */
-	if (fotg210->rh_state != FOTG210_RH_RUNNING ||
-			(fotg210->enabled_hrtimer_events &
-			BIT(FOTG210_HRTIMER_IO_WATCHDOG)))
-		return;
-
-	/*
-	 * Isochronous transfers always need the watchdog.
-	 * For other sorts we use it only if the flag is set.
-	 */
-	if (fotg210->isoc_count > 0 || (fotg210->need_io_watchdog &&
-			fotg210->async_count + fotg210->intr_count > 0))
-		fotg210_enable_event(fotg210, FOTG210_HRTIMER_IO_WATCHDOG,
-				true);
-}
-
-
-/* Handler functions for the hrtimer event types.
- * Keep this array in the same order as the event types indexed by
- * enum fotg210_hrtimer_event in fotg210.h.
- */
-static void (*event_handlers[])(struct fotg210_hcd *) = {
-	fotg210_poll_ASS,			/* FOTG210_HRTIMER_POLL_ASS */
-	fotg210_poll_PSS,			/* FOTG210_HRTIMER_POLL_PSS */
-	fotg210_handle_controller_death,	/* FOTG210_HRTIMER_POLL_DEAD */
-	fotg210_handle_intr_unlinks,	/* FOTG210_HRTIMER_UNLINK_INTR */
-	end_free_itds,			/* FOTG210_HRTIMER_FREE_ITDS */
-	unlink_empty_async,		/* FOTG210_HRTIMER_ASYNC_UNLINKS */
-	fotg210_iaa_watchdog,		/* FOTG210_HRTIMER_IAA_WATCHDOG */
-	fotg210_disable_PSE,		/* FOTG210_HRTIMER_DISABLE_PERIODIC */
-	fotg210_disable_ASE,		/* FOTG210_HRTIMER_DISABLE_ASYNC */
-	fotg210_work,			/* FOTG210_HRTIMER_IO_WATCHDOG */
-};
-
-static enum hrtimer_restart fotg210_hrtimer_func(struct hrtimer *t)
-{
-	struct fotg210_hcd *fotg210 =
-			container_of(t, struct fotg210_hcd, hrtimer);
-	ktime_t now;
-	unsigned long events;
-	unsigned long flags;
-	unsigned e;
-
-	spin_lock_irqsave(&fotg210->lock, flags);
-
-	events = fotg210->enabled_hrtimer_events;
-	fotg210->enabled_hrtimer_events = 0;
-	fotg210->next_hrtimer_event = FOTG210_HRTIMER_NO_EVENT;
-
-	/*
-	 * Check each pending event.  If its time has expired, handle
-	 * the event; otherwise re-enable it.
-	 */
-	now = ktime_get();
-	for_each_set_bit(e, &events, FOTG210_HRTIMER_NUM_EVENTS) {
-		if (ktime_compare(now, fotg210->hr_timeouts[e]) >= 0)
-			event_handlers[e](fotg210);
-		else
-			fotg210_enable_event(fotg210, e, false);
-	}
-
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-	return HRTIMER_NORESTART;
-}
-
-#define fotg210_bus_suspend NULL
-#define fotg210_bus_resume NULL
-
-static int check_reset_complete(struct fotg210_hcd *fotg210, int index,
-		u32 __iomem *status_reg, int port_status)
-{
-	if (!(port_status & PORT_CONNECT))
-		return port_status;
-
-	/* if reset finished and it's still not enabled -- handoff */
-	if (!(port_status & PORT_PE))
-		/* with integrated TT, there's nobody to hand it to! */
-		fotg210_dbg(fotg210, "Failed to enable port %d on root hub TT\n",
-				index + 1);
-	else
-		fotg210_dbg(fotg210, "port %d reset complete, port enabled\n",
-				index + 1);
-
-	return port_status;
-}
-
-
-/* build "status change" packet (one or two bytes) from HC registers */
-
-static int fotg210_hub_status_data(struct usb_hcd *hcd, char *buf)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-	u32 temp, status;
-	u32 mask;
-	int retval = 1;
-	unsigned long flags;
-
-	/* init status to no-changes */
-	buf[0] = 0;
-
-	/* Inform the core about resumes-in-progress by returning
-	 * a non-zero value even if there are no status changes.
-	 */
-	status = fotg210->resuming_ports;
-
-	mask = PORT_CSC | PORT_PEC;
-	/* PORT_RESUME from hardware ~= PORT_STAT_C_SUSPEND */
-
-	/* no hub change reports (bit 0) for now (power, ...) */
-
-	/* port N changes (bit N)? */
-	spin_lock_irqsave(&fotg210->lock, flags);
-
-	temp = fotg210_readl(fotg210, &fotg210->regs->port_status);
-
-	/*
-	 * Return status information even for ports with OWNER set.
-	 * Otherwise hub_wq wouldn't see the disconnect event when a
-	 * high-speed device is switched over to the companion
-	 * controller by the user.
-	 */
-
-	if ((temp & mask) != 0 || test_bit(0, &fotg210->port_c_suspend) ||
-			(fotg210->reset_done[0] &&
-			time_after_eq(jiffies, fotg210->reset_done[0]))) {
-		buf[0] |= 1 << 1;
-		status = STS_PCD;
-	}
-	/* FIXME autosuspend idle root hubs */
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-	return status ? retval : 0;
-}
-
-static void fotg210_hub_descriptor(struct fotg210_hcd *fotg210,
-		struct usb_hub_descriptor *desc)
-{
-	int ports = HCS_N_PORTS(fotg210->hcs_params);
-	u16 temp;
-
-	desc->bDescriptorType = USB_DT_HUB;
-	desc->bPwrOn2PwrGood = 10;	/* fotg210 1.0, 2.3.9 says 20ms max */
-	desc->bHubContrCurrent = 0;
-
-	desc->bNbrPorts = ports;
-	temp = 1 + (ports / 8);
-	desc->bDescLength = 7 + 2 * temp;
-
-	/* two bitmaps:  ports removable, and usb 1.0 legacy PortPwrCtrlMask */
-	memset(&desc->u.hs.DeviceRemovable[0], 0, temp);
-	memset(&desc->u.hs.DeviceRemovable[temp], 0xff, temp);
-
-	temp = HUB_CHAR_INDV_PORT_OCPM;	/* per-port overcurrent reporting */
-	temp |= HUB_CHAR_NO_LPSM;	/* no power switching */
-	desc->wHubCharacteristics = cpu_to_le16(temp);
-}
-
-static int fotg210_hub_control(struct usb_hcd *hcd, u16 typeReq, u16 wValue,
-		u16 wIndex, char *buf, u16 wLength)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-	int ports = HCS_N_PORTS(fotg210->hcs_params);
-	u32 __iomem *status_reg = &fotg210->regs->port_status;
-	u32 temp, temp1, status;
-	unsigned long flags;
-	int retval = 0;
-	unsigned selector;
-
-	/*
-	 * FIXME:  support SetPortFeatures USB_PORT_FEAT_INDICATOR.
-	 * HCS_INDICATOR may say we can change LEDs to off/amber/green.
-	 * (track current state ourselves) ... blink for diagnostics,
-	 * power, "this is the one", etc.  EHCI spec supports this.
-	 */
-
-	spin_lock_irqsave(&fotg210->lock, flags);
-	switch (typeReq) {
-	case ClearHubFeature:
-		switch (wValue) {
-		case C_HUB_LOCAL_POWER:
-		case C_HUB_OVER_CURRENT:
-			/* no hub-wide feature/status flags */
-			break;
-		default:
-			goto error;
-		}
-		break;
-	case ClearPortFeature:
-		if (!wIndex || wIndex > ports)
-			goto error;
-		wIndex--;
-		temp = fotg210_readl(fotg210, status_reg);
-		temp &= ~PORT_RWC_BITS;
-
-		/*
-		 * Even if OWNER is set, so the port is owned by the
-		 * companion controller, hub_wq needs to be able to clear
-		 * the port-change status bits (especially
-		 * USB_PORT_STAT_C_CONNECTION).
-		 */
-
-		switch (wValue) {
-		case USB_PORT_FEAT_ENABLE:
-			fotg210_writel(fotg210, temp & ~PORT_PE, status_reg);
-			break;
-		case USB_PORT_FEAT_C_ENABLE:
-			fotg210_writel(fotg210, temp | PORT_PEC, status_reg);
-			break;
-		case USB_PORT_FEAT_SUSPEND:
-			if (temp & PORT_RESET)
-				goto error;
-			if (!(temp & PORT_SUSPEND))
-				break;
-			if ((temp & PORT_PE) == 0)
-				goto error;
-
-			/* resume signaling for 20 msec */
-			fotg210_writel(fotg210, temp | PORT_RESUME, status_reg);
-			fotg210->reset_done[wIndex] = jiffies
-					+ msecs_to_jiffies(USB_RESUME_TIMEOUT);
-			break;
-		case USB_PORT_FEAT_C_SUSPEND:
-			clear_bit(wIndex, &fotg210->port_c_suspend);
-			break;
-		case USB_PORT_FEAT_C_CONNECTION:
-			fotg210_writel(fotg210, temp | PORT_CSC, status_reg);
-			break;
-		case USB_PORT_FEAT_C_OVER_CURRENT:
-			fotg210_writel(fotg210, temp | OTGISR_OVC,
-					&fotg210->regs->otgisr);
-			break;
-		case USB_PORT_FEAT_C_RESET:
-			/* GetPortStatus clears reset */
-			break;
-		default:
-			goto error;
-		}
-		fotg210_readl(fotg210, &fotg210->regs->command);
-		break;
-	case GetHubDescriptor:
-		fotg210_hub_descriptor(fotg210, (struct usb_hub_descriptor *)
-				buf);
-		break;
-	case GetHubStatus:
-		/* no hub-wide feature/status flags */
-		memset(buf, 0, 4);
-		/*cpu_to_le32s ((u32 *) buf); */
-		break;
-	case GetPortStatus:
-		if (!wIndex || wIndex > ports)
-			goto error;
-		wIndex--;
-		status = 0;
-		temp = fotg210_readl(fotg210, status_reg);
-
-		/* wPortChange bits */
-		if (temp & PORT_CSC)
-			status |= USB_PORT_STAT_C_CONNECTION << 16;
-		if (temp & PORT_PEC)
-			status |= USB_PORT_STAT_C_ENABLE << 16;
-
-		temp1 = fotg210_readl(fotg210, &fotg210->regs->otgisr);
-		if (temp1 & OTGISR_OVC)
-			status |= USB_PORT_STAT_C_OVERCURRENT << 16;
-
-		/* whoever resumes must GetPortStatus to complete it!! */
-		if (temp & PORT_RESUME) {
-
-			/* Remote Wakeup received? */
-			if (!fotg210->reset_done[wIndex]) {
-				/* resume signaling for 20 msec */
-				fotg210->reset_done[wIndex] = jiffies
-						+ msecs_to_jiffies(20);
-				/* check the port again */
-				mod_timer(&fotg210_to_hcd(fotg210)->rh_timer,
-						fotg210->reset_done[wIndex]);
-			}
-
-			/* resume completed? */
-			else if (time_after_eq(jiffies,
-					fotg210->reset_done[wIndex])) {
-				clear_bit(wIndex, &fotg210->suspended_ports);
-				set_bit(wIndex, &fotg210->port_c_suspend);
-				fotg210->reset_done[wIndex] = 0;
-
-				/* stop resume signaling */
-				temp = fotg210_readl(fotg210, status_reg);
-				fotg210_writel(fotg210, temp &
-						~(PORT_RWC_BITS | PORT_RESUME),
-						status_reg);
-				clear_bit(wIndex, &fotg210->resuming_ports);
-				retval = handshake(fotg210, status_reg,
-						PORT_RESUME, 0, 2000);/* 2ms */
-				if (retval != 0) {
-					fotg210_err(fotg210,
-							"port %d resume error %d\n",
-							wIndex + 1, retval);
-					goto error;
-				}
-				temp &= ~(PORT_SUSPEND|PORT_RESUME|(3<<10));
-			}
-		}
-
-		/* whoever resets must GetPortStatus to complete it!! */
-		if ((temp & PORT_RESET) && time_after_eq(jiffies,
-				fotg210->reset_done[wIndex])) {
-			status |= USB_PORT_STAT_C_RESET << 16;
-			fotg210->reset_done[wIndex] = 0;
-			clear_bit(wIndex, &fotg210->resuming_ports);
-
-			/* force reset to complete */
-			fotg210_writel(fotg210,
-					temp & ~(PORT_RWC_BITS | PORT_RESET),
-					status_reg);
-			/* REVISIT:  some hardware needs 550+ usec to clear
-			 * this bit; seems too long to spin routinely...
-			 */
-			retval = handshake(fotg210, status_reg,
-					PORT_RESET, 0, 1000);
-			if (retval != 0) {
-				fotg210_err(fotg210, "port %d reset error %d\n",
-						wIndex + 1, retval);
-				goto error;
-			}
-
-			/* see what we found out */
-			temp = check_reset_complete(fotg210, wIndex, status_reg,
-					fotg210_readl(fotg210, status_reg));
-
-			/* restart schedule */
-			fotg210->command |= CMD_RUN;
-			fotg210_writel(fotg210, fotg210->command, &fotg210->regs->command);
-		}
-
-		if (!(temp & (PORT_RESUME|PORT_RESET))) {
-			fotg210->reset_done[wIndex] = 0;
-			clear_bit(wIndex, &fotg210->resuming_ports);
-		}
-
-		/* transfer dedicated ports to the companion hc */
-		if ((temp & PORT_CONNECT) &&
-				test_bit(wIndex, &fotg210->companion_ports)) {
-			temp &= ~PORT_RWC_BITS;
-			fotg210_writel(fotg210, temp, status_reg);
-			fotg210_dbg(fotg210, "port %d --> companion\n",
-					wIndex + 1);
-			temp = fotg210_readl(fotg210, status_reg);
-		}
-
-		/*
-		 * Even if OWNER is set, there's no harm letting hub_wq
-		 * see the wPortStatus values (they should all be 0 except
-		 * for PORT_POWER anyway).
-		 */
-
-		if (temp & PORT_CONNECT) {
-			status |= USB_PORT_STAT_CONNECTION;
-			status |= fotg210_port_speed(fotg210, temp);
-		}
-		if (temp & PORT_PE)
-			status |= USB_PORT_STAT_ENABLE;
-
-		/* maybe the port was unsuspended without our knowledge */
-		if (temp & (PORT_SUSPEND|PORT_RESUME)) {
-			status |= USB_PORT_STAT_SUSPEND;
-		} else if (test_bit(wIndex, &fotg210->suspended_ports)) {
-			clear_bit(wIndex, &fotg210->suspended_ports);
-			clear_bit(wIndex, &fotg210->resuming_ports);
-			fotg210->reset_done[wIndex] = 0;
-			if (temp & PORT_PE)
-				set_bit(wIndex, &fotg210->port_c_suspend);
-		}
-
-		temp1 = fotg210_readl(fotg210, &fotg210->regs->otgisr);
-		if (temp1 & OTGISR_OVC)
-			status |= USB_PORT_STAT_OVERCURRENT;
-		if (temp & PORT_RESET)
-			status |= USB_PORT_STAT_RESET;
-		if (test_bit(wIndex, &fotg210->port_c_suspend))
-			status |= USB_PORT_STAT_C_SUSPEND << 16;
-
-		if (status & ~0xffff)	/* only if wPortChange is interesting */
-			dbg_port(fotg210, "GetStatus", wIndex + 1, temp);
-		put_unaligned_le32(status, buf);
-		break;
-	case SetHubFeature:
-		switch (wValue) {
-		case C_HUB_LOCAL_POWER:
-		case C_HUB_OVER_CURRENT:
-			/* no hub-wide feature/status flags */
-			break;
-		default:
-			goto error;
-		}
-		break;
-	case SetPortFeature:
-		selector = wIndex >> 8;
-		wIndex &= 0xff;
-
-		if (!wIndex || wIndex > ports)
-			goto error;
-		wIndex--;
-		temp = fotg210_readl(fotg210, status_reg);
-		temp &= ~PORT_RWC_BITS;
-		switch (wValue) {
-		case USB_PORT_FEAT_SUSPEND:
-			if ((temp & PORT_PE) == 0
-					|| (temp & PORT_RESET) != 0)
-				goto error;
-
-			/* After above check the port must be connected.
-			 * Set appropriate bit thus could put phy into low power
-			 * mode if we have hostpc feature
-			 */
-			fotg210_writel(fotg210, temp | PORT_SUSPEND,
-					status_reg);
-			set_bit(wIndex, &fotg210->suspended_ports);
-			break;
-		case USB_PORT_FEAT_RESET:
-			if (temp & PORT_RESUME)
-				goto error;
-			/* line status bits may report this as low speed,
-			 * which can be fine if this root hub has a
-			 * transaction translator built in.
-			 */
-			fotg210_dbg(fotg210, "port %d reset\n", wIndex + 1);
-			temp |= PORT_RESET;
-			temp &= ~PORT_PE;
-
-			/*
-			 * caller must wait, then call GetPortStatus
-			 * usb 2.0 spec says 50 ms resets on root
-			 */
-			fotg210->reset_done[wIndex] = jiffies
-					+ msecs_to_jiffies(50);
-			fotg210_writel(fotg210, temp, status_reg);
-			break;
-
-		/* For downstream facing ports (these):  one hub port is put
-		 * into test mode according to USB2 11.24.2.13, then the hub
-		 * must be reset (which for root hub now means rmmod+modprobe,
-		 * or else system reboot).  See EHCI 2.3.9 and 4.14 for info
-		 * about the EHCI-specific stuff.
-		 */
-		case USB_PORT_FEAT_TEST:
-			if (!selector || selector > 5)
-				goto error;
-			spin_unlock_irqrestore(&fotg210->lock, flags);
-			fotg210_quiesce(fotg210);
-			spin_lock_irqsave(&fotg210->lock, flags);
-
-			/* Put all enabled ports into suspend */
-			temp = fotg210_readl(fotg210, status_reg) &
-				~PORT_RWC_BITS;
-			if (temp & PORT_PE)
-				fotg210_writel(fotg210, temp | PORT_SUSPEND,
-						status_reg);
-
-			spin_unlock_irqrestore(&fotg210->lock, flags);
-			fotg210_halt(fotg210);
-			spin_lock_irqsave(&fotg210->lock, flags);
-
-			temp = fotg210_readl(fotg210, status_reg);
-			temp |= selector << 16;
-			fotg210_writel(fotg210, temp, status_reg);
-			break;
-
-		default:
-			goto error;
-		}
-		fotg210_readl(fotg210, &fotg210->regs->command);
-		break;
-
-	default:
-error:
-		/* "stall" on error */
-		retval = -EPIPE;
-	}
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-	return retval;
-}
-
-static void __maybe_unused fotg210_relinquish_port(struct usb_hcd *hcd,
-		int portnum)
-{
-	return;
-}
-
-static int __maybe_unused fotg210_port_handed_over(struct usb_hcd *hcd,
-		int portnum)
-{
-	return 0;
-}
-
-/* There's basically three types of memory:
- *	- data used only by the HCD ... kmalloc is fine
- *	- async and periodic schedules, shared by HC and HCD ... these
- *	  need to use dma_pool or dma_alloc_coherent
- *	- driver buffers, read/written by HC ... single shot DMA mapped
- *
- * There's also "register" data (e.g. PCI or SOC), which is memory mapped.
- * No memory seen by this driver is pageable.
- */
-
-/* Allocate the key transfer structures from the previously allocated pool */
-static inline void fotg210_qtd_init(struct fotg210_hcd *fotg210,
-		struct fotg210_qtd *qtd, dma_addr_t dma)
-{
-	memset(qtd, 0, sizeof(*qtd));
-	qtd->qtd_dma = dma;
-	qtd->hw_token = cpu_to_hc32(fotg210, QTD_STS_HALT);
-	qtd->hw_next = FOTG210_LIST_END(fotg210);
-	qtd->hw_alt_next = FOTG210_LIST_END(fotg210);
-	INIT_LIST_HEAD(&qtd->qtd_list);
-}
-
-static struct fotg210_qtd *fotg210_qtd_alloc(struct fotg210_hcd *fotg210,
-		gfp_t flags)
-{
-	struct fotg210_qtd *qtd;
-	dma_addr_t dma;
-
-	qtd = dma_pool_alloc(fotg210->qtd_pool, flags, &dma);
-	if (qtd != NULL)
-		fotg210_qtd_init(fotg210, qtd, dma);
-
-	return qtd;
-}
-
-static inline void fotg210_qtd_free(struct fotg210_hcd *fotg210,
-		struct fotg210_qtd *qtd)
-{
-	dma_pool_free(fotg210->qtd_pool, qtd, qtd->qtd_dma);
-}
-
-
-static void qh_destroy(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
-{
-	/* clean qtds first, and know this is not linked */
-	if (!list_empty(&qh->qtd_list) || qh->qh_next.ptr) {
-		fotg210_dbg(fotg210, "unused qh not empty!\n");
-		BUG();
-	}
-	if (qh->dummy)
-		fotg210_qtd_free(fotg210, qh->dummy);
-	dma_pool_free(fotg210->qh_pool, qh->hw, qh->qh_dma);
-	kfree(qh);
-}
-
-static struct fotg210_qh *fotg210_qh_alloc(struct fotg210_hcd *fotg210,
-		gfp_t flags)
-{
-	struct fotg210_qh *qh;
-	dma_addr_t dma;
-
-	qh = kzalloc(sizeof(*qh), GFP_ATOMIC);
-	if (!qh)
-		goto done;
-	qh->hw = (struct fotg210_qh_hw *)
-		dma_pool_zalloc(fotg210->qh_pool, flags, &dma);
-	if (!qh->hw)
-		goto fail;
-	qh->qh_dma = dma;
-	INIT_LIST_HEAD(&qh->qtd_list);
-
-	/* dummy td enables safe urb queuing */
-	qh->dummy = fotg210_qtd_alloc(fotg210, flags);
-	if (qh->dummy == NULL) {
-		fotg210_dbg(fotg210, "no dummy td\n");
-		goto fail1;
-	}
-done:
-	return qh;
-fail1:
-	dma_pool_free(fotg210->qh_pool, qh->hw, qh->qh_dma);
-fail:
-	kfree(qh);
-	return NULL;
-}
-
-/* The queue heads and transfer descriptors are managed from pools tied
- * to each of the "per device" structures.
- * This is the initialisation and cleanup code.
- */
-
-static void fotg210_mem_cleanup(struct fotg210_hcd *fotg210)
-{
-	if (fotg210->async)
-		qh_destroy(fotg210, fotg210->async);
-	fotg210->async = NULL;
-
-	if (fotg210->dummy)
-		qh_destroy(fotg210, fotg210->dummy);
-	fotg210->dummy = NULL;
-
-	/* DMA consistent memory and pools */
-	dma_pool_destroy(fotg210->qtd_pool);
-	fotg210->qtd_pool = NULL;
-
-	dma_pool_destroy(fotg210->qh_pool);
-	fotg210->qh_pool = NULL;
-
-	dma_pool_destroy(fotg210->itd_pool);
-	fotg210->itd_pool = NULL;
-
-	if (fotg210->periodic)
-		dma_free_coherent(fotg210_to_hcd(fotg210)->self.controller,
-				fotg210->periodic_size * sizeof(u32),
-				fotg210->periodic, fotg210->periodic_dma);
-	fotg210->periodic = NULL;
-
-	/* shadow periodic table */
-	kfree(fotg210->pshadow);
-	fotg210->pshadow = NULL;
-}
-
-/* remember to add cleanup code (above) if you add anything here */
-static int fotg210_mem_init(struct fotg210_hcd *fotg210, gfp_t flags)
-{
-	int i;
-
-	/* QTDs for control/bulk/intr transfers */
-	fotg210->qtd_pool = dma_pool_create("fotg210_qtd",
-			fotg210_to_hcd(fotg210)->self.controller,
-			sizeof(struct fotg210_qtd),
-			32 /* byte alignment (for hw parts) */,
-			4096 /* can't cross 4K */);
-	if (!fotg210->qtd_pool)
-		goto fail;
-
-	/* QHs for control/bulk/intr transfers */
-	fotg210->qh_pool = dma_pool_create("fotg210_qh",
-			fotg210_to_hcd(fotg210)->self.controller,
-			sizeof(struct fotg210_qh_hw),
-			32 /* byte alignment (for hw parts) */,
-			4096 /* can't cross 4K */);
-	if (!fotg210->qh_pool)
-		goto fail;
-
-	fotg210->async = fotg210_qh_alloc(fotg210, flags);
-	if (!fotg210->async)
-		goto fail;
-
-	/* ITD for high speed ISO transfers */
-	fotg210->itd_pool = dma_pool_create("fotg210_itd",
-			fotg210_to_hcd(fotg210)->self.controller,
-			sizeof(struct fotg210_itd),
-			64 /* byte alignment (for hw parts) */,
-			4096 /* can't cross 4K */);
-	if (!fotg210->itd_pool)
-		goto fail;
-
-	/* Hardware periodic table */
-	fotg210->periodic =
-		dma_alloc_coherent(fotg210_to_hcd(fotg210)->self.controller,
-				fotg210->periodic_size * sizeof(__le32),
-				&fotg210->periodic_dma, 0);
-	if (fotg210->periodic == NULL)
-		goto fail;
-
-	for (i = 0; i < fotg210->periodic_size; i++)
-		fotg210->periodic[i] = FOTG210_LIST_END(fotg210);
-
-	/* software shadow of hardware table */
-	fotg210->pshadow = kcalloc(fotg210->periodic_size, sizeof(void *),
-			flags);
-	if (fotg210->pshadow != NULL)
-		return 0;
-
-fail:
-	fotg210_dbg(fotg210, "couldn't init memory\n");
-	fotg210_mem_cleanup(fotg210);
-	return -ENOMEM;
-}
-/* EHCI hardware queue manipulation ... the core.  QH/QTD manipulation.
- *
- * Control, bulk, and interrupt traffic all use "qh" lists.  They list "qtd"
- * entries describing USB transactions, max 16-20kB/entry (with 4kB-aligned
- * buffers needed for the larger number).  We use one QH per endpoint, queue
- * multiple urbs (all three types) per endpoint.  URBs may need several qtds.
- *
- * ISO traffic uses "ISO TD" (itd) records, and (along with
- * interrupts) needs careful scheduling.  Performance improvements can be
- * an ongoing challenge.  That's in "ehci-sched.c".
- *
- * USB 1.1 devices are handled (a) by "companion" OHCI or UHCI root hubs,
- * or otherwise through transaction translators (TTs) in USB 2.0 hubs using
- * (b) special fields in qh entries or (c) split iso entries.  TTs will
- * buffer low/full speed data so the host collects it at high speed.
- */
-
-/* fill a qtd, returning how much of the buffer we were able to queue up */
-static int qtd_fill(struct fotg210_hcd *fotg210, struct fotg210_qtd *qtd,
-		dma_addr_t buf, size_t len, int token, int maxpacket)
-{
-	int i, count;
-	u64 addr = buf;
-
-	/* one buffer entry per 4K ... first might be short or unaligned */
-	qtd->hw_buf[0] = cpu_to_hc32(fotg210, (u32)addr);
-	qtd->hw_buf_hi[0] = cpu_to_hc32(fotg210, (u32)(addr >> 32));
-	count = 0x1000 - (buf & 0x0fff);	/* rest of that page */
-	if (likely(len < count))		/* ... iff needed */
-		count = len;
-	else {
-		buf +=  0x1000;
-		buf &= ~0x0fff;
-
-		/* per-qtd limit: from 16K to 20K (best alignment) */
-		for (i = 1; count < len && i < 5; i++) {
-			addr = buf;
-			qtd->hw_buf[i] = cpu_to_hc32(fotg210, (u32)addr);
-			qtd->hw_buf_hi[i] = cpu_to_hc32(fotg210,
-					(u32)(addr >> 32));
-			buf += 0x1000;
-			if ((count + 0x1000) < len)
-				count += 0x1000;
-			else
-				count = len;
-		}
-
-		/* short packets may only terminate transfers */
-		if (count != len)
-			count -= (count % maxpacket);
-	}
-	qtd->hw_token = cpu_to_hc32(fotg210, (count << 16) | token);
-	qtd->length = count;
-
-	return count;
-}
-
-static inline void qh_update(struct fotg210_hcd *fotg210,
-		struct fotg210_qh *qh, struct fotg210_qtd *qtd)
-{
-	struct fotg210_qh_hw *hw = qh->hw;
-
-	/* writes to an active overlay are unsafe */
-	BUG_ON(qh->qh_state != QH_STATE_IDLE);
-
-	hw->hw_qtd_next = QTD_NEXT(fotg210, qtd->qtd_dma);
-	hw->hw_alt_next = FOTG210_LIST_END(fotg210);
-
-	/* Except for control endpoints, we make hardware maintain data
-	 * toggle (like OHCI) ... here (re)initialize the toggle in the QH,
-	 * and set the pseudo-toggle in udev. Only usb_clear_halt() will
-	 * ever clear it.
-	 */
-	if (!(hw->hw_info1 & cpu_to_hc32(fotg210, QH_TOGGLE_CTL))) {
-		unsigned is_out, epnum;
-
-		is_out = qh->is_out;
-		epnum = (hc32_to_cpup(fotg210, &hw->hw_info1) >> 8) & 0x0f;
-		if (unlikely(!usb_gettoggle(qh->dev, epnum, is_out))) {
-			hw->hw_token &= ~cpu_to_hc32(fotg210, QTD_TOGGLE);
-			usb_settoggle(qh->dev, epnum, is_out, 1);
-		}
-	}
-
-	hw->hw_token &= cpu_to_hc32(fotg210, QTD_TOGGLE | QTD_STS_PING);
-}
-
-/* if it weren't for a common silicon quirk (writing the dummy into the qh
- * overlay, so qh->hw_token wrongly becomes inactive/halted), only fault
- * recovery (including urb dequeue) would need software changes to a QH...
- */
-static void qh_refresh(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
-{
-	struct fotg210_qtd *qtd;
-
-	if (list_empty(&qh->qtd_list))
-		qtd = qh->dummy;
-	else {
-		qtd = list_entry(qh->qtd_list.next,
-				struct fotg210_qtd, qtd_list);
-		/*
-		 * first qtd may already be partially processed.
-		 * If we come here during unlink, the QH overlay region
-		 * might have reference to the just unlinked qtd. The
-		 * qtd is updated in qh_completions(). Update the QH
-		 * overlay here.
-		 */
-		if (cpu_to_hc32(fotg210, qtd->qtd_dma) == qh->hw->hw_current) {
-			qh->hw->hw_qtd_next = qtd->hw_next;
-			qtd = NULL;
-		}
-	}
-
-	if (qtd)
-		qh_update(fotg210, qh, qtd);
-}
-
-static void qh_link_async(struct fotg210_hcd *fotg210, struct fotg210_qh *qh);
-
-static void fotg210_clear_tt_buffer_complete(struct usb_hcd *hcd,
-		struct usb_host_endpoint *ep)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-	struct fotg210_qh *qh = ep->hcpriv;
-	unsigned long flags;
-
-	spin_lock_irqsave(&fotg210->lock, flags);
-	qh->clearing_tt = 0;
-	if (qh->qh_state == QH_STATE_IDLE && !list_empty(&qh->qtd_list)
-			&& fotg210->rh_state == FOTG210_RH_RUNNING)
-		qh_link_async(fotg210, qh);
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-}
-
-static void fotg210_clear_tt_buffer(struct fotg210_hcd *fotg210,
-		struct fotg210_qh *qh, struct urb *urb, u32 token)
-{
-
-	/* If an async split transaction gets an error or is unlinked,
-	 * the TT buffer may be left in an indeterminate state.  We
-	 * have to clear the TT buffer.
-	 *
-	 * Note: this routine is never called for Isochronous transfers.
-	 */
-	if (urb->dev->tt && !usb_pipeint(urb->pipe) && !qh->clearing_tt) {
-		struct usb_device *tt = urb->dev->tt->hub;
-
-		dev_dbg(&tt->dev,
-				"clear tt buffer port %d, a%d ep%d t%08x\n",
-				urb->dev->ttport, urb->dev->devnum,
-				usb_pipeendpoint(urb->pipe), token);
-
-		if (urb->dev->tt->hub !=
-				fotg210_to_hcd(fotg210)->self.root_hub) {
-			if (usb_hub_clear_tt_buffer(urb) == 0)
-				qh->clearing_tt = 1;
-		}
-	}
-}
-
-static int qtd_copy_status(struct fotg210_hcd *fotg210, struct urb *urb,
-		size_t length, u32 token)
-{
-	int status = -EINPROGRESS;
-
-	/* count IN/OUT bytes, not SETUP (even short packets) */
-	if (likely(QTD_PID(token) != 2))
-		urb->actual_length += length - QTD_LENGTH(token);
-
-	/* don't modify error codes */
-	if (unlikely(urb->unlinked))
-		return status;
-
-	/* force cleanup after short read; not always an error */
-	if (unlikely(IS_SHORT_READ(token)))
-		status = -EREMOTEIO;
-
-	/* serious "can't proceed" faults reported by the hardware */
-	if (token & QTD_STS_HALT) {
-		if (token & QTD_STS_BABBLE) {
-			/* FIXME "must" disable babbling device's port too */
-			status = -EOVERFLOW;
-		/* CERR nonzero + halt --> stall */
-		} else if (QTD_CERR(token)) {
-			status = -EPIPE;
-
-		/* In theory, more than one of the following bits can be set
-		 * since they are sticky and the transaction is retried.
-		 * Which to test first is rather arbitrary.
-		 */
-		} else if (token & QTD_STS_MMF) {
-			/* fs/ls interrupt xfer missed the complete-split */
-			status = -EPROTO;
-		} else if (token & QTD_STS_DBE) {
-			status = (QTD_PID(token) == 1) /* IN ? */
-				? -ENOSR  /* hc couldn't read data */
-				: -ECOMM; /* hc couldn't write data */
-		} else if (token & QTD_STS_XACT) {
-			/* timeout, bad CRC, wrong PID, etc */
-			fotg210_dbg(fotg210, "devpath %s ep%d%s 3strikes\n",
-					urb->dev->devpath,
-					usb_pipeendpoint(urb->pipe),
-					usb_pipein(urb->pipe) ? "in" : "out");
-			status = -EPROTO;
-		} else {	/* unknown */
-			status = -EPROTO;
-		}
-
-		fotg210_dbg(fotg210,
-				"dev%d ep%d%s qtd token %08x --> status %d\n",
-				usb_pipedevice(urb->pipe),
-				usb_pipeendpoint(urb->pipe),
-				usb_pipein(urb->pipe) ? "in" : "out",
-				token, status);
-	}
-
-	return status;
-}
-
-static void fotg210_urb_done(struct fotg210_hcd *fotg210, struct urb *urb,
-		int status)
-__releases(fotg210->lock)
-__acquires(fotg210->lock)
-{
-	if (likely(urb->hcpriv != NULL)) {
-		struct fotg210_qh *qh = (struct fotg210_qh *) urb->hcpriv;
-
-		/* S-mask in a QH means it's an interrupt urb */
-		if ((qh->hw->hw_info2 & cpu_to_hc32(fotg210, QH_SMASK)) != 0) {
-
-			/* ... update hc-wide periodic stats (for usbfs) */
-			fotg210_to_hcd(fotg210)->self.bandwidth_int_reqs--;
-		}
-	}
-
-	if (unlikely(urb->unlinked)) {
-		INCR(fotg210->stats.unlink);
-	} else {
-		/* report non-error and short read status as zero */
-		if (status == -EINPROGRESS || status == -EREMOTEIO)
-			status = 0;
-		INCR(fotg210->stats.complete);
-	}
-
-#ifdef FOTG210_URB_TRACE
-	fotg210_dbg(fotg210,
-			"%s %s urb %p ep%d%s status %d len %d/%d\n",
-			__func__, urb->dev->devpath, urb,
-			usb_pipeendpoint(urb->pipe),
-			usb_pipein(urb->pipe) ? "in" : "out",
-			status,
-			urb->actual_length, urb->transfer_buffer_length);
-#endif
-
-	/* complete() can reenter this HCD */
-	usb_hcd_unlink_urb_from_ep(fotg210_to_hcd(fotg210), urb);
-	spin_unlock(&fotg210->lock);
-	usb_hcd_giveback_urb(fotg210_to_hcd(fotg210), urb, status);
-	spin_lock(&fotg210->lock);
-}
-
-static int qh_schedule(struct fotg210_hcd *fotg210, struct fotg210_qh *qh);
-
-/* Process and free completed qtds for a qh, returning URBs to drivers.
- * Chases up to qh->hw_current.  Returns number of completions called,
- * indicating how much "real" work we did.
- */
-static unsigned qh_completions(struct fotg210_hcd *fotg210,
-		struct fotg210_qh *qh)
-{
-	struct fotg210_qtd *last, *end = qh->dummy;
-	struct fotg210_qtd *qtd, *tmp;
-	int last_status;
-	int stopped;
-	unsigned count = 0;
-	u8 state;
-	struct fotg210_qh_hw *hw = qh->hw;
-
-	if (unlikely(list_empty(&qh->qtd_list)))
-		return count;
-
-	/* completions (or tasks on other cpus) must never clobber HALT
-	 * till we've gone through and cleaned everything up, even when
-	 * they add urbs to this qh's queue or mark them for unlinking.
-	 *
-	 * NOTE:  unlinking expects to be done in queue order.
-	 *
-	 * It's a bug for qh->qh_state to be anything other than
-	 * QH_STATE_IDLE, unless our caller is scan_async() or
-	 * scan_intr().
-	 */
-	state = qh->qh_state;
-	qh->qh_state = QH_STATE_COMPLETING;
-	stopped = (state == QH_STATE_IDLE);
-
-rescan:
-	last = NULL;
-	last_status = -EINPROGRESS;
-	qh->needs_rescan = 0;
-
-	/* remove de-activated QTDs from front of queue.
-	 * after faults (including short reads), cleanup this urb
-	 * then let the queue advance.
-	 * if queue is stopped, handles unlinks.
-	 */
-	list_for_each_entry_safe(qtd, tmp, &qh->qtd_list, qtd_list) {
-		struct urb *urb;
-		u32 token = 0;
-
-		urb = qtd->urb;
-
-		/* clean up any state from previous QTD ...*/
-		if (last) {
-			if (likely(last->urb != urb)) {
-				fotg210_urb_done(fotg210, last->urb,
-						last_status);
-				count++;
-				last_status = -EINPROGRESS;
-			}
-			fotg210_qtd_free(fotg210, last);
-			last = NULL;
-		}
-
-		/* ignore urbs submitted during completions we reported */
-		if (qtd == end)
-			break;
-
-		/* hardware copies qtd out of qh overlay */
-		rmb();
-		token = hc32_to_cpu(fotg210, qtd->hw_token);
-
-		/* always clean up qtds the hc de-activated */
-retry_xacterr:
-		if ((token & QTD_STS_ACTIVE) == 0) {
-
-			/* Report Data Buffer Error: non-fatal but useful */
-			if (token & QTD_STS_DBE)
-				fotg210_dbg(fotg210,
-					"detected DataBufferErr for urb %p ep%d%s len %d, qtd %p [qh %p]\n",
-					urb, usb_endpoint_num(&urb->ep->desc),
-					usb_endpoint_dir_in(&urb->ep->desc)
-						? "in" : "out",
-					urb->transfer_buffer_length, qtd, qh);
-
-			/* on STALL, error, and short reads this urb must
-			 * complete and all its qtds must be recycled.
-			 */
-			if ((token & QTD_STS_HALT) != 0) {
-
-				/* retry transaction errors until we
-				 * reach the software xacterr limit
-				 */
-				if ((token & QTD_STS_XACT) &&
-						QTD_CERR(token) == 0 &&
-						++qh->xacterrs < QH_XACTERR_MAX &&
-						!urb->unlinked) {
-					fotg210_dbg(fotg210,
-						"detected XactErr len %zu/%zu retry %d\n",
-						qtd->length - QTD_LENGTH(token),
-						qtd->length,
-						qh->xacterrs);
-
-					/* reset the token in the qtd and the
-					 * qh overlay (which still contains
-					 * the qtd) so that we pick up from
-					 * where we left off
-					 */
-					token &= ~QTD_STS_HALT;
-					token |= QTD_STS_ACTIVE |
-						 (FOTG210_TUNE_CERR << 10);
-					qtd->hw_token = cpu_to_hc32(fotg210,
-							token);
-					wmb();
-					hw->hw_token = cpu_to_hc32(fotg210,
-							token);
-					goto retry_xacterr;
-				}
-				stopped = 1;
-
-			/* magic dummy for some short reads; qh won't advance.
-			 * that silicon quirk can kick in with this dummy too.
-			 *
-			 * other short reads won't stop the queue, including
-			 * control transfers (status stage handles that) or
-			 * most other single-qtd reads ... the queue stops if
-			 * URB_SHORT_NOT_OK was set so the driver submitting
-			 * the urbs could clean it up.
-			 */
-			} else if (IS_SHORT_READ(token) &&
-					!(qtd->hw_alt_next &
-					FOTG210_LIST_END(fotg210))) {
-				stopped = 1;
-			}
-
-		/* stop scanning when we reach qtds the hc is using */
-		} else if (likely(!stopped
-				&& fotg210->rh_state >= FOTG210_RH_RUNNING)) {
-			break;
-
-		/* scan the whole queue for unlinks whenever it stops */
-		} else {
-			stopped = 1;
-
-			/* cancel everything if we halt, suspend, etc */
-			if (fotg210->rh_state < FOTG210_RH_RUNNING)
-				last_status = -ESHUTDOWN;
-
-			/* this qtd is active; skip it unless a previous qtd
-			 * for its urb faulted, or its urb was canceled.
-			 */
-			else if (last_status == -EINPROGRESS && !urb->unlinked)
-				continue;
-
-			/* qh unlinked; token in overlay may be most current */
-			if (state == QH_STATE_IDLE &&
-					cpu_to_hc32(fotg210, qtd->qtd_dma)
-					== hw->hw_current) {
-				token = hc32_to_cpu(fotg210, hw->hw_token);
-
-				/* An unlink may leave an incomplete
-				 * async transaction in the TT buffer.
-				 * We have to clear it.
-				 */
-				fotg210_clear_tt_buffer(fotg210, qh, urb,
-						token);
-			}
-		}
-
-		/* unless we already know the urb's status, collect qtd status
-		 * and update count of bytes transferred.  in common short read
-		 * cases with only one data qtd (including control transfers),
-		 * queue processing won't halt.  but with two or more qtds (for
-		 * example, with a 32 KB transfer), when the first qtd gets a
-		 * short read the second must be removed by hand.
-		 */
-		if (last_status == -EINPROGRESS) {
-			last_status = qtd_copy_status(fotg210, urb,
-					qtd->length, token);
-			if (last_status == -EREMOTEIO &&
-					(qtd->hw_alt_next &
-					FOTG210_LIST_END(fotg210)))
-				last_status = -EINPROGRESS;
-
-			/* As part of low/full-speed endpoint-halt processing
-			 * we must clear the TT buffer (11.17.5).
-			 */
-			if (unlikely(last_status != -EINPROGRESS &&
-					last_status != -EREMOTEIO)) {
-				/* The TT's in some hubs malfunction when they
-				 * receive this request following a STALL (they
-				 * stop sending isochronous packets).  Since a
-				 * STALL can't leave the TT buffer in a busy
-				 * state (if you believe Figures 11-48 - 11-51
-				 * in the USB 2.0 spec), we won't clear the TT
-				 * buffer in this case.  Strictly speaking this
-				 * is a violation of the spec.
-				 */
-				if (last_status != -EPIPE)
-					fotg210_clear_tt_buffer(fotg210, qh,
-							urb, token);
-			}
-		}
-
-		/* if we're removing something not at the queue head,
-		 * patch the hardware queue pointer.
-		 */
-		if (stopped && qtd->qtd_list.prev != &qh->qtd_list) {
-			last = list_entry(qtd->qtd_list.prev,
-					struct fotg210_qtd, qtd_list);
-			last->hw_next = qtd->hw_next;
-		}
-
-		/* remove qtd; it's recycled after possible urb completion */
-		list_del(&qtd->qtd_list);
-		last = qtd;
-
-		/* reinit the xacterr counter for the next qtd */
-		qh->xacterrs = 0;
-	}
-
-	/* last urb's completion might still need calling */
-	if (likely(last != NULL)) {
-		fotg210_urb_done(fotg210, last->urb, last_status);
-		count++;
-		fotg210_qtd_free(fotg210, last);
-	}
-
-	/* Do we need to rescan for URBs dequeued during a giveback? */
-	if (unlikely(qh->needs_rescan)) {
-		/* If the QH is already unlinked, do the rescan now. */
-		if (state == QH_STATE_IDLE)
-			goto rescan;
-
-		/* Otherwise we have to wait until the QH is fully unlinked.
-		 * Our caller will start an unlink if qh->needs_rescan is
-		 * set.  But if an unlink has already started, nothing needs
-		 * to be done.
-		 */
-		if (state != QH_STATE_LINKED)
-			qh->needs_rescan = 0;
-	}
-
-	/* restore original state; caller must unlink or relink */
-	qh->qh_state = state;
-
-	/* be sure the hardware's done with the qh before refreshing
-	 * it after fault cleanup, or recovering from silicon wrongly
-	 * overlaying the dummy qtd (which reduces DMA chatter).
-	 */
-	if (stopped != 0 || hw->hw_qtd_next == FOTG210_LIST_END(fotg210)) {
-		switch (state) {
-		case QH_STATE_IDLE:
-			qh_refresh(fotg210, qh);
-			break;
-		case QH_STATE_LINKED:
-			/* We won't refresh a QH that's linked (after the HC
-			 * stopped the queue).  That avoids a race:
-			 *  - HC reads first part of QH;
-			 *  - CPU updates that first part and the token;
-			 *  - HC reads rest of that QH, including token
-			 * Result:  HC gets an inconsistent image, and then
-			 * DMAs to/from the wrong memory (corrupting it).
-			 *
-			 * That should be rare for interrupt transfers,
-			 * except maybe high bandwidth ...
-			 */
-
-			/* Tell the caller to start an unlink */
-			qh->needs_rescan = 1;
-			break;
-		/* otherwise, unlink already started */
-		}
-	}
-
-	return count;
-}
-
-/* reverse of qh_urb_transaction:  free a list of TDs.
- * used for cleanup after errors, before HC sees an URB's TDs.
- */
-static void qtd_list_free(struct fotg210_hcd *fotg210, struct urb *urb,
-		struct list_head *head)
-{
-	struct fotg210_qtd *qtd, *temp;
-
-	list_for_each_entry_safe(qtd, temp, head, qtd_list) {
-		list_del(&qtd->qtd_list);
-		fotg210_qtd_free(fotg210, qtd);
-	}
-}
-
-/* create a list of filled qtds for this URB; won't link into qh.
- */
-static struct list_head *qh_urb_transaction(struct fotg210_hcd *fotg210,
-		struct urb *urb, struct list_head *head, gfp_t flags)
-{
-	struct fotg210_qtd *qtd, *qtd_prev;
-	dma_addr_t buf;
-	int len, this_sg_len, maxpacket;
-	int is_input;
-	u32 token;
-	int i;
-	struct scatterlist *sg;
-
-	/*
-	 * URBs map to sequences of QTDs:  one logical transaction
-	 */
-	qtd = fotg210_qtd_alloc(fotg210, flags);
-	if (unlikely(!qtd))
-		return NULL;
-	list_add_tail(&qtd->qtd_list, head);
-	qtd->urb = urb;
-
-	token = QTD_STS_ACTIVE;
-	token |= (FOTG210_TUNE_CERR << 10);
-	/* for split transactions, SplitXState initialized to zero */
-
-	len = urb->transfer_buffer_length;
-	is_input = usb_pipein(urb->pipe);
-	if (usb_pipecontrol(urb->pipe)) {
-		/* SETUP pid */
-		qtd_fill(fotg210, qtd, urb->setup_dma,
-				sizeof(struct usb_ctrlrequest),
-				token | (2 /* "setup" */ << 8), 8);
-
-		/* ... and always at least one more pid */
-		token ^= QTD_TOGGLE;
-		qtd_prev = qtd;
-		qtd = fotg210_qtd_alloc(fotg210, flags);
-		if (unlikely(!qtd))
-			goto cleanup;
-		qtd->urb = urb;
-		qtd_prev->hw_next = QTD_NEXT(fotg210, qtd->qtd_dma);
-		list_add_tail(&qtd->qtd_list, head);
-
-		/* for zero length DATA stages, STATUS is always IN */
-		if (len == 0)
-			token |= (1 /* "in" */ << 8);
-	}
-
-	/*
-	 * data transfer stage:  buffer setup
-	 */
-	i = urb->num_mapped_sgs;
-	if (len > 0 && i > 0) {
-		sg = urb->sg;
-		buf = sg_dma_address(sg);
-
-		/* urb->transfer_buffer_length may be smaller than the
-		 * size of the scatterlist (or vice versa)
-		 */
-		this_sg_len = min_t(int, sg_dma_len(sg), len);
-	} else {
-		sg = NULL;
-		buf = urb->transfer_dma;
-		this_sg_len = len;
-	}
-
-	if (is_input)
-		token |= (1 /* "in" */ << 8);
-	/* else it's already initted to "out" pid (0 << 8) */
-
-	maxpacket = usb_maxpacket(urb->dev, urb->pipe);
-
-	/*
-	 * buffer gets wrapped in one or more qtds;
-	 * last one may be "short" (including zero len)
-	 * and may serve as a control status ack
-	 */
-	for (;;) {
-		int this_qtd_len;
-
-		this_qtd_len = qtd_fill(fotg210, qtd, buf, this_sg_len, token,
-				maxpacket);
-		this_sg_len -= this_qtd_len;
-		len -= this_qtd_len;
-		buf += this_qtd_len;
-
-		/*
-		 * short reads advance to a "magic" dummy instead of the next
-		 * qtd ... that forces the queue to stop, for manual cleanup.
-		 * (this will usually be overridden later.)
-		 */
-		if (is_input)
-			qtd->hw_alt_next = fotg210->async->hw->hw_alt_next;
-
-		/* qh makes control packets use qtd toggle; maybe switch it */
-		if ((maxpacket & (this_qtd_len + (maxpacket - 1))) == 0)
-			token ^= QTD_TOGGLE;
-
-		if (likely(this_sg_len <= 0)) {
-			if (--i <= 0 || len <= 0)
-				break;
-			sg = sg_next(sg);
-			buf = sg_dma_address(sg);
-			this_sg_len = min_t(int, sg_dma_len(sg), len);
-		}
-
-		qtd_prev = qtd;
-		qtd = fotg210_qtd_alloc(fotg210, flags);
-		if (unlikely(!qtd))
-			goto cleanup;
-		qtd->urb = urb;
-		qtd_prev->hw_next = QTD_NEXT(fotg210, qtd->qtd_dma);
-		list_add_tail(&qtd->qtd_list, head);
-	}
-
-	/*
-	 * unless the caller requires manual cleanup after short reads,
-	 * have the alt_next mechanism keep the queue running after the
-	 * last data qtd (the only one, for control and most other cases).
-	 */
-	if (likely((urb->transfer_flags & URB_SHORT_NOT_OK) == 0 ||
-			usb_pipecontrol(urb->pipe)))
-		qtd->hw_alt_next = FOTG210_LIST_END(fotg210);
-
-	/*
-	 * control requests may need a terminating data "status" ack;
-	 * other OUT ones may need a terminating short packet
-	 * (zero length).
-	 */
-	if (likely(urb->transfer_buffer_length != 0)) {
-		int one_more = 0;
-
-		if (usb_pipecontrol(urb->pipe)) {
-			one_more = 1;
-			token ^= 0x0100;	/* "in" <--> "out"  */
-			token |= QTD_TOGGLE;	/* force DATA1 */
-		} else if (usb_pipeout(urb->pipe)
-				&& (urb->transfer_flags & URB_ZERO_PACKET)
-				&& !(urb->transfer_buffer_length % maxpacket)) {
-			one_more = 1;
-		}
-		if (one_more) {
-			qtd_prev = qtd;
-			qtd = fotg210_qtd_alloc(fotg210, flags);
-			if (unlikely(!qtd))
-				goto cleanup;
-			qtd->urb = urb;
-			qtd_prev->hw_next = QTD_NEXT(fotg210, qtd->qtd_dma);
-			list_add_tail(&qtd->qtd_list, head);
-
-			/* never any data in such packets */
-			qtd_fill(fotg210, qtd, 0, 0, token, 0);
-		}
-	}
-
-	/* by default, enable interrupt on urb completion */
-	if (likely(!(urb->transfer_flags & URB_NO_INTERRUPT)))
-		qtd->hw_token |= cpu_to_hc32(fotg210, QTD_IOC);
-	return head;
-
-cleanup:
-	qtd_list_free(fotg210, urb, head);
-	return NULL;
-}
-
-/* Would be best to create all qh's from config descriptors,
- * when each interface/altsetting is established.  Unlink
- * any previous qh and cancel its urbs first; endpoints are
- * implicitly reset then (data toggle too).
- * That'd mean updating how usbcore talks to HCDs. (2.7?)
- */
-
-
-/* Each QH holds a qtd list; a QH is used for everything except iso.
- *
- * For interrupt urbs, the scheduler must set the microframe scheduling
- * mask(s) each time the QH gets scheduled.  For highspeed, that's
- * just one microframe in the s-mask.  For split interrupt transactions
- * there are additional complications: c-mask, maybe FSTNs.
- */
-static struct fotg210_qh *qh_make(struct fotg210_hcd *fotg210, struct urb *urb,
-		gfp_t flags)
-{
-	struct fotg210_qh *qh = fotg210_qh_alloc(fotg210, flags);
-	struct usb_host_endpoint *ep;
-	u32 info1 = 0, info2 = 0;
-	int is_input, type;
-	int maxp = 0;
-	int mult;
-	struct usb_tt *tt = urb->dev->tt;
-	struct fotg210_qh_hw *hw;
-
-	if (!qh)
-		return qh;
-
-	/*
-	 * init endpoint/device data for this QH
-	 */
-	info1 |= usb_pipeendpoint(urb->pipe) << 8;
-	info1 |= usb_pipedevice(urb->pipe) << 0;
-
-	is_input = usb_pipein(urb->pipe);
-	type = usb_pipetype(urb->pipe);
-	ep = usb_pipe_endpoint(urb->dev, urb->pipe);
-	maxp = usb_endpoint_maxp(&ep->desc);
-	mult = usb_endpoint_maxp_mult(&ep->desc);
-
-	/* 1024 byte maxpacket is a hardware ceiling.  High bandwidth
-	 * acts like up to 3KB, but is built from smaller packets.
-	 */
-	if (maxp > 1024) {
-		fotg210_dbg(fotg210, "bogus qh maxpacket %d\n", maxp);
-		goto done;
-	}
-
-	/* Compute interrupt scheduling parameters just once, and save.
-	 * - allowing for high bandwidth, how many nsec/uframe are used?
-	 * - split transactions need a second CSPLIT uframe; same question
-	 * - splits also need a schedule gap (for full/low speed I/O)
-	 * - qh has a polling interval
-	 *
-	 * For control/bulk requests, the HC or TT handles these.
-	 */
-	if (type == PIPE_INTERRUPT) {
-		qh->usecs = NS_TO_US(usb_calc_bus_time(USB_SPEED_HIGH,
-				is_input, 0, mult * maxp));
-		qh->start = NO_FRAME;
-
-		if (urb->dev->speed == USB_SPEED_HIGH) {
-			qh->c_usecs = 0;
-			qh->gap_uf = 0;
-
-			qh->period = urb->interval >> 3;
-			if (qh->period == 0 && urb->interval != 1) {
-				/* NOTE interval 2 or 4 uframes could work.
-				 * But interval 1 scheduling is simpler, and
-				 * includes high bandwidth.
-				 */
-				urb->interval = 1;
-			} else if (qh->period > fotg210->periodic_size) {
-				qh->period = fotg210->periodic_size;
-				urb->interval = qh->period << 3;
-			}
-		} else {
-			int think_time;
-
-			/* gap is f(FS/LS transfer times) */
-			qh->gap_uf = 1 + usb_calc_bus_time(urb->dev->speed,
-					is_input, 0, maxp) / (125 * 1000);
-
-			/* FIXME this just approximates SPLIT/CSPLIT times */
-			if (is_input) {		/* SPLIT, gap, CSPLIT+DATA */
-				qh->c_usecs = qh->usecs + HS_USECS(0);
-				qh->usecs = HS_USECS(1);
-			} else {		/* SPLIT+DATA, gap, CSPLIT */
-				qh->usecs += HS_USECS(1);
-				qh->c_usecs = HS_USECS(0);
-			}
-
-			think_time = tt ? tt->think_time : 0;
-			qh->tt_usecs = NS_TO_US(think_time +
-					usb_calc_bus_time(urb->dev->speed,
-					is_input, 0, maxp));
-			qh->period = urb->interval;
-			if (qh->period > fotg210->periodic_size) {
-				qh->period = fotg210->periodic_size;
-				urb->interval = qh->period;
-			}
-		}
-	}
-
-	/* support for tt scheduling, and access to toggles */
-	qh->dev = urb->dev;
-
-	/* using TT? */
-	switch (urb->dev->speed) {
-	case USB_SPEED_LOW:
-		info1 |= QH_LOW_SPEED;
-		fallthrough;
-
-	case USB_SPEED_FULL:
-		/* EPS 0 means "full" */
-		if (type != PIPE_INTERRUPT)
-			info1 |= (FOTG210_TUNE_RL_TT << 28);
-		if (type == PIPE_CONTROL) {
-			info1 |= QH_CONTROL_EP;		/* for TT */
-			info1 |= QH_TOGGLE_CTL;		/* toggle from qtd */
-		}
-		info1 |= maxp << 16;
-
-		info2 |= (FOTG210_TUNE_MULT_TT << 30);
-
-		/* Some Freescale processors have an erratum in which the
-		 * port number in the queue head was 0..N-1 instead of 1..N.
-		 */
-		if (fotg210_has_fsl_portno_bug(fotg210))
-			info2 |= (urb->dev->ttport-1) << 23;
-		else
-			info2 |= urb->dev->ttport << 23;
-
-		/* set the address of the TT; for TDI's integrated
-		 * root hub tt, leave it zeroed.
-		 */
-		if (tt && tt->hub != fotg210_to_hcd(fotg210)->self.root_hub)
-			info2 |= tt->hub->devnum << 16;
-
-		/* NOTE:  if (PIPE_INTERRUPT) { scheduler sets c-mask } */
-
-		break;
-
-	case USB_SPEED_HIGH:		/* no TT involved */
-		info1 |= QH_HIGH_SPEED;
-		if (type == PIPE_CONTROL) {
-			info1 |= (FOTG210_TUNE_RL_HS << 28);
-			info1 |= 64 << 16;	/* usb2 fixed maxpacket */
-			info1 |= QH_TOGGLE_CTL;	/* toggle from qtd */
-			info2 |= (FOTG210_TUNE_MULT_HS << 30);
-		} else if (type == PIPE_BULK) {
-			info1 |= (FOTG210_TUNE_RL_HS << 28);
-			/* The USB spec says that high speed bulk endpoints
-			 * always use 512 byte maxpacket.  But some device
-			 * vendors decided to ignore that, and MSFT is happy
-			 * to help them do so.  So now people expect to use
-			 * such nonconformant devices with Linux too; sigh.
-			 */
-			info1 |= maxp << 16;
-			info2 |= (FOTG210_TUNE_MULT_HS << 30);
-		} else {		/* PIPE_INTERRUPT */
-			info1 |= maxp << 16;
-			info2 |= mult << 30;
-		}
-		break;
-	default:
-		fotg210_dbg(fotg210, "bogus dev %p speed %d\n", urb->dev,
-				urb->dev->speed);
-done:
-		qh_destroy(fotg210, qh);
-		return NULL;
-	}
-
-	/* NOTE:  if (PIPE_INTERRUPT) { scheduler sets s-mask } */
-
-	/* init as live, toggle clear, advance to dummy */
-	qh->qh_state = QH_STATE_IDLE;
-	hw = qh->hw;
-	hw->hw_info1 = cpu_to_hc32(fotg210, info1);
-	hw->hw_info2 = cpu_to_hc32(fotg210, info2);
-	qh->is_out = !is_input;
-	usb_settoggle(urb->dev, usb_pipeendpoint(urb->pipe), !is_input, 1);
-	qh_refresh(fotg210, qh);
-	return qh;
-}
-
-static void enable_async(struct fotg210_hcd *fotg210)
-{
-	if (fotg210->async_count++)
-		return;
-
-	/* Stop waiting to turn off the async schedule */
-	fotg210->enabled_hrtimer_events &= ~BIT(FOTG210_HRTIMER_DISABLE_ASYNC);
-
-	/* Don't start the schedule until ASS is 0 */
-	fotg210_poll_ASS(fotg210);
-	turn_on_io_watchdog(fotg210);
-}
-
-static void disable_async(struct fotg210_hcd *fotg210)
-{
-	if (--fotg210->async_count)
-		return;
-
-	/* The async schedule and async_unlink list are supposed to be empty */
-	WARN_ON(fotg210->async->qh_next.qh || fotg210->async_unlink);
-
-	/* Don't turn off the schedule until ASS is 1 */
-	fotg210_poll_ASS(fotg210);
-}
-
-/* move qh (and its qtds) onto async queue; maybe enable queue.  */
-
-static void qh_link_async(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
-{
-	__hc32 dma = QH_NEXT(fotg210, qh->qh_dma);
-	struct fotg210_qh *head;
-
-	/* Don't link a QH if there's a Clear-TT-Buffer pending */
-	if (unlikely(qh->clearing_tt))
-		return;
-
-	WARN_ON(qh->qh_state != QH_STATE_IDLE);
-
-	/* clear halt and/or toggle; and maybe recover from silicon quirk */
-	qh_refresh(fotg210, qh);
-
-	/* splice right after start */
-	head = fotg210->async;
-	qh->qh_next = head->qh_next;
-	qh->hw->hw_next = head->hw->hw_next;
-	wmb();
-
-	head->qh_next.qh = qh;
-	head->hw->hw_next = dma;
-
-	qh->xacterrs = 0;
-	qh->qh_state = QH_STATE_LINKED;
-	/* qtd completions reported later by interrupt */
-
-	enable_async(fotg210);
-}
-
-/* For control/bulk/interrupt, return QH with these TDs appended.
- * Allocates and initializes the QH if necessary.
- * Returns null if it can't allocate a QH it needs to.
- * If the QH has TDs (urbs) already, that's great.
- */
-static struct fotg210_qh *qh_append_tds(struct fotg210_hcd *fotg210,
-		struct urb *urb, struct list_head *qtd_list,
-		int epnum, void **ptr)
-{
-	struct fotg210_qh *qh = NULL;
-	__hc32 qh_addr_mask = cpu_to_hc32(fotg210, 0x7f);
-
-	qh = (struct fotg210_qh *) *ptr;
-	if (unlikely(qh == NULL)) {
-		/* can't sleep here, we have fotg210->lock... */
-		qh = qh_make(fotg210, urb, GFP_ATOMIC);
-		*ptr = qh;
-	}
-	if (likely(qh != NULL)) {
-		struct fotg210_qtd *qtd;
-
-		if (unlikely(list_empty(qtd_list)))
-			qtd = NULL;
-		else
-			qtd = list_entry(qtd_list->next, struct fotg210_qtd,
-					qtd_list);
-
-		/* control qh may need patching ... */
-		if (unlikely(epnum == 0)) {
-			/* usb_reset_device() briefly reverts to address 0 */
-			if (usb_pipedevice(urb->pipe) == 0)
-				qh->hw->hw_info1 &= ~qh_addr_mask;
-		}
-
-		/* just one way to queue requests: swap with the dummy qtd.
-		 * only hc or qh_refresh() ever modify the overlay.
-		 */
-		if (likely(qtd != NULL)) {
-			struct fotg210_qtd *dummy;
-			dma_addr_t dma;
-			__hc32 token;
-
-			/* to avoid racing the HC, use the dummy td instead of
-			 * the first td of our list (becomes new dummy).  both
-			 * tds stay deactivated until we're done, when the
-			 * HC is allowed to fetch the old dummy (4.10.2).
-			 */
-			token = qtd->hw_token;
-			qtd->hw_token = HALT_BIT(fotg210);
-
-			dummy = qh->dummy;
-
-			dma = dummy->qtd_dma;
-			*dummy = *qtd;
-			dummy->qtd_dma = dma;
-
-			list_del(&qtd->qtd_list);
-			list_add(&dummy->qtd_list, qtd_list);
-			list_splice_tail(qtd_list, &qh->qtd_list);
-
-			fotg210_qtd_init(fotg210, qtd, qtd->qtd_dma);
-			qh->dummy = qtd;
-
-			/* hc must see the new dummy at list end */
-			dma = qtd->qtd_dma;
-			qtd = list_entry(qh->qtd_list.prev,
-					struct fotg210_qtd, qtd_list);
-			qtd->hw_next = QTD_NEXT(fotg210, dma);
-
-			/* let the hc process these next qtds */
-			wmb();
-			dummy->hw_token = token;
-
-			urb->hcpriv = qh;
-		}
-	}
-	return qh;
-}
-
-static int submit_async(struct fotg210_hcd *fotg210, struct urb *urb,
-		struct list_head *qtd_list, gfp_t mem_flags)
-{
-	int epnum;
-	unsigned long flags;
-	struct fotg210_qh *qh = NULL;
-	int rc;
-
-	epnum = urb->ep->desc.bEndpointAddress;
-
-#ifdef FOTG210_URB_TRACE
-	{
-		struct fotg210_qtd *qtd;
-
-		qtd = list_entry(qtd_list->next, struct fotg210_qtd, qtd_list);
-		fotg210_dbg(fotg210,
-				"%s %s urb %p ep%d%s len %d, qtd %p [qh %p]\n",
-				__func__, urb->dev->devpath, urb,
-				epnum & 0x0f, (epnum & USB_DIR_IN)
-					? "in" : "out",
-				urb->transfer_buffer_length,
-				qtd, urb->ep->hcpriv);
-	}
-#endif
-
-	spin_lock_irqsave(&fotg210->lock, flags);
-	if (unlikely(!HCD_HW_ACCESSIBLE(fotg210_to_hcd(fotg210)))) {
-		rc = -ESHUTDOWN;
-		goto done;
-	}
-	rc = usb_hcd_link_urb_to_ep(fotg210_to_hcd(fotg210), urb);
-	if (unlikely(rc))
-		goto done;
-
-	qh = qh_append_tds(fotg210, urb, qtd_list, epnum, &urb->ep->hcpriv);
-	if (unlikely(qh == NULL)) {
-		usb_hcd_unlink_urb_from_ep(fotg210_to_hcd(fotg210), urb);
-		rc = -ENOMEM;
-		goto done;
-	}
-
-	/* Control/bulk operations through TTs don't need scheduling,
-	 * the HC and TT handle it when the TT has a buffer ready.
-	 */
-	if (likely(qh->qh_state == QH_STATE_IDLE))
-		qh_link_async(fotg210, qh);
-done:
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-	if (unlikely(qh == NULL))
-		qtd_list_free(fotg210, urb, qtd_list);
-	return rc;
-}
-
-static void single_unlink_async(struct fotg210_hcd *fotg210,
-		struct fotg210_qh *qh)
-{
-	struct fotg210_qh *prev;
-
-	/* Add to the end of the list of QHs waiting for the next IAAD */
-	qh->qh_state = QH_STATE_UNLINK;
-	if (fotg210->async_unlink)
-		fotg210->async_unlink_last->unlink_next = qh;
-	else
-		fotg210->async_unlink = qh;
-	fotg210->async_unlink_last = qh;
-
-	/* Unlink it from the schedule */
-	prev = fotg210->async;
-	while (prev->qh_next.qh != qh)
-		prev = prev->qh_next.qh;
-
-	prev->hw->hw_next = qh->hw->hw_next;
-	prev->qh_next = qh->qh_next;
-	if (fotg210->qh_scan_next == qh)
-		fotg210->qh_scan_next = qh->qh_next.qh;
-}
-
-static void start_iaa_cycle(struct fotg210_hcd *fotg210, bool nested)
-{
-	/*
-	 * Do nothing if an IAA cycle is already running or
-	 * if one will be started shortly.
-	 */
-	if (fotg210->async_iaa || fotg210->async_unlinking)
-		return;
-
-	/* Do all the waiting QHs at once */
-	fotg210->async_iaa = fotg210->async_unlink;
-	fotg210->async_unlink = NULL;
-
-	/* If the controller isn't running, we don't have to wait for it */
-	if (unlikely(fotg210->rh_state < FOTG210_RH_RUNNING)) {
-		if (!nested)		/* Avoid recursion */
-			end_unlink_async(fotg210);
-
-	/* Otherwise start a new IAA cycle */
-	} else if (likely(fotg210->rh_state == FOTG210_RH_RUNNING)) {
-		/* Make sure the unlinks are all visible to the hardware */
-		wmb();
-
-		fotg210_writel(fotg210, fotg210->command | CMD_IAAD,
-				&fotg210->regs->command);
-		fotg210_readl(fotg210, &fotg210->regs->command);
-		fotg210_enable_event(fotg210, FOTG210_HRTIMER_IAA_WATCHDOG,
-				true);
-	}
-}
-
-/* the async qh for the qtds being unlinked are now gone from the HC */
-
-static void end_unlink_async(struct fotg210_hcd *fotg210)
-{
-	struct fotg210_qh *qh;
-
-	/* Process the idle QHs */
-restart:
-	fotg210->async_unlinking = true;
-	while (fotg210->async_iaa) {
-		qh = fotg210->async_iaa;
-		fotg210->async_iaa = qh->unlink_next;
-		qh->unlink_next = NULL;
-
-		qh->qh_state = QH_STATE_IDLE;
-		qh->qh_next.qh = NULL;
-
-		qh_completions(fotg210, qh);
-		if (!list_empty(&qh->qtd_list) &&
-				fotg210->rh_state == FOTG210_RH_RUNNING)
-			qh_link_async(fotg210, qh);
-		disable_async(fotg210);
-	}
-	fotg210->async_unlinking = false;
-
-	/* Start a new IAA cycle if any QHs are waiting for it */
-	if (fotg210->async_unlink) {
-		start_iaa_cycle(fotg210, true);
-		if (unlikely(fotg210->rh_state < FOTG210_RH_RUNNING))
-			goto restart;
-	}
-}
-
-static void unlink_empty_async(struct fotg210_hcd *fotg210)
-{
-	struct fotg210_qh *qh, *next;
-	bool stopped = (fotg210->rh_state < FOTG210_RH_RUNNING);
-	bool check_unlinks_later = false;
-
-	/* Unlink all the async QHs that have been empty for a timer cycle */
-	next = fotg210->async->qh_next.qh;
-	while (next) {
-		qh = next;
-		next = qh->qh_next.qh;
-
-		if (list_empty(&qh->qtd_list) &&
-				qh->qh_state == QH_STATE_LINKED) {
-			if (!stopped && qh->unlink_cycle ==
-					fotg210->async_unlink_cycle)
-				check_unlinks_later = true;
-			else
-				single_unlink_async(fotg210, qh);
-		}
-	}
-
-	/* Start a new IAA cycle if any QHs are waiting for it */
-	if (fotg210->async_unlink)
-		start_iaa_cycle(fotg210, false);
-
-	/* QHs that haven't been empty for long enough will be handled later */
-	if (check_unlinks_later) {
-		fotg210_enable_event(fotg210, FOTG210_HRTIMER_ASYNC_UNLINKS,
-				true);
-		++fotg210->async_unlink_cycle;
-	}
-}
-
-/* makes sure the async qh will become idle */
-/* caller must own fotg210->lock */
-
-static void start_unlink_async(struct fotg210_hcd *fotg210,
-		struct fotg210_qh *qh)
-{
-	/*
-	 * If the QH isn't linked then there's nothing we can do
-	 * unless we were called during a giveback, in which case
-	 * qh_completions() has to deal with it.
-	 */
-	if (qh->qh_state != QH_STATE_LINKED) {
-		if (qh->qh_state == QH_STATE_COMPLETING)
-			qh->needs_rescan = 1;
-		return;
-	}
-
-	single_unlink_async(fotg210, qh);
-	start_iaa_cycle(fotg210, false);
-}
-
-static void scan_async(struct fotg210_hcd *fotg210)
-{
-	struct fotg210_qh *qh;
-	bool check_unlinks_later = false;
-
-	fotg210->qh_scan_next = fotg210->async->qh_next.qh;
-	while (fotg210->qh_scan_next) {
-		qh = fotg210->qh_scan_next;
-		fotg210->qh_scan_next = qh->qh_next.qh;
-rescan:
-		/* clean any finished work for this qh */
-		if (!list_empty(&qh->qtd_list)) {
-			int temp;
-
-			/*
-			 * Unlinks could happen here; completion reporting
-			 * drops the lock.  That's why fotg210->qh_scan_next
-			 * always holds the next qh to scan; if the next qh
-			 * gets unlinked then fotg210->qh_scan_next is adjusted
-			 * in single_unlink_async().
-			 */
-			temp = qh_completions(fotg210, qh);
-			if (qh->needs_rescan) {
-				start_unlink_async(fotg210, qh);
-			} else if (list_empty(&qh->qtd_list)
-					&& qh->qh_state == QH_STATE_LINKED) {
-				qh->unlink_cycle = fotg210->async_unlink_cycle;
-				check_unlinks_later = true;
-			} else if (temp != 0)
-				goto rescan;
-		}
-	}
-
-	/*
-	 * Unlink empty entries, reducing DMA usage as well
-	 * as HCD schedule-scanning costs.  Delay for any qh
-	 * we just scanned, there's a not-unusual case that it
-	 * doesn't stay idle for long.
-	 */
-	if (check_unlinks_later && fotg210->rh_state == FOTG210_RH_RUNNING &&
-			!(fotg210->enabled_hrtimer_events &
-			BIT(FOTG210_HRTIMER_ASYNC_UNLINKS))) {
-		fotg210_enable_event(fotg210,
-				FOTG210_HRTIMER_ASYNC_UNLINKS, true);
-		++fotg210->async_unlink_cycle;
-	}
-}
-/* EHCI scheduled transaction support:  interrupt, iso, split iso
- * These are called "periodic" transactions in the EHCI spec.
- *
- * Note that for interrupt transfers, the QH/QTD manipulation is shared
- * with the "asynchronous" transaction support (control/bulk transfers).
- * The only real difference is in how interrupt transfers are scheduled.
- *
- * For ISO, we make an "iso_stream" head to serve the same role as a QH.
- * It keeps track of every ITD (or SITD) that's linked, and holds enough
- * pre-calculated schedule data to make appending to the queue be quick.
- */
-static int fotg210_get_frame(struct usb_hcd *hcd);
-
-/* periodic_next_shadow - return "next" pointer on shadow list
- * @periodic: host pointer to qh/itd
- * @tag: hardware tag for type of this record
- */
-static union fotg210_shadow *periodic_next_shadow(struct fotg210_hcd *fotg210,
-		union fotg210_shadow *periodic, __hc32 tag)
-{
-	switch (hc32_to_cpu(fotg210, tag)) {
-	case Q_TYPE_QH:
-		return &periodic->qh->qh_next;
-	case Q_TYPE_FSTN:
-		return &periodic->fstn->fstn_next;
-	default:
-		return &periodic->itd->itd_next;
-	}
-}
-
-static __hc32 *shadow_next_periodic(struct fotg210_hcd *fotg210,
-		union fotg210_shadow *periodic, __hc32 tag)
-{
-	switch (hc32_to_cpu(fotg210, tag)) {
-	/* our fotg210_shadow.qh is actually software part */
-	case Q_TYPE_QH:
-		return &periodic->qh->hw->hw_next;
-	/* others are hw parts */
-	default:
-		return periodic->hw_next;
-	}
-}
-
-/* caller must hold fotg210->lock */
-static void periodic_unlink(struct fotg210_hcd *fotg210, unsigned frame,
-		void *ptr)
-{
-	union fotg210_shadow *prev_p = &fotg210->pshadow[frame];
-	__hc32 *hw_p = &fotg210->periodic[frame];
-	union fotg210_shadow here = *prev_p;
-
-	/* find predecessor of "ptr"; hw and shadow lists are in sync */
-	while (here.ptr && here.ptr != ptr) {
-		prev_p = periodic_next_shadow(fotg210, prev_p,
-				Q_NEXT_TYPE(fotg210, *hw_p));
-		hw_p = shadow_next_periodic(fotg210, &here,
-				Q_NEXT_TYPE(fotg210, *hw_p));
-		here = *prev_p;
-	}
-	/* an interrupt entry (at list end) could have been shared */
-	if (!here.ptr)
-		return;
-
-	/* update shadow and hardware lists ... the old "next" pointers
-	 * from ptr may still be in use, the caller updates them.
-	 */
-	*prev_p = *periodic_next_shadow(fotg210, &here,
-			Q_NEXT_TYPE(fotg210, *hw_p));
-
-	*hw_p = *shadow_next_periodic(fotg210, &here,
-			Q_NEXT_TYPE(fotg210, *hw_p));
-}
-
-/* how many of the uframe's 125 usecs are allocated? */
-static unsigned short periodic_usecs(struct fotg210_hcd *fotg210,
-		unsigned frame, unsigned uframe)
-{
-	__hc32 *hw_p = &fotg210->periodic[frame];
-	union fotg210_shadow *q = &fotg210->pshadow[frame];
-	unsigned usecs = 0;
-	struct fotg210_qh_hw *hw;
-
-	while (q->ptr) {
-		switch (hc32_to_cpu(fotg210, Q_NEXT_TYPE(fotg210, *hw_p))) {
-		case Q_TYPE_QH:
-			hw = q->qh->hw;
-			/* is it in the S-mask? */
-			if (hw->hw_info2 & cpu_to_hc32(fotg210, 1 << uframe))
-				usecs += q->qh->usecs;
-			/* ... or C-mask? */
-			if (hw->hw_info2 & cpu_to_hc32(fotg210,
-					1 << (8 + uframe)))
-				usecs += q->qh->c_usecs;
-			hw_p = &hw->hw_next;
-			q = &q->qh->qh_next;
-			break;
-		/* case Q_TYPE_FSTN: */
-		default:
-			/* for "save place" FSTNs, count the relevant INTR
-			 * bandwidth from the previous frame
-			 */
-			if (q->fstn->hw_prev != FOTG210_LIST_END(fotg210))
-				fotg210_dbg(fotg210, "ignoring FSTN cost ...\n");
-
-			hw_p = &q->fstn->hw_next;
-			q = &q->fstn->fstn_next;
-			break;
-		case Q_TYPE_ITD:
-			if (q->itd->hw_transaction[uframe])
-				usecs += q->itd->stream->usecs;
-			hw_p = &q->itd->hw_next;
-			q = &q->itd->itd_next;
-			break;
-		}
-	}
-	if (usecs > fotg210->uframe_periodic_max)
-		fotg210_err(fotg210, "uframe %d sched overrun: %d usecs\n",
-				frame * 8 + uframe, usecs);
-	return usecs;
-}
-
-static int same_tt(struct usb_device *dev1, struct usb_device *dev2)
-{
-	if (!dev1->tt || !dev2->tt)
-		return 0;
-	if (dev1->tt != dev2->tt)
-		return 0;
-	if (dev1->tt->multi)
-		return dev1->ttport == dev2->ttport;
-	else
-		return 1;
-}
-
-/* return true iff the device's transaction translator is available
- * for a periodic transfer starting at the specified frame, using
- * all the uframes in the mask.
- */
-static int tt_no_collision(struct fotg210_hcd *fotg210, unsigned period,
-		struct usb_device *dev, unsigned frame, u32 uf_mask)
-{
-	if (period == 0)	/* error */
-		return 0;
-
-	/* note bandwidth wastage:  split never follows csplit
-	 * (different dev or endpoint) until the next uframe.
-	 * calling convention doesn't make that distinction.
-	 */
-	for (; frame < fotg210->periodic_size; frame += period) {
-		union fotg210_shadow here;
-		__hc32 type;
-		struct fotg210_qh_hw *hw;
-
-		here = fotg210->pshadow[frame];
-		type = Q_NEXT_TYPE(fotg210, fotg210->periodic[frame]);
-		while (here.ptr) {
-			switch (hc32_to_cpu(fotg210, type)) {
-			case Q_TYPE_ITD:
-				type = Q_NEXT_TYPE(fotg210, here.itd->hw_next);
-				here = here.itd->itd_next;
-				continue;
-			case Q_TYPE_QH:
-				hw = here.qh->hw;
-				if (same_tt(dev, here.qh->dev)) {
-					u32 mask;
-
-					mask = hc32_to_cpu(fotg210,
-							hw->hw_info2);
-					/* "knows" no gap is needed */
-					mask |= mask >> 8;
-					if (mask & uf_mask)
-						break;
-				}
-				type = Q_NEXT_TYPE(fotg210, hw->hw_next);
-				here = here.qh->qh_next;
-				continue;
-			/* case Q_TYPE_FSTN: */
-			default:
-				fotg210_dbg(fotg210,
-						"periodic frame %d bogus type %d\n",
-						frame, type);
-			}
-
-			/* collision or error */
-			return 0;
-		}
-	}
-
-	/* no collision */
-	return 1;
-}
-
-static void enable_periodic(struct fotg210_hcd *fotg210)
-{
-	if (fotg210->periodic_count++)
-		return;
-
-	/* Stop waiting to turn off the periodic schedule */
-	fotg210->enabled_hrtimer_events &=
-		~BIT(FOTG210_HRTIMER_DISABLE_PERIODIC);
-
-	/* Don't start the schedule until PSS is 0 */
-	fotg210_poll_PSS(fotg210);
-	turn_on_io_watchdog(fotg210);
-}
-
-static void disable_periodic(struct fotg210_hcd *fotg210)
-{
-	if (--fotg210->periodic_count)
-		return;
-
-	/* Don't turn off the schedule until PSS is 1 */
-	fotg210_poll_PSS(fotg210);
-}
-
-/* periodic schedule slots have iso tds (normal or split) first, then a
- * sparse tree for active interrupt transfers.
- *
- * this just links in a qh; caller guarantees uframe masks are set right.
- * no FSTN support (yet; fotg210 0.96+)
- */
-static void qh_link_periodic(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
-{
-	unsigned i;
-	unsigned period = qh->period;
-
-	dev_dbg(&qh->dev->dev,
-			"link qh%d-%04x/%p start %d [%d/%d us]\n", period,
-			hc32_to_cpup(fotg210, &qh->hw->hw_info2) &
-			(QH_CMASK | QH_SMASK), qh, qh->start, qh->usecs,
-			qh->c_usecs);
-
-	/* high bandwidth, or otherwise every microframe */
-	if (period == 0)
-		period = 1;
-
-	for (i = qh->start; i < fotg210->periodic_size; i += period) {
-		union fotg210_shadow *prev = &fotg210->pshadow[i];
-		__hc32 *hw_p = &fotg210->periodic[i];
-		union fotg210_shadow here = *prev;
-		__hc32 type = 0;
-
-		/* skip the iso nodes at list head */
-		while (here.ptr) {
-			type = Q_NEXT_TYPE(fotg210, *hw_p);
-			if (type == cpu_to_hc32(fotg210, Q_TYPE_QH))
-				break;
-			prev = periodic_next_shadow(fotg210, prev, type);
-			hw_p = shadow_next_periodic(fotg210, &here, type);
-			here = *prev;
-		}
-
-		/* sorting each branch by period (slow-->fast)
-		 * enables sharing interior tree nodes
-		 */
-		while (here.ptr && qh != here.qh) {
-			if (qh->period > here.qh->period)
-				break;
-			prev = &here.qh->qh_next;
-			hw_p = &here.qh->hw->hw_next;
-			here = *prev;
-		}
-		/* link in this qh, unless some earlier pass did that */
-		if (qh != here.qh) {
-			qh->qh_next = here;
-			if (here.qh)
-				qh->hw->hw_next = *hw_p;
-			wmb();
-			prev->qh = qh;
-			*hw_p = QH_NEXT(fotg210, qh->qh_dma);
-		}
-	}
-	qh->qh_state = QH_STATE_LINKED;
-	qh->xacterrs = 0;
-
-	/* update per-qh bandwidth for usbfs */
-	fotg210_to_hcd(fotg210)->self.bandwidth_allocated += qh->period
-		? ((qh->usecs + qh->c_usecs) / qh->period)
-		: (qh->usecs * 8);
-
-	list_add(&qh->intr_node, &fotg210->intr_qh_list);
-
-	/* maybe enable periodic schedule processing */
-	++fotg210->intr_count;
-	enable_periodic(fotg210);
-}
-
-static void qh_unlink_periodic(struct fotg210_hcd *fotg210,
-		struct fotg210_qh *qh)
-{
-	unsigned i;
-	unsigned period;
-
-	/*
-	 * If qh is for a low/full-speed device, simply unlinking it
-	 * could interfere with an ongoing split transaction.  To unlink
-	 * it safely would require setting the QH_INACTIVATE bit and
-	 * waiting at least one frame, as described in EHCI 4.12.2.5.
-	 *
-	 * We won't bother with any of this.  Instead, we assume that the
-	 * only reason for unlinking an interrupt QH while the current URB
-	 * is still active is to dequeue all the URBs (flush the whole
-	 * endpoint queue).
-	 *
-	 * If rebalancing the periodic schedule is ever implemented, this
-	 * approach will no longer be valid.
-	 */
-
-	/* high bandwidth, or otherwise part of every microframe */
-	period = qh->period;
-	if (!period)
-		period = 1;
-
-	for (i = qh->start; i < fotg210->periodic_size; i += period)
-		periodic_unlink(fotg210, i, qh);
-
-	/* update per-qh bandwidth for usbfs */
-	fotg210_to_hcd(fotg210)->self.bandwidth_allocated -= qh->period
-		? ((qh->usecs + qh->c_usecs) / qh->period)
-		: (qh->usecs * 8);
-
-	dev_dbg(&qh->dev->dev,
-			"unlink qh%d-%04x/%p start %d [%d/%d us]\n",
-			qh->period, hc32_to_cpup(fotg210, &qh->hw->hw_info2) &
-			(QH_CMASK | QH_SMASK), qh, qh->start, qh->usecs,
-			qh->c_usecs);
-
-	/* qh->qh_next still "live" to HC */
-	qh->qh_state = QH_STATE_UNLINK;
-	qh->qh_next.ptr = NULL;
-
-	if (fotg210->qh_scan_next == qh)
-		fotg210->qh_scan_next = list_entry(qh->intr_node.next,
-				struct fotg210_qh, intr_node);
-	list_del(&qh->intr_node);
-}
-
-static void start_unlink_intr(struct fotg210_hcd *fotg210,
-		struct fotg210_qh *qh)
-{
-	/* If the QH isn't linked then there's nothing we can do
-	 * unless we were called during a giveback, in which case
-	 * qh_completions() has to deal with it.
-	 */
-	if (qh->qh_state != QH_STATE_LINKED) {
-		if (qh->qh_state == QH_STATE_COMPLETING)
-			qh->needs_rescan = 1;
-		return;
-	}
-
-	qh_unlink_periodic(fotg210, qh);
-
-	/* Make sure the unlinks are visible before starting the timer */
-	wmb();
-
-	/*
-	 * The EHCI spec doesn't say how long it takes the controller to
-	 * stop accessing an unlinked interrupt QH.  The timer delay is
-	 * 9 uframes; presumably that will be long enough.
-	 */
-	qh->unlink_cycle = fotg210->intr_unlink_cycle;
-
-	/* New entries go at the end of the intr_unlink list */
-	if (fotg210->intr_unlink)
-		fotg210->intr_unlink_last->unlink_next = qh;
-	else
-		fotg210->intr_unlink = qh;
-	fotg210->intr_unlink_last = qh;
-
-	if (fotg210->intr_unlinking)
-		;	/* Avoid recursive calls */
-	else if (fotg210->rh_state < FOTG210_RH_RUNNING)
-		fotg210_handle_intr_unlinks(fotg210);
-	else if (fotg210->intr_unlink == qh) {
-		fotg210_enable_event(fotg210, FOTG210_HRTIMER_UNLINK_INTR,
-				true);
-		++fotg210->intr_unlink_cycle;
-	}
-}
-
-static void end_unlink_intr(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
-{
-	struct fotg210_qh_hw *hw = qh->hw;
-	int rc;
-
-	qh->qh_state = QH_STATE_IDLE;
-	hw->hw_next = FOTG210_LIST_END(fotg210);
-
-	qh_completions(fotg210, qh);
-
-	/* reschedule QH iff another request is queued */
-	if (!list_empty(&qh->qtd_list) &&
-			fotg210->rh_state == FOTG210_RH_RUNNING) {
-		rc = qh_schedule(fotg210, qh);
-
-		/* An error here likely indicates handshake failure
-		 * or no space left in the schedule.  Neither fault
-		 * should happen often ...
-		 *
-		 * FIXME kill the now-dysfunctional queued urbs
-		 */
-		if (rc != 0)
-			fotg210_err(fotg210, "can't reschedule qh %p, err %d\n",
-					qh, rc);
-	}
-
-	/* maybe turn off periodic schedule */
-	--fotg210->intr_count;
-	disable_periodic(fotg210);
-}
-
-static int check_period(struct fotg210_hcd *fotg210, unsigned frame,
-		unsigned uframe, unsigned period, unsigned usecs)
-{
-	int claimed;
-
-	/* complete split running into next frame?
-	 * given FSTN support, we could sometimes check...
-	 */
-	if (uframe >= 8)
-		return 0;
-
-	/* convert "usecs we need" to "max already claimed" */
-	usecs = fotg210->uframe_periodic_max - usecs;
-
-	/* we "know" 2 and 4 uframe intervals were rejected; so
-	 * for period 0, check _every_ microframe in the schedule.
-	 */
-	if (unlikely(period == 0)) {
-		do {
-			for (uframe = 0; uframe < 7; uframe++) {
-				claimed = periodic_usecs(fotg210, frame,
-						uframe);
-				if (claimed > usecs)
-					return 0;
-			}
-		} while ((frame += 1) < fotg210->periodic_size);
-
-	/* just check the specified uframe, at that period */
-	} else {
-		do {
-			claimed = periodic_usecs(fotg210, frame, uframe);
-			if (claimed > usecs)
-				return 0;
-		} while ((frame += period) < fotg210->periodic_size);
-	}
-
-	/* success! */
-	return 1;
-}
-
-static int check_intr_schedule(struct fotg210_hcd *fotg210, unsigned frame,
-		unsigned uframe, const struct fotg210_qh *qh, __hc32 *c_maskp)
-{
-	int retval = -ENOSPC;
-	u8 mask = 0;
-
-	if (qh->c_usecs && uframe >= 6)		/* FSTN territory? */
-		goto done;
-
-	if (!check_period(fotg210, frame, uframe, qh->period, qh->usecs))
-		goto done;
-	if (!qh->c_usecs) {
-		retval = 0;
-		*c_maskp = 0;
-		goto done;
-	}
-
-	/* Make sure this tt's buffer is also available for CSPLITs.
-	 * We pessimize a bit; probably the typical full speed case
-	 * doesn't need the second CSPLIT.
-	 *
-	 * NOTE:  both SPLIT and CSPLIT could be checked in just
-	 * one smart pass...
-	 */
-	mask = 0x03 << (uframe + qh->gap_uf);
-	*c_maskp = cpu_to_hc32(fotg210, mask << 8);
-
-	mask |= 1 << uframe;
-	if (tt_no_collision(fotg210, qh->period, qh->dev, frame, mask)) {
-		if (!check_period(fotg210, frame, uframe + qh->gap_uf + 1,
-				qh->period, qh->c_usecs))
-			goto done;
-		if (!check_period(fotg210, frame, uframe + qh->gap_uf,
-				qh->period, qh->c_usecs))
-			goto done;
-		retval = 0;
-	}
-done:
-	return retval;
-}
-
-/* "first fit" scheduling policy used the first time through,
- * or when the previous schedule slot can't be re-used.
- */
-static int qh_schedule(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
-{
-	int status;
-	unsigned uframe;
-	__hc32 c_mask;
-	unsigned frame;	/* 0..(qh->period - 1), or NO_FRAME */
-	struct fotg210_qh_hw *hw = qh->hw;
-
-	qh_refresh(fotg210, qh);
-	hw->hw_next = FOTG210_LIST_END(fotg210);
-	frame = qh->start;
-
-	/* reuse the previous schedule slots, if we can */
-	if (frame < qh->period) {
-		uframe = ffs(hc32_to_cpup(fotg210, &hw->hw_info2) & QH_SMASK);
-		status = check_intr_schedule(fotg210, frame, --uframe,
-				qh, &c_mask);
-	} else {
-		uframe = 0;
-		c_mask = 0;
-		status = -ENOSPC;
-	}
-
-	/* else scan the schedule to find a group of slots such that all
-	 * uframes have enough periodic bandwidth available.
-	 */
-	if (status) {
-		/* "normal" case, uframing flexible except with splits */
-		if (qh->period) {
-			int i;
-
-			for (i = qh->period; status && i > 0; --i) {
-				frame = ++fotg210->random_frame % qh->period;
-				for (uframe = 0; uframe < 8; uframe++) {
-					status = check_intr_schedule(fotg210,
-							frame, uframe, qh,
-							&c_mask);
-					if (status == 0)
-						break;
-				}
-			}
-
-		/* qh->period == 0 means every uframe */
-		} else {
-			frame = 0;
-			status = check_intr_schedule(fotg210, 0, 0, qh,
-					&c_mask);
-		}
-		if (status)
-			goto done;
-		qh->start = frame;
-
-		/* reset S-frame and (maybe) C-frame masks */
-		hw->hw_info2 &= cpu_to_hc32(fotg210, ~(QH_CMASK | QH_SMASK));
-		hw->hw_info2 |= qh->period
-			? cpu_to_hc32(fotg210, 1 << uframe)
-			: cpu_to_hc32(fotg210, QH_SMASK);
-		hw->hw_info2 |= c_mask;
-	} else
-		fotg210_dbg(fotg210, "reused qh %p schedule\n", qh);
-
-	/* stuff into the periodic schedule */
-	qh_link_periodic(fotg210, qh);
-done:
-	return status;
-}
-
-static int intr_submit(struct fotg210_hcd *fotg210, struct urb *urb,
-		struct list_head *qtd_list, gfp_t mem_flags)
-{
-	unsigned epnum;
-	unsigned long flags;
-	struct fotg210_qh *qh;
-	int status;
-	struct list_head empty;
-
-	/* get endpoint and transfer/schedule data */
-	epnum = urb->ep->desc.bEndpointAddress;
-
-	spin_lock_irqsave(&fotg210->lock, flags);
-
-	if (unlikely(!HCD_HW_ACCESSIBLE(fotg210_to_hcd(fotg210)))) {
-		status = -ESHUTDOWN;
-		goto done_not_linked;
-	}
-	status = usb_hcd_link_urb_to_ep(fotg210_to_hcd(fotg210), urb);
-	if (unlikely(status))
-		goto done_not_linked;
-
-	/* get qh and force any scheduling errors */
-	INIT_LIST_HEAD(&empty);
-	qh = qh_append_tds(fotg210, urb, &empty, epnum, &urb->ep->hcpriv);
-	if (qh == NULL) {
-		status = -ENOMEM;
-		goto done;
-	}
-	if (qh->qh_state == QH_STATE_IDLE) {
-		status = qh_schedule(fotg210, qh);
-		if (status)
-			goto done;
-	}
-
-	/* then queue the urb's tds to the qh */
-	qh = qh_append_tds(fotg210, urb, qtd_list, epnum, &urb->ep->hcpriv);
-	BUG_ON(qh == NULL);
-
-	/* ... update usbfs periodic stats */
-	fotg210_to_hcd(fotg210)->self.bandwidth_int_reqs++;
-
-done:
-	if (unlikely(status))
-		usb_hcd_unlink_urb_from_ep(fotg210_to_hcd(fotg210), urb);
-done_not_linked:
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-	if (status)
-		qtd_list_free(fotg210, urb, qtd_list);
-
-	return status;
-}
-
-static void scan_intr(struct fotg210_hcd *fotg210)
-{
-	struct fotg210_qh *qh;
-
-	list_for_each_entry_safe(qh, fotg210->qh_scan_next,
-			&fotg210->intr_qh_list, intr_node) {
-rescan:
-		/* clean any finished work for this qh */
-		if (!list_empty(&qh->qtd_list)) {
-			int temp;
-
-			/*
-			 * Unlinks could happen here; completion reporting
-			 * drops the lock.  That's why fotg210->qh_scan_next
-			 * always holds the next qh to scan; if the next qh
-			 * gets unlinked then fotg210->qh_scan_next is adjusted
-			 * in qh_unlink_periodic().
-			 */
-			temp = qh_completions(fotg210, qh);
-			if (unlikely(qh->needs_rescan ||
-					(list_empty(&qh->qtd_list) &&
-					qh->qh_state == QH_STATE_LINKED)))
-				start_unlink_intr(fotg210, qh);
-			else if (temp != 0)
-				goto rescan;
-		}
-	}
-}
-
-/* fotg210_iso_stream ops work with both ITD and SITD */
-
-static struct fotg210_iso_stream *iso_stream_alloc(gfp_t mem_flags)
-{
-	struct fotg210_iso_stream *stream;
-
-	stream = kzalloc(sizeof(*stream), mem_flags);
-	if (likely(stream != NULL)) {
-		INIT_LIST_HEAD(&stream->td_list);
-		INIT_LIST_HEAD(&stream->free_list);
-		stream->next_uframe = -1;
-	}
-	return stream;
-}
-
-static void iso_stream_init(struct fotg210_hcd *fotg210,
-		struct fotg210_iso_stream *stream, struct usb_device *dev,
-		int pipe, unsigned interval)
-{
-	u32 buf1;
-	unsigned epnum, maxp;
-	int is_input;
-	long bandwidth;
-	unsigned multi;
-	struct usb_host_endpoint *ep;
-
-	/*
-	 * this might be a "high bandwidth" highspeed endpoint,
-	 * as encoded in the ep descriptor's wMaxPacket field
-	 */
-	epnum = usb_pipeendpoint(pipe);
-	is_input = usb_pipein(pipe) ? USB_DIR_IN : 0;
-	ep = usb_pipe_endpoint(dev, pipe);
-	maxp = usb_endpoint_maxp(&ep->desc);
-	if (is_input)
-		buf1 = (1 << 11);
-	else
-		buf1 = 0;
-
-	multi = usb_endpoint_maxp_mult(&ep->desc);
-	buf1 |= maxp;
-	maxp *= multi;
-
-	stream->buf0 = cpu_to_hc32(fotg210, (epnum << 8) | dev->devnum);
-	stream->buf1 = cpu_to_hc32(fotg210, buf1);
-	stream->buf2 = cpu_to_hc32(fotg210, multi);
-
-	/* usbfs wants to report the average usecs per frame tied up
-	 * when transfers on this endpoint are scheduled ...
-	 */
-	if (dev->speed == USB_SPEED_FULL) {
-		interval <<= 3;
-		stream->usecs = NS_TO_US(usb_calc_bus_time(dev->speed,
-				is_input, 1, maxp));
-		stream->usecs /= 8;
-	} else {
-		stream->highspeed = 1;
-		stream->usecs = HS_USECS_ISO(maxp);
-	}
-	bandwidth = stream->usecs * 8;
-	bandwidth /= interval;
-
-	stream->bandwidth = bandwidth;
-	stream->udev = dev;
-	stream->bEndpointAddress = is_input | epnum;
-	stream->interval = interval;
-	stream->maxp = maxp;
-}
-
-static struct fotg210_iso_stream *iso_stream_find(struct fotg210_hcd *fotg210,
-		struct urb *urb)
-{
-	unsigned epnum;
-	struct fotg210_iso_stream *stream;
-	struct usb_host_endpoint *ep;
-	unsigned long flags;
-
-	epnum = usb_pipeendpoint(urb->pipe);
-	if (usb_pipein(urb->pipe))
-		ep = urb->dev->ep_in[epnum];
-	else
-		ep = urb->dev->ep_out[epnum];
-
-	spin_lock_irqsave(&fotg210->lock, flags);
-	stream = ep->hcpriv;
-
-	if (unlikely(stream == NULL)) {
-		stream = iso_stream_alloc(GFP_ATOMIC);
-		if (likely(stream != NULL)) {
-			ep->hcpriv = stream;
-			stream->ep = ep;
-			iso_stream_init(fotg210, stream, urb->dev, urb->pipe,
-					urb->interval);
-		}
-
-	/* if dev->ep[epnum] is a QH, hw is set */
-	} else if (unlikely(stream->hw != NULL)) {
-		fotg210_dbg(fotg210, "dev %s ep%d%s, not iso??\n",
-				urb->dev->devpath, epnum,
-				usb_pipein(urb->pipe) ? "in" : "out");
-		stream = NULL;
-	}
-
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-	return stream;
-}
-
-/* fotg210_iso_sched ops can be ITD-only or SITD-only */
-
-static struct fotg210_iso_sched *iso_sched_alloc(unsigned packets,
-		gfp_t mem_flags)
-{
-	struct fotg210_iso_sched *iso_sched;
-
-	iso_sched = kzalloc(struct_size(iso_sched, packet, packets), mem_flags);
-	if (likely(iso_sched != NULL))
-		INIT_LIST_HEAD(&iso_sched->td_list);
-
-	return iso_sched;
-}
-
-static inline void itd_sched_init(struct fotg210_hcd *fotg210,
-		struct fotg210_iso_sched *iso_sched,
-		struct fotg210_iso_stream *stream, struct urb *urb)
-{
-	unsigned i;
-	dma_addr_t dma = urb->transfer_dma;
-
-	/* how many uframes are needed for these transfers */
-	iso_sched->span = urb->number_of_packets * stream->interval;
-
-	/* figure out per-uframe itd fields that we'll need later
-	 * when we fit new itds into the schedule.
-	 */
-	for (i = 0; i < urb->number_of_packets; i++) {
-		struct fotg210_iso_packet *uframe = &iso_sched->packet[i];
-		unsigned length;
-		dma_addr_t buf;
-		u32 trans;
-
-		length = urb->iso_frame_desc[i].length;
-		buf = dma + urb->iso_frame_desc[i].offset;
-
-		trans = FOTG210_ISOC_ACTIVE;
-		trans |= buf & 0x0fff;
-		if (unlikely(((i + 1) == urb->number_of_packets))
-				&& !(urb->transfer_flags & URB_NO_INTERRUPT))
-			trans |= FOTG210_ITD_IOC;
-		trans |= length << 16;
-		uframe->transaction = cpu_to_hc32(fotg210, trans);
-
-		/* might need to cross a buffer page within a uframe */
-		uframe->bufp = (buf & ~(u64)0x0fff);
-		buf += length;
-		if (unlikely((uframe->bufp != (buf & ~(u64)0x0fff))))
-			uframe->cross = 1;
-	}
-}
-
-static void iso_sched_free(struct fotg210_iso_stream *stream,
-		struct fotg210_iso_sched *iso_sched)
-{
-	if (!iso_sched)
-		return;
-	/* caller must hold fotg210->lock!*/
-	list_splice(&iso_sched->td_list, &stream->free_list);
-	kfree(iso_sched);
-}
-
-static int itd_urb_transaction(struct fotg210_iso_stream *stream,
-		struct fotg210_hcd *fotg210, struct urb *urb, gfp_t mem_flags)
-{
-	struct fotg210_itd *itd;
-	dma_addr_t itd_dma;
-	int i;
-	unsigned num_itds;
-	struct fotg210_iso_sched *sched;
-	unsigned long flags;
-
-	sched = iso_sched_alloc(urb->number_of_packets, mem_flags);
-	if (unlikely(sched == NULL))
-		return -ENOMEM;
-
-	itd_sched_init(fotg210, sched, stream, urb);
-
-	if (urb->interval < 8)
-		num_itds = 1 + (sched->span + 7) / 8;
-	else
-		num_itds = urb->number_of_packets;
-
-	/* allocate/init ITDs */
-	spin_lock_irqsave(&fotg210->lock, flags);
-	for (i = 0; i < num_itds; i++) {
-
-		/*
-		 * Use iTDs from the free list, but not iTDs that may
-		 * still be in use by the hardware.
-		 */
-		if (likely(!list_empty(&stream->free_list))) {
-			itd = list_first_entry(&stream->free_list,
-					struct fotg210_itd, itd_list);
-			if (itd->frame == fotg210->now_frame)
-				goto alloc_itd;
-			list_del(&itd->itd_list);
-			itd_dma = itd->itd_dma;
-		} else {
-alloc_itd:
-			spin_unlock_irqrestore(&fotg210->lock, flags);
-			itd = dma_pool_alloc(fotg210->itd_pool, mem_flags,
-					&itd_dma);
-			spin_lock_irqsave(&fotg210->lock, flags);
-			if (!itd) {
-				iso_sched_free(stream, sched);
-				spin_unlock_irqrestore(&fotg210->lock, flags);
-				return -ENOMEM;
-			}
-		}
-
-		memset(itd, 0, sizeof(*itd));
-		itd->itd_dma = itd_dma;
-		list_add(&itd->itd_list, &sched->td_list);
-	}
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-
-	/* temporarily store schedule info in hcpriv */
-	urb->hcpriv = sched;
-	urb->error_count = 0;
-	return 0;
-}
-
-static inline int itd_slot_ok(struct fotg210_hcd *fotg210, u32 mod, u32 uframe,
-		u8 usecs, u32 period)
-{
-	uframe %= period;
-	do {
-		/* can't commit more than uframe_periodic_max usec */
-		if (periodic_usecs(fotg210, uframe >> 3, uframe & 0x7)
-				> (fotg210->uframe_periodic_max - usecs))
-			return 0;
-
-		/* we know urb->interval is 2^N uframes */
-		uframe += period;
-	} while (uframe < mod);
-	return 1;
-}
-
-/* This scheduler plans almost as far into the future as it has actual
- * periodic schedule slots.  (Affected by TUNE_FLS, which defaults to
- * "as small as possible" to be cache-friendlier.)  That limits the size
- * transfers you can stream reliably; avoid more than 64 msec per urb.
- * Also avoid queue depths of less than fotg210's worst irq latency (affected
- * by the per-urb URB_NO_INTERRUPT hint, the log2_irq_thresh module parameter,
- * and other factors); or more than about 230 msec total (for portability,
- * given FOTG210_TUNE_FLS and the slop).  Or, write a smarter scheduler!
- */
-
-#define SCHEDULE_SLOP 80 /* microframes */
-
-static int iso_stream_schedule(struct fotg210_hcd *fotg210, struct urb *urb,
-		struct fotg210_iso_stream *stream)
-{
-	u32 now, next, start, period, span;
-	int status;
-	unsigned mod = fotg210->periodic_size << 3;
-	struct fotg210_iso_sched *sched = urb->hcpriv;
-
-	period = urb->interval;
-	span = sched->span;
-
-	if (span > mod - SCHEDULE_SLOP) {
-		fotg210_dbg(fotg210, "iso request %p too long\n", urb);
-		status = -EFBIG;
-		goto fail;
-	}
-
-	now = fotg210_read_frame_index(fotg210) & (mod - 1);
-
-	/* Typical case: reuse current schedule, stream is still active.
-	 * Hopefully there are no gaps from the host falling behind
-	 * (irq delays etc), but if there are we'll take the next
-	 * slot in the schedule, implicitly assuming URB_ISO_ASAP.
-	 */
-	if (likely(!list_empty(&stream->td_list))) {
-		u32 excess;
-
-		/* For high speed devices, allow scheduling within the
-		 * isochronous scheduling threshold.  For full speed devices
-		 * and Intel PCI-based controllers, don't (work around for
-		 * Intel ICH9 bug).
-		 */
-		if (!stream->highspeed && fotg210->fs_i_thresh)
-			next = now + fotg210->i_thresh;
-		else
-			next = now;
-
-		/* Fell behind (by up to twice the slop amount)?
-		 * We decide based on the time of the last currently-scheduled
-		 * slot, not the time of the next available slot.
-		 */
-		excess = (stream->next_uframe - period - next) & (mod - 1);
-		if (excess >= mod - 2 * SCHEDULE_SLOP)
-			start = next + excess - mod + period *
-					DIV_ROUND_UP(mod - excess, period);
-		else
-			start = next + excess + period;
-		if (start - now >= mod) {
-			fotg210_dbg(fotg210, "request %p would overflow (%d+%d >= %d)\n",
-					urb, start - now - period, period,
-					mod);
-			status = -EFBIG;
-			goto fail;
-		}
-	}
-
-	/* need to schedule; when's the next (u)frame we could start?
-	 * this is bigger than fotg210->i_thresh allows; scheduling itself
-	 * isn't free, the slop should handle reasonably slow cpus.  it
-	 * can also help high bandwidth if the dma and irq loads don't
-	 * jump until after the queue is primed.
-	 */
-	else {
-		int done = 0;
-
-		start = SCHEDULE_SLOP + (now & ~0x07);
-
-		/* NOTE:  assumes URB_ISO_ASAP, to limit complexity/bugs */
-
-		/* find a uframe slot with enough bandwidth.
-		 * Early uframes are more precious because full-speed
-		 * iso IN transfers can't use late uframes,
-		 * and therefore they should be allocated last.
-		 */
-		next = start;
-		start += period;
-		do {
-			start--;
-			/* check schedule: enough space? */
-			if (itd_slot_ok(fotg210, mod, start,
-					stream->usecs, period))
-				done = 1;
-		} while (start > next && !done);
-
-		/* no room in the schedule */
-		if (!done) {
-			fotg210_dbg(fotg210, "iso resched full %p (now %d max %d)\n",
-					urb, now, now + mod);
-			status = -ENOSPC;
-			goto fail;
-		}
-	}
-
-	/* Tried to schedule too far into the future? */
-	if (unlikely(start - now + span - period >=
-			mod - 2 * SCHEDULE_SLOP)) {
-		fotg210_dbg(fotg210, "request %p would overflow (%d+%d >= %d)\n",
-				urb, start - now, span - period,
-				mod - 2 * SCHEDULE_SLOP);
-		status = -EFBIG;
-		goto fail;
-	}
-
-	stream->next_uframe = start & (mod - 1);
-
-	/* report high speed start in uframes; full speed, in frames */
-	urb->start_frame = stream->next_uframe;
-	if (!stream->highspeed)
-		urb->start_frame >>= 3;
-
-	/* Make sure scan_isoc() sees these */
-	if (fotg210->isoc_count == 0)
-		fotg210->next_frame = now >> 3;
-	return 0;
-
-fail:
-	iso_sched_free(stream, sched);
-	urb->hcpriv = NULL;
-	return status;
-}
-
-static inline void itd_init(struct fotg210_hcd *fotg210,
-		struct fotg210_iso_stream *stream, struct fotg210_itd *itd)
-{
-	int i;
-
-	/* it's been recently zeroed */
-	itd->hw_next = FOTG210_LIST_END(fotg210);
-	itd->hw_bufp[0] = stream->buf0;
-	itd->hw_bufp[1] = stream->buf1;
-	itd->hw_bufp[2] = stream->buf2;
-
-	for (i = 0; i < 8; i++)
-		itd->index[i] = -1;
-
-	/* All other fields are filled when scheduling */
-}
-
-static inline void itd_patch(struct fotg210_hcd *fotg210,
-		struct fotg210_itd *itd, struct fotg210_iso_sched *iso_sched,
-		unsigned index, u16 uframe)
-{
-	struct fotg210_iso_packet *uf = &iso_sched->packet[index];
-	unsigned pg = itd->pg;
-
-	uframe &= 0x07;
-	itd->index[uframe] = index;
-
-	itd->hw_transaction[uframe] = uf->transaction;
-	itd->hw_transaction[uframe] |= cpu_to_hc32(fotg210, pg << 12);
-	itd->hw_bufp[pg] |= cpu_to_hc32(fotg210, uf->bufp & ~(u32)0);
-	itd->hw_bufp_hi[pg] |= cpu_to_hc32(fotg210, (u32)(uf->bufp >> 32));
-
-	/* iso_frame_desc[].offset must be strictly increasing */
-	if (unlikely(uf->cross)) {
-		u64 bufp = uf->bufp + 4096;
-
-		itd->pg = ++pg;
-		itd->hw_bufp[pg] |= cpu_to_hc32(fotg210, bufp & ~(u32)0);
-		itd->hw_bufp_hi[pg] |= cpu_to_hc32(fotg210, (u32)(bufp >> 32));
-	}
-}
-
-static inline void itd_link(struct fotg210_hcd *fotg210, unsigned frame,
-		struct fotg210_itd *itd)
-{
-	union fotg210_shadow *prev = &fotg210->pshadow[frame];
-	__hc32 *hw_p = &fotg210->periodic[frame];
-	union fotg210_shadow here = *prev;
-	__hc32 type = 0;
-
-	/* skip any iso nodes which might belong to previous microframes */
-	while (here.ptr) {
-		type = Q_NEXT_TYPE(fotg210, *hw_p);
-		if (type == cpu_to_hc32(fotg210, Q_TYPE_QH))
-			break;
-		prev = periodic_next_shadow(fotg210, prev, type);
-		hw_p = shadow_next_periodic(fotg210, &here, type);
-		here = *prev;
-	}
-
-	itd->itd_next = here;
-	itd->hw_next = *hw_p;
-	prev->itd = itd;
-	itd->frame = frame;
-	wmb();
-	*hw_p = cpu_to_hc32(fotg210, itd->itd_dma | Q_TYPE_ITD);
-}
-
-/* fit urb's itds into the selected schedule slot; activate as needed */
-static void itd_link_urb(struct fotg210_hcd *fotg210, struct urb *urb,
-		unsigned mod, struct fotg210_iso_stream *stream)
-{
-	int packet;
-	unsigned next_uframe, uframe, frame;
-	struct fotg210_iso_sched *iso_sched = urb->hcpriv;
-	struct fotg210_itd *itd;
-
-	next_uframe = stream->next_uframe & (mod - 1);
-
-	if (unlikely(list_empty(&stream->td_list))) {
-		fotg210_to_hcd(fotg210)->self.bandwidth_allocated
-				+= stream->bandwidth;
-		fotg210_dbg(fotg210,
-			"schedule devp %s ep%d%s-iso period %d start %d.%d\n",
-			urb->dev->devpath, stream->bEndpointAddress & 0x0f,
-			(stream->bEndpointAddress & USB_DIR_IN) ? "in" : "out",
-			urb->interval,
-			next_uframe >> 3, next_uframe & 0x7);
-	}
-
-	/* fill iTDs uframe by uframe */
-	for (packet = 0, itd = NULL; packet < urb->number_of_packets;) {
-		if (itd == NULL) {
-			/* ASSERT:  we have all necessary itds */
-
-			/* ASSERT:  no itds for this endpoint in this uframe */
-
-			itd = list_entry(iso_sched->td_list.next,
-					struct fotg210_itd, itd_list);
-			list_move_tail(&itd->itd_list, &stream->td_list);
-			itd->stream = stream;
-			itd->urb = urb;
-			itd_init(fotg210, stream, itd);
-		}
-
-		uframe = next_uframe & 0x07;
-		frame = next_uframe >> 3;
-
-		itd_patch(fotg210, itd, iso_sched, packet, uframe);
-
-		next_uframe += stream->interval;
-		next_uframe &= mod - 1;
-		packet++;
-
-		/* link completed itds into the schedule */
-		if (((next_uframe >> 3) != frame)
-				|| packet == urb->number_of_packets) {
-			itd_link(fotg210, frame & (fotg210->periodic_size - 1),
-					itd);
-			itd = NULL;
-		}
-	}
-	stream->next_uframe = next_uframe;
-
-	/* don't need that schedule data any more */
-	iso_sched_free(stream, iso_sched);
-	urb->hcpriv = NULL;
-
-	++fotg210->isoc_count;
-	enable_periodic(fotg210);
-}
-
-#define ISO_ERRS (FOTG210_ISOC_BUF_ERR | FOTG210_ISOC_BABBLE |\
-		FOTG210_ISOC_XACTERR)
-
-/* Process and recycle a completed ITD.  Return true iff its urb completed,
- * and hence its completion callback probably added things to the hardware
- * schedule.
- *
- * Note that we carefully avoid recycling this descriptor until after any
- * completion callback runs, so that it won't be reused quickly.  That is,
- * assuming (a) no more than two urbs per frame on this endpoint, and also
- * (b) only this endpoint's completions submit URBs.  It seems some silicon
- * corrupts things if you reuse completed descriptors very quickly...
- */
-static bool itd_complete(struct fotg210_hcd *fotg210, struct fotg210_itd *itd)
-{
-	struct urb *urb = itd->urb;
-	struct usb_iso_packet_descriptor *desc;
-	u32 t;
-	unsigned uframe;
-	int urb_index = -1;
-	struct fotg210_iso_stream *stream = itd->stream;
-	struct usb_device *dev;
-	bool retval = false;
-
-	/* for each uframe with a packet */
-	for (uframe = 0; uframe < 8; uframe++) {
-		if (likely(itd->index[uframe] == -1))
-			continue;
-		urb_index = itd->index[uframe];
-		desc = &urb->iso_frame_desc[urb_index];
-
-		t = hc32_to_cpup(fotg210, &itd->hw_transaction[uframe]);
-		itd->hw_transaction[uframe] = 0;
-
-		/* report transfer status */
-		if (unlikely(t & ISO_ERRS)) {
-			urb->error_count++;
-			if (t & FOTG210_ISOC_BUF_ERR)
-				desc->status = usb_pipein(urb->pipe)
-					? -ENOSR  /* hc couldn't read */
-					: -ECOMM; /* hc couldn't write */
-			else if (t & FOTG210_ISOC_BABBLE)
-				desc->status = -EOVERFLOW;
-			else /* (t & FOTG210_ISOC_XACTERR) */
-				desc->status = -EPROTO;
-
-			/* HC need not update length with this error */
-			if (!(t & FOTG210_ISOC_BABBLE)) {
-				desc->actual_length = FOTG210_ITD_LENGTH(t);
-				urb->actual_length += desc->actual_length;
-			}
-		} else if (likely((t & FOTG210_ISOC_ACTIVE) == 0)) {
-			desc->status = 0;
-			desc->actual_length = FOTG210_ITD_LENGTH(t);
-			urb->actual_length += desc->actual_length;
-		} else {
-			/* URB was too late */
-			desc->status = -EXDEV;
-		}
-	}
-
-	/* handle completion now? */
-	if (likely((urb_index + 1) != urb->number_of_packets))
-		goto done;
-
-	/* ASSERT: it's really the last itd for this urb
-	 * list_for_each_entry (itd, &stream->td_list, itd_list)
-	 *	BUG_ON (itd->urb == urb);
-	 */
-
-	/* give urb back to the driver; completion often (re)submits */
-	dev = urb->dev;
-	fotg210_urb_done(fotg210, urb, 0);
-	retval = true;
-	urb = NULL;
-
-	--fotg210->isoc_count;
-	disable_periodic(fotg210);
-
-	if (unlikely(list_is_singular(&stream->td_list))) {
-		fotg210_to_hcd(fotg210)->self.bandwidth_allocated
-				-= stream->bandwidth;
-		fotg210_dbg(fotg210,
-			"deschedule devp %s ep%d%s-iso\n",
-			dev->devpath, stream->bEndpointAddress & 0x0f,
-			(stream->bEndpointAddress & USB_DIR_IN) ? "in" : "out");
-	}
-
-done:
-	itd->urb = NULL;
-
-	/* Add to the end of the free list for later reuse */
-	list_move_tail(&itd->itd_list, &stream->free_list);
-
-	/* Recycle the iTDs when the pipeline is empty (ep no longer in use) */
-	if (list_empty(&stream->td_list)) {
-		list_splice_tail_init(&stream->free_list,
-				&fotg210->cached_itd_list);
-		start_free_itds(fotg210);
-	}
-
-	return retval;
-}
-
-static int itd_submit(struct fotg210_hcd *fotg210, struct urb *urb,
-		gfp_t mem_flags)
-{
-	int status = -EINVAL;
-	unsigned long flags;
-	struct fotg210_iso_stream *stream;
-
-	/* Get iso_stream head */
-	stream = iso_stream_find(fotg210, urb);
-	if (unlikely(stream == NULL)) {
-		fotg210_dbg(fotg210, "can't get iso stream\n");
-		return -ENOMEM;
-	}
-	if (unlikely(urb->interval != stream->interval &&
-			fotg210_port_speed(fotg210, 0) ==
-			USB_PORT_STAT_HIGH_SPEED)) {
-		fotg210_dbg(fotg210, "can't change iso interval %d --> %d\n",
-				stream->interval, urb->interval);
-		goto done;
-	}
-
-#ifdef FOTG210_URB_TRACE
-	fotg210_dbg(fotg210,
-			"%s %s urb %p ep%d%s len %d, %d pkts %d uframes[%p]\n",
-			__func__, urb->dev->devpath, urb,
-			usb_pipeendpoint(urb->pipe),
-			usb_pipein(urb->pipe) ? "in" : "out",
-			urb->transfer_buffer_length,
-			urb->number_of_packets, urb->interval,
-			stream);
-#endif
-
-	/* allocate ITDs w/o locking anything */
-	status = itd_urb_transaction(stream, fotg210, urb, mem_flags);
-	if (unlikely(status < 0)) {
-		fotg210_dbg(fotg210, "can't init itds\n");
-		goto done;
-	}
-
-	/* schedule ... need to lock */
-	spin_lock_irqsave(&fotg210->lock, flags);
-	if (unlikely(!HCD_HW_ACCESSIBLE(fotg210_to_hcd(fotg210)))) {
-		status = -ESHUTDOWN;
-		goto done_not_linked;
-	}
-	status = usb_hcd_link_urb_to_ep(fotg210_to_hcd(fotg210), urb);
-	if (unlikely(status))
-		goto done_not_linked;
-	status = iso_stream_schedule(fotg210, urb, stream);
-	if (likely(status == 0))
-		itd_link_urb(fotg210, urb, fotg210->periodic_size << 3, stream);
-	else
-		usb_hcd_unlink_urb_from_ep(fotg210_to_hcd(fotg210), urb);
-done_not_linked:
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-done:
-	return status;
-}
-
-static inline int scan_frame_queue(struct fotg210_hcd *fotg210, unsigned frame,
-		unsigned now_frame, bool live)
-{
-	unsigned uf;
-	bool modified;
-	union fotg210_shadow q, *q_p;
-	__hc32 type, *hw_p;
-
-	/* scan each element in frame's queue for completions */
-	q_p = &fotg210->pshadow[frame];
-	hw_p = &fotg210->periodic[frame];
-	q.ptr = q_p->ptr;
-	type = Q_NEXT_TYPE(fotg210, *hw_p);
-	modified = false;
-
-	while (q.ptr) {
-		switch (hc32_to_cpu(fotg210, type)) {
-		case Q_TYPE_ITD:
-			/* If this ITD is still active, leave it for
-			 * later processing ... check the next entry.
-			 * No need to check for activity unless the
-			 * frame is current.
-			 */
-			if (frame == now_frame && live) {
-				rmb();
-				for (uf = 0; uf < 8; uf++) {
-					if (q.itd->hw_transaction[uf] &
-							ITD_ACTIVE(fotg210))
-						break;
-				}
-				if (uf < 8) {
-					q_p = &q.itd->itd_next;
-					hw_p = &q.itd->hw_next;
-					type = Q_NEXT_TYPE(fotg210,
-							q.itd->hw_next);
-					q = *q_p;
-					break;
-				}
-			}
-
-			/* Take finished ITDs out of the schedule
-			 * and process them:  recycle, maybe report
-			 * URB completion.  HC won't cache the
-			 * pointer for much longer, if at all.
-			 */
-			*q_p = q.itd->itd_next;
-			*hw_p = q.itd->hw_next;
-			type = Q_NEXT_TYPE(fotg210, q.itd->hw_next);
-			wmb();
-			modified = itd_complete(fotg210, q.itd);
-			q = *q_p;
-			break;
-		default:
-			fotg210_dbg(fotg210, "corrupt type %d frame %d shadow %p\n",
-					type, frame, q.ptr);
-			fallthrough;
-		case Q_TYPE_QH:
-		case Q_TYPE_FSTN:
-			/* End of the iTDs and siTDs */
-			q.ptr = NULL;
-			break;
-		}
-
-		/* assume completion callbacks modify the queue */
-		if (unlikely(modified && fotg210->isoc_count > 0))
-			return -EINVAL;
-	}
-	return 0;
-}
-
-static void scan_isoc(struct fotg210_hcd *fotg210)
-{
-	unsigned uf, now_frame, frame, ret;
-	unsigned fmask = fotg210->periodic_size - 1;
-	bool live;
-
-	/*
-	 * When running, scan from last scan point up to "now"
-	 * else clean up by scanning everything that's left.
-	 * Touches as few pages as possible:  cache-friendly.
-	 */
-	if (fotg210->rh_state >= FOTG210_RH_RUNNING) {
-		uf = fotg210_read_frame_index(fotg210);
-		now_frame = (uf >> 3) & fmask;
-		live = true;
-	} else  {
-		now_frame = (fotg210->next_frame - 1) & fmask;
-		live = false;
-	}
-	fotg210->now_frame = now_frame;
-
-	frame = fotg210->next_frame;
-	for (;;) {
-		ret = 1;
-		while (ret != 0)
-			ret = scan_frame_queue(fotg210, frame,
-					now_frame, live);
-
-		/* Stop when we have reached the current frame */
-		if (frame == now_frame)
-			break;
-		frame = (frame + 1) & fmask;
-	}
-	fotg210->next_frame = now_frame;
-}
-
-/* Display / Set uframe_periodic_max
- */
-static ssize_t uframe_periodic_max_show(struct device *dev,
-		struct device_attribute *attr, char *buf)
-{
-	struct fotg210_hcd *fotg210;
-	int n;
-
-	fotg210 = hcd_to_fotg210(bus_to_hcd(dev_get_drvdata(dev)));
-	n = scnprintf(buf, PAGE_SIZE, "%d\n", fotg210->uframe_periodic_max);
-	return n;
-}
-
-
-static ssize_t uframe_periodic_max_store(struct device *dev,
-		struct device_attribute *attr, const char *buf, size_t count)
-{
-	struct fotg210_hcd *fotg210;
-	unsigned uframe_periodic_max;
-	unsigned frame, uframe;
-	unsigned short allocated_max;
-	unsigned long flags;
-	ssize_t ret;
-
-	fotg210 = hcd_to_fotg210(bus_to_hcd(dev_get_drvdata(dev)));
-	if (kstrtouint(buf, 0, &uframe_periodic_max) < 0)
-		return -EINVAL;
-
-	if (uframe_periodic_max < 100 || uframe_periodic_max >= 125) {
-		fotg210_info(fotg210, "rejecting invalid request for uframe_periodic_max=%u\n",
-				uframe_periodic_max);
-		return -EINVAL;
-	}
-
-	ret = -EINVAL;
-
-	/*
-	 * lock, so that our checking does not race with possible periodic
-	 * bandwidth allocation through submitting new urbs.
-	 */
-	spin_lock_irqsave(&fotg210->lock, flags);
-
-	/*
-	 * for request to decrease max periodic bandwidth, we have to check
-	 * every microframe in the schedule to see whether the decrease is
-	 * possible.
-	 */
-	if (uframe_periodic_max < fotg210->uframe_periodic_max) {
-		allocated_max = 0;
-
-		for (frame = 0; frame < fotg210->periodic_size; ++frame)
-			for (uframe = 0; uframe < 7; ++uframe)
-				allocated_max = max(allocated_max,
-						periodic_usecs(fotg210, frame,
-						uframe));
-
-		if (allocated_max > uframe_periodic_max) {
-			fotg210_info(fotg210,
-					"cannot decrease uframe_periodic_max because periodic bandwidth is already allocated (%u > %u)\n",
-					allocated_max, uframe_periodic_max);
-			goto out_unlock;
-		}
-	}
-
-	/* increasing is always ok */
-
-	fotg210_info(fotg210,
-			"setting max periodic bandwidth to %u%% (== %u usec/uframe)\n",
-			100 * uframe_periodic_max/125, uframe_periodic_max);
-
-	if (uframe_periodic_max != 100)
-		fotg210_warn(fotg210, "max periodic bandwidth set is non-standard\n");
-
-	fotg210->uframe_periodic_max = uframe_periodic_max;
-	ret = count;
-
-out_unlock:
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-	return ret;
-}
-
-static DEVICE_ATTR_RW(uframe_periodic_max);
-
-static inline int create_sysfs_files(struct fotg210_hcd *fotg210)
-{
-	struct device *controller = fotg210_to_hcd(fotg210)->self.controller;
-
-	return device_create_file(controller, &dev_attr_uframe_periodic_max);
-}
-
-static inline void remove_sysfs_files(struct fotg210_hcd *fotg210)
-{
-	struct device *controller = fotg210_to_hcd(fotg210)->self.controller;
-
-	device_remove_file(controller, &dev_attr_uframe_periodic_max);
-}
-/* On some systems, leaving remote wakeup enabled prevents system shutdown.
- * The firmware seems to think that powering off is a wakeup event!
- * This routine turns off remote wakeup and everything else, on all ports.
- */
-static void fotg210_turn_off_all_ports(struct fotg210_hcd *fotg210)
-{
-	u32 __iomem *status_reg = &fotg210->regs->port_status;
-
-	fotg210_writel(fotg210, PORT_RWC_BITS, status_reg);
-}
-
-/* Halt HC, turn off all ports, and let the BIOS use the companion controllers.
- * Must be called with interrupts enabled and the lock not held.
- */
-static void fotg210_silence_controller(struct fotg210_hcd *fotg210)
-{
-	fotg210_halt(fotg210);
-
-	spin_lock_irq(&fotg210->lock);
-	fotg210->rh_state = FOTG210_RH_HALTED;
-	fotg210_turn_off_all_ports(fotg210);
-	spin_unlock_irq(&fotg210->lock);
-}
-
-/* fotg210_shutdown kick in for silicon on any bus (not just pci, etc).
- * This forcibly disables dma and IRQs, helping kexec and other cases
- * where the next system software may expect clean state.
- */
-static void fotg210_shutdown(struct usb_hcd *hcd)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-
-	spin_lock_irq(&fotg210->lock);
-	fotg210->shutdown = true;
-	fotg210->rh_state = FOTG210_RH_STOPPING;
-	fotg210->enabled_hrtimer_events = 0;
-	spin_unlock_irq(&fotg210->lock);
-
-	fotg210_silence_controller(fotg210);
-
-	hrtimer_cancel(&fotg210->hrtimer);
-}
-
-/* fotg210_work is called from some interrupts, timers, and so on.
- * it calls driver completion functions, after dropping fotg210->lock.
- */
-static void fotg210_work(struct fotg210_hcd *fotg210)
-{
-	/* another CPU may drop fotg210->lock during a schedule scan while
-	 * it reports urb completions.  this flag guards against bogus
-	 * attempts at re-entrant schedule scanning.
-	 */
-	if (fotg210->scanning) {
-		fotg210->need_rescan = true;
-		return;
-	}
-	fotg210->scanning = true;
-
-rescan:
-	fotg210->need_rescan = false;
-	if (fotg210->async_count)
-		scan_async(fotg210);
-	if (fotg210->intr_count > 0)
-		scan_intr(fotg210);
-	if (fotg210->isoc_count > 0)
-		scan_isoc(fotg210);
-	if (fotg210->need_rescan)
-		goto rescan;
-	fotg210->scanning = false;
-
-	/* the IO watchdog guards against hardware or driver bugs that
-	 * misplace IRQs, and should let us run completely without IRQs.
-	 * such lossage has been observed on both VT6202 and VT8235.
-	 */
-	turn_on_io_watchdog(fotg210);
-}
-
-/* Called when the fotg210_hcd module is removed.
- */
-static void fotg210_stop(struct usb_hcd *hcd)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-
-	fotg210_dbg(fotg210, "stop\n");
-
-	/* no more interrupts ... */
-
-	spin_lock_irq(&fotg210->lock);
-	fotg210->enabled_hrtimer_events = 0;
-	spin_unlock_irq(&fotg210->lock);
-
-	fotg210_quiesce(fotg210);
-	fotg210_silence_controller(fotg210);
-	fotg210_reset(fotg210);
-
-	hrtimer_cancel(&fotg210->hrtimer);
-	remove_sysfs_files(fotg210);
-	remove_debug_files(fotg210);
-
-	/* root hub is shut down separately (first, when possible) */
-	spin_lock_irq(&fotg210->lock);
-	end_free_itds(fotg210);
-	spin_unlock_irq(&fotg210->lock);
-	fotg210_mem_cleanup(fotg210);
-
-#ifdef FOTG210_STATS
-	fotg210_dbg(fotg210, "irq normal %ld err %ld iaa %ld (lost %ld)\n",
-			fotg210->stats.normal, fotg210->stats.error,
-			fotg210->stats.iaa, fotg210->stats.lost_iaa);
-	fotg210_dbg(fotg210, "complete %ld unlink %ld\n",
-			fotg210->stats.complete, fotg210->stats.unlink);
-#endif
-
-	dbg_status(fotg210, "fotg210_stop completed",
-			fotg210_readl(fotg210, &fotg210->regs->status));
-}
-
-/* one-time init, only for memory state */
-static int hcd_fotg210_init(struct usb_hcd *hcd)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-	u32 temp;
-	int retval;
-	u32 hcc_params;
-	struct fotg210_qh_hw *hw;
-
-	spin_lock_init(&fotg210->lock);
-
-	/*
-	 * keep io watchdog by default, those good HCDs could turn off it later
-	 */
-	fotg210->need_io_watchdog = 1;
-
-	hrtimer_init(&fotg210->hrtimer, CLOCK_MONOTONIC, HRTIMER_MODE_ABS);
-	fotg210->hrtimer.function = fotg210_hrtimer_func;
-	fotg210->next_hrtimer_event = FOTG210_HRTIMER_NO_EVENT;
-
-	hcc_params = fotg210_readl(fotg210, &fotg210->caps->hcc_params);
-
-	/*
-	 * by default set standard 80% (== 100 usec/uframe) max periodic
-	 * bandwidth as required by USB 2.0
-	 */
-	fotg210->uframe_periodic_max = 100;
-
-	/*
-	 * hw default: 1K periodic list heads, one per frame.
-	 * periodic_size can shrink by USBCMD update if hcc_params allows.
-	 */
-	fotg210->periodic_size = DEFAULT_I_TDPS;
-	INIT_LIST_HEAD(&fotg210->intr_qh_list);
-	INIT_LIST_HEAD(&fotg210->cached_itd_list);
-
-	if (HCC_PGM_FRAMELISTLEN(hcc_params)) {
-		/* periodic schedule size can be smaller than default */
-		switch (FOTG210_TUNE_FLS) {
-		case 0:
-			fotg210->periodic_size = 1024;
-			break;
-		case 1:
-			fotg210->periodic_size = 512;
-			break;
-		case 2:
-			fotg210->periodic_size = 256;
-			break;
-		default:
-			BUG();
-		}
-	}
-	retval = fotg210_mem_init(fotg210, GFP_KERNEL);
-	if (retval < 0)
-		return retval;
-
-	/* controllers may cache some of the periodic schedule ... */
-	fotg210->i_thresh = 2;
-
-	/*
-	 * dedicate a qh for the async ring head, since we couldn't unlink
-	 * a 'real' qh without stopping the async schedule [4.8].  use it
-	 * as the 'reclamation list head' too.
-	 * its dummy is used in hw_alt_next of many tds, to prevent the qh
-	 * from automatically advancing to the next td after short reads.
-	 */
-	fotg210->async->qh_next.qh = NULL;
-	hw = fotg210->async->hw;
-	hw->hw_next = QH_NEXT(fotg210, fotg210->async->qh_dma);
-	hw->hw_info1 = cpu_to_hc32(fotg210, QH_HEAD);
-	hw->hw_token = cpu_to_hc32(fotg210, QTD_STS_HALT);
-	hw->hw_qtd_next = FOTG210_LIST_END(fotg210);
-	fotg210->async->qh_state = QH_STATE_LINKED;
-	hw->hw_alt_next = QTD_NEXT(fotg210, fotg210->async->dummy->qtd_dma);
-
-	/* clear interrupt enables, set irq latency */
-	if (log2_irq_thresh < 0 || log2_irq_thresh > 6)
-		log2_irq_thresh = 0;
-	temp = 1 << (16 + log2_irq_thresh);
-	if (HCC_CANPARK(hcc_params)) {
-		/* HW default park == 3, on hardware that supports it (like
-		 * NVidia and ALI silicon), maximizes throughput on the async
-		 * schedule by avoiding QH fetches between transfers.
-		 *
-		 * With fast usb storage devices and NForce2, "park" seems to
-		 * make problems:  throughput reduction (!), data errors...
-		 */
-		if (park) {
-			park = min_t(unsigned, park, 3);
-			temp |= CMD_PARK;
-			temp |= park << 8;
-		}
-		fotg210_dbg(fotg210, "park %d\n", park);
-	}
-	if (HCC_PGM_FRAMELISTLEN(hcc_params)) {
-		/* periodic schedule size can be smaller than default */
-		temp &= ~(3 << 2);
-		temp |= (FOTG210_TUNE_FLS << 2);
-	}
-	fotg210->command = temp;
-
-	/* Accept arbitrarily long scatter-gather lists */
-	if (!hcd->localmem_pool)
-		hcd->self.sg_tablesize = ~0;
-	return 0;
-}
-
-/* start HC running; it's halted, hcd_fotg210_init() has been run (once) */
-static int fotg210_run(struct usb_hcd *hcd)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-	u32 temp;
-
-	hcd->uses_new_polling = 1;
-
-	/* EHCI spec section 4.1 */
-
-	fotg210_writel(fotg210, fotg210->periodic_dma,
-			&fotg210->regs->frame_list);
-	fotg210_writel(fotg210, (u32)fotg210->async->qh_dma,
-			&fotg210->regs->async_next);
-
-	/*
-	 * hcc_params controls whether fotg210->regs->segment must (!!!)
-	 * be used; it constrains QH/ITD/SITD and QTD locations.
-	 * dma_pool consistent memory always uses segment zero.
-	 * streaming mappings for I/O buffers, like dma_map_single(),
-	 * can return segments above 4GB, if the device allows.
-	 *
-	 * NOTE:  the dma mask is visible through dev->dma_mask, so
-	 * drivers can pass this info along ... like NETIF_F_HIGHDMA,
-	 * Scsi_Host.highmem_io, and so forth.  It's readonly to all
-	 * host side drivers though.
-	 */
-	fotg210_readl(fotg210, &fotg210->caps->hcc_params);
-
-	/*
-	 * Philips, Intel, and maybe others need CMD_RUN before the
-	 * root hub will detect new devices (why?); NEC doesn't
-	 */
-	fotg210->command &= ~(CMD_IAAD|CMD_PSE|CMD_ASE|CMD_RESET);
-	fotg210->command |= CMD_RUN;
-	fotg210_writel(fotg210, fotg210->command, &fotg210->regs->command);
-	dbg_cmd(fotg210, "init", fotg210->command);
-
-	/*
-	 * Start, enabling full USB 2.0 functionality ... usb 1.1 devices
-	 * are explicitly handed to companion controller(s), so no TT is
-	 * involved with the root hub.  (Except where one is integrated,
-	 * and there's no companion controller unless maybe for USB OTG.)
-	 *
-	 * Turning on the CF flag will transfer ownership of all ports
-	 * from the companions to the EHCI controller.  If any of the
-	 * companions are in the middle of a port reset at the time, it
-	 * could cause trouble.  Write-locking ehci_cf_port_reset_rwsem
-	 * guarantees that no resets are in progress.  After we set CF,
-	 * a short delay lets the hardware catch up; new resets shouldn't
-	 * be started before the port switching actions could complete.
-	 */
-	down_write(&ehci_cf_port_reset_rwsem);
-	fotg210->rh_state = FOTG210_RH_RUNNING;
-	/* unblock posted writes */
-	fotg210_readl(fotg210, &fotg210->regs->command);
-	usleep_range(5000, 10000);
-	up_write(&ehci_cf_port_reset_rwsem);
-	fotg210->last_periodic_enable = ktime_get_real();
-
-	temp = HC_VERSION(fotg210,
-			fotg210_readl(fotg210, &fotg210->caps->hc_capbase));
-	fotg210_info(fotg210,
-			"USB %x.%x started, EHCI %x.%02x\n",
-			((fotg210->sbrn & 0xf0) >> 4), (fotg210->sbrn & 0x0f),
-			temp >> 8, temp & 0xff);
-
-	fotg210_writel(fotg210, INTR_MASK,
-			&fotg210->regs->intr_enable); /* Turn On Interrupts */
-
-	/* GRR this is run-once init(), being done every time the HC starts.
-	 * So long as they're part of class devices, we can't do it init()
-	 * since the class device isn't created that early.
-	 */
-	create_debug_files(fotg210);
-	create_sysfs_files(fotg210);
-
-	return 0;
-}
-
-static int fotg210_setup(struct usb_hcd *hcd)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-	int retval;
-
-	fotg210->regs = (void __iomem *)fotg210->caps +
-			HC_LENGTH(fotg210,
-			fotg210_readl(fotg210, &fotg210->caps->hc_capbase));
-	dbg_hcs_params(fotg210, "reset");
-	dbg_hcc_params(fotg210, "reset");
-
-	/* cache this readonly data; minimize chip reads */
-	fotg210->hcs_params = fotg210_readl(fotg210,
-			&fotg210->caps->hcs_params);
-
-	fotg210->sbrn = HCD_USB2;
-
-	/* data structure init */
-	retval = hcd_fotg210_init(hcd);
-	if (retval)
-		return retval;
-
-	retval = fotg210_halt(fotg210);
-	if (retval)
-		return retval;
-
-	fotg210_reset(fotg210);
-
-	return 0;
-}
-
-static irqreturn_t fotg210_irq(struct usb_hcd *hcd)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-	u32 status, masked_status, pcd_status = 0, cmd;
-	int bh;
-
-	spin_lock(&fotg210->lock);
-
-	status = fotg210_readl(fotg210, &fotg210->regs->status);
-
-	/* e.g. cardbus physical eject */
-	if (status == ~(u32) 0) {
-		fotg210_dbg(fotg210, "device removed\n");
-		goto dead;
-	}
-
-	/*
-	 * We don't use STS_FLR, but some controllers don't like it to
-	 * remain on, so mask it out along with the other status bits.
-	 */
-	masked_status = status & (INTR_MASK | STS_FLR);
-
-	/* Shared IRQ? */
-	if (!masked_status ||
-			unlikely(fotg210->rh_state == FOTG210_RH_HALTED)) {
-		spin_unlock(&fotg210->lock);
-		return IRQ_NONE;
-	}
-
-	/* clear (just) interrupts */
-	fotg210_writel(fotg210, masked_status, &fotg210->regs->status);
-	cmd = fotg210_readl(fotg210, &fotg210->regs->command);
-	bh = 0;
-
-	/* unrequested/ignored: Frame List Rollover */
-	dbg_status(fotg210, "irq", status);
-
-	/* INT, ERR, and IAA interrupt rates can be throttled */
-
-	/* normal [4.15.1.2] or error [4.15.1.1] completion */
-	if (likely((status & (STS_INT|STS_ERR)) != 0)) {
-		if (likely((status & STS_ERR) == 0))
-			INCR(fotg210->stats.normal);
-		else
-			INCR(fotg210->stats.error);
-		bh = 1;
-	}
-
-	/* complete the unlinking of some qh [4.15.2.3] */
-	if (status & STS_IAA) {
-
-		/* Turn off the IAA watchdog */
-		fotg210->enabled_hrtimer_events &=
-			~BIT(FOTG210_HRTIMER_IAA_WATCHDOG);
-
-		/*
-		 * Mild optimization: Allow another IAAD to reset the
-		 * hrtimer, if one occurs before the next expiration.
-		 * In theory we could always cancel the hrtimer, but
-		 * tests show that about half the time it will be reset
-		 * for some other event anyway.
-		 */
-		if (fotg210->next_hrtimer_event == FOTG210_HRTIMER_IAA_WATCHDOG)
-			++fotg210->next_hrtimer_event;
-
-		/* guard against (alleged) silicon errata */
-		if (cmd & CMD_IAAD)
-			fotg210_dbg(fotg210, "IAA with IAAD still set?\n");
-		if (fotg210->async_iaa) {
-			INCR(fotg210->stats.iaa);
-			end_unlink_async(fotg210);
-		} else
-			fotg210_dbg(fotg210, "IAA with nothing unlinked?\n");
-	}
-
-	/* remote wakeup [4.3.1] */
-	if (status & STS_PCD) {
-		int pstatus;
-		u32 __iomem *status_reg = &fotg210->regs->port_status;
-
-		/* kick root hub later */
-		pcd_status = status;
-
-		/* resume root hub? */
-		if (fotg210->rh_state == FOTG210_RH_SUSPENDED)
-			usb_hcd_resume_root_hub(hcd);
-
-		pstatus = fotg210_readl(fotg210, status_reg);
-
-		if (test_bit(0, &fotg210->suspended_ports) &&
-				((pstatus & PORT_RESUME) ||
-				!(pstatus & PORT_SUSPEND)) &&
-				(pstatus & PORT_PE) &&
-				fotg210->reset_done[0] == 0) {
-
-			/* start 20 msec resume signaling from this port,
-			 * and make hub_wq collect PORT_STAT_C_SUSPEND to
-			 * stop that signaling.  Use 5 ms extra for safety,
-			 * like usb_port_resume() does.
-			 */
-			fotg210->reset_done[0] = jiffies + msecs_to_jiffies(25);
-			set_bit(0, &fotg210->resuming_ports);
-			fotg210_dbg(fotg210, "port 1 remote wakeup\n");
-			mod_timer(&hcd->rh_timer, fotg210->reset_done[0]);
-		}
-	}
-
-	/* PCI errors [4.15.2.4] */
-	if (unlikely((status & STS_FATAL) != 0)) {
-		fotg210_err(fotg210, "fatal error\n");
-		dbg_cmd(fotg210, "fatal", cmd);
-		dbg_status(fotg210, "fatal", status);
-dead:
-		usb_hc_died(hcd);
-
-		/* Don't let the controller do anything more */
-		fotg210->shutdown = true;
-		fotg210->rh_state = FOTG210_RH_STOPPING;
-		fotg210->command &= ~(CMD_RUN | CMD_ASE | CMD_PSE);
-		fotg210_writel(fotg210, fotg210->command,
-				&fotg210->regs->command);
-		fotg210_writel(fotg210, 0, &fotg210->regs->intr_enable);
-		fotg210_handle_controller_death(fotg210);
-
-		/* Handle completions when the controller stops */
-		bh = 0;
-	}
-
-	if (bh)
-		fotg210_work(fotg210);
-	spin_unlock(&fotg210->lock);
-	if (pcd_status)
-		usb_hcd_poll_rh_status(hcd);
-	return IRQ_HANDLED;
-}
-
-/* non-error returns are a promise to giveback() the urb later
- * we drop ownership so next owner (or urb unlink) can get it
- *
- * urb + dev is in hcd.self.controller.urb_list
- * we're queueing TDs onto software and hardware lists
- *
- * hcd-specific init for hcpriv hasn't been done yet
- *
- * NOTE:  control, bulk, and interrupt share the same code to append TDs
- * to a (possibly active) QH, and the same QH scanning code.
- */
-static int fotg210_urb_enqueue(struct usb_hcd *hcd, struct urb *urb,
-		gfp_t mem_flags)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-	struct list_head qtd_list;
-
-	INIT_LIST_HEAD(&qtd_list);
-
-	switch (usb_pipetype(urb->pipe)) {
-	case PIPE_CONTROL:
-		/* qh_completions() code doesn't handle all the fault cases
-		 * in multi-TD control transfers.  Even 1KB is rare anyway.
-		 */
-		if (urb->transfer_buffer_length > (16 * 1024))
-			return -EMSGSIZE;
-		fallthrough;
-	/* case PIPE_BULK: */
-	default:
-		if (!qh_urb_transaction(fotg210, urb, &qtd_list, mem_flags))
-			return -ENOMEM;
-		return submit_async(fotg210, urb, &qtd_list, mem_flags);
-
-	case PIPE_INTERRUPT:
-		if (!qh_urb_transaction(fotg210, urb, &qtd_list, mem_flags))
-			return -ENOMEM;
-		return intr_submit(fotg210, urb, &qtd_list, mem_flags);
-
-	case PIPE_ISOCHRONOUS:
-		return itd_submit(fotg210, urb, mem_flags);
-	}
-}
-
-/* remove from hardware lists
- * completions normally happen asynchronously
- */
-
-static int fotg210_urb_dequeue(struct usb_hcd *hcd, struct urb *urb, int status)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-	struct fotg210_qh *qh;
-	unsigned long flags;
-	int rc;
-
-	spin_lock_irqsave(&fotg210->lock, flags);
-	rc = usb_hcd_check_unlink_urb(hcd, urb, status);
-	if (rc)
-		goto done;
-
-	switch (usb_pipetype(urb->pipe)) {
-	/* case PIPE_CONTROL: */
-	/* case PIPE_BULK:*/
-	default:
-		qh = (struct fotg210_qh *) urb->hcpriv;
-		if (!qh)
-			break;
-		switch (qh->qh_state) {
-		case QH_STATE_LINKED:
-		case QH_STATE_COMPLETING:
-			start_unlink_async(fotg210, qh);
-			break;
-		case QH_STATE_UNLINK:
-		case QH_STATE_UNLINK_WAIT:
-			/* already started */
-			break;
-		case QH_STATE_IDLE:
-			/* QH might be waiting for a Clear-TT-Buffer */
-			qh_completions(fotg210, qh);
-			break;
-		}
-		break;
-
-	case PIPE_INTERRUPT:
-		qh = (struct fotg210_qh *) urb->hcpriv;
-		if (!qh)
-			break;
-		switch (qh->qh_state) {
-		case QH_STATE_LINKED:
-		case QH_STATE_COMPLETING:
-			start_unlink_intr(fotg210, qh);
-			break;
-		case QH_STATE_IDLE:
-			qh_completions(fotg210, qh);
-			break;
-		default:
-			fotg210_dbg(fotg210, "bogus qh %p state %d\n",
-					qh, qh->qh_state);
-			goto done;
-		}
-		break;
-
-	case PIPE_ISOCHRONOUS:
-		/* itd... */
-
-		/* wait till next completion, do it then. */
-		/* completion irqs can wait up to 1024 msec, */
-		break;
-	}
-done:
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-	return rc;
-}
-
-/* bulk qh holds the data toggle */
-
-static void fotg210_endpoint_disable(struct usb_hcd *hcd,
-		struct usb_host_endpoint *ep)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-	unsigned long flags;
-	struct fotg210_qh *qh, *tmp;
-
-	/* ASSERT:  any requests/urbs are being unlinked */
-	/* ASSERT:  nobody can be submitting urbs for this any more */
-
-rescan:
-	spin_lock_irqsave(&fotg210->lock, flags);
-	qh = ep->hcpriv;
-	if (!qh)
-		goto done;
-
-	/* endpoints can be iso streams.  for now, we don't
-	 * accelerate iso completions ... so spin a while.
-	 */
-	if (qh->hw == NULL) {
-		struct fotg210_iso_stream *stream = ep->hcpriv;
-
-		if (!list_empty(&stream->td_list))
-			goto idle_timeout;
-
-		/* BUG_ON(!list_empty(&stream->free_list)); */
-		kfree(stream);
-		goto done;
-	}
-
-	if (fotg210->rh_state < FOTG210_RH_RUNNING)
-		qh->qh_state = QH_STATE_IDLE;
-	switch (qh->qh_state) {
-	case QH_STATE_LINKED:
-	case QH_STATE_COMPLETING:
-		for (tmp = fotg210->async->qh_next.qh;
-				tmp && tmp != qh;
-				tmp = tmp->qh_next.qh)
-			continue;
-		/* periodic qh self-unlinks on empty, and a COMPLETING qh
-		 * may already be unlinked.
-		 */
-		if (tmp)
-			start_unlink_async(fotg210, qh);
-		fallthrough;
-	case QH_STATE_UNLINK:		/* wait for hw to finish? */
-	case QH_STATE_UNLINK_WAIT:
-idle_timeout:
-		spin_unlock_irqrestore(&fotg210->lock, flags);
-		schedule_timeout_uninterruptible(1);
-		goto rescan;
-	case QH_STATE_IDLE:		/* fully unlinked */
-		if (qh->clearing_tt)
-			goto idle_timeout;
-		if (list_empty(&qh->qtd_list)) {
-			qh_destroy(fotg210, qh);
-			break;
-		}
-		fallthrough;
-	default:
-		/* caller was supposed to have unlinked any requests;
-		 * that's not our job.  just leak this memory.
-		 */
-		fotg210_err(fotg210, "qh %p (#%02x) state %d%s\n",
-				qh, ep->desc.bEndpointAddress, qh->qh_state,
-				list_empty(&qh->qtd_list) ? "" : "(has tds)");
-		break;
-	}
-done:
-	ep->hcpriv = NULL;
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-}
-
-static void fotg210_endpoint_reset(struct usb_hcd *hcd,
-		struct usb_host_endpoint *ep)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-	struct fotg210_qh *qh;
-	int eptype = usb_endpoint_type(&ep->desc);
-	int epnum = usb_endpoint_num(&ep->desc);
-	int is_out = usb_endpoint_dir_out(&ep->desc);
-	unsigned long flags;
-
-	if (eptype != USB_ENDPOINT_XFER_BULK && eptype != USB_ENDPOINT_XFER_INT)
-		return;
-
-	spin_lock_irqsave(&fotg210->lock, flags);
-	qh = ep->hcpriv;
-
-	/* For Bulk and Interrupt endpoints we maintain the toggle state
-	 * in the hardware; the toggle bits in udev aren't used at all.
-	 * When an endpoint is reset by usb_clear_halt() we must reset
-	 * the toggle bit in the QH.
-	 */
-	if (qh) {
-		usb_settoggle(qh->dev, epnum, is_out, 0);
-		if (!list_empty(&qh->qtd_list)) {
-			WARN_ONCE(1, "clear_halt for a busy endpoint\n");
-		} else if (qh->qh_state == QH_STATE_LINKED ||
-				qh->qh_state == QH_STATE_COMPLETING) {
-
-			/* The toggle value in the QH can't be updated
-			 * while the QH is active.  Unlink it now;
-			 * re-linking will call qh_refresh().
-			 */
-			if (eptype == USB_ENDPOINT_XFER_BULK)
-				start_unlink_async(fotg210, qh);
-			else
-				start_unlink_intr(fotg210, qh);
-		}
-	}
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-}
-
-static int fotg210_get_frame(struct usb_hcd *hcd)
-{
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-
-	return (fotg210_read_frame_index(fotg210) >> 3) %
-		fotg210->periodic_size;
-}
-
-/* The EHCI in ChipIdea HDRC cannot be a separate module or device,
- * because its registers (and irq) are shared between host/gadget/otg
- * functions  and in order to facilitate role switching we cannot
- * give the fotg210 driver exclusive access to those.
- */
-MODULE_DESCRIPTION(DRIVER_DESC);
-MODULE_AUTHOR(DRIVER_AUTHOR);
-MODULE_LICENSE("GPL");
-
-static const struct hc_driver fotg210_fotg210_hc_driver = {
-	.description		= hcd_name,
-	.product_desc		= "Faraday USB2.0 Host Controller",
-	.hcd_priv_size		= sizeof(struct fotg210_hcd),
-
-	/*
-	 * generic hardware linkage
-	 */
-	.irq			= fotg210_irq,
-	.flags			= HCD_MEMORY | HCD_DMA | HCD_USB2,
-
-	/*
-	 * basic lifecycle operations
-	 */
-	.reset			= hcd_fotg210_init,
-	.start			= fotg210_run,
-	.stop			= fotg210_stop,
-	.shutdown		= fotg210_shutdown,
-
-	/*
-	 * managing i/o requests and associated device resources
-	 */
-	.urb_enqueue		= fotg210_urb_enqueue,
-	.urb_dequeue		= fotg210_urb_dequeue,
-	.endpoint_disable	= fotg210_endpoint_disable,
-	.endpoint_reset		= fotg210_endpoint_reset,
-
-	/*
-	 * scheduling support
-	 */
-	.get_frame_number	= fotg210_get_frame,
-
-	/*
-	 * root hub support
-	 */
-	.hub_status_data	= fotg210_hub_status_data,
-	.hub_control		= fotg210_hub_control,
-	.bus_suspend		= fotg210_bus_suspend,
-	.bus_resume		= fotg210_bus_resume,
-
-	.relinquish_port	= fotg210_relinquish_port,
-	.port_handed_over	= fotg210_port_handed_over,
-
-	.clear_tt_buffer_complete = fotg210_clear_tt_buffer_complete,
-};
-
-static void fotg210_init(struct fotg210_hcd *fotg210)
-{
-	u32 value;
-
-	iowrite32(GMIR_MDEV_INT | GMIR_MOTG_INT | GMIR_INT_POLARITY,
-			&fotg210->regs->gmir);
-
-	value = ioread32(&fotg210->regs->otgcsr);
-	value &= ~OTGCSR_A_BUS_DROP;
-	value |= OTGCSR_A_BUS_REQ;
-	iowrite32(value, &fotg210->regs->otgcsr);
-}
-
-/*
- * fotg210_hcd_probe - initialize faraday FOTG210 HCDs
- *
- * Allocates basic resources for this USB host controller, and
- * then invokes the start() method for the HCD associated with it
- * through the hotplug entry's driver_data.
- */
-static int fotg210_hcd_probe(struct platform_device *pdev)
-{
-	struct device *dev = &pdev->dev;
-	struct usb_hcd *hcd;
-	struct resource *res;
-	int irq;
-	int retval;
-	struct fotg210_hcd *fotg210;
-
-	if (usb_disabled())
-		return -ENODEV;
-
-	pdev->dev.power.power_state = PMSG_ON;
-
-	irq = platform_get_irq(pdev, 0);
-	if (irq < 0)
-		return irq;
-
-	hcd = usb_create_hcd(&fotg210_fotg210_hc_driver, dev,
-			dev_name(dev));
-	if (!hcd) {
-		dev_err(dev, "failed to create hcd\n");
-		retval = -ENOMEM;
-		goto fail_create_hcd;
-	}
-
-	hcd->has_tt = 1;
-
-	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
-	hcd->regs = devm_ioremap_resource(&pdev->dev, res);
-	if (IS_ERR(hcd->regs)) {
-		retval = PTR_ERR(hcd->regs);
-		goto failed_put_hcd;
-	}
-
-	hcd->rsrc_start = res->start;
-	hcd->rsrc_len = resource_size(res);
-
-	fotg210 = hcd_to_fotg210(hcd);
-
-	fotg210->caps = hcd->regs;
-
-	/* It's OK not to supply this clock */
-	fotg210->pclk = clk_get(dev, "PCLK");
-	if (!IS_ERR(fotg210->pclk)) {
-		retval = clk_prepare_enable(fotg210->pclk);
-		if (retval) {
-			dev_err(dev, "failed to enable PCLK\n");
-			goto failed_put_hcd;
-		}
-	} else if (PTR_ERR(fotg210->pclk) == -EPROBE_DEFER) {
-		/*
-		 * Percolate deferrals, for anything else,
-		 * just live without the clocking.
-		 */
-		retval = PTR_ERR(fotg210->pclk);
-		goto failed_dis_clk;
-	}
-
-	retval = fotg210_setup(hcd);
-	if (retval)
-		goto failed_dis_clk;
-
-	fotg210_init(fotg210);
-
-	retval = usb_add_hcd(hcd, irq, IRQF_SHARED);
-	if (retval) {
-		dev_err(dev, "failed to add hcd with err %d\n", retval);
-		goto failed_dis_clk;
-	}
-	device_wakeup_enable(hcd->self.controller);
-	platform_set_drvdata(pdev, hcd);
-
-	return retval;
-
-failed_dis_clk:
-	if (!IS_ERR(fotg210->pclk)) {
-		clk_disable_unprepare(fotg210->pclk);
-		clk_put(fotg210->pclk);
-	}
-failed_put_hcd:
-	usb_put_hcd(hcd);
-fail_create_hcd:
-	dev_err(dev, "init %s fail, %d\n", dev_name(dev), retval);
-	return retval;
-}
-
-/*
- * fotg210_hcd_remove - shutdown processing for EHCI HCDs
- * @dev: USB Host Controller being removed
- *
- */
-static int fotg210_hcd_remove(struct platform_device *pdev)
-{
-	struct usb_hcd *hcd = platform_get_drvdata(pdev);
-	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
-
-	if (!IS_ERR(fotg210->pclk)) {
-		clk_disable_unprepare(fotg210->pclk);
-		clk_put(fotg210->pclk);
-	}
-
-	usb_remove_hcd(hcd);
-	usb_put_hcd(hcd);
-
-	return 0;
-}
-
-#ifdef CONFIG_OF
-static const struct of_device_id fotg210_of_match[] = {
-	{ .compatible = "faraday,fotg210" },
-	{},
-};
-MODULE_DEVICE_TABLE(of, fotg210_of_match);
-#endif
-
-static struct platform_driver fotg210_hcd_driver = {
-	.driver = {
-		.name   = "fotg210-hcd",
-		.of_match_table = of_match_ptr(fotg210_of_match),
-	},
-	.probe  = fotg210_hcd_probe,
-	.remove = fotg210_hcd_remove,
-};
-
-static int __init fotg210_hcd_init(void)
-{
-	int retval = 0;
-
-	if (usb_disabled())
-		return -ENODEV;
-
-	set_bit(USB_EHCI_LOADED, &usb_hcds_loaded);
-	if (test_bit(USB_UHCI_LOADED, &usb_hcds_loaded) ||
-			test_bit(USB_OHCI_LOADED, &usb_hcds_loaded))
-		pr_warn("Warning! fotg210_hcd should always be loaded before uhci_hcd and ohci_hcd, not after\n");
-
-	pr_debug("%s: block sizes: qh %zd qtd %zd itd %zd\n",
-			hcd_name, sizeof(struct fotg210_qh),
-			sizeof(struct fotg210_qtd),
-			sizeof(struct fotg210_itd));
-
-	fotg210_debug_root = debugfs_create_dir("fotg210", usb_debug_root);
-
-	retval = platform_driver_register(&fotg210_hcd_driver);
-	if (retval < 0)
-		goto clean;
-	return retval;
-
-clean:
-	debugfs_remove(fotg210_debug_root);
-	fotg210_debug_root = NULL;
-
-	clear_bit(USB_EHCI_LOADED, &usb_hcds_loaded);
-	return retval;
-}
-module_init(fotg210_hcd_init);
-
-static void __exit fotg210_hcd_cleanup(void)
-{
-	platform_driver_unregister(&fotg210_hcd_driver);
-	debugfs_remove(fotg210_debug_root);
-	clear_bit(USB_EHCI_LOADED, &usb_hcds_loaded);
-}
-module_exit(fotg210_hcd_cleanup);
--- /dev/null
+++ b/drivers/usb/fotg210/fotg210-hcd.c
@@ -0,0 +1,5727 @@
+// SPDX-License-Identifier: GPL-2.0+
+/* Faraday FOTG210 EHCI-like driver
+ *
+ * Copyright (c) 2013 Faraday Technology Corporation
+ *
+ * Author: Yuan-Hsin Chen <yhchen@faraday-tech.com>
+ *	   Feng-Hsin Chiang <john453@faraday-tech.com>
+ *	   Po-Yu Chuang <ratbert.chuang@gmail.com>
+ *
+ * Most of code borrowed from the Linux-3.7 EHCI driver
+ */
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/device.h>
+#include <linux/dmapool.h>
+#include <linux/kernel.h>
+#include <linux/delay.h>
+#include <linux/ioport.h>
+#include <linux/sched.h>
+#include <linux/vmalloc.h>
+#include <linux/errno.h>
+#include <linux/init.h>
+#include <linux/hrtimer.h>
+#include <linux/list.h>
+#include <linux/interrupt.h>
+#include <linux/usb.h>
+#include <linux/usb/hcd.h>
+#include <linux/moduleparam.h>
+#include <linux/dma-mapping.h>
+#include <linux/debugfs.h>
+#include <linux/slab.h>
+#include <linux/uaccess.h>
+#include <linux/platform_device.h>
+#include <linux/io.h>
+#include <linux/iopoll.h>
+#include <linux/clk.h>
+
+#include <asm/byteorder.h>
+#include <asm/irq.h>
+#include <asm/unaligned.h>
+
+#define DRIVER_AUTHOR "Yuan-Hsin Chen"
+#define DRIVER_DESC "FOTG210 Host Controller (EHCI) Driver"
+static const char hcd_name[] = "fotg210_hcd";
+
+#undef FOTG210_URB_TRACE
+#define FOTG210_STATS
+
+/* magic numbers that can affect system performance */
+#define FOTG210_TUNE_CERR	3 /* 0-3 qtd retries; 0 == don't stop */
+#define FOTG210_TUNE_RL_HS	4 /* nak throttle; see 4.9 */
+#define FOTG210_TUNE_RL_TT	0
+#define FOTG210_TUNE_MULT_HS	1 /* 1-3 transactions/uframe; 4.10.3 */
+#define FOTG210_TUNE_MULT_TT	1
+
+/* Some drivers think it's safe to schedule isochronous transfers more than 256
+ * ms into the future (partly as a result of an old bug in the scheduling
+ * code).  In an attempt to avoid trouble, we will use a minimum scheduling
+ * length of 512 frames instead of 256.
+ */
+#define FOTG210_TUNE_FLS 1 /* (medium) 512-frame schedule */
+
+/* Initial IRQ latency:  faster than hw default */
+static int log2_irq_thresh; /* 0 to 6 */
+module_param(log2_irq_thresh, int, S_IRUGO);
+MODULE_PARM_DESC(log2_irq_thresh, "log2 IRQ latency, 1-64 microframes");
+
+/* initial park setting:  slower than hw default */
+static unsigned park;
+module_param(park, uint, S_IRUGO);
+MODULE_PARM_DESC(park, "park setting; 1-3 back-to-back async packets");
+
+/* for link power management(LPM) feature */
+static unsigned int hird;
+module_param(hird, int, S_IRUGO);
+MODULE_PARM_DESC(hird, "host initiated resume duration, +1 for each 75us");
+
+#define INTR_MASK (STS_IAA | STS_FATAL | STS_PCD | STS_ERR | STS_INT)
+
+#include "fotg210-hcd.h"
+
+#define fotg210_dbg(fotg210, fmt, args...) \
+	dev_dbg(fotg210_to_hcd(fotg210)->self.controller, fmt, ## args)
+#define fotg210_err(fotg210, fmt, args...) \
+	dev_err(fotg210_to_hcd(fotg210)->self.controller, fmt, ## args)
+#define fotg210_info(fotg210, fmt, args...) \
+	dev_info(fotg210_to_hcd(fotg210)->self.controller, fmt, ## args)
+#define fotg210_warn(fotg210, fmt, args...) \
+	dev_warn(fotg210_to_hcd(fotg210)->self.controller, fmt, ## args)
+
+/* check the values in the HCSPARAMS register (host controller _Structural_
+ * parameters) see EHCI spec, Table 2-4 for each value
+ */
+static void dbg_hcs_params(struct fotg210_hcd *fotg210, char *label)
+{
+	u32 params = fotg210_readl(fotg210, &fotg210->caps->hcs_params);
+
+	fotg210_dbg(fotg210, "%s hcs_params 0x%x ports=%d\n", label, params,
+			HCS_N_PORTS(params));
+}
+
+/* check the values in the HCCPARAMS register (host controller _Capability_
+ * parameters) see EHCI Spec, Table 2-5 for each value
+ */
+static void dbg_hcc_params(struct fotg210_hcd *fotg210, char *label)
+{
+	u32 params = fotg210_readl(fotg210, &fotg210->caps->hcc_params);
+
+	fotg210_dbg(fotg210, "%s hcc_params %04x uframes %s%s\n", label,
+			params,
+			HCC_PGM_FRAMELISTLEN(params) ? "256/512/1024" : "1024",
+			HCC_CANPARK(params) ? " park" : "");
+}
+
+static void __maybe_unused
+dbg_qtd(const char *label, struct fotg210_hcd *fotg210, struct fotg210_qtd *qtd)
+{
+	fotg210_dbg(fotg210, "%s td %p n%08x %08x t%08x p0=%08x\n", label, qtd,
+			hc32_to_cpup(fotg210, &qtd->hw_next),
+			hc32_to_cpup(fotg210, &qtd->hw_alt_next),
+			hc32_to_cpup(fotg210, &qtd->hw_token),
+			hc32_to_cpup(fotg210, &qtd->hw_buf[0]));
+	if (qtd->hw_buf[1])
+		fotg210_dbg(fotg210, "  p1=%08x p2=%08x p3=%08x p4=%08x\n",
+				hc32_to_cpup(fotg210, &qtd->hw_buf[1]),
+				hc32_to_cpup(fotg210, &qtd->hw_buf[2]),
+				hc32_to_cpup(fotg210, &qtd->hw_buf[3]),
+				hc32_to_cpup(fotg210, &qtd->hw_buf[4]));
+}
+
+static void __maybe_unused
+dbg_qh(const char *label, struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
+{
+	struct fotg210_qh_hw *hw = qh->hw;
+
+	fotg210_dbg(fotg210, "%s qh %p n%08x info %x %x qtd %x\n", label, qh,
+			hw->hw_next, hw->hw_info1, hw->hw_info2,
+			hw->hw_current);
+
+	dbg_qtd("overlay", fotg210, (struct fotg210_qtd *) &hw->hw_qtd_next);
+}
+
+static void __maybe_unused
+dbg_itd(const char *label, struct fotg210_hcd *fotg210, struct fotg210_itd *itd)
+{
+	fotg210_dbg(fotg210, "%s[%d] itd %p, next %08x, urb %p\n", label,
+			itd->frame, itd, hc32_to_cpu(fotg210, itd->hw_next),
+			itd->urb);
+
+	fotg210_dbg(fotg210,
+			"  trans: %08x %08x %08x %08x %08x %08x %08x %08x\n",
+			hc32_to_cpu(fotg210, itd->hw_transaction[0]),
+			hc32_to_cpu(fotg210, itd->hw_transaction[1]),
+			hc32_to_cpu(fotg210, itd->hw_transaction[2]),
+			hc32_to_cpu(fotg210, itd->hw_transaction[3]),
+			hc32_to_cpu(fotg210, itd->hw_transaction[4]),
+			hc32_to_cpu(fotg210, itd->hw_transaction[5]),
+			hc32_to_cpu(fotg210, itd->hw_transaction[6]),
+			hc32_to_cpu(fotg210, itd->hw_transaction[7]));
+
+	fotg210_dbg(fotg210,
+			"  buf:   %08x %08x %08x %08x %08x %08x %08x\n",
+			hc32_to_cpu(fotg210, itd->hw_bufp[0]),
+			hc32_to_cpu(fotg210, itd->hw_bufp[1]),
+			hc32_to_cpu(fotg210, itd->hw_bufp[2]),
+			hc32_to_cpu(fotg210, itd->hw_bufp[3]),
+			hc32_to_cpu(fotg210, itd->hw_bufp[4]),
+			hc32_to_cpu(fotg210, itd->hw_bufp[5]),
+			hc32_to_cpu(fotg210, itd->hw_bufp[6]));
+
+	fotg210_dbg(fotg210, "  index: %d %d %d %d %d %d %d %d\n",
+			itd->index[0], itd->index[1], itd->index[2],
+			itd->index[3], itd->index[4], itd->index[5],
+			itd->index[6], itd->index[7]);
+}
+
+static int __maybe_unused
+dbg_status_buf(char *buf, unsigned len, const char *label, u32 status)
+{
+	return scnprintf(buf, len, "%s%sstatus %04x%s%s%s%s%s%s%s%s%s%s",
+			label, label[0] ? " " : "", status,
+			(status & STS_ASS) ? " Async" : "",
+			(status & STS_PSS) ? " Periodic" : "",
+			(status & STS_RECL) ? " Recl" : "",
+			(status & STS_HALT) ? " Halt" : "",
+			(status & STS_IAA) ? " IAA" : "",
+			(status & STS_FATAL) ? " FATAL" : "",
+			(status & STS_FLR) ? " FLR" : "",
+			(status & STS_PCD) ? " PCD" : "",
+			(status & STS_ERR) ? " ERR" : "",
+			(status & STS_INT) ? " INT" : "");
+}
+
+static int __maybe_unused
+dbg_intr_buf(char *buf, unsigned len, const char *label, u32 enable)
+{
+	return scnprintf(buf, len, "%s%sintrenable %02x%s%s%s%s%s%s",
+			label, label[0] ? " " : "", enable,
+			(enable & STS_IAA) ? " IAA" : "",
+			(enable & STS_FATAL) ? " FATAL" : "",
+			(enable & STS_FLR) ? " FLR" : "",
+			(enable & STS_PCD) ? " PCD" : "",
+			(enable & STS_ERR) ? " ERR" : "",
+			(enable & STS_INT) ? " INT" : "");
+}
+
+static const char *const fls_strings[] = { "1024", "512", "256", "??" };
+
+static int dbg_command_buf(char *buf, unsigned len, const char *label,
+		u32 command)
+{
+	return scnprintf(buf, len,
+			"%s%scommand %07x %s=%d ithresh=%d%s%s%s period=%s%s %s",
+			label, label[0] ? " " : "", command,
+			(command & CMD_PARK) ? " park" : "(park)",
+			CMD_PARK_CNT(command),
+			(command >> 16) & 0x3f,
+			(command & CMD_IAAD) ? " IAAD" : "",
+			(command & CMD_ASE) ? " Async" : "",
+			(command & CMD_PSE) ? " Periodic" : "",
+			fls_strings[(command >> 2) & 0x3],
+			(command & CMD_RESET) ? " Reset" : "",
+			(command & CMD_RUN) ? "RUN" : "HALT");
+}
+
+static char *dbg_port_buf(char *buf, unsigned len, const char *label, int port,
+		u32 status)
+{
+	char *sig;
+
+	/* signaling state */
+	switch (status & (3 << 10)) {
+	case 0 << 10:
+		sig = "se0";
+		break;
+	case 1 << 10:
+		sig = "k";
+		break; /* low speed */
+	case 2 << 10:
+		sig = "j";
+		break;
+	default:
+		sig = "?";
+		break;
+	}
+
+	scnprintf(buf, len, "%s%sport:%d status %06x %d sig=%s%s%s%s%s%s%s%s",
+			label, label[0] ? " " : "", port, status,
+			status >> 25, /*device address */
+			sig,
+			(status & PORT_RESET) ? " RESET" : "",
+			(status & PORT_SUSPEND) ? " SUSPEND" : "",
+			(status & PORT_RESUME) ? " RESUME" : "",
+			(status & PORT_PEC) ? " PEC" : "",
+			(status & PORT_PE) ? " PE" : "",
+			(status & PORT_CSC) ? " CSC" : "",
+			(status & PORT_CONNECT) ? " CONNECT" : "");
+
+	return buf;
+}
+
+/* functions have the "wrong" filename when they're output... */
+#define dbg_status(fotg210, label, status) {			\
+	char _buf[80];						\
+	dbg_status_buf(_buf, sizeof(_buf), label, status);	\
+	fotg210_dbg(fotg210, "%s\n", _buf);			\
+}
+
+#define dbg_cmd(fotg210, label, command) {			\
+	char _buf[80];						\
+	dbg_command_buf(_buf, sizeof(_buf), label, command);	\
+	fotg210_dbg(fotg210, "%s\n", _buf);			\
+}
+
+#define dbg_port(fotg210, label, port, status) {			       \
+	char _buf[80];							       \
+	fotg210_dbg(fotg210, "%s\n",					       \
+			dbg_port_buf(_buf, sizeof(_buf), label, port, status));\
+}
+
+/* troubleshooting help: expose state in debugfs */
+static int debug_async_open(struct inode *, struct file *);
+static int debug_periodic_open(struct inode *, struct file *);
+static int debug_registers_open(struct inode *, struct file *);
+static int debug_async_open(struct inode *, struct file *);
+
+static ssize_t debug_output(struct file*, char __user*, size_t, loff_t*);
+static int debug_close(struct inode *, struct file *);
+
+static const struct file_operations debug_async_fops = {
+	.owner		= THIS_MODULE,
+	.open		= debug_async_open,
+	.read		= debug_output,
+	.release	= debug_close,
+	.llseek		= default_llseek,
+};
+static const struct file_operations debug_periodic_fops = {
+	.owner		= THIS_MODULE,
+	.open		= debug_periodic_open,
+	.read		= debug_output,
+	.release	= debug_close,
+	.llseek		= default_llseek,
+};
+static const struct file_operations debug_registers_fops = {
+	.owner		= THIS_MODULE,
+	.open		= debug_registers_open,
+	.read		= debug_output,
+	.release	= debug_close,
+	.llseek		= default_llseek,
+};
+
+static struct dentry *fotg210_debug_root;
+
+struct debug_buffer {
+	ssize_t (*fill_func)(struct debug_buffer *);	/* fill method */
+	struct usb_bus *bus;
+	struct mutex mutex;	/* protect filling of buffer */
+	size_t count;		/* number of characters filled into buffer */
+	char *output_buf;
+	size_t alloc_size;
+};
+
+static inline char speed_char(u32 scratch)
+{
+	switch (scratch & (3 << 12)) {
+	case QH_FULL_SPEED:
+		return 'f';
+
+	case QH_LOW_SPEED:
+		return 'l';
+
+	case QH_HIGH_SPEED:
+		return 'h';
+
+	default:
+		return '?';
+	}
+}
+
+static inline char token_mark(struct fotg210_hcd *fotg210, __hc32 token)
+{
+	__u32 v = hc32_to_cpu(fotg210, token);
+
+	if (v & QTD_STS_ACTIVE)
+		return '*';
+	if (v & QTD_STS_HALT)
+		return '-';
+	if (!IS_SHORT_READ(v))
+		return ' ';
+	/* tries to advance through hw_alt_next */
+	return '/';
+}
+
+static void qh_lines(struct fotg210_hcd *fotg210, struct fotg210_qh *qh,
+		char **nextp, unsigned *sizep)
+{
+	u32 scratch;
+	u32 hw_curr;
+	struct fotg210_qtd *td;
+	unsigned temp;
+	unsigned size = *sizep;
+	char *next = *nextp;
+	char mark;
+	__le32 list_end = FOTG210_LIST_END(fotg210);
+	struct fotg210_qh_hw *hw = qh->hw;
+
+	if (hw->hw_qtd_next == list_end) /* NEC does this */
+		mark = '@';
+	else
+		mark = token_mark(fotg210, hw->hw_token);
+	if (mark == '/') { /* qh_alt_next controls qh advance? */
+		if ((hw->hw_alt_next & QTD_MASK(fotg210)) ==
+		    fotg210->async->hw->hw_alt_next)
+			mark = '#'; /* blocked */
+		else if (hw->hw_alt_next == list_end)
+			mark = '.'; /* use hw_qtd_next */
+		/* else alt_next points to some other qtd */
+	}
+	scratch = hc32_to_cpup(fotg210, &hw->hw_info1);
+	hw_curr = (mark == '*') ? hc32_to_cpup(fotg210, &hw->hw_current) : 0;
+	temp = scnprintf(next, size,
+			"qh/%p dev%d %cs ep%d %08x %08x(%08x%c %s nak%d)",
+			qh, scratch & 0x007f,
+			speed_char(scratch),
+			(scratch >> 8) & 0x000f,
+			scratch, hc32_to_cpup(fotg210, &hw->hw_info2),
+			hc32_to_cpup(fotg210, &hw->hw_token), mark,
+			(cpu_to_hc32(fotg210, QTD_TOGGLE) & hw->hw_token)
+				? "data1" : "data0",
+			(hc32_to_cpup(fotg210, &hw->hw_alt_next) >> 1) & 0x0f);
+	size -= temp;
+	next += temp;
+
+	/* hc may be modifying the list as we read it ... */
+	list_for_each_entry(td, &qh->qtd_list, qtd_list) {
+		scratch = hc32_to_cpup(fotg210, &td->hw_token);
+		mark = ' ';
+		if (hw_curr == td->qtd_dma)
+			mark = '*';
+		else if (hw->hw_qtd_next == cpu_to_hc32(fotg210, td->qtd_dma))
+			mark = '+';
+		else if (QTD_LENGTH(scratch)) {
+			if (td->hw_alt_next == fotg210->async->hw->hw_alt_next)
+				mark = '#';
+			else if (td->hw_alt_next != list_end)
+				mark = '/';
+		}
+		temp = snprintf(next, size,
+				"\n\t%p%c%s len=%d %08x urb %p",
+				td, mark, ({ char *tmp;
+				switch ((scratch>>8)&0x03) {
+				case 0:
+					tmp = "out";
+					break;
+				case 1:
+					tmp = "in";
+					break;
+				case 2:
+					tmp = "setup";
+					break;
+				default:
+					tmp = "?";
+					break;
+				 } tmp; }),
+				(scratch >> 16) & 0x7fff,
+				scratch,
+				td->urb);
+		if (size < temp)
+			temp = size;
+		size -= temp;
+		next += temp;
+		if (temp == size)
+			goto done;
+	}
+
+	temp = snprintf(next, size, "\n");
+	if (size < temp)
+		temp = size;
+
+	size -= temp;
+	next += temp;
+
+done:
+	*sizep = size;
+	*nextp = next;
+}
+
+static ssize_t fill_async_buffer(struct debug_buffer *buf)
+{
+	struct usb_hcd *hcd;
+	struct fotg210_hcd *fotg210;
+	unsigned long flags;
+	unsigned temp, size;
+	char *next;
+	struct fotg210_qh *qh;
+
+	hcd = bus_to_hcd(buf->bus);
+	fotg210 = hcd_to_fotg210(hcd);
+	next = buf->output_buf;
+	size = buf->alloc_size;
+
+	*next = 0;
+
+	/* dumps a snapshot of the async schedule.
+	 * usually empty except for long-term bulk reads, or head.
+	 * one QH per line, and TDs we know about
+	 */
+	spin_lock_irqsave(&fotg210->lock, flags);
+	for (qh = fotg210->async->qh_next.qh; size > 0 && qh;
+			qh = qh->qh_next.qh)
+		qh_lines(fotg210, qh, &next, &size);
+	if (fotg210->async_unlink && size > 0) {
+		temp = scnprintf(next, size, "\nunlink =\n");
+		size -= temp;
+		next += temp;
+
+		for (qh = fotg210->async_unlink; size > 0 && qh;
+				qh = qh->unlink_next)
+			qh_lines(fotg210, qh, &next, &size);
+	}
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+
+	return strlen(buf->output_buf);
+}
+
+/* count tds, get ep direction */
+static unsigned output_buf_tds_dir(char *buf, struct fotg210_hcd *fotg210,
+		struct fotg210_qh_hw *hw, struct fotg210_qh *qh, unsigned size)
+{
+	u32 scratch = hc32_to_cpup(fotg210, &hw->hw_info1);
+	struct fotg210_qtd *qtd;
+	char *type = "";
+	unsigned temp = 0;
+
+	/* count tds, get ep direction */
+	list_for_each_entry(qtd, &qh->qtd_list, qtd_list) {
+		temp++;
+		switch ((hc32_to_cpu(fotg210, qtd->hw_token) >> 8) & 0x03) {
+		case 0:
+			type = "out";
+			continue;
+		case 1:
+			type = "in";
+			continue;
+		}
+	}
+
+	return scnprintf(buf, size, "(%c%d ep%d%s [%d/%d] q%d p%d)",
+			speed_char(scratch), scratch & 0x007f,
+			(scratch >> 8) & 0x000f, type, qh->usecs,
+			qh->c_usecs, temp, (scratch >> 16) & 0x7ff);
+}
+
+#define DBG_SCHED_LIMIT 64
+static ssize_t fill_periodic_buffer(struct debug_buffer *buf)
+{
+	struct usb_hcd *hcd;
+	struct fotg210_hcd *fotg210;
+	unsigned long flags;
+	union fotg210_shadow p, *seen;
+	unsigned temp, size, seen_count;
+	char *next;
+	unsigned i;
+	__hc32 tag;
+
+	seen = kmalloc_array(DBG_SCHED_LIMIT, sizeof(*seen), GFP_ATOMIC);
+	if (!seen)
+		return 0;
+
+	seen_count = 0;
+
+	hcd = bus_to_hcd(buf->bus);
+	fotg210 = hcd_to_fotg210(hcd);
+	next = buf->output_buf;
+	size = buf->alloc_size;
+
+	temp = scnprintf(next, size, "size = %d\n", fotg210->periodic_size);
+	size -= temp;
+	next += temp;
+
+	/* dump a snapshot of the periodic schedule.
+	 * iso changes, interrupt usually doesn't.
+	 */
+	spin_lock_irqsave(&fotg210->lock, flags);
+	for (i = 0; i < fotg210->periodic_size; i++) {
+		p = fotg210->pshadow[i];
+		if (likely(!p.ptr))
+			continue;
+
+		tag = Q_NEXT_TYPE(fotg210, fotg210->periodic[i]);
+
+		temp = scnprintf(next, size, "%4d: ", i);
+		size -= temp;
+		next += temp;
+
+		do {
+			struct fotg210_qh_hw *hw;
+
+			switch (hc32_to_cpu(fotg210, tag)) {
+			case Q_TYPE_QH:
+				hw = p.qh->hw;
+				temp = scnprintf(next, size, " qh%d-%04x/%p",
+						p.qh->period,
+						hc32_to_cpup(fotg210,
+							&hw->hw_info2)
+							/* uframe masks */
+							& (QH_CMASK | QH_SMASK),
+						p.qh);
+				size -= temp;
+				next += temp;
+				/* don't repeat what follows this qh */
+				for (temp = 0; temp < seen_count; temp++) {
+					if (seen[temp].ptr != p.ptr)
+						continue;
+					if (p.qh->qh_next.ptr) {
+						temp = scnprintf(next, size,
+								" ...");
+						size -= temp;
+						next += temp;
+					}
+					break;
+				}
+				/* show more info the first time around */
+				if (temp == seen_count) {
+					temp = output_buf_tds_dir(next,
+							fotg210, hw,
+							p.qh, size);
+
+					if (seen_count < DBG_SCHED_LIMIT)
+						seen[seen_count++].qh = p.qh;
+				} else
+					temp = 0;
+				tag = Q_NEXT_TYPE(fotg210, hw->hw_next);
+				p = p.qh->qh_next;
+				break;
+			case Q_TYPE_FSTN:
+				temp = scnprintf(next, size,
+						" fstn-%8x/%p",
+						p.fstn->hw_prev, p.fstn);
+				tag = Q_NEXT_TYPE(fotg210, p.fstn->hw_next);
+				p = p.fstn->fstn_next;
+				break;
+			case Q_TYPE_ITD:
+				temp = scnprintf(next, size,
+						" itd/%p", p.itd);
+				tag = Q_NEXT_TYPE(fotg210, p.itd->hw_next);
+				p = p.itd->itd_next;
+				break;
+			}
+			size -= temp;
+			next += temp;
+		} while (p.ptr);
+
+		temp = scnprintf(next, size, "\n");
+		size -= temp;
+		next += temp;
+	}
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+	kfree(seen);
+
+	return buf->alloc_size - size;
+}
+#undef DBG_SCHED_LIMIT
+
+static const char *rh_state_string(struct fotg210_hcd *fotg210)
+{
+	switch (fotg210->rh_state) {
+	case FOTG210_RH_HALTED:
+		return "halted";
+	case FOTG210_RH_SUSPENDED:
+		return "suspended";
+	case FOTG210_RH_RUNNING:
+		return "running";
+	case FOTG210_RH_STOPPING:
+		return "stopping";
+	}
+	return "?";
+}
+
+static ssize_t fill_registers_buffer(struct debug_buffer *buf)
+{
+	struct usb_hcd *hcd;
+	struct fotg210_hcd *fotg210;
+	unsigned long flags;
+	unsigned temp, size, i;
+	char *next, scratch[80];
+	static const char fmt[] = "%*s\n";
+	static const char label[] = "";
+
+	hcd = bus_to_hcd(buf->bus);
+	fotg210 = hcd_to_fotg210(hcd);
+	next = buf->output_buf;
+	size = buf->alloc_size;
+
+	spin_lock_irqsave(&fotg210->lock, flags);
+
+	if (!HCD_HW_ACCESSIBLE(hcd)) {
+		size = scnprintf(next, size,
+				"bus %s, device %s\n"
+				"%s\n"
+				"SUSPENDED(no register access)\n",
+				hcd->self.controller->bus->name,
+				dev_name(hcd->self.controller),
+				hcd->product_desc);
+		goto done;
+	}
+
+	/* Capability Registers */
+	i = HC_VERSION(fotg210, fotg210_readl(fotg210,
+			&fotg210->caps->hc_capbase));
+	temp = scnprintf(next, size,
+			"bus %s, device %s\n"
+			"%s\n"
+			"EHCI %x.%02x, rh state %s\n",
+			hcd->self.controller->bus->name,
+			dev_name(hcd->self.controller),
+			hcd->product_desc,
+			i >> 8, i & 0x0ff, rh_state_string(fotg210));
+	size -= temp;
+	next += temp;
+
+	/* FIXME interpret both types of params */
+	i = fotg210_readl(fotg210, &fotg210->caps->hcs_params);
+	temp = scnprintf(next, size, "structural params 0x%08x\n", i);
+	size -= temp;
+	next += temp;
+
+	i = fotg210_readl(fotg210, &fotg210->caps->hcc_params);
+	temp = scnprintf(next, size, "capability params 0x%08x\n", i);
+	size -= temp;
+	next += temp;
+
+	/* Operational Registers */
+	temp = dbg_status_buf(scratch, sizeof(scratch), label,
+			fotg210_readl(fotg210, &fotg210->regs->status));
+	temp = scnprintf(next, size, fmt, temp, scratch);
+	size -= temp;
+	next += temp;
+
+	temp = dbg_command_buf(scratch, sizeof(scratch), label,
+			fotg210_readl(fotg210, &fotg210->regs->command));
+	temp = scnprintf(next, size, fmt, temp, scratch);
+	size -= temp;
+	next += temp;
+
+	temp = dbg_intr_buf(scratch, sizeof(scratch), label,
+			fotg210_readl(fotg210, &fotg210->regs->intr_enable));
+	temp = scnprintf(next, size, fmt, temp, scratch);
+	size -= temp;
+	next += temp;
+
+	temp = scnprintf(next, size, "uframe %04x\n",
+			fotg210_read_frame_index(fotg210));
+	size -= temp;
+	next += temp;
+
+	if (fotg210->async_unlink) {
+		temp = scnprintf(next, size, "async unlink qh %p\n",
+				fotg210->async_unlink);
+		size -= temp;
+		next += temp;
+	}
+
+#ifdef FOTG210_STATS
+	temp = scnprintf(next, size,
+			"irq normal %ld err %ld iaa %ld(lost %ld)\n",
+			fotg210->stats.normal, fotg210->stats.error,
+			fotg210->stats.iaa, fotg210->stats.lost_iaa);
+	size -= temp;
+	next += temp;
+
+	temp = scnprintf(next, size, "complete %ld unlink %ld\n",
+			fotg210->stats.complete, fotg210->stats.unlink);
+	size -= temp;
+	next += temp;
+#endif
+
+done:
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+
+	return buf->alloc_size - size;
+}
+
+static struct debug_buffer
+*alloc_buffer(struct usb_bus *bus, ssize_t (*fill_func)(struct debug_buffer *))
+{
+	struct debug_buffer *buf;
+
+	buf = kzalloc(sizeof(struct debug_buffer), GFP_KERNEL);
+
+	if (buf) {
+		buf->bus = bus;
+		buf->fill_func = fill_func;
+		mutex_init(&buf->mutex);
+		buf->alloc_size = PAGE_SIZE;
+	}
+
+	return buf;
+}
+
+static int fill_buffer(struct debug_buffer *buf)
+{
+	int ret = 0;
+
+	if (!buf->output_buf)
+		buf->output_buf = vmalloc(buf->alloc_size);
+
+	if (!buf->output_buf) {
+		ret = -ENOMEM;
+		goto out;
+	}
+
+	ret = buf->fill_func(buf);
+
+	if (ret >= 0) {
+		buf->count = ret;
+		ret = 0;
+	}
+
+out:
+	return ret;
+}
+
+static ssize_t debug_output(struct file *file, char __user *user_buf,
+		size_t len, loff_t *offset)
+{
+	struct debug_buffer *buf = file->private_data;
+	int ret = 0;
+
+	mutex_lock(&buf->mutex);
+	if (buf->count == 0) {
+		ret = fill_buffer(buf);
+		if (ret != 0) {
+			mutex_unlock(&buf->mutex);
+			goto out;
+		}
+	}
+	mutex_unlock(&buf->mutex);
+
+	ret = simple_read_from_buffer(user_buf, len, offset,
+			buf->output_buf, buf->count);
+
+out:
+	return ret;
+
+}
+
+static int debug_close(struct inode *inode, struct file *file)
+{
+	struct debug_buffer *buf = file->private_data;
+
+	if (buf) {
+		vfree(buf->output_buf);
+		kfree(buf);
+	}
+
+	return 0;
+}
+static int debug_async_open(struct inode *inode, struct file *file)
+{
+	file->private_data = alloc_buffer(inode->i_private, fill_async_buffer);
+
+	return file->private_data ? 0 : -ENOMEM;
+}
+
+static int debug_periodic_open(struct inode *inode, struct file *file)
+{
+	struct debug_buffer *buf;
+
+	buf = alloc_buffer(inode->i_private, fill_periodic_buffer);
+	if (!buf)
+		return -ENOMEM;
+
+	buf->alloc_size = (sizeof(void *) == 4 ? 6 : 8)*PAGE_SIZE;
+	file->private_data = buf;
+	return 0;
+}
+
+static int debug_registers_open(struct inode *inode, struct file *file)
+{
+	file->private_data = alloc_buffer(inode->i_private,
+			fill_registers_buffer);
+
+	return file->private_data ? 0 : -ENOMEM;
+}
+
+static inline void create_debug_files(struct fotg210_hcd *fotg210)
+{
+	struct usb_bus *bus = &fotg210_to_hcd(fotg210)->self;
+	struct dentry *root;
+
+	root = debugfs_create_dir(bus->bus_name, fotg210_debug_root);
+
+	debugfs_create_file("async", S_IRUGO, root, bus, &debug_async_fops);
+	debugfs_create_file("periodic", S_IRUGO, root, bus,
+			    &debug_periodic_fops);
+	debugfs_create_file("registers", S_IRUGO, root, bus,
+			    &debug_registers_fops);
+}
+
+static inline void remove_debug_files(struct fotg210_hcd *fotg210)
+{
+	struct usb_bus *bus = &fotg210_to_hcd(fotg210)->self;
+
+	debugfs_lookup_and_remove(bus->bus_name, fotg210_debug_root);
+}
+
+/* handshake - spin reading hc until handshake completes or fails
+ * @ptr: address of hc register to be read
+ * @mask: bits to look at in result of read
+ * @done: value of those bits when handshake succeeds
+ * @usec: timeout in microseconds
+ *
+ * Returns negative errno, or zero on success
+ *
+ * Success happens when the "mask" bits have the specified value (hardware
+ * handshake done).  There are two failure modes:  "usec" have passed (major
+ * hardware flakeout), or the register reads as all-ones (hardware removed).
+ *
+ * That last failure should_only happen in cases like physical cardbus eject
+ * before driver shutdown. But it also seems to be caused by bugs in cardbus
+ * bridge shutdown:  shutting down the bridge before the devices using it.
+ */
+static int handshake(struct fotg210_hcd *fotg210, void __iomem *ptr,
+		u32 mask, u32 done, int usec)
+{
+	u32 result;
+	int ret;
+
+	ret = readl_poll_timeout_atomic(ptr, result,
+					((result & mask) == done ||
+					 result == U32_MAX), 1, usec);
+	if (result == U32_MAX)		/* card removed */
+		return -ENODEV;
+
+	return ret;
+}
+
+/* Force HC to halt state from unknown (EHCI spec section 2.3).
+ * Must be called with interrupts enabled and the lock not held.
+ */
+static int fotg210_halt(struct fotg210_hcd *fotg210)
+{
+	u32 temp;
+
+	spin_lock_irq(&fotg210->lock);
+
+	/* disable any irqs left enabled by previous code */
+	fotg210_writel(fotg210, 0, &fotg210->regs->intr_enable);
+
+	/*
+	 * This routine gets called during probe before fotg210->command
+	 * has been initialized, so we can't rely on its value.
+	 */
+	fotg210->command &= ~CMD_RUN;
+	temp = fotg210_readl(fotg210, &fotg210->regs->command);
+	temp &= ~(CMD_RUN | CMD_IAAD);
+	fotg210_writel(fotg210, temp, &fotg210->regs->command);
+
+	spin_unlock_irq(&fotg210->lock);
+	synchronize_irq(fotg210_to_hcd(fotg210)->irq);
+
+	return handshake(fotg210, &fotg210->regs->status,
+			STS_HALT, STS_HALT, 16 * 125);
+}
+
+/* Reset a non-running (STS_HALT == 1) controller.
+ * Must be called with interrupts enabled and the lock not held.
+ */
+static int fotg210_reset(struct fotg210_hcd *fotg210)
+{
+	int retval;
+	u32 command = fotg210_readl(fotg210, &fotg210->regs->command);
+
+	/* If the EHCI debug controller is active, special care must be
+	 * taken before and after a host controller reset
+	 */
+	if (fotg210->debug && !dbgp_reset_prep(fotg210_to_hcd(fotg210)))
+		fotg210->debug = NULL;
+
+	command |= CMD_RESET;
+	dbg_cmd(fotg210, "reset", command);
+	fotg210_writel(fotg210, command, &fotg210->regs->command);
+	fotg210->rh_state = FOTG210_RH_HALTED;
+	fotg210->next_statechange = jiffies;
+	retval = handshake(fotg210, &fotg210->regs->command,
+			CMD_RESET, 0, 250 * 1000);
+
+	if (retval)
+		return retval;
+
+	if (fotg210->debug)
+		dbgp_external_startup(fotg210_to_hcd(fotg210));
+
+	fotg210->port_c_suspend = fotg210->suspended_ports =
+			fotg210->resuming_ports = 0;
+	return retval;
+}
+
+/* Idle the controller (turn off the schedules).
+ * Must be called with interrupts enabled and the lock not held.
+ */
+static void fotg210_quiesce(struct fotg210_hcd *fotg210)
+{
+	u32 temp;
+
+	if (fotg210->rh_state != FOTG210_RH_RUNNING)
+		return;
+
+	/* wait for any schedule enables/disables to take effect */
+	temp = (fotg210->command << 10) & (STS_ASS | STS_PSS);
+	handshake(fotg210, &fotg210->regs->status, STS_ASS | STS_PSS, temp,
+			16 * 125);
+
+	/* then disable anything that's still active */
+	spin_lock_irq(&fotg210->lock);
+	fotg210->command &= ~(CMD_ASE | CMD_PSE);
+	fotg210_writel(fotg210, fotg210->command, &fotg210->regs->command);
+	spin_unlock_irq(&fotg210->lock);
+
+	/* hardware can take 16 microframes to turn off ... */
+	handshake(fotg210, &fotg210->regs->status, STS_ASS | STS_PSS, 0,
+			16 * 125);
+}
+
+static void end_unlink_async(struct fotg210_hcd *fotg210);
+static void unlink_empty_async(struct fotg210_hcd *fotg210);
+static void fotg210_work(struct fotg210_hcd *fotg210);
+static void start_unlink_intr(struct fotg210_hcd *fotg210,
+			      struct fotg210_qh *qh);
+static void end_unlink_intr(struct fotg210_hcd *fotg210, struct fotg210_qh *qh);
+
+/* Set a bit in the USBCMD register */
+static void fotg210_set_command_bit(struct fotg210_hcd *fotg210, u32 bit)
+{
+	fotg210->command |= bit;
+	fotg210_writel(fotg210, fotg210->command, &fotg210->regs->command);
+
+	/* unblock posted write */
+	fotg210_readl(fotg210, &fotg210->regs->command);
+}
+
+/* Clear a bit in the USBCMD register */
+static void fotg210_clear_command_bit(struct fotg210_hcd *fotg210, u32 bit)
+{
+	fotg210->command &= ~bit;
+	fotg210_writel(fotg210, fotg210->command, &fotg210->regs->command);
+
+	/* unblock posted write */
+	fotg210_readl(fotg210, &fotg210->regs->command);
+}
+
+/* EHCI timer support...  Now using hrtimers.
+ *
+ * Lots of different events are triggered from fotg210->hrtimer.  Whenever
+ * the timer routine runs, it checks each possible event; events that are
+ * currently enabled and whose expiration time has passed get handled.
+ * The set of enabled events is stored as a collection of bitflags in
+ * fotg210->enabled_hrtimer_events, and they are numbered in order of
+ * increasing delay values (ranging between 1 ms and 100 ms).
+ *
+ * Rather than implementing a sorted list or tree of all pending events,
+ * we keep track only of the lowest-numbered pending event, in
+ * fotg210->next_hrtimer_event.  Whenever fotg210->hrtimer gets restarted, its
+ * expiration time is set to the timeout value for this event.
+ *
+ * As a result, events might not get handled right away; the actual delay
+ * could be anywhere up to twice the requested delay.  This doesn't
+ * matter, because none of the events are especially time-critical.  The
+ * ones that matter most all have a delay of 1 ms, so they will be
+ * handled after 2 ms at most, which is okay.  In addition to this, we
+ * allow for an expiration range of 1 ms.
+ */
+
+/* Delay lengths for the hrtimer event types.
+ * Keep this list sorted by delay length, in the same order as
+ * the event types indexed by enum fotg210_hrtimer_event in fotg210.h.
+ */
+static unsigned event_delays_ns[] = {
+	1 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_POLL_ASS */
+	1 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_POLL_PSS */
+	1 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_POLL_DEAD */
+	1125 * NSEC_PER_USEC,	/* FOTG210_HRTIMER_UNLINK_INTR */
+	2 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_FREE_ITDS */
+	6 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_ASYNC_UNLINKS */
+	10 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_IAA_WATCHDOG */
+	10 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_DISABLE_PERIODIC */
+	15 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_DISABLE_ASYNC */
+	100 * NSEC_PER_MSEC,	/* FOTG210_HRTIMER_IO_WATCHDOG */
+};
+
+/* Enable a pending hrtimer event */
+static void fotg210_enable_event(struct fotg210_hcd *fotg210, unsigned event,
+		bool resched)
+{
+	ktime_t *timeout = &fotg210->hr_timeouts[event];
+
+	if (resched)
+		*timeout = ktime_add(ktime_get(), event_delays_ns[event]);
+	fotg210->enabled_hrtimer_events |= (1 << event);
+
+	/* Track only the lowest-numbered pending event */
+	if (event < fotg210->next_hrtimer_event) {
+		fotg210->next_hrtimer_event = event;
+		hrtimer_start_range_ns(&fotg210->hrtimer, *timeout,
+				NSEC_PER_MSEC, HRTIMER_MODE_ABS);
+	}
+}
+
+
+/* Poll the STS_ASS status bit; see when it agrees with CMD_ASE */
+static void fotg210_poll_ASS(struct fotg210_hcd *fotg210)
+{
+	unsigned actual, want;
+
+	/* Don't enable anything if the controller isn't running (e.g., died) */
+	if (fotg210->rh_state != FOTG210_RH_RUNNING)
+		return;
+
+	want = (fotg210->command & CMD_ASE) ? STS_ASS : 0;
+	actual = fotg210_readl(fotg210, &fotg210->regs->status) & STS_ASS;
+
+	if (want != actual) {
+
+		/* Poll again later, but give up after about 20 ms */
+		if (fotg210->ASS_poll_count++ < 20) {
+			fotg210_enable_event(fotg210, FOTG210_HRTIMER_POLL_ASS,
+					true);
+			return;
+		}
+		fotg210_dbg(fotg210, "Waited too long for the async schedule status (%x/%x), giving up\n",
+				want, actual);
+	}
+	fotg210->ASS_poll_count = 0;
+
+	/* The status is up-to-date; restart or stop the schedule as needed */
+	if (want == 0) {	/* Stopped */
+		if (fotg210->async_count > 0)
+			fotg210_set_command_bit(fotg210, CMD_ASE);
+
+	} else {		/* Running */
+		if (fotg210->async_count == 0) {
+
+			/* Turn off the schedule after a while */
+			fotg210_enable_event(fotg210,
+					FOTG210_HRTIMER_DISABLE_ASYNC,
+					true);
+		}
+	}
+}
+
+/* Turn off the async schedule after a brief delay */
+static void fotg210_disable_ASE(struct fotg210_hcd *fotg210)
+{
+	fotg210_clear_command_bit(fotg210, CMD_ASE);
+}
+
+
+/* Poll the STS_PSS status bit; see when it agrees with CMD_PSE */
+static void fotg210_poll_PSS(struct fotg210_hcd *fotg210)
+{
+	unsigned actual, want;
+
+	/* Don't do anything if the controller isn't running (e.g., died) */
+	if (fotg210->rh_state != FOTG210_RH_RUNNING)
+		return;
+
+	want = (fotg210->command & CMD_PSE) ? STS_PSS : 0;
+	actual = fotg210_readl(fotg210, &fotg210->regs->status) & STS_PSS;
+
+	if (want != actual) {
+
+		/* Poll again later, but give up after about 20 ms */
+		if (fotg210->PSS_poll_count++ < 20) {
+			fotg210_enable_event(fotg210, FOTG210_HRTIMER_POLL_PSS,
+					true);
+			return;
+		}
+		fotg210_dbg(fotg210, "Waited too long for the periodic schedule status (%x/%x), giving up\n",
+				want, actual);
+	}
+	fotg210->PSS_poll_count = 0;
+
+	/* The status is up-to-date; restart or stop the schedule as needed */
+	if (want == 0) {	/* Stopped */
+		if (fotg210->periodic_count > 0)
+			fotg210_set_command_bit(fotg210, CMD_PSE);
+
+	} else {		/* Running */
+		if (fotg210->periodic_count == 0) {
+
+			/* Turn off the schedule after a while */
+			fotg210_enable_event(fotg210,
+					FOTG210_HRTIMER_DISABLE_PERIODIC,
+					true);
+		}
+	}
+}
+
+/* Turn off the periodic schedule after a brief delay */
+static void fotg210_disable_PSE(struct fotg210_hcd *fotg210)
+{
+	fotg210_clear_command_bit(fotg210, CMD_PSE);
+}
+
+
+/* Poll the STS_HALT status bit; see when a dead controller stops */
+static void fotg210_handle_controller_death(struct fotg210_hcd *fotg210)
+{
+	if (!(fotg210_readl(fotg210, &fotg210->regs->status) & STS_HALT)) {
+
+		/* Give up after a few milliseconds */
+		if (fotg210->died_poll_count++ < 5) {
+			/* Try again later */
+			fotg210_enable_event(fotg210,
+					FOTG210_HRTIMER_POLL_DEAD, true);
+			return;
+		}
+		fotg210_warn(fotg210, "Waited too long for the controller to stop, giving up\n");
+	}
+
+	/* Clean up the mess */
+	fotg210->rh_state = FOTG210_RH_HALTED;
+	fotg210_writel(fotg210, 0, &fotg210->regs->intr_enable);
+	fotg210_work(fotg210);
+	end_unlink_async(fotg210);
+
+	/* Not in process context, so don't try to reset the controller */
+}
+
+
+/* Handle unlinked interrupt QHs once they are gone from the hardware */
+static void fotg210_handle_intr_unlinks(struct fotg210_hcd *fotg210)
+{
+	bool stopped = (fotg210->rh_state < FOTG210_RH_RUNNING);
+
+	/*
+	 * Process all the QHs on the intr_unlink list that were added
+	 * before the current unlink cycle began.  The list is in
+	 * temporal order, so stop when we reach the first entry in the
+	 * current cycle.  But if the root hub isn't running then
+	 * process all the QHs on the list.
+	 */
+	fotg210->intr_unlinking = true;
+	while (fotg210->intr_unlink) {
+		struct fotg210_qh *qh = fotg210->intr_unlink;
+
+		if (!stopped && qh->unlink_cycle == fotg210->intr_unlink_cycle)
+			break;
+		fotg210->intr_unlink = qh->unlink_next;
+		qh->unlink_next = NULL;
+		end_unlink_intr(fotg210, qh);
+	}
+
+	/* Handle remaining entries later */
+	if (fotg210->intr_unlink) {
+		fotg210_enable_event(fotg210, FOTG210_HRTIMER_UNLINK_INTR,
+				true);
+		++fotg210->intr_unlink_cycle;
+	}
+	fotg210->intr_unlinking = false;
+}
+
+
+/* Start another free-iTDs/siTDs cycle */
+static void start_free_itds(struct fotg210_hcd *fotg210)
+{
+	if (!(fotg210->enabled_hrtimer_events &
+			BIT(FOTG210_HRTIMER_FREE_ITDS))) {
+		fotg210->last_itd_to_free = list_entry(
+				fotg210->cached_itd_list.prev,
+				struct fotg210_itd, itd_list);
+		fotg210_enable_event(fotg210, FOTG210_HRTIMER_FREE_ITDS, true);
+	}
+}
+
+/* Wait for controller to stop using old iTDs and siTDs */
+static void end_free_itds(struct fotg210_hcd *fotg210)
+{
+	struct fotg210_itd *itd, *n;
+
+	if (fotg210->rh_state < FOTG210_RH_RUNNING)
+		fotg210->last_itd_to_free = NULL;
+
+	list_for_each_entry_safe(itd, n, &fotg210->cached_itd_list, itd_list) {
+		list_del(&itd->itd_list);
+		dma_pool_free(fotg210->itd_pool, itd, itd->itd_dma);
+		if (itd == fotg210->last_itd_to_free)
+			break;
+	}
+
+	if (!list_empty(&fotg210->cached_itd_list))
+		start_free_itds(fotg210);
+}
+
+
+/* Handle lost (or very late) IAA interrupts */
+static void fotg210_iaa_watchdog(struct fotg210_hcd *fotg210)
+{
+	if (fotg210->rh_state != FOTG210_RH_RUNNING)
+		return;
+
+	/*
+	 * Lost IAA irqs wedge things badly; seen first with a vt8235.
+	 * So we need this watchdog, but must protect it against both
+	 * (a) SMP races against real IAA firing and retriggering, and
+	 * (b) clean HC shutdown, when IAA watchdog was pending.
+	 */
+	if (fotg210->async_iaa) {
+		u32 cmd, status;
+
+		/* If we get here, IAA is *REALLY* late.  It's barely
+		 * conceivable that the system is so busy that CMD_IAAD
+		 * is still legitimately set, so let's be sure it's
+		 * clear before we read STS_IAA.  (The HC should clear
+		 * CMD_IAAD when it sets STS_IAA.)
+		 */
+		cmd = fotg210_readl(fotg210, &fotg210->regs->command);
+
+		/*
+		 * If IAA is set here it either legitimately triggered
+		 * after the watchdog timer expired (_way_ late, so we'll
+		 * still count it as lost) ... or a silicon erratum:
+		 * - VIA seems to set IAA without triggering the IRQ;
+		 * - IAAD potentially cleared without setting IAA.
+		 */
+		status = fotg210_readl(fotg210, &fotg210->regs->status);
+		if ((status & STS_IAA) || !(cmd & CMD_IAAD)) {
+			INCR(fotg210->stats.lost_iaa);
+			fotg210_writel(fotg210, STS_IAA,
+					&fotg210->regs->status);
+		}
+
+		fotg210_dbg(fotg210, "IAA watchdog: status %x cmd %x\n",
+				status, cmd);
+		end_unlink_async(fotg210);
+	}
+}
+
+
+/* Enable the I/O watchdog, if appropriate */
+static void turn_on_io_watchdog(struct fotg210_hcd *fotg210)
+{
+	/* Not needed if the controller isn't running or it's already enabled */
+	if (fotg210->rh_state != FOTG210_RH_RUNNING ||
+			(fotg210->enabled_hrtimer_events &
+			BIT(FOTG210_HRTIMER_IO_WATCHDOG)))
+		return;
+
+	/*
+	 * Isochronous transfers always need the watchdog.
+	 * For other sorts we use it only if the flag is set.
+	 */
+	if (fotg210->isoc_count > 0 || (fotg210->need_io_watchdog &&
+			fotg210->async_count + fotg210->intr_count > 0))
+		fotg210_enable_event(fotg210, FOTG210_HRTIMER_IO_WATCHDOG,
+				true);
+}
+
+
+/* Handler functions for the hrtimer event types.
+ * Keep this array in the same order as the event types indexed by
+ * enum fotg210_hrtimer_event in fotg210.h.
+ */
+static void (*event_handlers[])(struct fotg210_hcd *) = {
+	fotg210_poll_ASS,			/* FOTG210_HRTIMER_POLL_ASS */
+	fotg210_poll_PSS,			/* FOTG210_HRTIMER_POLL_PSS */
+	fotg210_handle_controller_death,	/* FOTG210_HRTIMER_POLL_DEAD */
+	fotg210_handle_intr_unlinks,	/* FOTG210_HRTIMER_UNLINK_INTR */
+	end_free_itds,			/* FOTG210_HRTIMER_FREE_ITDS */
+	unlink_empty_async,		/* FOTG210_HRTIMER_ASYNC_UNLINKS */
+	fotg210_iaa_watchdog,		/* FOTG210_HRTIMER_IAA_WATCHDOG */
+	fotg210_disable_PSE,		/* FOTG210_HRTIMER_DISABLE_PERIODIC */
+	fotg210_disable_ASE,		/* FOTG210_HRTIMER_DISABLE_ASYNC */
+	fotg210_work,			/* FOTG210_HRTIMER_IO_WATCHDOG */
+};
+
+static enum hrtimer_restart fotg210_hrtimer_func(struct hrtimer *t)
+{
+	struct fotg210_hcd *fotg210 =
+			container_of(t, struct fotg210_hcd, hrtimer);
+	ktime_t now;
+	unsigned long events;
+	unsigned long flags;
+	unsigned e;
+
+	spin_lock_irqsave(&fotg210->lock, flags);
+
+	events = fotg210->enabled_hrtimer_events;
+	fotg210->enabled_hrtimer_events = 0;
+	fotg210->next_hrtimer_event = FOTG210_HRTIMER_NO_EVENT;
+
+	/*
+	 * Check each pending event.  If its time has expired, handle
+	 * the event; otherwise re-enable it.
+	 */
+	now = ktime_get();
+	for_each_set_bit(e, &events, FOTG210_HRTIMER_NUM_EVENTS) {
+		if (ktime_compare(now, fotg210->hr_timeouts[e]) >= 0)
+			event_handlers[e](fotg210);
+		else
+			fotg210_enable_event(fotg210, e, false);
+	}
+
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+	return HRTIMER_NORESTART;
+}
+
+#define fotg210_bus_suspend NULL
+#define fotg210_bus_resume NULL
+
+static int check_reset_complete(struct fotg210_hcd *fotg210, int index,
+		u32 __iomem *status_reg, int port_status)
+{
+	if (!(port_status & PORT_CONNECT))
+		return port_status;
+
+	/* if reset finished and it's still not enabled -- handoff */
+	if (!(port_status & PORT_PE))
+		/* with integrated TT, there's nobody to hand it to! */
+		fotg210_dbg(fotg210, "Failed to enable port %d on root hub TT\n",
+				index + 1);
+	else
+		fotg210_dbg(fotg210, "port %d reset complete, port enabled\n",
+				index + 1);
+
+	return port_status;
+}
+
+
+/* build "status change" packet (one or two bytes) from HC registers */
+
+static int fotg210_hub_status_data(struct usb_hcd *hcd, char *buf)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+	u32 temp, status;
+	u32 mask;
+	int retval = 1;
+	unsigned long flags;
+
+	/* init status to no-changes */
+	buf[0] = 0;
+
+	/* Inform the core about resumes-in-progress by returning
+	 * a non-zero value even if there are no status changes.
+	 */
+	status = fotg210->resuming_ports;
+
+	mask = PORT_CSC | PORT_PEC;
+	/* PORT_RESUME from hardware ~= PORT_STAT_C_SUSPEND */
+
+	/* no hub change reports (bit 0) for now (power, ...) */
+
+	/* port N changes (bit N)? */
+	spin_lock_irqsave(&fotg210->lock, flags);
+
+	temp = fotg210_readl(fotg210, &fotg210->regs->port_status);
+
+	/*
+	 * Return status information even for ports with OWNER set.
+	 * Otherwise hub_wq wouldn't see the disconnect event when a
+	 * high-speed device is switched over to the companion
+	 * controller by the user.
+	 */
+
+	if ((temp & mask) != 0 || test_bit(0, &fotg210->port_c_suspend) ||
+			(fotg210->reset_done[0] &&
+			time_after_eq(jiffies, fotg210->reset_done[0]))) {
+		buf[0] |= 1 << 1;
+		status = STS_PCD;
+	}
+	/* FIXME autosuspend idle root hubs */
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+	return status ? retval : 0;
+}
+
+static void fotg210_hub_descriptor(struct fotg210_hcd *fotg210,
+		struct usb_hub_descriptor *desc)
+{
+	int ports = HCS_N_PORTS(fotg210->hcs_params);
+	u16 temp;
+
+	desc->bDescriptorType = USB_DT_HUB;
+	desc->bPwrOn2PwrGood = 10;	/* fotg210 1.0, 2.3.9 says 20ms max */
+	desc->bHubContrCurrent = 0;
+
+	desc->bNbrPorts = ports;
+	temp = 1 + (ports / 8);
+	desc->bDescLength = 7 + 2 * temp;
+
+	/* two bitmaps:  ports removable, and usb 1.0 legacy PortPwrCtrlMask */
+	memset(&desc->u.hs.DeviceRemovable[0], 0, temp);
+	memset(&desc->u.hs.DeviceRemovable[temp], 0xff, temp);
+
+	temp = HUB_CHAR_INDV_PORT_OCPM;	/* per-port overcurrent reporting */
+	temp |= HUB_CHAR_NO_LPSM;	/* no power switching */
+	desc->wHubCharacteristics = cpu_to_le16(temp);
+}
+
+static int fotg210_hub_control(struct usb_hcd *hcd, u16 typeReq, u16 wValue,
+		u16 wIndex, char *buf, u16 wLength)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+	int ports = HCS_N_PORTS(fotg210->hcs_params);
+	u32 __iomem *status_reg = &fotg210->regs->port_status;
+	u32 temp, temp1, status;
+	unsigned long flags;
+	int retval = 0;
+	unsigned selector;
+
+	/*
+	 * FIXME:  support SetPortFeatures USB_PORT_FEAT_INDICATOR.
+	 * HCS_INDICATOR may say we can change LEDs to off/amber/green.
+	 * (track current state ourselves) ... blink for diagnostics,
+	 * power, "this is the one", etc.  EHCI spec supports this.
+	 */
+
+	spin_lock_irqsave(&fotg210->lock, flags);
+	switch (typeReq) {
+	case ClearHubFeature:
+		switch (wValue) {
+		case C_HUB_LOCAL_POWER:
+		case C_HUB_OVER_CURRENT:
+			/* no hub-wide feature/status flags */
+			break;
+		default:
+			goto error;
+		}
+		break;
+	case ClearPortFeature:
+		if (!wIndex || wIndex > ports)
+			goto error;
+		wIndex--;
+		temp = fotg210_readl(fotg210, status_reg);
+		temp &= ~PORT_RWC_BITS;
+
+		/*
+		 * Even if OWNER is set, so the port is owned by the
+		 * companion controller, hub_wq needs to be able to clear
+		 * the port-change status bits (especially
+		 * USB_PORT_STAT_C_CONNECTION).
+		 */
+
+		switch (wValue) {
+		case USB_PORT_FEAT_ENABLE:
+			fotg210_writel(fotg210, temp & ~PORT_PE, status_reg);
+			break;
+		case USB_PORT_FEAT_C_ENABLE:
+			fotg210_writel(fotg210, temp | PORT_PEC, status_reg);
+			break;
+		case USB_PORT_FEAT_SUSPEND:
+			if (temp & PORT_RESET)
+				goto error;
+			if (!(temp & PORT_SUSPEND))
+				break;
+			if ((temp & PORT_PE) == 0)
+				goto error;
+
+			/* resume signaling for 20 msec */
+			fotg210_writel(fotg210, temp | PORT_RESUME, status_reg);
+			fotg210->reset_done[wIndex] = jiffies
+					+ msecs_to_jiffies(USB_RESUME_TIMEOUT);
+			break;
+		case USB_PORT_FEAT_C_SUSPEND:
+			clear_bit(wIndex, &fotg210->port_c_suspend);
+			break;
+		case USB_PORT_FEAT_C_CONNECTION:
+			fotg210_writel(fotg210, temp | PORT_CSC, status_reg);
+			break;
+		case USB_PORT_FEAT_C_OVER_CURRENT:
+			fotg210_writel(fotg210, temp | OTGISR_OVC,
+					&fotg210->regs->otgisr);
+			break;
+		case USB_PORT_FEAT_C_RESET:
+			/* GetPortStatus clears reset */
+			break;
+		default:
+			goto error;
+		}
+		fotg210_readl(fotg210, &fotg210->regs->command);
+		break;
+	case GetHubDescriptor:
+		fotg210_hub_descriptor(fotg210, (struct usb_hub_descriptor *)
+				buf);
+		break;
+	case GetHubStatus:
+		/* no hub-wide feature/status flags */
+		memset(buf, 0, 4);
+		/*cpu_to_le32s ((u32 *) buf); */
+		break;
+	case GetPortStatus:
+		if (!wIndex || wIndex > ports)
+			goto error;
+		wIndex--;
+		status = 0;
+		temp = fotg210_readl(fotg210, status_reg);
+
+		/* wPortChange bits */
+		if (temp & PORT_CSC)
+			status |= USB_PORT_STAT_C_CONNECTION << 16;
+		if (temp & PORT_PEC)
+			status |= USB_PORT_STAT_C_ENABLE << 16;
+
+		temp1 = fotg210_readl(fotg210, &fotg210->regs->otgisr);
+		if (temp1 & OTGISR_OVC)
+			status |= USB_PORT_STAT_C_OVERCURRENT << 16;
+
+		/* whoever resumes must GetPortStatus to complete it!! */
+		if (temp & PORT_RESUME) {
+
+			/* Remote Wakeup received? */
+			if (!fotg210->reset_done[wIndex]) {
+				/* resume signaling for 20 msec */
+				fotg210->reset_done[wIndex] = jiffies
+						+ msecs_to_jiffies(20);
+				/* check the port again */
+				mod_timer(&fotg210_to_hcd(fotg210)->rh_timer,
+						fotg210->reset_done[wIndex]);
+			}
+
+			/* resume completed? */
+			else if (time_after_eq(jiffies,
+					fotg210->reset_done[wIndex])) {
+				clear_bit(wIndex, &fotg210->suspended_ports);
+				set_bit(wIndex, &fotg210->port_c_suspend);
+				fotg210->reset_done[wIndex] = 0;
+
+				/* stop resume signaling */
+				temp = fotg210_readl(fotg210, status_reg);
+				fotg210_writel(fotg210, temp &
+						~(PORT_RWC_BITS | PORT_RESUME),
+						status_reg);
+				clear_bit(wIndex, &fotg210->resuming_ports);
+				retval = handshake(fotg210, status_reg,
+						PORT_RESUME, 0, 2000);/* 2ms */
+				if (retval != 0) {
+					fotg210_err(fotg210,
+							"port %d resume error %d\n",
+							wIndex + 1, retval);
+					goto error;
+				}
+				temp &= ~(PORT_SUSPEND|PORT_RESUME|(3<<10));
+			}
+		}
+
+		/* whoever resets must GetPortStatus to complete it!! */
+		if ((temp & PORT_RESET) && time_after_eq(jiffies,
+				fotg210->reset_done[wIndex])) {
+			status |= USB_PORT_STAT_C_RESET << 16;
+			fotg210->reset_done[wIndex] = 0;
+			clear_bit(wIndex, &fotg210->resuming_ports);
+
+			/* force reset to complete */
+			fotg210_writel(fotg210,
+					temp & ~(PORT_RWC_BITS | PORT_RESET),
+					status_reg);
+			/* REVISIT:  some hardware needs 550+ usec to clear
+			 * this bit; seems too long to spin routinely...
+			 */
+			retval = handshake(fotg210, status_reg,
+					PORT_RESET, 0, 1000);
+			if (retval != 0) {
+				fotg210_err(fotg210, "port %d reset error %d\n",
+						wIndex + 1, retval);
+				goto error;
+			}
+
+			/* see what we found out */
+			temp = check_reset_complete(fotg210, wIndex, status_reg,
+					fotg210_readl(fotg210, status_reg));
+
+			/* restart schedule */
+			fotg210->command |= CMD_RUN;
+			fotg210_writel(fotg210, fotg210->command, &fotg210->regs->command);
+		}
+
+		if (!(temp & (PORT_RESUME|PORT_RESET))) {
+			fotg210->reset_done[wIndex] = 0;
+			clear_bit(wIndex, &fotg210->resuming_ports);
+		}
+
+		/* transfer dedicated ports to the companion hc */
+		if ((temp & PORT_CONNECT) &&
+				test_bit(wIndex, &fotg210->companion_ports)) {
+			temp &= ~PORT_RWC_BITS;
+			fotg210_writel(fotg210, temp, status_reg);
+			fotg210_dbg(fotg210, "port %d --> companion\n",
+					wIndex + 1);
+			temp = fotg210_readl(fotg210, status_reg);
+		}
+
+		/*
+		 * Even if OWNER is set, there's no harm letting hub_wq
+		 * see the wPortStatus values (they should all be 0 except
+		 * for PORT_POWER anyway).
+		 */
+
+		if (temp & PORT_CONNECT) {
+			status |= USB_PORT_STAT_CONNECTION;
+			status |= fotg210_port_speed(fotg210, temp);
+		}
+		if (temp & PORT_PE)
+			status |= USB_PORT_STAT_ENABLE;
+
+		/* maybe the port was unsuspended without our knowledge */
+		if (temp & (PORT_SUSPEND|PORT_RESUME)) {
+			status |= USB_PORT_STAT_SUSPEND;
+		} else if (test_bit(wIndex, &fotg210->suspended_ports)) {
+			clear_bit(wIndex, &fotg210->suspended_ports);
+			clear_bit(wIndex, &fotg210->resuming_ports);
+			fotg210->reset_done[wIndex] = 0;
+			if (temp & PORT_PE)
+				set_bit(wIndex, &fotg210->port_c_suspend);
+		}
+
+		temp1 = fotg210_readl(fotg210, &fotg210->regs->otgisr);
+		if (temp1 & OTGISR_OVC)
+			status |= USB_PORT_STAT_OVERCURRENT;
+		if (temp & PORT_RESET)
+			status |= USB_PORT_STAT_RESET;
+		if (test_bit(wIndex, &fotg210->port_c_suspend))
+			status |= USB_PORT_STAT_C_SUSPEND << 16;
+
+		if (status & ~0xffff)	/* only if wPortChange is interesting */
+			dbg_port(fotg210, "GetStatus", wIndex + 1, temp);
+		put_unaligned_le32(status, buf);
+		break;
+	case SetHubFeature:
+		switch (wValue) {
+		case C_HUB_LOCAL_POWER:
+		case C_HUB_OVER_CURRENT:
+			/* no hub-wide feature/status flags */
+			break;
+		default:
+			goto error;
+		}
+		break;
+	case SetPortFeature:
+		selector = wIndex >> 8;
+		wIndex &= 0xff;
+
+		if (!wIndex || wIndex > ports)
+			goto error;
+		wIndex--;
+		temp = fotg210_readl(fotg210, status_reg);
+		temp &= ~PORT_RWC_BITS;
+		switch (wValue) {
+		case USB_PORT_FEAT_SUSPEND:
+			if ((temp & PORT_PE) == 0
+					|| (temp & PORT_RESET) != 0)
+				goto error;
+
+			/* After above check the port must be connected.
+			 * Set appropriate bit thus could put phy into low power
+			 * mode if we have hostpc feature
+			 */
+			fotg210_writel(fotg210, temp | PORT_SUSPEND,
+					status_reg);
+			set_bit(wIndex, &fotg210->suspended_ports);
+			break;
+		case USB_PORT_FEAT_RESET:
+			if (temp & PORT_RESUME)
+				goto error;
+			/* line status bits may report this as low speed,
+			 * which can be fine if this root hub has a
+			 * transaction translator built in.
+			 */
+			fotg210_dbg(fotg210, "port %d reset\n", wIndex + 1);
+			temp |= PORT_RESET;
+			temp &= ~PORT_PE;
+
+			/*
+			 * caller must wait, then call GetPortStatus
+			 * usb 2.0 spec says 50 ms resets on root
+			 */
+			fotg210->reset_done[wIndex] = jiffies
+					+ msecs_to_jiffies(50);
+			fotg210_writel(fotg210, temp, status_reg);
+			break;
+
+		/* For downstream facing ports (these):  one hub port is put
+		 * into test mode according to USB2 11.24.2.13, then the hub
+		 * must be reset (which for root hub now means rmmod+modprobe,
+		 * or else system reboot).  See EHCI 2.3.9 and 4.14 for info
+		 * about the EHCI-specific stuff.
+		 */
+		case USB_PORT_FEAT_TEST:
+			if (!selector || selector > 5)
+				goto error;
+			spin_unlock_irqrestore(&fotg210->lock, flags);
+			fotg210_quiesce(fotg210);
+			spin_lock_irqsave(&fotg210->lock, flags);
+
+			/* Put all enabled ports into suspend */
+			temp = fotg210_readl(fotg210, status_reg) &
+				~PORT_RWC_BITS;
+			if (temp & PORT_PE)
+				fotg210_writel(fotg210, temp | PORT_SUSPEND,
+						status_reg);
+
+			spin_unlock_irqrestore(&fotg210->lock, flags);
+			fotg210_halt(fotg210);
+			spin_lock_irqsave(&fotg210->lock, flags);
+
+			temp = fotg210_readl(fotg210, status_reg);
+			temp |= selector << 16;
+			fotg210_writel(fotg210, temp, status_reg);
+			break;
+
+		default:
+			goto error;
+		}
+		fotg210_readl(fotg210, &fotg210->regs->command);
+		break;
+
+	default:
+error:
+		/* "stall" on error */
+		retval = -EPIPE;
+	}
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+	return retval;
+}
+
+static void __maybe_unused fotg210_relinquish_port(struct usb_hcd *hcd,
+		int portnum)
+{
+	return;
+}
+
+static int __maybe_unused fotg210_port_handed_over(struct usb_hcd *hcd,
+		int portnum)
+{
+	return 0;
+}
+
+/* There's basically three types of memory:
+ *	- data used only by the HCD ... kmalloc is fine
+ *	- async and periodic schedules, shared by HC and HCD ... these
+ *	  need to use dma_pool or dma_alloc_coherent
+ *	- driver buffers, read/written by HC ... single shot DMA mapped
+ *
+ * There's also "register" data (e.g. PCI or SOC), which is memory mapped.
+ * No memory seen by this driver is pageable.
+ */
+
+/* Allocate the key transfer structures from the previously allocated pool */
+static inline void fotg210_qtd_init(struct fotg210_hcd *fotg210,
+		struct fotg210_qtd *qtd, dma_addr_t dma)
+{
+	memset(qtd, 0, sizeof(*qtd));
+	qtd->qtd_dma = dma;
+	qtd->hw_token = cpu_to_hc32(fotg210, QTD_STS_HALT);
+	qtd->hw_next = FOTG210_LIST_END(fotg210);
+	qtd->hw_alt_next = FOTG210_LIST_END(fotg210);
+	INIT_LIST_HEAD(&qtd->qtd_list);
+}
+
+static struct fotg210_qtd *fotg210_qtd_alloc(struct fotg210_hcd *fotg210,
+		gfp_t flags)
+{
+	struct fotg210_qtd *qtd;
+	dma_addr_t dma;
+
+	qtd = dma_pool_alloc(fotg210->qtd_pool, flags, &dma);
+	if (qtd != NULL)
+		fotg210_qtd_init(fotg210, qtd, dma);
+
+	return qtd;
+}
+
+static inline void fotg210_qtd_free(struct fotg210_hcd *fotg210,
+		struct fotg210_qtd *qtd)
+{
+	dma_pool_free(fotg210->qtd_pool, qtd, qtd->qtd_dma);
+}
+
+
+static void qh_destroy(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
+{
+	/* clean qtds first, and know this is not linked */
+	if (!list_empty(&qh->qtd_list) || qh->qh_next.ptr) {
+		fotg210_dbg(fotg210, "unused qh not empty!\n");
+		BUG();
+	}
+	if (qh->dummy)
+		fotg210_qtd_free(fotg210, qh->dummy);
+	dma_pool_free(fotg210->qh_pool, qh->hw, qh->qh_dma);
+	kfree(qh);
+}
+
+static struct fotg210_qh *fotg210_qh_alloc(struct fotg210_hcd *fotg210,
+		gfp_t flags)
+{
+	struct fotg210_qh *qh;
+	dma_addr_t dma;
+
+	qh = kzalloc(sizeof(*qh), GFP_ATOMIC);
+	if (!qh)
+		goto done;
+	qh->hw = (struct fotg210_qh_hw *)
+		dma_pool_zalloc(fotg210->qh_pool, flags, &dma);
+	if (!qh->hw)
+		goto fail;
+	qh->qh_dma = dma;
+	INIT_LIST_HEAD(&qh->qtd_list);
+
+	/* dummy td enables safe urb queuing */
+	qh->dummy = fotg210_qtd_alloc(fotg210, flags);
+	if (qh->dummy == NULL) {
+		fotg210_dbg(fotg210, "no dummy td\n");
+		goto fail1;
+	}
+done:
+	return qh;
+fail1:
+	dma_pool_free(fotg210->qh_pool, qh->hw, qh->qh_dma);
+fail:
+	kfree(qh);
+	return NULL;
+}
+
+/* The queue heads and transfer descriptors are managed from pools tied
+ * to each of the "per device" structures.
+ * This is the initialisation and cleanup code.
+ */
+
+static void fotg210_mem_cleanup(struct fotg210_hcd *fotg210)
+{
+	if (fotg210->async)
+		qh_destroy(fotg210, fotg210->async);
+	fotg210->async = NULL;
+
+	if (fotg210->dummy)
+		qh_destroy(fotg210, fotg210->dummy);
+	fotg210->dummy = NULL;
+
+	/* DMA consistent memory and pools */
+	dma_pool_destroy(fotg210->qtd_pool);
+	fotg210->qtd_pool = NULL;
+
+	dma_pool_destroy(fotg210->qh_pool);
+	fotg210->qh_pool = NULL;
+
+	dma_pool_destroy(fotg210->itd_pool);
+	fotg210->itd_pool = NULL;
+
+	if (fotg210->periodic)
+		dma_free_coherent(fotg210_to_hcd(fotg210)->self.controller,
+				fotg210->periodic_size * sizeof(u32),
+				fotg210->periodic, fotg210->periodic_dma);
+	fotg210->periodic = NULL;
+
+	/* shadow periodic table */
+	kfree(fotg210->pshadow);
+	fotg210->pshadow = NULL;
+}
+
+/* remember to add cleanup code (above) if you add anything here */
+static int fotg210_mem_init(struct fotg210_hcd *fotg210, gfp_t flags)
+{
+	int i;
+
+	/* QTDs for control/bulk/intr transfers */
+	fotg210->qtd_pool = dma_pool_create("fotg210_qtd",
+			fotg210_to_hcd(fotg210)->self.controller,
+			sizeof(struct fotg210_qtd),
+			32 /* byte alignment (for hw parts) */,
+			4096 /* can't cross 4K */);
+	if (!fotg210->qtd_pool)
+		goto fail;
+
+	/* QHs for control/bulk/intr transfers */
+	fotg210->qh_pool = dma_pool_create("fotg210_qh",
+			fotg210_to_hcd(fotg210)->self.controller,
+			sizeof(struct fotg210_qh_hw),
+			32 /* byte alignment (for hw parts) */,
+			4096 /* can't cross 4K */);
+	if (!fotg210->qh_pool)
+		goto fail;
+
+	fotg210->async = fotg210_qh_alloc(fotg210, flags);
+	if (!fotg210->async)
+		goto fail;
+
+	/* ITD for high speed ISO transfers */
+	fotg210->itd_pool = dma_pool_create("fotg210_itd",
+			fotg210_to_hcd(fotg210)->self.controller,
+			sizeof(struct fotg210_itd),
+			64 /* byte alignment (for hw parts) */,
+			4096 /* can't cross 4K */);
+	if (!fotg210->itd_pool)
+		goto fail;
+
+	/* Hardware periodic table */
+	fotg210->periodic =
+		dma_alloc_coherent(fotg210_to_hcd(fotg210)->self.controller,
+				fotg210->periodic_size * sizeof(__le32),
+				&fotg210->periodic_dma, 0);
+	if (fotg210->periodic == NULL)
+		goto fail;
+
+	for (i = 0; i < fotg210->periodic_size; i++)
+		fotg210->periodic[i] = FOTG210_LIST_END(fotg210);
+
+	/* software shadow of hardware table */
+	fotg210->pshadow = kcalloc(fotg210->periodic_size, sizeof(void *),
+			flags);
+	if (fotg210->pshadow != NULL)
+		return 0;
+
+fail:
+	fotg210_dbg(fotg210, "couldn't init memory\n");
+	fotg210_mem_cleanup(fotg210);
+	return -ENOMEM;
+}
+/* EHCI hardware queue manipulation ... the core.  QH/QTD manipulation.
+ *
+ * Control, bulk, and interrupt traffic all use "qh" lists.  They list "qtd"
+ * entries describing USB transactions, max 16-20kB/entry (with 4kB-aligned
+ * buffers needed for the larger number).  We use one QH per endpoint, queue
+ * multiple urbs (all three types) per endpoint.  URBs may need several qtds.
+ *
+ * ISO traffic uses "ISO TD" (itd) records, and (along with
+ * interrupts) needs careful scheduling.  Performance improvements can be
+ * an ongoing challenge.  That's in "ehci-sched.c".
+ *
+ * USB 1.1 devices are handled (a) by "companion" OHCI or UHCI root hubs,
+ * or otherwise through transaction translators (TTs) in USB 2.0 hubs using
+ * (b) special fields in qh entries or (c) split iso entries.  TTs will
+ * buffer low/full speed data so the host collects it at high speed.
+ */
+
+/* fill a qtd, returning how much of the buffer we were able to queue up */
+static int qtd_fill(struct fotg210_hcd *fotg210, struct fotg210_qtd *qtd,
+		dma_addr_t buf, size_t len, int token, int maxpacket)
+{
+	int i, count;
+	u64 addr = buf;
+
+	/* one buffer entry per 4K ... first might be short or unaligned */
+	qtd->hw_buf[0] = cpu_to_hc32(fotg210, (u32)addr);
+	qtd->hw_buf_hi[0] = cpu_to_hc32(fotg210, (u32)(addr >> 32));
+	count = 0x1000 - (buf & 0x0fff);	/* rest of that page */
+	if (likely(len < count))		/* ... iff needed */
+		count = len;
+	else {
+		buf +=  0x1000;
+		buf &= ~0x0fff;
+
+		/* per-qtd limit: from 16K to 20K (best alignment) */
+		for (i = 1; count < len && i < 5; i++) {
+			addr = buf;
+			qtd->hw_buf[i] = cpu_to_hc32(fotg210, (u32)addr);
+			qtd->hw_buf_hi[i] = cpu_to_hc32(fotg210,
+					(u32)(addr >> 32));
+			buf += 0x1000;
+			if ((count + 0x1000) < len)
+				count += 0x1000;
+			else
+				count = len;
+		}
+
+		/* short packets may only terminate transfers */
+		if (count != len)
+			count -= (count % maxpacket);
+	}
+	qtd->hw_token = cpu_to_hc32(fotg210, (count << 16) | token);
+	qtd->length = count;
+
+	return count;
+}
+
+static inline void qh_update(struct fotg210_hcd *fotg210,
+		struct fotg210_qh *qh, struct fotg210_qtd *qtd)
+{
+	struct fotg210_qh_hw *hw = qh->hw;
+
+	/* writes to an active overlay are unsafe */
+	BUG_ON(qh->qh_state != QH_STATE_IDLE);
+
+	hw->hw_qtd_next = QTD_NEXT(fotg210, qtd->qtd_dma);
+	hw->hw_alt_next = FOTG210_LIST_END(fotg210);
+
+	/* Except for control endpoints, we make hardware maintain data
+	 * toggle (like OHCI) ... here (re)initialize the toggle in the QH,
+	 * and set the pseudo-toggle in udev. Only usb_clear_halt() will
+	 * ever clear it.
+	 */
+	if (!(hw->hw_info1 & cpu_to_hc32(fotg210, QH_TOGGLE_CTL))) {
+		unsigned is_out, epnum;
+
+		is_out = qh->is_out;
+		epnum = (hc32_to_cpup(fotg210, &hw->hw_info1) >> 8) & 0x0f;
+		if (unlikely(!usb_gettoggle(qh->dev, epnum, is_out))) {
+			hw->hw_token &= ~cpu_to_hc32(fotg210, QTD_TOGGLE);
+			usb_settoggle(qh->dev, epnum, is_out, 1);
+		}
+	}
+
+	hw->hw_token &= cpu_to_hc32(fotg210, QTD_TOGGLE | QTD_STS_PING);
+}
+
+/* if it weren't for a common silicon quirk (writing the dummy into the qh
+ * overlay, so qh->hw_token wrongly becomes inactive/halted), only fault
+ * recovery (including urb dequeue) would need software changes to a QH...
+ */
+static void qh_refresh(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
+{
+	struct fotg210_qtd *qtd;
+
+	if (list_empty(&qh->qtd_list))
+		qtd = qh->dummy;
+	else {
+		qtd = list_entry(qh->qtd_list.next,
+				struct fotg210_qtd, qtd_list);
+		/*
+		 * first qtd may already be partially processed.
+		 * If we come here during unlink, the QH overlay region
+		 * might have reference to the just unlinked qtd. The
+		 * qtd is updated in qh_completions(). Update the QH
+		 * overlay here.
+		 */
+		if (cpu_to_hc32(fotg210, qtd->qtd_dma) == qh->hw->hw_current) {
+			qh->hw->hw_qtd_next = qtd->hw_next;
+			qtd = NULL;
+		}
+	}
+
+	if (qtd)
+		qh_update(fotg210, qh, qtd);
+}
+
+static void qh_link_async(struct fotg210_hcd *fotg210, struct fotg210_qh *qh);
+
+static void fotg210_clear_tt_buffer_complete(struct usb_hcd *hcd,
+		struct usb_host_endpoint *ep)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+	struct fotg210_qh *qh = ep->hcpriv;
+	unsigned long flags;
+
+	spin_lock_irqsave(&fotg210->lock, flags);
+	qh->clearing_tt = 0;
+	if (qh->qh_state == QH_STATE_IDLE && !list_empty(&qh->qtd_list)
+			&& fotg210->rh_state == FOTG210_RH_RUNNING)
+		qh_link_async(fotg210, qh);
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+}
+
+static void fotg210_clear_tt_buffer(struct fotg210_hcd *fotg210,
+		struct fotg210_qh *qh, struct urb *urb, u32 token)
+{
+
+	/* If an async split transaction gets an error or is unlinked,
+	 * the TT buffer may be left in an indeterminate state.  We
+	 * have to clear the TT buffer.
+	 *
+	 * Note: this routine is never called for Isochronous transfers.
+	 */
+	if (urb->dev->tt && !usb_pipeint(urb->pipe) && !qh->clearing_tt) {
+		struct usb_device *tt = urb->dev->tt->hub;
+
+		dev_dbg(&tt->dev,
+				"clear tt buffer port %d, a%d ep%d t%08x\n",
+				urb->dev->ttport, urb->dev->devnum,
+				usb_pipeendpoint(urb->pipe), token);
+
+		if (urb->dev->tt->hub !=
+				fotg210_to_hcd(fotg210)->self.root_hub) {
+			if (usb_hub_clear_tt_buffer(urb) == 0)
+				qh->clearing_tt = 1;
+		}
+	}
+}
+
+static int qtd_copy_status(struct fotg210_hcd *fotg210, struct urb *urb,
+		size_t length, u32 token)
+{
+	int status = -EINPROGRESS;
+
+	/* count IN/OUT bytes, not SETUP (even short packets) */
+	if (likely(QTD_PID(token) != 2))
+		urb->actual_length += length - QTD_LENGTH(token);
+
+	/* don't modify error codes */
+	if (unlikely(urb->unlinked))
+		return status;
+
+	/* force cleanup after short read; not always an error */
+	if (unlikely(IS_SHORT_READ(token)))
+		status = -EREMOTEIO;
+
+	/* serious "can't proceed" faults reported by the hardware */
+	if (token & QTD_STS_HALT) {
+		if (token & QTD_STS_BABBLE) {
+			/* FIXME "must" disable babbling device's port too */
+			status = -EOVERFLOW;
+		/* CERR nonzero + halt --> stall */
+		} else if (QTD_CERR(token)) {
+			status = -EPIPE;
+
+		/* In theory, more than one of the following bits can be set
+		 * since they are sticky and the transaction is retried.
+		 * Which to test first is rather arbitrary.
+		 */
+		} else if (token & QTD_STS_MMF) {
+			/* fs/ls interrupt xfer missed the complete-split */
+			status = -EPROTO;
+		} else if (token & QTD_STS_DBE) {
+			status = (QTD_PID(token) == 1) /* IN ? */
+				? -ENOSR  /* hc couldn't read data */
+				: -ECOMM; /* hc couldn't write data */
+		} else if (token & QTD_STS_XACT) {
+			/* timeout, bad CRC, wrong PID, etc */
+			fotg210_dbg(fotg210, "devpath %s ep%d%s 3strikes\n",
+					urb->dev->devpath,
+					usb_pipeendpoint(urb->pipe),
+					usb_pipein(urb->pipe) ? "in" : "out");
+			status = -EPROTO;
+		} else {	/* unknown */
+			status = -EPROTO;
+		}
+
+		fotg210_dbg(fotg210,
+				"dev%d ep%d%s qtd token %08x --> status %d\n",
+				usb_pipedevice(urb->pipe),
+				usb_pipeendpoint(urb->pipe),
+				usb_pipein(urb->pipe) ? "in" : "out",
+				token, status);
+	}
+
+	return status;
+}
+
+static void fotg210_urb_done(struct fotg210_hcd *fotg210, struct urb *urb,
+		int status)
+__releases(fotg210->lock)
+__acquires(fotg210->lock)
+{
+	if (likely(urb->hcpriv != NULL)) {
+		struct fotg210_qh *qh = (struct fotg210_qh *) urb->hcpriv;
+
+		/* S-mask in a QH means it's an interrupt urb */
+		if ((qh->hw->hw_info2 & cpu_to_hc32(fotg210, QH_SMASK)) != 0) {
+
+			/* ... update hc-wide periodic stats (for usbfs) */
+			fotg210_to_hcd(fotg210)->self.bandwidth_int_reqs--;
+		}
+	}
+
+	if (unlikely(urb->unlinked)) {
+		INCR(fotg210->stats.unlink);
+	} else {
+		/* report non-error and short read status as zero */
+		if (status == -EINPROGRESS || status == -EREMOTEIO)
+			status = 0;
+		INCR(fotg210->stats.complete);
+	}
+
+#ifdef FOTG210_URB_TRACE
+	fotg210_dbg(fotg210,
+			"%s %s urb %p ep%d%s status %d len %d/%d\n",
+			__func__, urb->dev->devpath, urb,
+			usb_pipeendpoint(urb->pipe),
+			usb_pipein(urb->pipe) ? "in" : "out",
+			status,
+			urb->actual_length, urb->transfer_buffer_length);
+#endif
+
+	/* complete() can reenter this HCD */
+	usb_hcd_unlink_urb_from_ep(fotg210_to_hcd(fotg210), urb);
+	spin_unlock(&fotg210->lock);
+	usb_hcd_giveback_urb(fotg210_to_hcd(fotg210), urb, status);
+	spin_lock(&fotg210->lock);
+}
+
+static int qh_schedule(struct fotg210_hcd *fotg210, struct fotg210_qh *qh);
+
+/* Process and free completed qtds for a qh, returning URBs to drivers.
+ * Chases up to qh->hw_current.  Returns number of completions called,
+ * indicating how much "real" work we did.
+ */
+static unsigned qh_completions(struct fotg210_hcd *fotg210,
+		struct fotg210_qh *qh)
+{
+	struct fotg210_qtd *last, *end = qh->dummy;
+	struct fotg210_qtd *qtd, *tmp;
+	int last_status;
+	int stopped;
+	unsigned count = 0;
+	u8 state;
+	struct fotg210_qh_hw *hw = qh->hw;
+
+	if (unlikely(list_empty(&qh->qtd_list)))
+		return count;
+
+	/* completions (or tasks on other cpus) must never clobber HALT
+	 * till we've gone through and cleaned everything up, even when
+	 * they add urbs to this qh's queue or mark them for unlinking.
+	 *
+	 * NOTE:  unlinking expects to be done in queue order.
+	 *
+	 * It's a bug for qh->qh_state to be anything other than
+	 * QH_STATE_IDLE, unless our caller is scan_async() or
+	 * scan_intr().
+	 */
+	state = qh->qh_state;
+	qh->qh_state = QH_STATE_COMPLETING;
+	stopped = (state == QH_STATE_IDLE);
+
+rescan:
+	last = NULL;
+	last_status = -EINPROGRESS;
+	qh->needs_rescan = 0;
+
+	/* remove de-activated QTDs from front of queue.
+	 * after faults (including short reads), cleanup this urb
+	 * then let the queue advance.
+	 * if queue is stopped, handles unlinks.
+	 */
+	list_for_each_entry_safe(qtd, tmp, &qh->qtd_list, qtd_list) {
+		struct urb *urb;
+		u32 token = 0;
+
+		urb = qtd->urb;
+
+		/* clean up any state from previous QTD ...*/
+		if (last) {
+			if (likely(last->urb != urb)) {
+				fotg210_urb_done(fotg210, last->urb,
+						last_status);
+				count++;
+				last_status = -EINPROGRESS;
+			}
+			fotg210_qtd_free(fotg210, last);
+			last = NULL;
+		}
+
+		/* ignore urbs submitted during completions we reported */
+		if (qtd == end)
+			break;
+
+		/* hardware copies qtd out of qh overlay */
+		rmb();
+		token = hc32_to_cpu(fotg210, qtd->hw_token);
+
+		/* always clean up qtds the hc de-activated */
+retry_xacterr:
+		if ((token & QTD_STS_ACTIVE) == 0) {
+
+			/* Report Data Buffer Error: non-fatal but useful */
+			if (token & QTD_STS_DBE)
+				fotg210_dbg(fotg210,
+					"detected DataBufferErr for urb %p ep%d%s len %d, qtd %p [qh %p]\n",
+					urb, usb_endpoint_num(&urb->ep->desc),
+					usb_endpoint_dir_in(&urb->ep->desc)
+						? "in" : "out",
+					urb->transfer_buffer_length, qtd, qh);
+
+			/* on STALL, error, and short reads this urb must
+			 * complete and all its qtds must be recycled.
+			 */
+			if ((token & QTD_STS_HALT) != 0) {
+
+				/* retry transaction errors until we
+				 * reach the software xacterr limit
+				 */
+				if ((token & QTD_STS_XACT) &&
+						QTD_CERR(token) == 0 &&
+						++qh->xacterrs < QH_XACTERR_MAX &&
+						!urb->unlinked) {
+					fotg210_dbg(fotg210,
+						"detected XactErr len %zu/%zu retry %d\n",
+						qtd->length - QTD_LENGTH(token),
+						qtd->length,
+						qh->xacterrs);
+
+					/* reset the token in the qtd and the
+					 * qh overlay (which still contains
+					 * the qtd) so that we pick up from
+					 * where we left off
+					 */
+					token &= ~QTD_STS_HALT;
+					token |= QTD_STS_ACTIVE |
+						 (FOTG210_TUNE_CERR << 10);
+					qtd->hw_token = cpu_to_hc32(fotg210,
+							token);
+					wmb();
+					hw->hw_token = cpu_to_hc32(fotg210,
+							token);
+					goto retry_xacterr;
+				}
+				stopped = 1;
+
+			/* magic dummy for some short reads; qh won't advance.
+			 * that silicon quirk can kick in with this dummy too.
+			 *
+			 * other short reads won't stop the queue, including
+			 * control transfers (status stage handles that) or
+			 * most other single-qtd reads ... the queue stops if
+			 * URB_SHORT_NOT_OK was set so the driver submitting
+			 * the urbs could clean it up.
+			 */
+			} else if (IS_SHORT_READ(token) &&
+					!(qtd->hw_alt_next &
+					FOTG210_LIST_END(fotg210))) {
+				stopped = 1;
+			}
+
+		/* stop scanning when we reach qtds the hc is using */
+		} else if (likely(!stopped
+				&& fotg210->rh_state >= FOTG210_RH_RUNNING)) {
+			break;
+
+		/* scan the whole queue for unlinks whenever it stops */
+		} else {
+			stopped = 1;
+
+			/* cancel everything if we halt, suspend, etc */
+			if (fotg210->rh_state < FOTG210_RH_RUNNING)
+				last_status = -ESHUTDOWN;
+
+			/* this qtd is active; skip it unless a previous qtd
+			 * for its urb faulted, or its urb was canceled.
+			 */
+			else if (last_status == -EINPROGRESS && !urb->unlinked)
+				continue;
+
+			/* qh unlinked; token in overlay may be most current */
+			if (state == QH_STATE_IDLE &&
+					cpu_to_hc32(fotg210, qtd->qtd_dma)
+					== hw->hw_current) {
+				token = hc32_to_cpu(fotg210, hw->hw_token);
+
+				/* An unlink may leave an incomplete
+				 * async transaction in the TT buffer.
+				 * We have to clear it.
+				 */
+				fotg210_clear_tt_buffer(fotg210, qh, urb,
+						token);
+			}
+		}
+
+		/* unless we already know the urb's status, collect qtd status
+		 * and update count of bytes transferred.  in common short read
+		 * cases with only one data qtd (including control transfers),
+		 * queue processing won't halt.  but with two or more qtds (for
+		 * example, with a 32 KB transfer), when the first qtd gets a
+		 * short read the second must be removed by hand.
+		 */
+		if (last_status == -EINPROGRESS) {
+			last_status = qtd_copy_status(fotg210, urb,
+					qtd->length, token);
+			if (last_status == -EREMOTEIO &&
+					(qtd->hw_alt_next &
+					FOTG210_LIST_END(fotg210)))
+				last_status = -EINPROGRESS;
+
+			/* As part of low/full-speed endpoint-halt processing
+			 * we must clear the TT buffer (11.17.5).
+			 */
+			if (unlikely(last_status != -EINPROGRESS &&
+					last_status != -EREMOTEIO)) {
+				/* The TT's in some hubs malfunction when they
+				 * receive this request following a STALL (they
+				 * stop sending isochronous packets).  Since a
+				 * STALL can't leave the TT buffer in a busy
+				 * state (if you believe Figures 11-48 - 11-51
+				 * in the USB 2.0 spec), we won't clear the TT
+				 * buffer in this case.  Strictly speaking this
+				 * is a violation of the spec.
+				 */
+				if (last_status != -EPIPE)
+					fotg210_clear_tt_buffer(fotg210, qh,
+							urb, token);
+			}
+		}
+
+		/* if we're removing something not at the queue head,
+		 * patch the hardware queue pointer.
+		 */
+		if (stopped && qtd->qtd_list.prev != &qh->qtd_list) {
+			last = list_entry(qtd->qtd_list.prev,
+					struct fotg210_qtd, qtd_list);
+			last->hw_next = qtd->hw_next;
+		}
+
+		/* remove qtd; it's recycled after possible urb completion */
+		list_del(&qtd->qtd_list);
+		last = qtd;
+
+		/* reinit the xacterr counter for the next qtd */
+		qh->xacterrs = 0;
+	}
+
+	/* last urb's completion might still need calling */
+	if (likely(last != NULL)) {
+		fotg210_urb_done(fotg210, last->urb, last_status);
+		count++;
+		fotg210_qtd_free(fotg210, last);
+	}
+
+	/* Do we need to rescan for URBs dequeued during a giveback? */
+	if (unlikely(qh->needs_rescan)) {
+		/* If the QH is already unlinked, do the rescan now. */
+		if (state == QH_STATE_IDLE)
+			goto rescan;
+
+		/* Otherwise we have to wait until the QH is fully unlinked.
+		 * Our caller will start an unlink if qh->needs_rescan is
+		 * set.  But if an unlink has already started, nothing needs
+		 * to be done.
+		 */
+		if (state != QH_STATE_LINKED)
+			qh->needs_rescan = 0;
+	}
+
+	/* restore original state; caller must unlink or relink */
+	qh->qh_state = state;
+
+	/* be sure the hardware's done with the qh before refreshing
+	 * it after fault cleanup, or recovering from silicon wrongly
+	 * overlaying the dummy qtd (which reduces DMA chatter).
+	 */
+	if (stopped != 0 || hw->hw_qtd_next == FOTG210_LIST_END(fotg210)) {
+		switch (state) {
+		case QH_STATE_IDLE:
+			qh_refresh(fotg210, qh);
+			break;
+		case QH_STATE_LINKED:
+			/* We won't refresh a QH that's linked (after the HC
+			 * stopped the queue).  That avoids a race:
+			 *  - HC reads first part of QH;
+			 *  - CPU updates that first part and the token;
+			 *  - HC reads rest of that QH, including token
+			 * Result:  HC gets an inconsistent image, and then
+			 * DMAs to/from the wrong memory (corrupting it).
+			 *
+			 * That should be rare for interrupt transfers,
+			 * except maybe high bandwidth ...
+			 */
+
+			/* Tell the caller to start an unlink */
+			qh->needs_rescan = 1;
+			break;
+		/* otherwise, unlink already started */
+		}
+	}
+
+	return count;
+}
+
+/* reverse of qh_urb_transaction:  free a list of TDs.
+ * used for cleanup after errors, before HC sees an URB's TDs.
+ */
+static void qtd_list_free(struct fotg210_hcd *fotg210, struct urb *urb,
+		struct list_head *head)
+{
+	struct fotg210_qtd *qtd, *temp;
+
+	list_for_each_entry_safe(qtd, temp, head, qtd_list) {
+		list_del(&qtd->qtd_list);
+		fotg210_qtd_free(fotg210, qtd);
+	}
+}
+
+/* create a list of filled qtds for this URB; won't link into qh.
+ */
+static struct list_head *qh_urb_transaction(struct fotg210_hcd *fotg210,
+		struct urb *urb, struct list_head *head, gfp_t flags)
+{
+	struct fotg210_qtd *qtd, *qtd_prev;
+	dma_addr_t buf;
+	int len, this_sg_len, maxpacket;
+	int is_input;
+	u32 token;
+	int i;
+	struct scatterlist *sg;
+
+	/*
+	 * URBs map to sequences of QTDs:  one logical transaction
+	 */
+	qtd = fotg210_qtd_alloc(fotg210, flags);
+	if (unlikely(!qtd))
+		return NULL;
+	list_add_tail(&qtd->qtd_list, head);
+	qtd->urb = urb;
+
+	token = QTD_STS_ACTIVE;
+	token |= (FOTG210_TUNE_CERR << 10);
+	/* for split transactions, SplitXState initialized to zero */
+
+	len = urb->transfer_buffer_length;
+	is_input = usb_pipein(urb->pipe);
+	if (usb_pipecontrol(urb->pipe)) {
+		/* SETUP pid */
+		qtd_fill(fotg210, qtd, urb->setup_dma,
+				sizeof(struct usb_ctrlrequest),
+				token | (2 /* "setup" */ << 8), 8);
+
+		/* ... and always at least one more pid */
+		token ^= QTD_TOGGLE;
+		qtd_prev = qtd;
+		qtd = fotg210_qtd_alloc(fotg210, flags);
+		if (unlikely(!qtd))
+			goto cleanup;
+		qtd->urb = urb;
+		qtd_prev->hw_next = QTD_NEXT(fotg210, qtd->qtd_dma);
+		list_add_tail(&qtd->qtd_list, head);
+
+		/* for zero length DATA stages, STATUS is always IN */
+		if (len == 0)
+			token |= (1 /* "in" */ << 8);
+	}
+
+	/*
+	 * data transfer stage:  buffer setup
+	 */
+	i = urb->num_mapped_sgs;
+	if (len > 0 && i > 0) {
+		sg = urb->sg;
+		buf = sg_dma_address(sg);
+
+		/* urb->transfer_buffer_length may be smaller than the
+		 * size of the scatterlist (or vice versa)
+		 */
+		this_sg_len = min_t(int, sg_dma_len(sg), len);
+	} else {
+		sg = NULL;
+		buf = urb->transfer_dma;
+		this_sg_len = len;
+	}
+
+	if (is_input)
+		token |= (1 /* "in" */ << 8);
+	/* else it's already initted to "out" pid (0 << 8) */
+
+	maxpacket = usb_maxpacket(urb->dev, urb->pipe);
+
+	/*
+	 * buffer gets wrapped in one or more qtds;
+	 * last one may be "short" (including zero len)
+	 * and may serve as a control status ack
+	 */
+	for (;;) {
+		int this_qtd_len;
+
+		this_qtd_len = qtd_fill(fotg210, qtd, buf, this_sg_len, token,
+				maxpacket);
+		this_sg_len -= this_qtd_len;
+		len -= this_qtd_len;
+		buf += this_qtd_len;
+
+		/*
+		 * short reads advance to a "magic" dummy instead of the next
+		 * qtd ... that forces the queue to stop, for manual cleanup.
+		 * (this will usually be overridden later.)
+		 */
+		if (is_input)
+			qtd->hw_alt_next = fotg210->async->hw->hw_alt_next;
+
+		/* qh makes control packets use qtd toggle; maybe switch it */
+		if ((maxpacket & (this_qtd_len + (maxpacket - 1))) == 0)
+			token ^= QTD_TOGGLE;
+
+		if (likely(this_sg_len <= 0)) {
+			if (--i <= 0 || len <= 0)
+				break;
+			sg = sg_next(sg);
+			buf = sg_dma_address(sg);
+			this_sg_len = min_t(int, sg_dma_len(sg), len);
+		}
+
+		qtd_prev = qtd;
+		qtd = fotg210_qtd_alloc(fotg210, flags);
+		if (unlikely(!qtd))
+			goto cleanup;
+		qtd->urb = urb;
+		qtd_prev->hw_next = QTD_NEXT(fotg210, qtd->qtd_dma);
+		list_add_tail(&qtd->qtd_list, head);
+	}
+
+	/*
+	 * unless the caller requires manual cleanup after short reads,
+	 * have the alt_next mechanism keep the queue running after the
+	 * last data qtd (the only one, for control and most other cases).
+	 */
+	if (likely((urb->transfer_flags & URB_SHORT_NOT_OK) == 0 ||
+			usb_pipecontrol(urb->pipe)))
+		qtd->hw_alt_next = FOTG210_LIST_END(fotg210);
+
+	/*
+	 * control requests may need a terminating data "status" ack;
+	 * other OUT ones may need a terminating short packet
+	 * (zero length).
+	 */
+	if (likely(urb->transfer_buffer_length != 0)) {
+		int one_more = 0;
+
+		if (usb_pipecontrol(urb->pipe)) {
+			one_more = 1;
+			token ^= 0x0100;	/* "in" <--> "out"  */
+			token |= QTD_TOGGLE;	/* force DATA1 */
+		} else if (usb_pipeout(urb->pipe)
+				&& (urb->transfer_flags & URB_ZERO_PACKET)
+				&& !(urb->transfer_buffer_length % maxpacket)) {
+			one_more = 1;
+		}
+		if (one_more) {
+			qtd_prev = qtd;
+			qtd = fotg210_qtd_alloc(fotg210, flags);
+			if (unlikely(!qtd))
+				goto cleanup;
+			qtd->urb = urb;
+			qtd_prev->hw_next = QTD_NEXT(fotg210, qtd->qtd_dma);
+			list_add_tail(&qtd->qtd_list, head);
+
+			/* never any data in such packets */
+			qtd_fill(fotg210, qtd, 0, 0, token, 0);
+		}
+	}
+
+	/* by default, enable interrupt on urb completion */
+	if (likely(!(urb->transfer_flags & URB_NO_INTERRUPT)))
+		qtd->hw_token |= cpu_to_hc32(fotg210, QTD_IOC);
+	return head;
+
+cleanup:
+	qtd_list_free(fotg210, urb, head);
+	return NULL;
+}
+
+/* Would be best to create all qh's from config descriptors,
+ * when each interface/altsetting is established.  Unlink
+ * any previous qh and cancel its urbs first; endpoints are
+ * implicitly reset then (data toggle too).
+ * That'd mean updating how usbcore talks to HCDs. (2.7?)
+ */
+
+
+/* Each QH holds a qtd list; a QH is used for everything except iso.
+ *
+ * For interrupt urbs, the scheduler must set the microframe scheduling
+ * mask(s) each time the QH gets scheduled.  For highspeed, that's
+ * just one microframe in the s-mask.  For split interrupt transactions
+ * there are additional complications: c-mask, maybe FSTNs.
+ */
+static struct fotg210_qh *qh_make(struct fotg210_hcd *fotg210, struct urb *urb,
+		gfp_t flags)
+{
+	struct fotg210_qh *qh = fotg210_qh_alloc(fotg210, flags);
+	struct usb_host_endpoint *ep;
+	u32 info1 = 0, info2 = 0;
+	int is_input, type;
+	int maxp = 0;
+	int mult;
+	struct usb_tt *tt = urb->dev->tt;
+	struct fotg210_qh_hw *hw;
+
+	if (!qh)
+		return qh;
+
+	/*
+	 * init endpoint/device data for this QH
+	 */
+	info1 |= usb_pipeendpoint(urb->pipe) << 8;
+	info1 |= usb_pipedevice(urb->pipe) << 0;
+
+	is_input = usb_pipein(urb->pipe);
+	type = usb_pipetype(urb->pipe);
+	ep = usb_pipe_endpoint(urb->dev, urb->pipe);
+	maxp = usb_endpoint_maxp(&ep->desc);
+	mult = usb_endpoint_maxp_mult(&ep->desc);
+
+	/* 1024 byte maxpacket is a hardware ceiling.  High bandwidth
+	 * acts like up to 3KB, but is built from smaller packets.
+	 */
+	if (maxp > 1024) {
+		fotg210_dbg(fotg210, "bogus qh maxpacket %d\n", maxp);
+		goto done;
+	}
+
+	/* Compute interrupt scheduling parameters just once, and save.
+	 * - allowing for high bandwidth, how many nsec/uframe are used?
+	 * - split transactions need a second CSPLIT uframe; same question
+	 * - splits also need a schedule gap (for full/low speed I/O)
+	 * - qh has a polling interval
+	 *
+	 * For control/bulk requests, the HC or TT handles these.
+	 */
+	if (type == PIPE_INTERRUPT) {
+		qh->usecs = NS_TO_US(usb_calc_bus_time(USB_SPEED_HIGH,
+				is_input, 0, mult * maxp));
+		qh->start = NO_FRAME;
+
+		if (urb->dev->speed == USB_SPEED_HIGH) {
+			qh->c_usecs = 0;
+			qh->gap_uf = 0;
+
+			qh->period = urb->interval >> 3;
+			if (qh->period == 0 && urb->interval != 1) {
+				/* NOTE interval 2 or 4 uframes could work.
+				 * But interval 1 scheduling is simpler, and
+				 * includes high bandwidth.
+				 */
+				urb->interval = 1;
+			} else if (qh->period > fotg210->periodic_size) {
+				qh->period = fotg210->periodic_size;
+				urb->interval = qh->period << 3;
+			}
+		} else {
+			int think_time;
+
+			/* gap is f(FS/LS transfer times) */
+			qh->gap_uf = 1 + usb_calc_bus_time(urb->dev->speed,
+					is_input, 0, maxp) / (125 * 1000);
+
+			/* FIXME this just approximates SPLIT/CSPLIT times */
+			if (is_input) {		/* SPLIT, gap, CSPLIT+DATA */
+				qh->c_usecs = qh->usecs + HS_USECS(0);
+				qh->usecs = HS_USECS(1);
+			} else {		/* SPLIT+DATA, gap, CSPLIT */
+				qh->usecs += HS_USECS(1);
+				qh->c_usecs = HS_USECS(0);
+			}
+
+			think_time = tt ? tt->think_time : 0;
+			qh->tt_usecs = NS_TO_US(think_time +
+					usb_calc_bus_time(urb->dev->speed,
+					is_input, 0, maxp));
+			qh->period = urb->interval;
+			if (qh->period > fotg210->periodic_size) {
+				qh->period = fotg210->periodic_size;
+				urb->interval = qh->period;
+			}
+		}
+	}
+
+	/* support for tt scheduling, and access to toggles */
+	qh->dev = urb->dev;
+
+	/* using TT? */
+	switch (urb->dev->speed) {
+	case USB_SPEED_LOW:
+		info1 |= QH_LOW_SPEED;
+		fallthrough;
+
+	case USB_SPEED_FULL:
+		/* EPS 0 means "full" */
+		if (type != PIPE_INTERRUPT)
+			info1 |= (FOTG210_TUNE_RL_TT << 28);
+		if (type == PIPE_CONTROL) {
+			info1 |= QH_CONTROL_EP;		/* for TT */
+			info1 |= QH_TOGGLE_CTL;		/* toggle from qtd */
+		}
+		info1 |= maxp << 16;
+
+		info2 |= (FOTG210_TUNE_MULT_TT << 30);
+
+		/* Some Freescale processors have an erratum in which the
+		 * port number in the queue head was 0..N-1 instead of 1..N.
+		 */
+		if (fotg210_has_fsl_portno_bug(fotg210))
+			info2 |= (urb->dev->ttport-1) << 23;
+		else
+			info2 |= urb->dev->ttport << 23;
+
+		/* set the address of the TT; for TDI's integrated
+		 * root hub tt, leave it zeroed.
+		 */
+		if (tt && tt->hub != fotg210_to_hcd(fotg210)->self.root_hub)
+			info2 |= tt->hub->devnum << 16;
+
+		/* NOTE:  if (PIPE_INTERRUPT) { scheduler sets c-mask } */
+
+		break;
+
+	case USB_SPEED_HIGH:		/* no TT involved */
+		info1 |= QH_HIGH_SPEED;
+		if (type == PIPE_CONTROL) {
+			info1 |= (FOTG210_TUNE_RL_HS << 28);
+			info1 |= 64 << 16;	/* usb2 fixed maxpacket */
+			info1 |= QH_TOGGLE_CTL;	/* toggle from qtd */
+			info2 |= (FOTG210_TUNE_MULT_HS << 30);
+		} else if (type == PIPE_BULK) {
+			info1 |= (FOTG210_TUNE_RL_HS << 28);
+			/* The USB spec says that high speed bulk endpoints
+			 * always use 512 byte maxpacket.  But some device
+			 * vendors decided to ignore that, and MSFT is happy
+			 * to help them do so.  So now people expect to use
+			 * such nonconformant devices with Linux too; sigh.
+			 */
+			info1 |= maxp << 16;
+			info2 |= (FOTG210_TUNE_MULT_HS << 30);
+		} else {		/* PIPE_INTERRUPT */
+			info1 |= maxp << 16;
+			info2 |= mult << 30;
+		}
+		break;
+	default:
+		fotg210_dbg(fotg210, "bogus dev %p speed %d\n", urb->dev,
+				urb->dev->speed);
+done:
+		qh_destroy(fotg210, qh);
+		return NULL;
+	}
+
+	/* NOTE:  if (PIPE_INTERRUPT) { scheduler sets s-mask } */
+
+	/* init as live, toggle clear, advance to dummy */
+	qh->qh_state = QH_STATE_IDLE;
+	hw = qh->hw;
+	hw->hw_info1 = cpu_to_hc32(fotg210, info1);
+	hw->hw_info2 = cpu_to_hc32(fotg210, info2);
+	qh->is_out = !is_input;
+	usb_settoggle(urb->dev, usb_pipeendpoint(urb->pipe), !is_input, 1);
+	qh_refresh(fotg210, qh);
+	return qh;
+}
+
+static void enable_async(struct fotg210_hcd *fotg210)
+{
+	if (fotg210->async_count++)
+		return;
+
+	/* Stop waiting to turn off the async schedule */
+	fotg210->enabled_hrtimer_events &= ~BIT(FOTG210_HRTIMER_DISABLE_ASYNC);
+
+	/* Don't start the schedule until ASS is 0 */
+	fotg210_poll_ASS(fotg210);
+	turn_on_io_watchdog(fotg210);
+}
+
+static void disable_async(struct fotg210_hcd *fotg210)
+{
+	if (--fotg210->async_count)
+		return;
+
+	/* The async schedule and async_unlink list are supposed to be empty */
+	WARN_ON(fotg210->async->qh_next.qh || fotg210->async_unlink);
+
+	/* Don't turn off the schedule until ASS is 1 */
+	fotg210_poll_ASS(fotg210);
+}
+
+/* move qh (and its qtds) onto async queue; maybe enable queue.  */
+
+static void qh_link_async(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
+{
+	__hc32 dma = QH_NEXT(fotg210, qh->qh_dma);
+	struct fotg210_qh *head;
+
+	/* Don't link a QH if there's a Clear-TT-Buffer pending */
+	if (unlikely(qh->clearing_tt))
+		return;
+
+	WARN_ON(qh->qh_state != QH_STATE_IDLE);
+
+	/* clear halt and/or toggle; and maybe recover from silicon quirk */
+	qh_refresh(fotg210, qh);
+
+	/* splice right after start */
+	head = fotg210->async;
+	qh->qh_next = head->qh_next;
+	qh->hw->hw_next = head->hw->hw_next;
+	wmb();
+
+	head->qh_next.qh = qh;
+	head->hw->hw_next = dma;
+
+	qh->xacterrs = 0;
+	qh->qh_state = QH_STATE_LINKED;
+	/* qtd completions reported later by interrupt */
+
+	enable_async(fotg210);
+}
+
+/* For control/bulk/interrupt, return QH with these TDs appended.
+ * Allocates and initializes the QH if necessary.
+ * Returns null if it can't allocate a QH it needs to.
+ * If the QH has TDs (urbs) already, that's great.
+ */
+static struct fotg210_qh *qh_append_tds(struct fotg210_hcd *fotg210,
+		struct urb *urb, struct list_head *qtd_list,
+		int epnum, void **ptr)
+{
+	struct fotg210_qh *qh = NULL;
+	__hc32 qh_addr_mask = cpu_to_hc32(fotg210, 0x7f);
+
+	qh = (struct fotg210_qh *) *ptr;
+	if (unlikely(qh == NULL)) {
+		/* can't sleep here, we have fotg210->lock... */
+		qh = qh_make(fotg210, urb, GFP_ATOMIC);
+		*ptr = qh;
+	}
+	if (likely(qh != NULL)) {
+		struct fotg210_qtd *qtd;
+
+		if (unlikely(list_empty(qtd_list)))
+			qtd = NULL;
+		else
+			qtd = list_entry(qtd_list->next, struct fotg210_qtd,
+					qtd_list);
+
+		/* control qh may need patching ... */
+		if (unlikely(epnum == 0)) {
+			/* usb_reset_device() briefly reverts to address 0 */
+			if (usb_pipedevice(urb->pipe) == 0)
+				qh->hw->hw_info1 &= ~qh_addr_mask;
+		}
+
+		/* just one way to queue requests: swap with the dummy qtd.
+		 * only hc or qh_refresh() ever modify the overlay.
+		 */
+		if (likely(qtd != NULL)) {
+			struct fotg210_qtd *dummy;
+			dma_addr_t dma;
+			__hc32 token;
+
+			/* to avoid racing the HC, use the dummy td instead of
+			 * the first td of our list (becomes new dummy).  both
+			 * tds stay deactivated until we're done, when the
+			 * HC is allowed to fetch the old dummy (4.10.2).
+			 */
+			token = qtd->hw_token;
+			qtd->hw_token = HALT_BIT(fotg210);
+
+			dummy = qh->dummy;
+
+			dma = dummy->qtd_dma;
+			*dummy = *qtd;
+			dummy->qtd_dma = dma;
+
+			list_del(&qtd->qtd_list);
+			list_add(&dummy->qtd_list, qtd_list);
+			list_splice_tail(qtd_list, &qh->qtd_list);
+
+			fotg210_qtd_init(fotg210, qtd, qtd->qtd_dma);
+			qh->dummy = qtd;
+
+			/* hc must see the new dummy at list end */
+			dma = qtd->qtd_dma;
+			qtd = list_entry(qh->qtd_list.prev,
+					struct fotg210_qtd, qtd_list);
+			qtd->hw_next = QTD_NEXT(fotg210, dma);
+
+			/* let the hc process these next qtds */
+			wmb();
+			dummy->hw_token = token;
+
+			urb->hcpriv = qh;
+		}
+	}
+	return qh;
+}
+
+static int submit_async(struct fotg210_hcd *fotg210, struct urb *urb,
+		struct list_head *qtd_list, gfp_t mem_flags)
+{
+	int epnum;
+	unsigned long flags;
+	struct fotg210_qh *qh = NULL;
+	int rc;
+
+	epnum = urb->ep->desc.bEndpointAddress;
+
+#ifdef FOTG210_URB_TRACE
+	{
+		struct fotg210_qtd *qtd;
+
+		qtd = list_entry(qtd_list->next, struct fotg210_qtd, qtd_list);
+		fotg210_dbg(fotg210,
+				"%s %s urb %p ep%d%s len %d, qtd %p [qh %p]\n",
+				__func__, urb->dev->devpath, urb,
+				epnum & 0x0f, (epnum & USB_DIR_IN)
+					? "in" : "out",
+				urb->transfer_buffer_length,
+				qtd, urb->ep->hcpriv);
+	}
+#endif
+
+	spin_lock_irqsave(&fotg210->lock, flags);
+	if (unlikely(!HCD_HW_ACCESSIBLE(fotg210_to_hcd(fotg210)))) {
+		rc = -ESHUTDOWN;
+		goto done;
+	}
+	rc = usb_hcd_link_urb_to_ep(fotg210_to_hcd(fotg210), urb);
+	if (unlikely(rc))
+		goto done;
+
+	qh = qh_append_tds(fotg210, urb, qtd_list, epnum, &urb->ep->hcpriv);
+	if (unlikely(qh == NULL)) {
+		usb_hcd_unlink_urb_from_ep(fotg210_to_hcd(fotg210), urb);
+		rc = -ENOMEM;
+		goto done;
+	}
+
+	/* Control/bulk operations through TTs don't need scheduling,
+	 * the HC and TT handle it when the TT has a buffer ready.
+	 */
+	if (likely(qh->qh_state == QH_STATE_IDLE))
+		qh_link_async(fotg210, qh);
+done:
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+	if (unlikely(qh == NULL))
+		qtd_list_free(fotg210, urb, qtd_list);
+	return rc;
+}
+
+static void single_unlink_async(struct fotg210_hcd *fotg210,
+		struct fotg210_qh *qh)
+{
+	struct fotg210_qh *prev;
+
+	/* Add to the end of the list of QHs waiting for the next IAAD */
+	qh->qh_state = QH_STATE_UNLINK;
+	if (fotg210->async_unlink)
+		fotg210->async_unlink_last->unlink_next = qh;
+	else
+		fotg210->async_unlink = qh;
+	fotg210->async_unlink_last = qh;
+
+	/* Unlink it from the schedule */
+	prev = fotg210->async;
+	while (prev->qh_next.qh != qh)
+		prev = prev->qh_next.qh;
+
+	prev->hw->hw_next = qh->hw->hw_next;
+	prev->qh_next = qh->qh_next;
+	if (fotg210->qh_scan_next == qh)
+		fotg210->qh_scan_next = qh->qh_next.qh;
+}
+
+static void start_iaa_cycle(struct fotg210_hcd *fotg210, bool nested)
+{
+	/*
+	 * Do nothing if an IAA cycle is already running or
+	 * if one will be started shortly.
+	 */
+	if (fotg210->async_iaa || fotg210->async_unlinking)
+		return;
+
+	/* Do all the waiting QHs at once */
+	fotg210->async_iaa = fotg210->async_unlink;
+	fotg210->async_unlink = NULL;
+
+	/* If the controller isn't running, we don't have to wait for it */
+	if (unlikely(fotg210->rh_state < FOTG210_RH_RUNNING)) {
+		if (!nested)		/* Avoid recursion */
+			end_unlink_async(fotg210);
+
+	/* Otherwise start a new IAA cycle */
+	} else if (likely(fotg210->rh_state == FOTG210_RH_RUNNING)) {
+		/* Make sure the unlinks are all visible to the hardware */
+		wmb();
+
+		fotg210_writel(fotg210, fotg210->command | CMD_IAAD,
+				&fotg210->regs->command);
+		fotg210_readl(fotg210, &fotg210->regs->command);
+		fotg210_enable_event(fotg210, FOTG210_HRTIMER_IAA_WATCHDOG,
+				true);
+	}
+}
+
+/* the async qh for the qtds being unlinked are now gone from the HC */
+
+static void end_unlink_async(struct fotg210_hcd *fotg210)
+{
+	struct fotg210_qh *qh;
+
+	/* Process the idle QHs */
+restart:
+	fotg210->async_unlinking = true;
+	while (fotg210->async_iaa) {
+		qh = fotg210->async_iaa;
+		fotg210->async_iaa = qh->unlink_next;
+		qh->unlink_next = NULL;
+
+		qh->qh_state = QH_STATE_IDLE;
+		qh->qh_next.qh = NULL;
+
+		qh_completions(fotg210, qh);
+		if (!list_empty(&qh->qtd_list) &&
+				fotg210->rh_state == FOTG210_RH_RUNNING)
+			qh_link_async(fotg210, qh);
+		disable_async(fotg210);
+	}
+	fotg210->async_unlinking = false;
+
+	/* Start a new IAA cycle if any QHs are waiting for it */
+	if (fotg210->async_unlink) {
+		start_iaa_cycle(fotg210, true);
+		if (unlikely(fotg210->rh_state < FOTG210_RH_RUNNING))
+			goto restart;
+	}
+}
+
+static void unlink_empty_async(struct fotg210_hcd *fotg210)
+{
+	struct fotg210_qh *qh, *next;
+	bool stopped = (fotg210->rh_state < FOTG210_RH_RUNNING);
+	bool check_unlinks_later = false;
+
+	/* Unlink all the async QHs that have been empty for a timer cycle */
+	next = fotg210->async->qh_next.qh;
+	while (next) {
+		qh = next;
+		next = qh->qh_next.qh;
+
+		if (list_empty(&qh->qtd_list) &&
+				qh->qh_state == QH_STATE_LINKED) {
+			if (!stopped && qh->unlink_cycle ==
+					fotg210->async_unlink_cycle)
+				check_unlinks_later = true;
+			else
+				single_unlink_async(fotg210, qh);
+		}
+	}
+
+	/* Start a new IAA cycle if any QHs are waiting for it */
+	if (fotg210->async_unlink)
+		start_iaa_cycle(fotg210, false);
+
+	/* QHs that haven't been empty for long enough will be handled later */
+	if (check_unlinks_later) {
+		fotg210_enable_event(fotg210, FOTG210_HRTIMER_ASYNC_UNLINKS,
+				true);
+		++fotg210->async_unlink_cycle;
+	}
+}
+
+/* makes sure the async qh will become idle */
+/* caller must own fotg210->lock */
+
+static void start_unlink_async(struct fotg210_hcd *fotg210,
+		struct fotg210_qh *qh)
+{
+	/*
+	 * If the QH isn't linked then there's nothing we can do
+	 * unless we were called during a giveback, in which case
+	 * qh_completions() has to deal with it.
+	 */
+	if (qh->qh_state != QH_STATE_LINKED) {
+		if (qh->qh_state == QH_STATE_COMPLETING)
+			qh->needs_rescan = 1;
+		return;
+	}
+
+	single_unlink_async(fotg210, qh);
+	start_iaa_cycle(fotg210, false);
+}
+
+static void scan_async(struct fotg210_hcd *fotg210)
+{
+	struct fotg210_qh *qh;
+	bool check_unlinks_later = false;
+
+	fotg210->qh_scan_next = fotg210->async->qh_next.qh;
+	while (fotg210->qh_scan_next) {
+		qh = fotg210->qh_scan_next;
+		fotg210->qh_scan_next = qh->qh_next.qh;
+rescan:
+		/* clean any finished work for this qh */
+		if (!list_empty(&qh->qtd_list)) {
+			int temp;
+
+			/*
+			 * Unlinks could happen here; completion reporting
+			 * drops the lock.  That's why fotg210->qh_scan_next
+			 * always holds the next qh to scan; if the next qh
+			 * gets unlinked then fotg210->qh_scan_next is adjusted
+			 * in single_unlink_async().
+			 */
+			temp = qh_completions(fotg210, qh);
+			if (qh->needs_rescan) {
+				start_unlink_async(fotg210, qh);
+			} else if (list_empty(&qh->qtd_list)
+					&& qh->qh_state == QH_STATE_LINKED) {
+				qh->unlink_cycle = fotg210->async_unlink_cycle;
+				check_unlinks_later = true;
+			} else if (temp != 0)
+				goto rescan;
+		}
+	}
+
+	/*
+	 * Unlink empty entries, reducing DMA usage as well
+	 * as HCD schedule-scanning costs.  Delay for any qh
+	 * we just scanned, there's a not-unusual case that it
+	 * doesn't stay idle for long.
+	 */
+	if (check_unlinks_later && fotg210->rh_state == FOTG210_RH_RUNNING &&
+			!(fotg210->enabled_hrtimer_events &
+			BIT(FOTG210_HRTIMER_ASYNC_UNLINKS))) {
+		fotg210_enable_event(fotg210,
+				FOTG210_HRTIMER_ASYNC_UNLINKS, true);
+		++fotg210->async_unlink_cycle;
+	}
+}
+/* EHCI scheduled transaction support:  interrupt, iso, split iso
+ * These are called "periodic" transactions in the EHCI spec.
+ *
+ * Note that for interrupt transfers, the QH/QTD manipulation is shared
+ * with the "asynchronous" transaction support (control/bulk transfers).
+ * The only real difference is in how interrupt transfers are scheduled.
+ *
+ * For ISO, we make an "iso_stream" head to serve the same role as a QH.
+ * It keeps track of every ITD (or SITD) that's linked, and holds enough
+ * pre-calculated schedule data to make appending to the queue be quick.
+ */
+static int fotg210_get_frame(struct usb_hcd *hcd);
+
+/* periodic_next_shadow - return "next" pointer on shadow list
+ * @periodic: host pointer to qh/itd
+ * @tag: hardware tag for type of this record
+ */
+static union fotg210_shadow *periodic_next_shadow(struct fotg210_hcd *fotg210,
+		union fotg210_shadow *periodic, __hc32 tag)
+{
+	switch (hc32_to_cpu(fotg210, tag)) {
+	case Q_TYPE_QH:
+		return &periodic->qh->qh_next;
+	case Q_TYPE_FSTN:
+		return &periodic->fstn->fstn_next;
+	default:
+		return &periodic->itd->itd_next;
+	}
+}
+
+static __hc32 *shadow_next_periodic(struct fotg210_hcd *fotg210,
+		union fotg210_shadow *periodic, __hc32 tag)
+{
+	switch (hc32_to_cpu(fotg210, tag)) {
+	/* our fotg210_shadow.qh is actually software part */
+	case Q_TYPE_QH:
+		return &periodic->qh->hw->hw_next;
+	/* others are hw parts */
+	default:
+		return periodic->hw_next;
+	}
+}
+
+/* caller must hold fotg210->lock */
+static void periodic_unlink(struct fotg210_hcd *fotg210, unsigned frame,
+		void *ptr)
+{
+	union fotg210_shadow *prev_p = &fotg210->pshadow[frame];
+	__hc32 *hw_p = &fotg210->periodic[frame];
+	union fotg210_shadow here = *prev_p;
+
+	/* find predecessor of "ptr"; hw and shadow lists are in sync */
+	while (here.ptr && here.ptr != ptr) {
+		prev_p = periodic_next_shadow(fotg210, prev_p,
+				Q_NEXT_TYPE(fotg210, *hw_p));
+		hw_p = shadow_next_periodic(fotg210, &here,
+				Q_NEXT_TYPE(fotg210, *hw_p));
+		here = *prev_p;
+	}
+	/* an interrupt entry (at list end) could have been shared */
+	if (!here.ptr)
+		return;
+
+	/* update shadow and hardware lists ... the old "next" pointers
+	 * from ptr may still be in use, the caller updates them.
+	 */
+	*prev_p = *periodic_next_shadow(fotg210, &here,
+			Q_NEXT_TYPE(fotg210, *hw_p));
+
+	*hw_p = *shadow_next_periodic(fotg210, &here,
+			Q_NEXT_TYPE(fotg210, *hw_p));
+}
+
+/* how many of the uframe's 125 usecs are allocated? */
+static unsigned short periodic_usecs(struct fotg210_hcd *fotg210,
+		unsigned frame, unsigned uframe)
+{
+	__hc32 *hw_p = &fotg210->periodic[frame];
+	union fotg210_shadow *q = &fotg210->pshadow[frame];
+	unsigned usecs = 0;
+	struct fotg210_qh_hw *hw;
+
+	while (q->ptr) {
+		switch (hc32_to_cpu(fotg210, Q_NEXT_TYPE(fotg210, *hw_p))) {
+		case Q_TYPE_QH:
+			hw = q->qh->hw;
+			/* is it in the S-mask? */
+			if (hw->hw_info2 & cpu_to_hc32(fotg210, 1 << uframe))
+				usecs += q->qh->usecs;
+			/* ... or C-mask? */
+			if (hw->hw_info2 & cpu_to_hc32(fotg210,
+					1 << (8 + uframe)))
+				usecs += q->qh->c_usecs;
+			hw_p = &hw->hw_next;
+			q = &q->qh->qh_next;
+			break;
+		/* case Q_TYPE_FSTN: */
+		default:
+			/* for "save place" FSTNs, count the relevant INTR
+			 * bandwidth from the previous frame
+			 */
+			if (q->fstn->hw_prev != FOTG210_LIST_END(fotg210))
+				fotg210_dbg(fotg210, "ignoring FSTN cost ...\n");
+
+			hw_p = &q->fstn->hw_next;
+			q = &q->fstn->fstn_next;
+			break;
+		case Q_TYPE_ITD:
+			if (q->itd->hw_transaction[uframe])
+				usecs += q->itd->stream->usecs;
+			hw_p = &q->itd->hw_next;
+			q = &q->itd->itd_next;
+			break;
+		}
+	}
+	if (usecs > fotg210->uframe_periodic_max)
+		fotg210_err(fotg210, "uframe %d sched overrun: %d usecs\n",
+				frame * 8 + uframe, usecs);
+	return usecs;
+}
+
+static int same_tt(struct usb_device *dev1, struct usb_device *dev2)
+{
+	if (!dev1->tt || !dev2->tt)
+		return 0;
+	if (dev1->tt != dev2->tt)
+		return 0;
+	if (dev1->tt->multi)
+		return dev1->ttport == dev2->ttport;
+	else
+		return 1;
+}
+
+/* return true iff the device's transaction translator is available
+ * for a periodic transfer starting at the specified frame, using
+ * all the uframes in the mask.
+ */
+static int tt_no_collision(struct fotg210_hcd *fotg210, unsigned period,
+		struct usb_device *dev, unsigned frame, u32 uf_mask)
+{
+	if (period == 0)	/* error */
+		return 0;
+
+	/* note bandwidth wastage:  split never follows csplit
+	 * (different dev or endpoint) until the next uframe.
+	 * calling convention doesn't make that distinction.
+	 */
+	for (; frame < fotg210->periodic_size; frame += period) {
+		union fotg210_shadow here;
+		__hc32 type;
+		struct fotg210_qh_hw *hw;
+
+		here = fotg210->pshadow[frame];
+		type = Q_NEXT_TYPE(fotg210, fotg210->periodic[frame]);
+		while (here.ptr) {
+			switch (hc32_to_cpu(fotg210, type)) {
+			case Q_TYPE_ITD:
+				type = Q_NEXT_TYPE(fotg210, here.itd->hw_next);
+				here = here.itd->itd_next;
+				continue;
+			case Q_TYPE_QH:
+				hw = here.qh->hw;
+				if (same_tt(dev, here.qh->dev)) {
+					u32 mask;
+
+					mask = hc32_to_cpu(fotg210,
+							hw->hw_info2);
+					/* "knows" no gap is needed */
+					mask |= mask >> 8;
+					if (mask & uf_mask)
+						break;
+				}
+				type = Q_NEXT_TYPE(fotg210, hw->hw_next);
+				here = here.qh->qh_next;
+				continue;
+			/* case Q_TYPE_FSTN: */
+			default:
+				fotg210_dbg(fotg210,
+						"periodic frame %d bogus type %d\n",
+						frame, type);
+			}
+
+			/* collision or error */
+			return 0;
+		}
+	}
+
+	/* no collision */
+	return 1;
+}
+
+static void enable_periodic(struct fotg210_hcd *fotg210)
+{
+	if (fotg210->periodic_count++)
+		return;
+
+	/* Stop waiting to turn off the periodic schedule */
+	fotg210->enabled_hrtimer_events &=
+		~BIT(FOTG210_HRTIMER_DISABLE_PERIODIC);
+
+	/* Don't start the schedule until PSS is 0 */
+	fotg210_poll_PSS(fotg210);
+	turn_on_io_watchdog(fotg210);
+}
+
+static void disable_periodic(struct fotg210_hcd *fotg210)
+{
+	if (--fotg210->periodic_count)
+		return;
+
+	/* Don't turn off the schedule until PSS is 1 */
+	fotg210_poll_PSS(fotg210);
+}
+
+/* periodic schedule slots have iso tds (normal or split) first, then a
+ * sparse tree for active interrupt transfers.
+ *
+ * this just links in a qh; caller guarantees uframe masks are set right.
+ * no FSTN support (yet; fotg210 0.96+)
+ */
+static void qh_link_periodic(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
+{
+	unsigned i;
+	unsigned period = qh->period;
+
+	dev_dbg(&qh->dev->dev,
+			"link qh%d-%04x/%p start %d [%d/%d us]\n", period,
+			hc32_to_cpup(fotg210, &qh->hw->hw_info2) &
+			(QH_CMASK | QH_SMASK), qh, qh->start, qh->usecs,
+			qh->c_usecs);
+
+	/* high bandwidth, or otherwise every microframe */
+	if (period == 0)
+		period = 1;
+
+	for (i = qh->start; i < fotg210->periodic_size; i += period) {
+		union fotg210_shadow *prev = &fotg210->pshadow[i];
+		__hc32 *hw_p = &fotg210->periodic[i];
+		union fotg210_shadow here = *prev;
+		__hc32 type = 0;
+
+		/* skip the iso nodes at list head */
+		while (here.ptr) {
+			type = Q_NEXT_TYPE(fotg210, *hw_p);
+			if (type == cpu_to_hc32(fotg210, Q_TYPE_QH))
+				break;
+			prev = periodic_next_shadow(fotg210, prev, type);
+			hw_p = shadow_next_periodic(fotg210, &here, type);
+			here = *prev;
+		}
+
+		/* sorting each branch by period (slow-->fast)
+		 * enables sharing interior tree nodes
+		 */
+		while (here.ptr && qh != here.qh) {
+			if (qh->period > here.qh->period)
+				break;
+			prev = &here.qh->qh_next;
+			hw_p = &here.qh->hw->hw_next;
+			here = *prev;
+		}
+		/* link in this qh, unless some earlier pass did that */
+		if (qh != here.qh) {
+			qh->qh_next = here;
+			if (here.qh)
+				qh->hw->hw_next = *hw_p;
+			wmb();
+			prev->qh = qh;
+			*hw_p = QH_NEXT(fotg210, qh->qh_dma);
+		}
+	}
+	qh->qh_state = QH_STATE_LINKED;
+	qh->xacterrs = 0;
+
+	/* update per-qh bandwidth for usbfs */
+	fotg210_to_hcd(fotg210)->self.bandwidth_allocated += qh->period
+		? ((qh->usecs + qh->c_usecs) / qh->period)
+		: (qh->usecs * 8);
+
+	list_add(&qh->intr_node, &fotg210->intr_qh_list);
+
+	/* maybe enable periodic schedule processing */
+	++fotg210->intr_count;
+	enable_periodic(fotg210);
+}
+
+static void qh_unlink_periodic(struct fotg210_hcd *fotg210,
+		struct fotg210_qh *qh)
+{
+	unsigned i;
+	unsigned period;
+
+	/*
+	 * If qh is for a low/full-speed device, simply unlinking it
+	 * could interfere with an ongoing split transaction.  To unlink
+	 * it safely would require setting the QH_INACTIVATE bit and
+	 * waiting at least one frame, as described in EHCI 4.12.2.5.
+	 *
+	 * We won't bother with any of this.  Instead, we assume that the
+	 * only reason for unlinking an interrupt QH while the current URB
+	 * is still active is to dequeue all the URBs (flush the whole
+	 * endpoint queue).
+	 *
+	 * If rebalancing the periodic schedule is ever implemented, this
+	 * approach will no longer be valid.
+	 */
+
+	/* high bandwidth, or otherwise part of every microframe */
+	period = qh->period;
+	if (!period)
+		period = 1;
+
+	for (i = qh->start; i < fotg210->periodic_size; i += period)
+		periodic_unlink(fotg210, i, qh);
+
+	/* update per-qh bandwidth for usbfs */
+	fotg210_to_hcd(fotg210)->self.bandwidth_allocated -= qh->period
+		? ((qh->usecs + qh->c_usecs) / qh->period)
+		: (qh->usecs * 8);
+
+	dev_dbg(&qh->dev->dev,
+			"unlink qh%d-%04x/%p start %d [%d/%d us]\n",
+			qh->period, hc32_to_cpup(fotg210, &qh->hw->hw_info2) &
+			(QH_CMASK | QH_SMASK), qh, qh->start, qh->usecs,
+			qh->c_usecs);
+
+	/* qh->qh_next still "live" to HC */
+	qh->qh_state = QH_STATE_UNLINK;
+	qh->qh_next.ptr = NULL;
+
+	if (fotg210->qh_scan_next == qh)
+		fotg210->qh_scan_next = list_entry(qh->intr_node.next,
+				struct fotg210_qh, intr_node);
+	list_del(&qh->intr_node);
+}
+
+static void start_unlink_intr(struct fotg210_hcd *fotg210,
+		struct fotg210_qh *qh)
+{
+	/* If the QH isn't linked then there's nothing we can do
+	 * unless we were called during a giveback, in which case
+	 * qh_completions() has to deal with it.
+	 */
+	if (qh->qh_state != QH_STATE_LINKED) {
+		if (qh->qh_state == QH_STATE_COMPLETING)
+			qh->needs_rescan = 1;
+		return;
+	}
+
+	qh_unlink_periodic(fotg210, qh);
+
+	/* Make sure the unlinks are visible before starting the timer */
+	wmb();
+
+	/*
+	 * The EHCI spec doesn't say how long it takes the controller to
+	 * stop accessing an unlinked interrupt QH.  The timer delay is
+	 * 9 uframes; presumably that will be long enough.
+	 */
+	qh->unlink_cycle = fotg210->intr_unlink_cycle;
+
+	/* New entries go at the end of the intr_unlink list */
+	if (fotg210->intr_unlink)
+		fotg210->intr_unlink_last->unlink_next = qh;
+	else
+		fotg210->intr_unlink = qh;
+	fotg210->intr_unlink_last = qh;
+
+	if (fotg210->intr_unlinking)
+		;	/* Avoid recursive calls */
+	else if (fotg210->rh_state < FOTG210_RH_RUNNING)
+		fotg210_handle_intr_unlinks(fotg210);
+	else if (fotg210->intr_unlink == qh) {
+		fotg210_enable_event(fotg210, FOTG210_HRTIMER_UNLINK_INTR,
+				true);
+		++fotg210->intr_unlink_cycle;
+	}
+}
+
+static void end_unlink_intr(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
+{
+	struct fotg210_qh_hw *hw = qh->hw;
+	int rc;
+
+	qh->qh_state = QH_STATE_IDLE;
+	hw->hw_next = FOTG210_LIST_END(fotg210);
+
+	qh_completions(fotg210, qh);
+
+	/* reschedule QH iff another request is queued */
+	if (!list_empty(&qh->qtd_list) &&
+			fotg210->rh_state == FOTG210_RH_RUNNING) {
+		rc = qh_schedule(fotg210, qh);
+
+		/* An error here likely indicates handshake failure
+		 * or no space left in the schedule.  Neither fault
+		 * should happen often ...
+		 *
+		 * FIXME kill the now-dysfunctional queued urbs
+		 */
+		if (rc != 0)
+			fotg210_err(fotg210, "can't reschedule qh %p, err %d\n",
+					qh, rc);
+	}
+
+	/* maybe turn off periodic schedule */
+	--fotg210->intr_count;
+	disable_periodic(fotg210);
+}
+
+static int check_period(struct fotg210_hcd *fotg210, unsigned frame,
+		unsigned uframe, unsigned period, unsigned usecs)
+{
+	int claimed;
+
+	/* complete split running into next frame?
+	 * given FSTN support, we could sometimes check...
+	 */
+	if (uframe >= 8)
+		return 0;
+
+	/* convert "usecs we need" to "max already claimed" */
+	usecs = fotg210->uframe_periodic_max - usecs;
+
+	/* we "know" 2 and 4 uframe intervals were rejected; so
+	 * for period 0, check _every_ microframe in the schedule.
+	 */
+	if (unlikely(period == 0)) {
+		do {
+			for (uframe = 0; uframe < 7; uframe++) {
+				claimed = periodic_usecs(fotg210, frame,
+						uframe);
+				if (claimed > usecs)
+					return 0;
+			}
+		} while ((frame += 1) < fotg210->periodic_size);
+
+	/* just check the specified uframe, at that period */
+	} else {
+		do {
+			claimed = periodic_usecs(fotg210, frame, uframe);
+			if (claimed > usecs)
+				return 0;
+		} while ((frame += period) < fotg210->periodic_size);
+	}
+
+	/* success! */
+	return 1;
+}
+
+static int check_intr_schedule(struct fotg210_hcd *fotg210, unsigned frame,
+		unsigned uframe, const struct fotg210_qh *qh, __hc32 *c_maskp)
+{
+	int retval = -ENOSPC;
+	u8 mask = 0;
+
+	if (qh->c_usecs && uframe >= 6)		/* FSTN territory? */
+		goto done;
+
+	if (!check_period(fotg210, frame, uframe, qh->period, qh->usecs))
+		goto done;
+	if (!qh->c_usecs) {
+		retval = 0;
+		*c_maskp = 0;
+		goto done;
+	}
+
+	/* Make sure this tt's buffer is also available for CSPLITs.
+	 * We pessimize a bit; probably the typical full speed case
+	 * doesn't need the second CSPLIT.
+	 *
+	 * NOTE:  both SPLIT and CSPLIT could be checked in just
+	 * one smart pass...
+	 */
+	mask = 0x03 << (uframe + qh->gap_uf);
+	*c_maskp = cpu_to_hc32(fotg210, mask << 8);
+
+	mask |= 1 << uframe;
+	if (tt_no_collision(fotg210, qh->period, qh->dev, frame, mask)) {
+		if (!check_period(fotg210, frame, uframe + qh->gap_uf + 1,
+				qh->period, qh->c_usecs))
+			goto done;
+		if (!check_period(fotg210, frame, uframe + qh->gap_uf,
+				qh->period, qh->c_usecs))
+			goto done;
+		retval = 0;
+	}
+done:
+	return retval;
+}
+
+/* "first fit" scheduling policy used the first time through,
+ * or when the previous schedule slot can't be re-used.
+ */
+static int qh_schedule(struct fotg210_hcd *fotg210, struct fotg210_qh *qh)
+{
+	int status;
+	unsigned uframe;
+	__hc32 c_mask;
+	unsigned frame;	/* 0..(qh->period - 1), or NO_FRAME */
+	struct fotg210_qh_hw *hw = qh->hw;
+
+	qh_refresh(fotg210, qh);
+	hw->hw_next = FOTG210_LIST_END(fotg210);
+	frame = qh->start;
+
+	/* reuse the previous schedule slots, if we can */
+	if (frame < qh->period) {
+		uframe = ffs(hc32_to_cpup(fotg210, &hw->hw_info2) & QH_SMASK);
+		status = check_intr_schedule(fotg210, frame, --uframe,
+				qh, &c_mask);
+	} else {
+		uframe = 0;
+		c_mask = 0;
+		status = -ENOSPC;
+	}
+
+	/* else scan the schedule to find a group of slots such that all
+	 * uframes have enough periodic bandwidth available.
+	 */
+	if (status) {
+		/* "normal" case, uframing flexible except with splits */
+		if (qh->period) {
+			int i;
+
+			for (i = qh->period; status && i > 0; --i) {
+				frame = ++fotg210->random_frame % qh->period;
+				for (uframe = 0; uframe < 8; uframe++) {
+					status = check_intr_schedule(fotg210,
+							frame, uframe, qh,
+							&c_mask);
+					if (status == 0)
+						break;
+				}
+			}
+
+		/* qh->period == 0 means every uframe */
+		} else {
+			frame = 0;
+			status = check_intr_schedule(fotg210, 0, 0, qh,
+					&c_mask);
+		}
+		if (status)
+			goto done;
+		qh->start = frame;
+
+		/* reset S-frame and (maybe) C-frame masks */
+		hw->hw_info2 &= cpu_to_hc32(fotg210, ~(QH_CMASK | QH_SMASK));
+		hw->hw_info2 |= qh->period
+			? cpu_to_hc32(fotg210, 1 << uframe)
+			: cpu_to_hc32(fotg210, QH_SMASK);
+		hw->hw_info2 |= c_mask;
+	} else
+		fotg210_dbg(fotg210, "reused qh %p schedule\n", qh);
+
+	/* stuff into the periodic schedule */
+	qh_link_periodic(fotg210, qh);
+done:
+	return status;
+}
+
+static int intr_submit(struct fotg210_hcd *fotg210, struct urb *urb,
+		struct list_head *qtd_list, gfp_t mem_flags)
+{
+	unsigned epnum;
+	unsigned long flags;
+	struct fotg210_qh *qh;
+	int status;
+	struct list_head empty;
+
+	/* get endpoint and transfer/schedule data */
+	epnum = urb->ep->desc.bEndpointAddress;
+
+	spin_lock_irqsave(&fotg210->lock, flags);
+
+	if (unlikely(!HCD_HW_ACCESSIBLE(fotg210_to_hcd(fotg210)))) {
+		status = -ESHUTDOWN;
+		goto done_not_linked;
+	}
+	status = usb_hcd_link_urb_to_ep(fotg210_to_hcd(fotg210), urb);
+	if (unlikely(status))
+		goto done_not_linked;
+
+	/* get qh and force any scheduling errors */
+	INIT_LIST_HEAD(&empty);
+	qh = qh_append_tds(fotg210, urb, &empty, epnum, &urb->ep->hcpriv);
+	if (qh == NULL) {
+		status = -ENOMEM;
+		goto done;
+	}
+	if (qh->qh_state == QH_STATE_IDLE) {
+		status = qh_schedule(fotg210, qh);
+		if (status)
+			goto done;
+	}
+
+	/* then queue the urb's tds to the qh */
+	qh = qh_append_tds(fotg210, urb, qtd_list, epnum, &urb->ep->hcpriv);
+	BUG_ON(qh == NULL);
+
+	/* ... update usbfs periodic stats */
+	fotg210_to_hcd(fotg210)->self.bandwidth_int_reqs++;
+
+done:
+	if (unlikely(status))
+		usb_hcd_unlink_urb_from_ep(fotg210_to_hcd(fotg210), urb);
+done_not_linked:
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+	if (status)
+		qtd_list_free(fotg210, urb, qtd_list);
+
+	return status;
+}
+
+static void scan_intr(struct fotg210_hcd *fotg210)
+{
+	struct fotg210_qh *qh;
+
+	list_for_each_entry_safe(qh, fotg210->qh_scan_next,
+			&fotg210->intr_qh_list, intr_node) {
+rescan:
+		/* clean any finished work for this qh */
+		if (!list_empty(&qh->qtd_list)) {
+			int temp;
+
+			/*
+			 * Unlinks could happen here; completion reporting
+			 * drops the lock.  That's why fotg210->qh_scan_next
+			 * always holds the next qh to scan; if the next qh
+			 * gets unlinked then fotg210->qh_scan_next is adjusted
+			 * in qh_unlink_periodic().
+			 */
+			temp = qh_completions(fotg210, qh);
+			if (unlikely(qh->needs_rescan ||
+					(list_empty(&qh->qtd_list) &&
+					qh->qh_state == QH_STATE_LINKED)))
+				start_unlink_intr(fotg210, qh);
+			else if (temp != 0)
+				goto rescan;
+		}
+	}
+}
+
+/* fotg210_iso_stream ops work with both ITD and SITD */
+
+static struct fotg210_iso_stream *iso_stream_alloc(gfp_t mem_flags)
+{
+	struct fotg210_iso_stream *stream;
+
+	stream = kzalloc(sizeof(*stream), mem_flags);
+	if (likely(stream != NULL)) {
+		INIT_LIST_HEAD(&stream->td_list);
+		INIT_LIST_HEAD(&stream->free_list);
+		stream->next_uframe = -1;
+	}
+	return stream;
+}
+
+static void iso_stream_init(struct fotg210_hcd *fotg210,
+		struct fotg210_iso_stream *stream, struct usb_device *dev,
+		int pipe, unsigned interval)
+{
+	u32 buf1;
+	unsigned epnum, maxp;
+	int is_input;
+	long bandwidth;
+	unsigned multi;
+	struct usb_host_endpoint *ep;
+
+	/*
+	 * this might be a "high bandwidth" highspeed endpoint,
+	 * as encoded in the ep descriptor's wMaxPacket field
+	 */
+	epnum = usb_pipeendpoint(pipe);
+	is_input = usb_pipein(pipe) ? USB_DIR_IN : 0;
+	ep = usb_pipe_endpoint(dev, pipe);
+	maxp = usb_endpoint_maxp(&ep->desc);
+	if (is_input)
+		buf1 = (1 << 11);
+	else
+		buf1 = 0;
+
+	multi = usb_endpoint_maxp_mult(&ep->desc);
+	buf1 |= maxp;
+	maxp *= multi;
+
+	stream->buf0 = cpu_to_hc32(fotg210, (epnum << 8) | dev->devnum);
+	stream->buf1 = cpu_to_hc32(fotg210, buf1);
+	stream->buf2 = cpu_to_hc32(fotg210, multi);
+
+	/* usbfs wants to report the average usecs per frame tied up
+	 * when transfers on this endpoint are scheduled ...
+	 */
+	if (dev->speed == USB_SPEED_FULL) {
+		interval <<= 3;
+		stream->usecs = NS_TO_US(usb_calc_bus_time(dev->speed,
+				is_input, 1, maxp));
+		stream->usecs /= 8;
+	} else {
+		stream->highspeed = 1;
+		stream->usecs = HS_USECS_ISO(maxp);
+	}
+	bandwidth = stream->usecs * 8;
+	bandwidth /= interval;
+
+	stream->bandwidth = bandwidth;
+	stream->udev = dev;
+	stream->bEndpointAddress = is_input | epnum;
+	stream->interval = interval;
+	stream->maxp = maxp;
+}
+
+static struct fotg210_iso_stream *iso_stream_find(struct fotg210_hcd *fotg210,
+		struct urb *urb)
+{
+	unsigned epnum;
+	struct fotg210_iso_stream *stream;
+	struct usb_host_endpoint *ep;
+	unsigned long flags;
+
+	epnum = usb_pipeendpoint(urb->pipe);
+	if (usb_pipein(urb->pipe))
+		ep = urb->dev->ep_in[epnum];
+	else
+		ep = urb->dev->ep_out[epnum];
+
+	spin_lock_irqsave(&fotg210->lock, flags);
+	stream = ep->hcpriv;
+
+	if (unlikely(stream == NULL)) {
+		stream = iso_stream_alloc(GFP_ATOMIC);
+		if (likely(stream != NULL)) {
+			ep->hcpriv = stream;
+			stream->ep = ep;
+			iso_stream_init(fotg210, stream, urb->dev, urb->pipe,
+					urb->interval);
+		}
+
+	/* if dev->ep[epnum] is a QH, hw is set */
+	} else if (unlikely(stream->hw != NULL)) {
+		fotg210_dbg(fotg210, "dev %s ep%d%s, not iso??\n",
+				urb->dev->devpath, epnum,
+				usb_pipein(urb->pipe) ? "in" : "out");
+		stream = NULL;
+	}
+
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+	return stream;
+}
+
+/* fotg210_iso_sched ops can be ITD-only or SITD-only */
+
+static struct fotg210_iso_sched *iso_sched_alloc(unsigned packets,
+		gfp_t mem_flags)
+{
+	struct fotg210_iso_sched *iso_sched;
+
+	iso_sched = kzalloc(struct_size(iso_sched, packet, packets), mem_flags);
+	if (likely(iso_sched != NULL))
+		INIT_LIST_HEAD(&iso_sched->td_list);
+
+	return iso_sched;
+}
+
+static inline void itd_sched_init(struct fotg210_hcd *fotg210,
+		struct fotg210_iso_sched *iso_sched,
+		struct fotg210_iso_stream *stream, struct urb *urb)
+{
+	unsigned i;
+	dma_addr_t dma = urb->transfer_dma;
+
+	/* how many uframes are needed for these transfers */
+	iso_sched->span = urb->number_of_packets * stream->interval;
+
+	/* figure out per-uframe itd fields that we'll need later
+	 * when we fit new itds into the schedule.
+	 */
+	for (i = 0; i < urb->number_of_packets; i++) {
+		struct fotg210_iso_packet *uframe = &iso_sched->packet[i];
+		unsigned length;
+		dma_addr_t buf;
+		u32 trans;
+
+		length = urb->iso_frame_desc[i].length;
+		buf = dma + urb->iso_frame_desc[i].offset;
+
+		trans = FOTG210_ISOC_ACTIVE;
+		trans |= buf & 0x0fff;
+		if (unlikely(((i + 1) == urb->number_of_packets))
+				&& !(urb->transfer_flags & URB_NO_INTERRUPT))
+			trans |= FOTG210_ITD_IOC;
+		trans |= length << 16;
+		uframe->transaction = cpu_to_hc32(fotg210, trans);
+
+		/* might need to cross a buffer page within a uframe */
+		uframe->bufp = (buf & ~(u64)0x0fff);
+		buf += length;
+		if (unlikely((uframe->bufp != (buf & ~(u64)0x0fff))))
+			uframe->cross = 1;
+	}
+}
+
+static void iso_sched_free(struct fotg210_iso_stream *stream,
+		struct fotg210_iso_sched *iso_sched)
+{
+	if (!iso_sched)
+		return;
+	/* caller must hold fotg210->lock!*/
+	list_splice(&iso_sched->td_list, &stream->free_list);
+	kfree(iso_sched);
+}
+
+static int itd_urb_transaction(struct fotg210_iso_stream *stream,
+		struct fotg210_hcd *fotg210, struct urb *urb, gfp_t mem_flags)
+{
+	struct fotg210_itd *itd;
+	dma_addr_t itd_dma;
+	int i;
+	unsigned num_itds;
+	struct fotg210_iso_sched *sched;
+	unsigned long flags;
+
+	sched = iso_sched_alloc(urb->number_of_packets, mem_flags);
+	if (unlikely(sched == NULL))
+		return -ENOMEM;
+
+	itd_sched_init(fotg210, sched, stream, urb);
+
+	if (urb->interval < 8)
+		num_itds = 1 + (sched->span + 7) / 8;
+	else
+		num_itds = urb->number_of_packets;
+
+	/* allocate/init ITDs */
+	spin_lock_irqsave(&fotg210->lock, flags);
+	for (i = 0; i < num_itds; i++) {
+
+		/*
+		 * Use iTDs from the free list, but not iTDs that may
+		 * still be in use by the hardware.
+		 */
+		if (likely(!list_empty(&stream->free_list))) {
+			itd = list_first_entry(&stream->free_list,
+					struct fotg210_itd, itd_list);
+			if (itd->frame == fotg210->now_frame)
+				goto alloc_itd;
+			list_del(&itd->itd_list);
+			itd_dma = itd->itd_dma;
+		} else {
+alloc_itd:
+			spin_unlock_irqrestore(&fotg210->lock, flags);
+			itd = dma_pool_alloc(fotg210->itd_pool, mem_flags,
+					&itd_dma);
+			spin_lock_irqsave(&fotg210->lock, flags);
+			if (!itd) {
+				iso_sched_free(stream, sched);
+				spin_unlock_irqrestore(&fotg210->lock, flags);
+				return -ENOMEM;
+			}
+		}
+
+		memset(itd, 0, sizeof(*itd));
+		itd->itd_dma = itd_dma;
+		list_add(&itd->itd_list, &sched->td_list);
+	}
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+
+	/* temporarily store schedule info in hcpriv */
+	urb->hcpriv = sched;
+	urb->error_count = 0;
+	return 0;
+}
+
+static inline int itd_slot_ok(struct fotg210_hcd *fotg210, u32 mod, u32 uframe,
+		u8 usecs, u32 period)
+{
+	uframe %= period;
+	do {
+		/* can't commit more than uframe_periodic_max usec */
+		if (periodic_usecs(fotg210, uframe >> 3, uframe & 0x7)
+				> (fotg210->uframe_periodic_max - usecs))
+			return 0;
+
+		/* we know urb->interval is 2^N uframes */
+		uframe += period;
+	} while (uframe < mod);
+	return 1;
+}
+
+/* This scheduler plans almost as far into the future as it has actual
+ * periodic schedule slots.  (Affected by TUNE_FLS, which defaults to
+ * "as small as possible" to be cache-friendlier.)  That limits the size
+ * transfers you can stream reliably; avoid more than 64 msec per urb.
+ * Also avoid queue depths of less than fotg210's worst irq latency (affected
+ * by the per-urb URB_NO_INTERRUPT hint, the log2_irq_thresh module parameter,
+ * and other factors); or more than about 230 msec total (for portability,
+ * given FOTG210_TUNE_FLS and the slop).  Or, write a smarter scheduler!
+ */
+
+#define SCHEDULE_SLOP 80 /* microframes */
+
+static int iso_stream_schedule(struct fotg210_hcd *fotg210, struct urb *urb,
+		struct fotg210_iso_stream *stream)
+{
+	u32 now, next, start, period, span;
+	int status;
+	unsigned mod = fotg210->periodic_size << 3;
+	struct fotg210_iso_sched *sched = urb->hcpriv;
+
+	period = urb->interval;
+	span = sched->span;
+
+	if (span > mod - SCHEDULE_SLOP) {
+		fotg210_dbg(fotg210, "iso request %p too long\n", urb);
+		status = -EFBIG;
+		goto fail;
+	}
+
+	now = fotg210_read_frame_index(fotg210) & (mod - 1);
+
+	/* Typical case: reuse current schedule, stream is still active.
+	 * Hopefully there are no gaps from the host falling behind
+	 * (irq delays etc), but if there are we'll take the next
+	 * slot in the schedule, implicitly assuming URB_ISO_ASAP.
+	 */
+	if (likely(!list_empty(&stream->td_list))) {
+		u32 excess;
+
+		/* For high speed devices, allow scheduling within the
+		 * isochronous scheduling threshold.  For full speed devices
+		 * and Intel PCI-based controllers, don't (work around for
+		 * Intel ICH9 bug).
+		 */
+		if (!stream->highspeed && fotg210->fs_i_thresh)
+			next = now + fotg210->i_thresh;
+		else
+			next = now;
+
+		/* Fell behind (by up to twice the slop amount)?
+		 * We decide based on the time of the last currently-scheduled
+		 * slot, not the time of the next available slot.
+		 */
+		excess = (stream->next_uframe - period - next) & (mod - 1);
+		if (excess >= mod - 2 * SCHEDULE_SLOP)
+			start = next + excess - mod + period *
+					DIV_ROUND_UP(mod - excess, period);
+		else
+			start = next + excess + period;
+		if (start - now >= mod) {
+			fotg210_dbg(fotg210, "request %p would overflow (%d+%d >= %d)\n",
+					urb, start - now - period, period,
+					mod);
+			status = -EFBIG;
+			goto fail;
+		}
+	}
+
+	/* need to schedule; when's the next (u)frame we could start?
+	 * this is bigger than fotg210->i_thresh allows; scheduling itself
+	 * isn't free, the slop should handle reasonably slow cpus.  it
+	 * can also help high bandwidth if the dma and irq loads don't
+	 * jump until after the queue is primed.
+	 */
+	else {
+		int done = 0;
+
+		start = SCHEDULE_SLOP + (now & ~0x07);
+
+		/* NOTE:  assumes URB_ISO_ASAP, to limit complexity/bugs */
+
+		/* find a uframe slot with enough bandwidth.
+		 * Early uframes are more precious because full-speed
+		 * iso IN transfers can't use late uframes,
+		 * and therefore they should be allocated last.
+		 */
+		next = start;
+		start += period;
+		do {
+			start--;
+			/* check schedule: enough space? */
+			if (itd_slot_ok(fotg210, mod, start,
+					stream->usecs, period))
+				done = 1;
+		} while (start > next && !done);
+
+		/* no room in the schedule */
+		if (!done) {
+			fotg210_dbg(fotg210, "iso resched full %p (now %d max %d)\n",
+					urb, now, now + mod);
+			status = -ENOSPC;
+			goto fail;
+		}
+	}
+
+	/* Tried to schedule too far into the future? */
+	if (unlikely(start - now + span - period >=
+			mod - 2 * SCHEDULE_SLOP)) {
+		fotg210_dbg(fotg210, "request %p would overflow (%d+%d >= %d)\n",
+				urb, start - now, span - period,
+				mod - 2 * SCHEDULE_SLOP);
+		status = -EFBIG;
+		goto fail;
+	}
+
+	stream->next_uframe = start & (mod - 1);
+
+	/* report high speed start in uframes; full speed, in frames */
+	urb->start_frame = stream->next_uframe;
+	if (!stream->highspeed)
+		urb->start_frame >>= 3;
+
+	/* Make sure scan_isoc() sees these */
+	if (fotg210->isoc_count == 0)
+		fotg210->next_frame = now >> 3;
+	return 0;
+
+fail:
+	iso_sched_free(stream, sched);
+	urb->hcpriv = NULL;
+	return status;
+}
+
+static inline void itd_init(struct fotg210_hcd *fotg210,
+		struct fotg210_iso_stream *stream, struct fotg210_itd *itd)
+{
+	int i;
+
+	/* it's been recently zeroed */
+	itd->hw_next = FOTG210_LIST_END(fotg210);
+	itd->hw_bufp[0] = stream->buf0;
+	itd->hw_bufp[1] = stream->buf1;
+	itd->hw_bufp[2] = stream->buf2;
+
+	for (i = 0; i < 8; i++)
+		itd->index[i] = -1;
+
+	/* All other fields are filled when scheduling */
+}
+
+static inline void itd_patch(struct fotg210_hcd *fotg210,
+		struct fotg210_itd *itd, struct fotg210_iso_sched *iso_sched,
+		unsigned index, u16 uframe)
+{
+	struct fotg210_iso_packet *uf = &iso_sched->packet[index];
+	unsigned pg = itd->pg;
+
+	uframe &= 0x07;
+	itd->index[uframe] = index;
+
+	itd->hw_transaction[uframe] = uf->transaction;
+	itd->hw_transaction[uframe] |= cpu_to_hc32(fotg210, pg << 12);
+	itd->hw_bufp[pg] |= cpu_to_hc32(fotg210, uf->bufp & ~(u32)0);
+	itd->hw_bufp_hi[pg] |= cpu_to_hc32(fotg210, (u32)(uf->bufp >> 32));
+
+	/* iso_frame_desc[].offset must be strictly increasing */
+	if (unlikely(uf->cross)) {
+		u64 bufp = uf->bufp + 4096;
+
+		itd->pg = ++pg;
+		itd->hw_bufp[pg] |= cpu_to_hc32(fotg210, bufp & ~(u32)0);
+		itd->hw_bufp_hi[pg] |= cpu_to_hc32(fotg210, (u32)(bufp >> 32));
+	}
+}
+
+static inline void itd_link(struct fotg210_hcd *fotg210, unsigned frame,
+		struct fotg210_itd *itd)
+{
+	union fotg210_shadow *prev = &fotg210->pshadow[frame];
+	__hc32 *hw_p = &fotg210->periodic[frame];
+	union fotg210_shadow here = *prev;
+	__hc32 type = 0;
+
+	/* skip any iso nodes which might belong to previous microframes */
+	while (here.ptr) {
+		type = Q_NEXT_TYPE(fotg210, *hw_p);
+		if (type == cpu_to_hc32(fotg210, Q_TYPE_QH))
+			break;
+		prev = periodic_next_shadow(fotg210, prev, type);
+		hw_p = shadow_next_periodic(fotg210, &here, type);
+		here = *prev;
+	}
+
+	itd->itd_next = here;
+	itd->hw_next = *hw_p;
+	prev->itd = itd;
+	itd->frame = frame;
+	wmb();
+	*hw_p = cpu_to_hc32(fotg210, itd->itd_dma | Q_TYPE_ITD);
+}
+
+/* fit urb's itds into the selected schedule slot; activate as needed */
+static void itd_link_urb(struct fotg210_hcd *fotg210, struct urb *urb,
+		unsigned mod, struct fotg210_iso_stream *stream)
+{
+	int packet;
+	unsigned next_uframe, uframe, frame;
+	struct fotg210_iso_sched *iso_sched = urb->hcpriv;
+	struct fotg210_itd *itd;
+
+	next_uframe = stream->next_uframe & (mod - 1);
+
+	if (unlikely(list_empty(&stream->td_list))) {
+		fotg210_to_hcd(fotg210)->self.bandwidth_allocated
+				+= stream->bandwidth;
+		fotg210_dbg(fotg210,
+			"schedule devp %s ep%d%s-iso period %d start %d.%d\n",
+			urb->dev->devpath, stream->bEndpointAddress & 0x0f,
+			(stream->bEndpointAddress & USB_DIR_IN) ? "in" : "out",
+			urb->interval,
+			next_uframe >> 3, next_uframe & 0x7);
+	}
+
+	/* fill iTDs uframe by uframe */
+	for (packet = 0, itd = NULL; packet < urb->number_of_packets;) {
+		if (itd == NULL) {
+			/* ASSERT:  we have all necessary itds */
+
+			/* ASSERT:  no itds for this endpoint in this uframe */
+
+			itd = list_entry(iso_sched->td_list.next,
+					struct fotg210_itd, itd_list);
+			list_move_tail(&itd->itd_list, &stream->td_list);
+			itd->stream = stream;
+			itd->urb = urb;
+			itd_init(fotg210, stream, itd);
+		}
+
+		uframe = next_uframe & 0x07;
+		frame = next_uframe >> 3;
+
+		itd_patch(fotg210, itd, iso_sched, packet, uframe);
+
+		next_uframe += stream->interval;
+		next_uframe &= mod - 1;
+		packet++;
+
+		/* link completed itds into the schedule */
+		if (((next_uframe >> 3) != frame)
+				|| packet == urb->number_of_packets) {
+			itd_link(fotg210, frame & (fotg210->periodic_size - 1),
+					itd);
+			itd = NULL;
+		}
+	}
+	stream->next_uframe = next_uframe;
+
+	/* don't need that schedule data any more */
+	iso_sched_free(stream, iso_sched);
+	urb->hcpriv = NULL;
+
+	++fotg210->isoc_count;
+	enable_periodic(fotg210);
+}
+
+#define ISO_ERRS (FOTG210_ISOC_BUF_ERR | FOTG210_ISOC_BABBLE |\
+		FOTG210_ISOC_XACTERR)
+
+/* Process and recycle a completed ITD.  Return true iff its urb completed,
+ * and hence its completion callback probably added things to the hardware
+ * schedule.
+ *
+ * Note that we carefully avoid recycling this descriptor until after any
+ * completion callback runs, so that it won't be reused quickly.  That is,
+ * assuming (a) no more than two urbs per frame on this endpoint, and also
+ * (b) only this endpoint's completions submit URBs.  It seems some silicon
+ * corrupts things if you reuse completed descriptors very quickly...
+ */
+static bool itd_complete(struct fotg210_hcd *fotg210, struct fotg210_itd *itd)
+{
+	struct urb *urb = itd->urb;
+	struct usb_iso_packet_descriptor *desc;
+	u32 t;
+	unsigned uframe;
+	int urb_index = -1;
+	struct fotg210_iso_stream *stream = itd->stream;
+	struct usb_device *dev;
+	bool retval = false;
+
+	/* for each uframe with a packet */
+	for (uframe = 0; uframe < 8; uframe++) {
+		if (likely(itd->index[uframe] == -1))
+			continue;
+		urb_index = itd->index[uframe];
+		desc = &urb->iso_frame_desc[urb_index];
+
+		t = hc32_to_cpup(fotg210, &itd->hw_transaction[uframe]);
+		itd->hw_transaction[uframe] = 0;
+
+		/* report transfer status */
+		if (unlikely(t & ISO_ERRS)) {
+			urb->error_count++;
+			if (t & FOTG210_ISOC_BUF_ERR)
+				desc->status = usb_pipein(urb->pipe)
+					? -ENOSR  /* hc couldn't read */
+					: -ECOMM; /* hc couldn't write */
+			else if (t & FOTG210_ISOC_BABBLE)
+				desc->status = -EOVERFLOW;
+			else /* (t & FOTG210_ISOC_XACTERR) */
+				desc->status = -EPROTO;
+
+			/* HC need not update length with this error */
+			if (!(t & FOTG210_ISOC_BABBLE)) {
+				desc->actual_length = FOTG210_ITD_LENGTH(t);
+				urb->actual_length += desc->actual_length;
+			}
+		} else if (likely((t & FOTG210_ISOC_ACTIVE) == 0)) {
+			desc->status = 0;
+			desc->actual_length = FOTG210_ITD_LENGTH(t);
+			urb->actual_length += desc->actual_length;
+		} else {
+			/* URB was too late */
+			desc->status = -EXDEV;
+		}
+	}
+
+	/* handle completion now? */
+	if (likely((urb_index + 1) != urb->number_of_packets))
+		goto done;
+
+	/* ASSERT: it's really the last itd for this urb
+	 * list_for_each_entry (itd, &stream->td_list, itd_list)
+	 *	BUG_ON (itd->urb == urb);
+	 */
+
+	/* give urb back to the driver; completion often (re)submits */
+	dev = urb->dev;
+	fotg210_urb_done(fotg210, urb, 0);
+	retval = true;
+	urb = NULL;
+
+	--fotg210->isoc_count;
+	disable_periodic(fotg210);
+
+	if (unlikely(list_is_singular(&stream->td_list))) {
+		fotg210_to_hcd(fotg210)->self.bandwidth_allocated
+				-= stream->bandwidth;
+		fotg210_dbg(fotg210,
+			"deschedule devp %s ep%d%s-iso\n",
+			dev->devpath, stream->bEndpointAddress & 0x0f,
+			(stream->bEndpointAddress & USB_DIR_IN) ? "in" : "out");
+	}
+
+done:
+	itd->urb = NULL;
+
+	/* Add to the end of the free list for later reuse */
+	list_move_tail(&itd->itd_list, &stream->free_list);
+
+	/* Recycle the iTDs when the pipeline is empty (ep no longer in use) */
+	if (list_empty(&stream->td_list)) {
+		list_splice_tail_init(&stream->free_list,
+				&fotg210->cached_itd_list);
+		start_free_itds(fotg210);
+	}
+
+	return retval;
+}
+
+static int itd_submit(struct fotg210_hcd *fotg210, struct urb *urb,
+		gfp_t mem_flags)
+{
+	int status = -EINVAL;
+	unsigned long flags;
+	struct fotg210_iso_stream *stream;
+
+	/* Get iso_stream head */
+	stream = iso_stream_find(fotg210, urb);
+	if (unlikely(stream == NULL)) {
+		fotg210_dbg(fotg210, "can't get iso stream\n");
+		return -ENOMEM;
+	}
+	if (unlikely(urb->interval != stream->interval &&
+			fotg210_port_speed(fotg210, 0) ==
+			USB_PORT_STAT_HIGH_SPEED)) {
+		fotg210_dbg(fotg210, "can't change iso interval %d --> %d\n",
+				stream->interval, urb->interval);
+		goto done;
+	}
+
+#ifdef FOTG210_URB_TRACE
+	fotg210_dbg(fotg210,
+			"%s %s urb %p ep%d%s len %d, %d pkts %d uframes[%p]\n",
+			__func__, urb->dev->devpath, urb,
+			usb_pipeendpoint(urb->pipe),
+			usb_pipein(urb->pipe) ? "in" : "out",
+			urb->transfer_buffer_length,
+			urb->number_of_packets, urb->interval,
+			stream);
+#endif
+
+	/* allocate ITDs w/o locking anything */
+	status = itd_urb_transaction(stream, fotg210, urb, mem_flags);
+	if (unlikely(status < 0)) {
+		fotg210_dbg(fotg210, "can't init itds\n");
+		goto done;
+	}
+
+	/* schedule ... need to lock */
+	spin_lock_irqsave(&fotg210->lock, flags);
+	if (unlikely(!HCD_HW_ACCESSIBLE(fotg210_to_hcd(fotg210)))) {
+		status = -ESHUTDOWN;
+		goto done_not_linked;
+	}
+	status = usb_hcd_link_urb_to_ep(fotg210_to_hcd(fotg210), urb);
+	if (unlikely(status))
+		goto done_not_linked;
+	status = iso_stream_schedule(fotg210, urb, stream);
+	if (likely(status == 0))
+		itd_link_urb(fotg210, urb, fotg210->periodic_size << 3, stream);
+	else
+		usb_hcd_unlink_urb_from_ep(fotg210_to_hcd(fotg210), urb);
+done_not_linked:
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+done:
+	return status;
+}
+
+static inline int scan_frame_queue(struct fotg210_hcd *fotg210, unsigned frame,
+		unsigned now_frame, bool live)
+{
+	unsigned uf;
+	bool modified;
+	union fotg210_shadow q, *q_p;
+	__hc32 type, *hw_p;
+
+	/* scan each element in frame's queue for completions */
+	q_p = &fotg210->pshadow[frame];
+	hw_p = &fotg210->periodic[frame];
+	q.ptr = q_p->ptr;
+	type = Q_NEXT_TYPE(fotg210, *hw_p);
+	modified = false;
+
+	while (q.ptr) {
+		switch (hc32_to_cpu(fotg210, type)) {
+		case Q_TYPE_ITD:
+			/* If this ITD is still active, leave it for
+			 * later processing ... check the next entry.
+			 * No need to check for activity unless the
+			 * frame is current.
+			 */
+			if (frame == now_frame && live) {
+				rmb();
+				for (uf = 0; uf < 8; uf++) {
+					if (q.itd->hw_transaction[uf] &
+							ITD_ACTIVE(fotg210))
+						break;
+				}
+				if (uf < 8) {
+					q_p = &q.itd->itd_next;
+					hw_p = &q.itd->hw_next;
+					type = Q_NEXT_TYPE(fotg210,
+							q.itd->hw_next);
+					q = *q_p;
+					break;
+				}
+			}
+
+			/* Take finished ITDs out of the schedule
+			 * and process them:  recycle, maybe report
+			 * URB completion.  HC won't cache the
+			 * pointer for much longer, if at all.
+			 */
+			*q_p = q.itd->itd_next;
+			*hw_p = q.itd->hw_next;
+			type = Q_NEXT_TYPE(fotg210, q.itd->hw_next);
+			wmb();
+			modified = itd_complete(fotg210, q.itd);
+			q = *q_p;
+			break;
+		default:
+			fotg210_dbg(fotg210, "corrupt type %d frame %d shadow %p\n",
+					type, frame, q.ptr);
+			fallthrough;
+		case Q_TYPE_QH:
+		case Q_TYPE_FSTN:
+			/* End of the iTDs and siTDs */
+			q.ptr = NULL;
+			break;
+		}
+
+		/* assume completion callbacks modify the queue */
+		if (unlikely(modified && fotg210->isoc_count > 0))
+			return -EINVAL;
+	}
+	return 0;
+}
+
+static void scan_isoc(struct fotg210_hcd *fotg210)
+{
+	unsigned uf, now_frame, frame, ret;
+	unsigned fmask = fotg210->periodic_size - 1;
+	bool live;
+
+	/*
+	 * When running, scan from last scan point up to "now"
+	 * else clean up by scanning everything that's left.
+	 * Touches as few pages as possible:  cache-friendly.
+	 */
+	if (fotg210->rh_state >= FOTG210_RH_RUNNING) {
+		uf = fotg210_read_frame_index(fotg210);
+		now_frame = (uf >> 3) & fmask;
+		live = true;
+	} else  {
+		now_frame = (fotg210->next_frame - 1) & fmask;
+		live = false;
+	}
+	fotg210->now_frame = now_frame;
+
+	frame = fotg210->next_frame;
+	for (;;) {
+		ret = 1;
+		while (ret != 0)
+			ret = scan_frame_queue(fotg210, frame,
+					now_frame, live);
+
+		/* Stop when we have reached the current frame */
+		if (frame == now_frame)
+			break;
+		frame = (frame + 1) & fmask;
+	}
+	fotg210->next_frame = now_frame;
+}
+
+/* Display / Set uframe_periodic_max
+ */
+static ssize_t uframe_periodic_max_show(struct device *dev,
+		struct device_attribute *attr, char *buf)
+{
+	struct fotg210_hcd *fotg210;
+	int n;
+
+	fotg210 = hcd_to_fotg210(bus_to_hcd(dev_get_drvdata(dev)));
+	n = scnprintf(buf, PAGE_SIZE, "%d\n", fotg210->uframe_periodic_max);
+	return n;
+}
+
+
+static ssize_t uframe_periodic_max_store(struct device *dev,
+		struct device_attribute *attr, const char *buf, size_t count)
+{
+	struct fotg210_hcd *fotg210;
+	unsigned uframe_periodic_max;
+	unsigned frame, uframe;
+	unsigned short allocated_max;
+	unsigned long flags;
+	ssize_t ret;
+
+	fotg210 = hcd_to_fotg210(bus_to_hcd(dev_get_drvdata(dev)));
+	if (kstrtouint(buf, 0, &uframe_periodic_max) < 0)
+		return -EINVAL;
+
+	if (uframe_periodic_max < 100 || uframe_periodic_max >= 125) {
+		fotg210_info(fotg210, "rejecting invalid request for uframe_periodic_max=%u\n",
+				uframe_periodic_max);
+		return -EINVAL;
+	}
+
+	ret = -EINVAL;
+
+	/*
+	 * lock, so that our checking does not race with possible periodic
+	 * bandwidth allocation through submitting new urbs.
+	 */
+	spin_lock_irqsave(&fotg210->lock, flags);
+
+	/*
+	 * for request to decrease max periodic bandwidth, we have to check
+	 * every microframe in the schedule to see whether the decrease is
+	 * possible.
+	 */
+	if (uframe_periodic_max < fotg210->uframe_periodic_max) {
+		allocated_max = 0;
+
+		for (frame = 0; frame < fotg210->periodic_size; ++frame)
+			for (uframe = 0; uframe < 7; ++uframe)
+				allocated_max = max(allocated_max,
+						periodic_usecs(fotg210, frame,
+						uframe));
+
+		if (allocated_max > uframe_periodic_max) {
+			fotg210_info(fotg210,
+					"cannot decrease uframe_periodic_max because periodic bandwidth is already allocated (%u > %u)\n",
+					allocated_max, uframe_periodic_max);
+			goto out_unlock;
+		}
+	}
+
+	/* increasing is always ok */
+
+	fotg210_info(fotg210,
+			"setting max periodic bandwidth to %u%% (== %u usec/uframe)\n",
+			100 * uframe_periodic_max/125, uframe_periodic_max);
+
+	if (uframe_periodic_max != 100)
+		fotg210_warn(fotg210, "max periodic bandwidth set is non-standard\n");
+
+	fotg210->uframe_periodic_max = uframe_periodic_max;
+	ret = count;
+
+out_unlock:
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+	return ret;
+}
+
+static DEVICE_ATTR_RW(uframe_periodic_max);
+
+static inline int create_sysfs_files(struct fotg210_hcd *fotg210)
+{
+	struct device *controller = fotg210_to_hcd(fotg210)->self.controller;
+
+	return device_create_file(controller, &dev_attr_uframe_periodic_max);
+}
+
+static inline void remove_sysfs_files(struct fotg210_hcd *fotg210)
+{
+	struct device *controller = fotg210_to_hcd(fotg210)->self.controller;
+
+	device_remove_file(controller, &dev_attr_uframe_periodic_max);
+}
+/* On some systems, leaving remote wakeup enabled prevents system shutdown.
+ * The firmware seems to think that powering off is a wakeup event!
+ * This routine turns off remote wakeup and everything else, on all ports.
+ */
+static void fotg210_turn_off_all_ports(struct fotg210_hcd *fotg210)
+{
+	u32 __iomem *status_reg = &fotg210->regs->port_status;
+
+	fotg210_writel(fotg210, PORT_RWC_BITS, status_reg);
+}
+
+/* Halt HC, turn off all ports, and let the BIOS use the companion controllers.
+ * Must be called with interrupts enabled and the lock not held.
+ */
+static void fotg210_silence_controller(struct fotg210_hcd *fotg210)
+{
+	fotg210_halt(fotg210);
+
+	spin_lock_irq(&fotg210->lock);
+	fotg210->rh_state = FOTG210_RH_HALTED;
+	fotg210_turn_off_all_ports(fotg210);
+	spin_unlock_irq(&fotg210->lock);
+}
+
+/* fotg210_shutdown kick in for silicon on any bus (not just pci, etc).
+ * This forcibly disables dma and IRQs, helping kexec and other cases
+ * where the next system software may expect clean state.
+ */
+static void fotg210_shutdown(struct usb_hcd *hcd)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+
+	spin_lock_irq(&fotg210->lock);
+	fotg210->shutdown = true;
+	fotg210->rh_state = FOTG210_RH_STOPPING;
+	fotg210->enabled_hrtimer_events = 0;
+	spin_unlock_irq(&fotg210->lock);
+
+	fotg210_silence_controller(fotg210);
+
+	hrtimer_cancel(&fotg210->hrtimer);
+}
+
+/* fotg210_work is called from some interrupts, timers, and so on.
+ * it calls driver completion functions, after dropping fotg210->lock.
+ */
+static void fotg210_work(struct fotg210_hcd *fotg210)
+{
+	/* another CPU may drop fotg210->lock during a schedule scan while
+	 * it reports urb completions.  this flag guards against bogus
+	 * attempts at re-entrant schedule scanning.
+	 */
+	if (fotg210->scanning) {
+		fotg210->need_rescan = true;
+		return;
+	}
+	fotg210->scanning = true;
+
+rescan:
+	fotg210->need_rescan = false;
+	if (fotg210->async_count)
+		scan_async(fotg210);
+	if (fotg210->intr_count > 0)
+		scan_intr(fotg210);
+	if (fotg210->isoc_count > 0)
+		scan_isoc(fotg210);
+	if (fotg210->need_rescan)
+		goto rescan;
+	fotg210->scanning = false;
+
+	/* the IO watchdog guards against hardware or driver bugs that
+	 * misplace IRQs, and should let us run completely without IRQs.
+	 * such lossage has been observed on both VT6202 and VT8235.
+	 */
+	turn_on_io_watchdog(fotg210);
+}
+
+/* Called when the fotg210_hcd module is removed.
+ */
+static void fotg210_stop(struct usb_hcd *hcd)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+
+	fotg210_dbg(fotg210, "stop\n");
+
+	/* no more interrupts ... */
+
+	spin_lock_irq(&fotg210->lock);
+	fotg210->enabled_hrtimer_events = 0;
+	spin_unlock_irq(&fotg210->lock);
+
+	fotg210_quiesce(fotg210);
+	fotg210_silence_controller(fotg210);
+	fotg210_reset(fotg210);
+
+	hrtimer_cancel(&fotg210->hrtimer);
+	remove_sysfs_files(fotg210);
+	remove_debug_files(fotg210);
+
+	/* root hub is shut down separately (first, when possible) */
+	spin_lock_irq(&fotg210->lock);
+	end_free_itds(fotg210);
+	spin_unlock_irq(&fotg210->lock);
+	fotg210_mem_cleanup(fotg210);
+
+#ifdef FOTG210_STATS
+	fotg210_dbg(fotg210, "irq normal %ld err %ld iaa %ld (lost %ld)\n",
+			fotg210->stats.normal, fotg210->stats.error,
+			fotg210->stats.iaa, fotg210->stats.lost_iaa);
+	fotg210_dbg(fotg210, "complete %ld unlink %ld\n",
+			fotg210->stats.complete, fotg210->stats.unlink);
+#endif
+
+	dbg_status(fotg210, "fotg210_stop completed",
+			fotg210_readl(fotg210, &fotg210->regs->status));
+}
+
+/* one-time init, only for memory state */
+static int hcd_fotg210_init(struct usb_hcd *hcd)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+	u32 temp;
+	int retval;
+	u32 hcc_params;
+	struct fotg210_qh_hw *hw;
+
+	spin_lock_init(&fotg210->lock);
+
+	/*
+	 * keep io watchdog by default, those good HCDs could turn off it later
+	 */
+	fotg210->need_io_watchdog = 1;
+
+	hrtimer_init(&fotg210->hrtimer, CLOCK_MONOTONIC, HRTIMER_MODE_ABS);
+	fotg210->hrtimer.function = fotg210_hrtimer_func;
+	fotg210->next_hrtimer_event = FOTG210_HRTIMER_NO_EVENT;
+
+	hcc_params = fotg210_readl(fotg210, &fotg210->caps->hcc_params);
+
+	/*
+	 * by default set standard 80% (== 100 usec/uframe) max periodic
+	 * bandwidth as required by USB 2.0
+	 */
+	fotg210->uframe_periodic_max = 100;
+
+	/*
+	 * hw default: 1K periodic list heads, one per frame.
+	 * periodic_size can shrink by USBCMD update if hcc_params allows.
+	 */
+	fotg210->periodic_size = DEFAULT_I_TDPS;
+	INIT_LIST_HEAD(&fotg210->intr_qh_list);
+	INIT_LIST_HEAD(&fotg210->cached_itd_list);
+
+	if (HCC_PGM_FRAMELISTLEN(hcc_params)) {
+		/* periodic schedule size can be smaller than default */
+		switch (FOTG210_TUNE_FLS) {
+		case 0:
+			fotg210->periodic_size = 1024;
+			break;
+		case 1:
+			fotg210->periodic_size = 512;
+			break;
+		case 2:
+			fotg210->periodic_size = 256;
+			break;
+		default:
+			BUG();
+		}
+	}
+	retval = fotg210_mem_init(fotg210, GFP_KERNEL);
+	if (retval < 0)
+		return retval;
+
+	/* controllers may cache some of the periodic schedule ... */
+	fotg210->i_thresh = 2;
+
+	/*
+	 * dedicate a qh for the async ring head, since we couldn't unlink
+	 * a 'real' qh without stopping the async schedule [4.8].  use it
+	 * as the 'reclamation list head' too.
+	 * its dummy is used in hw_alt_next of many tds, to prevent the qh
+	 * from automatically advancing to the next td after short reads.
+	 */
+	fotg210->async->qh_next.qh = NULL;
+	hw = fotg210->async->hw;
+	hw->hw_next = QH_NEXT(fotg210, fotg210->async->qh_dma);
+	hw->hw_info1 = cpu_to_hc32(fotg210, QH_HEAD);
+	hw->hw_token = cpu_to_hc32(fotg210, QTD_STS_HALT);
+	hw->hw_qtd_next = FOTG210_LIST_END(fotg210);
+	fotg210->async->qh_state = QH_STATE_LINKED;
+	hw->hw_alt_next = QTD_NEXT(fotg210, fotg210->async->dummy->qtd_dma);
+
+	/* clear interrupt enables, set irq latency */
+	if (log2_irq_thresh < 0 || log2_irq_thresh > 6)
+		log2_irq_thresh = 0;
+	temp = 1 << (16 + log2_irq_thresh);
+	if (HCC_CANPARK(hcc_params)) {
+		/* HW default park == 3, on hardware that supports it (like
+		 * NVidia and ALI silicon), maximizes throughput on the async
+		 * schedule by avoiding QH fetches between transfers.
+		 *
+		 * With fast usb storage devices and NForce2, "park" seems to
+		 * make problems:  throughput reduction (!), data errors...
+		 */
+		if (park) {
+			park = min_t(unsigned, park, 3);
+			temp |= CMD_PARK;
+			temp |= park << 8;
+		}
+		fotg210_dbg(fotg210, "park %d\n", park);
+	}
+	if (HCC_PGM_FRAMELISTLEN(hcc_params)) {
+		/* periodic schedule size can be smaller than default */
+		temp &= ~(3 << 2);
+		temp |= (FOTG210_TUNE_FLS << 2);
+	}
+	fotg210->command = temp;
+
+	/* Accept arbitrarily long scatter-gather lists */
+	if (!hcd->localmem_pool)
+		hcd->self.sg_tablesize = ~0;
+	return 0;
+}
+
+/* start HC running; it's halted, hcd_fotg210_init() has been run (once) */
+static int fotg210_run(struct usb_hcd *hcd)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+	u32 temp;
+
+	hcd->uses_new_polling = 1;
+
+	/* EHCI spec section 4.1 */
+
+	fotg210_writel(fotg210, fotg210->periodic_dma,
+			&fotg210->regs->frame_list);
+	fotg210_writel(fotg210, (u32)fotg210->async->qh_dma,
+			&fotg210->regs->async_next);
+
+	/*
+	 * hcc_params controls whether fotg210->regs->segment must (!!!)
+	 * be used; it constrains QH/ITD/SITD and QTD locations.
+	 * dma_pool consistent memory always uses segment zero.
+	 * streaming mappings for I/O buffers, like dma_map_single(),
+	 * can return segments above 4GB, if the device allows.
+	 *
+	 * NOTE:  the dma mask is visible through dev->dma_mask, so
+	 * drivers can pass this info along ... like NETIF_F_HIGHDMA,
+	 * Scsi_Host.highmem_io, and so forth.  It's readonly to all
+	 * host side drivers though.
+	 */
+	fotg210_readl(fotg210, &fotg210->caps->hcc_params);
+
+	/*
+	 * Philips, Intel, and maybe others need CMD_RUN before the
+	 * root hub will detect new devices (why?); NEC doesn't
+	 */
+	fotg210->command &= ~(CMD_IAAD|CMD_PSE|CMD_ASE|CMD_RESET);
+	fotg210->command |= CMD_RUN;
+	fotg210_writel(fotg210, fotg210->command, &fotg210->regs->command);
+	dbg_cmd(fotg210, "init", fotg210->command);
+
+	/*
+	 * Start, enabling full USB 2.0 functionality ... usb 1.1 devices
+	 * are explicitly handed to companion controller(s), so no TT is
+	 * involved with the root hub.  (Except where one is integrated,
+	 * and there's no companion controller unless maybe for USB OTG.)
+	 *
+	 * Turning on the CF flag will transfer ownership of all ports
+	 * from the companions to the EHCI controller.  If any of the
+	 * companions are in the middle of a port reset at the time, it
+	 * could cause trouble.  Write-locking ehci_cf_port_reset_rwsem
+	 * guarantees that no resets are in progress.  After we set CF,
+	 * a short delay lets the hardware catch up; new resets shouldn't
+	 * be started before the port switching actions could complete.
+	 */
+	down_write(&ehci_cf_port_reset_rwsem);
+	fotg210->rh_state = FOTG210_RH_RUNNING;
+	/* unblock posted writes */
+	fotg210_readl(fotg210, &fotg210->regs->command);
+	usleep_range(5000, 10000);
+	up_write(&ehci_cf_port_reset_rwsem);
+	fotg210->last_periodic_enable = ktime_get_real();
+
+	temp = HC_VERSION(fotg210,
+			fotg210_readl(fotg210, &fotg210->caps->hc_capbase));
+	fotg210_info(fotg210,
+			"USB %x.%x started, EHCI %x.%02x\n",
+			((fotg210->sbrn & 0xf0) >> 4), (fotg210->sbrn & 0x0f),
+			temp >> 8, temp & 0xff);
+
+	fotg210_writel(fotg210, INTR_MASK,
+			&fotg210->regs->intr_enable); /* Turn On Interrupts */
+
+	/* GRR this is run-once init(), being done every time the HC starts.
+	 * So long as they're part of class devices, we can't do it init()
+	 * since the class device isn't created that early.
+	 */
+	create_debug_files(fotg210);
+	create_sysfs_files(fotg210);
+
+	return 0;
+}
+
+static int fotg210_setup(struct usb_hcd *hcd)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+	int retval;
+
+	fotg210->regs = (void __iomem *)fotg210->caps +
+			HC_LENGTH(fotg210,
+			fotg210_readl(fotg210, &fotg210->caps->hc_capbase));
+	dbg_hcs_params(fotg210, "reset");
+	dbg_hcc_params(fotg210, "reset");
+
+	/* cache this readonly data; minimize chip reads */
+	fotg210->hcs_params = fotg210_readl(fotg210,
+			&fotg210->caps->hcs_params);
+
+	fotg210->sbrn = HCD_USB2;
+
+	/* data structure init */
+	retval = hcd_fotg210_init(hcd);
+	if (retval)
+		return retval;
+
+	retval = fotg210_halt(fotg210);
+	if (retval)
+		return retval;
+
+	fotg210_reset(fotg210);
+
+	return 0;
+}
+
+static irqreturn_t fotg210_irq(struct usb_hcd *hcd)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+	u32 status, masked_status, pcd_status = 0, cmd;
+	int bh;
+
+	spin_lock(&fotg210->lock);
+
+	status = fotg210_readl(fotg210, &fotg210->regs->status);
+
+	/* e.g. cardbus physical eject */
+	if (status == ~(u32) 0) {
+		fotg210_dbg(fotg210, "device removed\n");
+		goto dead;
+	}
+
+	/*
+	 * We don't use STS_FLR, but some controllers don't like it to
+	 * remain on, so mask it out along with the other status bits.
+	 */
+	masked_status = status & (INTR_MASK | STS_FLR);
+
+	/* Shared IRQ? */
+	if (!masked_status ||
+			unlikely(fotg210->rh_state == FOTG210_RH_HALTED)) {
+		spin_unlock(&fotg210->lock);
+		return IRQ_NONE;
+	}
+
+	/* clear (just) interrupts */
+	fotg210_writel(fotg210, masked_status, &fotg210->regs->status);
+	cmd = fotg210_readl(fotg210, &fotg210->regs->command);
+	bh = 0;
+
+	/* unrequested/ignored: Frame List Rollover */
+	dbg_status(fotg210, "irq", status);
+
+	/* INT, ERR, and IAA interrupt rates can be throttled */
+
+	/* normal [4.15.1.2] or error [4.15.1.1] completion */
+	if (likely((status & (STS_INT|STS_ERR)) != 0)) {
+		if (likely((status & STS_ERR) == 0))
+			INCR(fotg210->stats.normal);
+		else
+			INCR(fotg210->stats.error);
+		bh = 1;
+	}
+
+	/* complete the unlinking of some qh [4.15.2.3] */
+	if (status & STS_IAA) {
+
+		/* Turn off the IAA watchdog */
+		fotg210->enabled_hrtimer_events &=
+			~BIT(FOTG210_HRTIMER_IAA_WATCHDOG);
+
+		/*
+		 * Mild optimization: Allow another IAAD to reset the
+		 * hrtimer, if one occurs before the next expiration.
+		 * In theory we could always cancel the hrtimer, but
+		 * tests show that about half the time it will be reset
+		 * for some other event anyway.
+		 */
+		if (fotg210->next_hrtimer_event == FOTG210_HRTIMER_IAA_WATCHDOG)
+			++fotg210->next_hrtimer_event;
+
+		/* guard against (alleged) silicon errata */
+		if (cmd & CMD_IAAD)
+			fotg210_dbg(fotg210, "IAA with IAAD still set?\n");
+		if (fotg210->async_iaa) {
+			INCR(fotg210->stats.iaa);
+			end_unlink_async(fotg210);
+		} else
+			fotg210_dbg(fotg210, "IAA with nothing unlinked?\n");
+	}
+
+	/* remote wakeup [4.3.1] */
+	if (status & STS_PCD) {
+		int pstatus;
+		u32 __iomem *status_reg = &fotg210->regs->port_status;
+
+		/* kick root hub later */
+		pcd_status = status;
+
+		/* resume root hub? */
+		if (fotg210->rh_state == FOTG210_RH_SUSPENDED)
+			usb_hcd_resume_root_hub(hcd);
+
+		pstatus = fotg210_readl(fotg210, status_reg);
+
+		if (test_bit(0, &fotg210->suspended_ports) &&
+				((pstatus & PORT_RESUME) ||
+				!(pstatus & PORT_SUSPEND)) &&
+				(pstatus & PORT_PE) &&
+				fotg210->reset_done[0] == 0) {
+
+			/* start 20 msec resume signaling from this port,
+			 * and make hub_wq collect PORT_STAT_C_SUSPEND to
+			 * stop that signaling.  Use 5 ms extra for safety,
+			 * like usb_port_resume() does.
+			 */
+			fotg210->reset_done[0] = jiffies + msecs_to_jiffies(25);
+			set_bit(0, &fotg210->resuming_ports);
+			fotg210_dbg(fotg210, "port 1 remote wakeup\n");
+			mod_timer(&hcd->rh_timer, fotg210->reset_done[0]);
+		}
+	}
+
+	/* PCI errors [4.15.2.4] */
+	if (unlikely((status & STS_FATAL) != 0)) {
+		fotg210_err(fotg210, "fatal error\n");
+		dbg_cmd(fotg210, "fatal", cmd);
+		dbg_status(fotg210, "fatal", status);
+dead:
+		usb_hc_died(hcd);
+
+		/* Don't let the controller do anything more */
+		fotg210->shutdown = true;
+		fotg210->rh_state = FOTG210_RH_STOPPING;
+		fotg210->command &= ~(CMD_RUN | CMD_ASE | CMD_PSE);
+		fotg210_writel(fotg210, fotg210->command,
+				&fotg210->regs->command);
+		fotg210_writel(fotg210, 0, &fotg210->regs->intr_enable);
+		fotg210_handle_controller_death(fotg210);
+
+		/* Handle completions when the controller stops */
+		bh = 0;
+	}
+
+	if (bh)
+		fotg210_work(fotg210);
+	spin_unlock(&fotg210->lock);
+	if (pcd_status)
+		usb_hcd_poll_rh_status(hcd);
+	return IRQ_HANDLED;
+}
+
+/* non-error returns are a promise to giveback() the urb later
+ * we drop ownership so next owner (or urb unlink) can get it
+ *
+ * urb + dev is in hcd.self.controller.urb_list
+ * we're queueing TDs onto software and hardware lists
+ *
+ * hcd-specific init for hcpriv hasn't been done yet
+ *
+ * NOTE:  control, bulk, and interrupt share the same code to append TDs
+ * to a (possibly active) QH, and the same QH scanning code.
+ */
+static int fotg210_urb_enqueue(struct usb_hcd *hcd, struct urb *urb,
+		gfp_t mem_flags)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+	struct list_head qtd_list;
+
+	INIT_LIST_HEAD(&qtd_list);
+
+	switch (usb_pipetype(urb->pipe)) {
+	case PIPE_CONTROL:
+		/* qh_completions() code doesn't handle all the fault cases
+		 * in multi-TD control transfers.  Even 1KB is rare anyway.
+		 */
+		if (urb->transfer_buffer_length > (16 * 1024))
+			return -EMSGSIZE;
+		fallthrough;
+	/* case PIPE_BULK: */
+	default:
+		if (!qh_urb_transaction(fotg210, urb, &qtd_list, mem_flags))
+			return -ENOMEM;
+		return submit_async(fotg210, urb, &qtd_list, mem_flags);
+
+	case PIPE_INTERRUPT:
+		if (!qh_urb_transaction(fotg210, urb, &qtd_list, mem_flags))
+			return -ENOMEM;
+		return intr_submit(fotg210, urb, &qtd_list, mem_flags);
+
+	case PIPE_ISOCHRONOUS:
+		return itd_submit(fotg210, urb, mem_flags);
+	}
+}
+
+/* remove from hardware lists
+ * completions normally happen asynchronously
+ */
+
+static int fotg210_urb_dequeue(struct usb_hcd *hcd, struct urb *urb, int status)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+	struct fotg210_qh *qh;
+	unsigned long flags;
+	int rc;
+
+	spin_lock_irqsave(&fotg210->lock, flags);
+	rc = usb_hcd_check_unlink_urb(hcd, urb, status);
+	if (rc)
+		goto done;
+
+	switch (usb_pipetype(urb->pipe)) {
+	/* case PIPE_CONTROL: */
+	/* case PIPE_BULK:*/
+	default:
+		qh = (struct fotg210_qh *) urb->hcpriv;
+		if (!qh)
+			break;
+		switch (qh->qh_state) {
+		case QH_STATE_LINKED:
+		case QH_STATE_COMPLETING:
+			start_unlink_async(fotg210, qh);
+			break;
+		case QH_STATE_UNLINK:
+		case QH_STATE_UNLINK_WAIT:
+			/* already started */
+			break;
+		case QH_STATE_IDLE:
+			/* QH might be waiting for a Clear-TT-Buffer */
+			qh_completions(fotg210, qh);
+			break;
+		}
+		break;
+
+	case PIPE_INTERRUPT:
+		qh = (struct fotg210_qh *) urb->hcpriv;
+		if (!qh)
+			break;
+		switch (qh->qh_state) {
+		case QH_STATE_LINKED:
+		case QH_STATE_COMPLETING:
+			start_unlink_intr(fotg210, qh);
+			break;
+		case QH_STATE_IDLE:
+			qh_completions(fotg210, qh);
+			break;
+		default:
+			fotg210_dbg(fotg210, "bogus qh %p state %d\n",
+					qh, qh->qh_state);
+			goto done;
+		}
+		break;
+
+	case PIPE_ISOCHRONOUS:
+		/* itd... */
+
+		/* wait till next completion, do it then. */
+		/* completion irqs can wait up to 1024 msec, */
+		break;
+	}
+done:
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+	return rc;
+}
+
+/* bulk qh holds the data toggle */
+
+static void fotg210_endpoint_disable(struct usb_hcd *hcd,
+		struct usb_host_endpoint *ep)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+	unsigned long flags;
+	struct fotg210_qh *qh, *tmp;
+
+	/* ASSERT:  any requests/urbs are being unlinked */
+	/* ASSERT:  nobody can be submitting urbs for this any more */
+
+rescan:
+	spin_lock_irqsave(&fotg210->lock, flags);
+	qh = ep->hcpriv;
+	if (!qh)
+		goto done;
+
+	/* endpoints can be iso streams.  for now, we don't
+	 * accelerate iso completions ... so spin a while.
+	 */
+	if (qh->hw == NULL) {
+		struct fotg210_iso_stream *stream = ep->hcpriv;
+
+		if (!list_empty(&stream->td_list))
+			goto idle_timeout;
+
+		/* BUG_ON(!list_empty(&stream->free_list)); */
+		kfree(stream);
+		goto done;
+	}
+
+	if (fotg210->rh_state < FOTG210_RH_RUNNING)
+		qh->qh_state = QH_STATE_IDLE;
+	switch (qh->qh_state) {
+	case QH_STATE_LINKED:
+	case QH_STATE_COMPLETING:
+		for (tmp = fotg210->async->qh_next.qh;
+				tmp && tmp != qh;
+				tmp = tmp->qh_next.qh)
+			continue;
+		/* periodic qh self-unlinks on empty, and a COMPLETING qh
+		 * may already be unlinked.
+		 */
+		if (tmp)
+			start_unlink_async(fotg210, qh);
+		fallthrough;
+	case QH_STATE_UNLINK:		/* wait for hw to finish? */
+	case QH_STATE_UNLINK_WAIT:
+idle_timeout:
+		spin_unlock_irqrestore(&fotg210->lock, flags);
+		schedule_timeout_uninterruptible(1);
+		goto rescan;
+	case QH_STATE_IDLE:		/* fully unlinked */
+		if (qh->clearing_tt)
+			goto idle_timeout;
+		if (list_empty(&qh->qtd_list)) {
+			qh_destroy(fotg210, qh);
+			break;
+		}
+		fallthrough;
+	default:
+		/* caller was supposed to have unlinked any requests;
+		 * that's not our job.  just leak this memory.
+		 */
+		fotg210_err(fotg210, "qh %p (#%02x) state %d%s\n",
+				qh, ep->desc.bEndpointAddress, qh->qh_state,
+				list_empty(&qh->qtd_list) ? "" : "(has tds)");
+		break;
+	}
+done:
+	ep->hcpriv = NULL;
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+}
+
+static void fotg210_endpoint_reset(struct usb_hcd *hcd,
+		struct usb_host_endpoint *ep)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+	struct fotg210_qh *qh;
+	int eptype = usb_endpoint_type(&ep->desc);
+	int epnum = usb_endpoint_num(&ep->desc);
+	int is_out = usb_endpoint_dir_out(&ep->desc);
+	unsigned long flags;
+
+	if (eptype != USB_ENDPOINT_XFER_BULK && eptype != USB_ENDPOINT_XFER_INT)
+		return;
+
+	spin_lock_irqsave(&fotg210->lock, flags);
+	qh = ep->hcpriv;
+
+	/* For Bulk and Interrupt endpoints we maintain the toggle state
+	 * in the hardware; the toggle bits in udev aren't used at all.
+	 * When an endpoint is reset by usb_clear_halt() we must reset
+	 * the toggle bit in the QH.
+	 */
+	if (qh) {
+		usb_settoggle(qh->dev, epnum, is_out, 0);
+		if (!list_empty(&qh->qtd_list)) {
+			WARN_ONCE(1, "clear_halt for a busy endpoint\n");
+		} else if (qh->qh_state == QH_STATE_LINKED ||
+				qh->qh_state == QH_STATE_COMPLETING) {
+
+			/* The toggle value in the QH can't be updated
+			 * while the QH is active.  Unlink it now;
+			 * re-linking will call qh_refresh().
+			 */
+			if (eptype == USB_ENDPOINT_XFER_BULK)
+				start_unlink_async(fotg210, qh);
+			else
+				start_unlink_intr(fotg210, qh);
+		}
+	}
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+}
+
+static int fotg210_get_frame(struct usb_hcd *hcd)
+{
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+
+	return (fotg210_read_frame_index(fotg210) >> 3) %
+		fotg210->periodic_size;
+}
+
+/* The EHCI in ChipIdea HDRC cannot be a separate module or device,
+ * because its registers (and irq) are shared between host/gadget/otg
+ * functions  and in order to facilitate role switching we cannot
+ * give the fotg210 driver exclusive access to those.
+ */
+MODULE_DESCRIPTION(DRIVER_DESC);
+MODULE_AUTHOR(DRIVER_AUTHOR);
+MODULE_LICENSE("GPL");
+
+static const struct hc_driver fotg210_fotg210_hc_driver = {
+	.description		= hcd_name,
+	.product_desc		= "Faraday USB2.0 Host Controller",
+	.hcd_priv_size		= sizeof(struct fotg210_hcd),
+
+	/*
+	 * generic hardware linkage
+	 */
+	.irq			= fotg210_irq,
+	.flags			= HCD_MEMORY | HCD_DMA | HCD_USB2,
+
+	/*
+	 * basic lifecycle operations
+	 */
+	.reset			= hcd_fotg210_init,
+	.start			= fotg210_run,
+	.stop			= fotg210_stop,
+	.shutdown		= fotg210_shutdown,
+
+	/*
+	 * managing i/o requests and associated device resources
+	 */
+	.urb_enqueue		= fotg210_urb_enqueue,
+	.urb_dequeue		= fotg210_urb_dequeue,
+	.endpoint_disable	= fotg210_endpoint_disable,
+	.endpoint_reset		= fotg210_endpoint_reset,
+
+	/*
+	 * scheduling support
+	 */
+	.get_frame_number	= fotg210_get_frame,
+
+	/*
+	 * root hub support
+	 */
+	.hub_status_data	= fotg210_hub_status_data,
+	.hub_control		= fotg210_hub_control,
+	.bus_suspend		= fotg210_bus_suspend,
+	.bus_resume		= fotg210_bus_resume,
+
+	.relinquish_port	= fotg210_relinquish_port,
+	.port_handed_over	= fotg210_port_handed_over,
+
+	.clear_tt_buffer_complete = fotg210_clear_tt_buffer_complete,
+};
+
+static void fotg210_init(struct fotg210_hcd *fotg210)
+{
+	u32 value;
+
+	iowrite32(GMIR_MDEV_INT | GMIR_MOTG_INT | GMIR_INT_POLARITY,
+			&fotg210->regs->gmir);
+
+	value = ioread32(&fotg210->regs->otgcsr);
+	value &= ~OTGCSR_A_BUS_DROP;
+	value |= OTGCSR_A_BUS_REQ;
+	iowrite32(value, &fotg210->regs->otgcsr);
+}
+
+/*
+ * fotg210_hcd_probe - initialize faraday FOTG210 HCDs
+ *
+ * Allocates basic resources for this USB host controller, and
+ * then invokes the start() method for the HCD associated with it
+ * through the hotplug entry's driver_data.
+ */
+static int fotg210_hcd_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct usb_hcd *hcd;
+	struct resource *res;
+	int irq;
+	int retval;
+	struct fotg210_hcd *fotg210;
+
+	if (usb_disabled())
+		return -ENODEV;
+
+	pdev->dev.power.power_state = PMSG_ON;
+
+	irq = platform_get_irq(pdev, 0);
+	if (irq < 0)
+		return irq;
+
+	hcd = usb_create_hcd(&fotg210_fotg210_hc_driver, dev,
+			dev_name(dev));
+	if (!hcd) {
+		dev_err(dev, "failed to create hcd\n");
+		retval = -ENOMEM;
+		goto fail_create_hcd;
+	}
+
+	hcd->has_tt = 1;
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	hcd->regs = devm_ioremap_resource(&pdev->dev, res);
+	if (IS_ERR(hcd->regs)) {
+		retval = PTR_ERR(hcd->regs);
+		goto failed_put_hcd;
+	}
+
+	hcd->rsrc_start = res->start;
+	hcd->rsrc_len = resource_size(res);
+
+	fotg210 = hcd_to_fotg210(hcd);
+
+	fotg210->caps = hcd->regs;
+
+	/* It's OK not to supply this clock */
+	fotg210->pclk = clk_get(dev, "PCLK");
+	if (!IS_ERR(fotg210->pclk)) {
+		retval = clk_prepare_enable(fotg210->pclk);
+		if (retval) {
+			dev_err(dev, "failed to enable PCLK\n");
+			goto failed_put_hcd;
+		}
+	} else if (PTR_ERR(fotg210->pclk) == -EPROBE_DEFER) {
+		/*
+		 * Percolate deferrals, for anything else,
+		 * just live without the clocking.
+		 */
+		retval = PTR_ERR(fotg210->pclk);
+		goto failed_dis_clk;
+	}
+
+	retval = fotg210_setup(hcd);
+	if (retval)
+		goto failed_dis_clk;
+
+	fotg210_init(fotg210);
+
+	retval = usb_add_hcd(hcd, irq, IRQF_SHARED);
+	if (retval) {
+		dev_err(dev, "failed to add hcd with err %d\n", retval);
+		goto failed_dis_clk;
+	}
+	device_wakeup_enable(hcd->self.controller);
+	platform_set_drvdata(pdev, hcd);
+
+	return retval;
+
+failed_dis_clk:
+	if (!IS_ERR(fotg210->pclk)) {
+		clk_disable_unprepare(fotg210->pclk);
+		clk_put(fotg210->pclk);
+	}
+failed_put_hcd:
+	usb_put_hcd(hcd);
+fail_create_hcd:
+	dev_err(dev, "init %s fail, %d\n", dev_name(dev), retval);
+	return retval;
+}
+
+/*
+ * fotg210_hcd_remove - shutdown processing for EHCI HCDs
+ * @dev: USB Host Controller being removed
+ *
+ */
+static int fotg210_hcd_remove(struct platform_device *pdev)
+{
+	struct usb_hcd *hcd = platform_get_drvdata(pdev);
+	struct fotg210_hcd *fotg210 = hcd_to_fotg210(hcd);
+
+	if (!IS_ERR(fotg210->pclk)) {
+		clk_disable_unprepare(fotg210->pclk);
+		clk_put(fotg210->pclk);
+	}
+
+	usb_remove_hcd(hcd);
+	usb_put_hcd(hcd);
+
+	return 0;
+}
+
+#ifdef CONFIG_OF
+static const struct of_device_id fotg210_of_match[] = {
+	{ .compatible = "faraday,fotg210" },
+	{},
+};
+MODULE_DEVICE_TABLE(of, fotg210_of_match);
+#endif
+
+static struct platform_driver fotg210_hcd_driver = {
+	.driver = {
+		.name   = "fotg210-hcd",
+		.of_match_table = of_match_ptr(fotg210_of_match),
+	},
+	.probe  = fotg210_hcd_probe,
+	.remove = fotg210_hcd_remove,
+};
+
+static int __init fotg210_hcd_init(void)
+{
+	int retval = 0;
+
+	if (usb_disabled())
+		return -ENODEV;
+
+	set_bit(USB_EHCI_LOADED, &usb_hcds_loaded);
+	if (test_bit(USB_UHCI_LOADED, &usb_hcds_loaded) ||
+			test_bit(USB_OHCI_LOADED, &usb_hcds_loaded))
+		pr_warn("Warning! fotg210_hcd should always be loaded before uhci_hcd and ohci_hcd, not after\n");
+
+	pr_debug("%s: block sizes: qh %zd qtd %zd itd %zd\n",
+			hcd_name, sizeof(struct fotg210_qh),
+			sizeof(struct fotg210_qtd),
+			sizeof(struct fotg210_itd));
+
+	fotg210_debug_root = debugfs_create_dir("fotg210", usb_debug_root);
+
+	retval = platform_driver_register(&fotg210_hcd_driver);
+	if (retval < 0)
+		goto clean;
+	return retval;
+
+clean:
+	debugfs_remove(fotg210_debug_root);
+	fotg210_debug_root = NULL;
+
+	clear_bit(USB_EHCI_LOADED, &usb_hcds_loaded);
+	return retval;
+}
+module_init(fotg210_hcd_init);
+
+static void __exit fotg210_hcd_cleanup(void)
+{
+	platform_driver_unregister(&fotg210_hcd_driver);
+	debugfs_remove(fotg210_debug_root);
+	clear_bit(USB_EHCI_LOADED, &usb_hcds_loaded);
+}
+module_exit(fotg210_hcd_cleanup);
--- a/drivers/usb/gadget/udc/fotg210-udc.c
+++ /dev/null
@@ -1,1239 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0
-/*
- * FOTG210 UDC Driver supports Bulk transfer so far
- *
- * Copyright (C) 2013 Faraday Technology Corporation
- *
- * Author : Yuan-Hsin Chen <yhchen@faraday-tech.com>
- */
-
-#include <linux/dma-mapping.h>
-#include <linux/err.h>
-#include <linux/interrupt.h>
-#include <linux/io.h>
-#include <linux/module.h>
-#include <linux/platform_device.h>
-#include <linux/usb/ch9.h>
-#include <linux/usb/gadget.h>
-
-#include "fotg210.h"
-
-#define	DRIVER_DESC	"FOTG210 USB Device Controller Driver"
-#define	DRIVER_VERSION	"30-April-2013"
-
-static const char udc_name[] = "fotg210_udc";
-static const char * const fotg210_ep_name[] = {
-	"ep0", "ep1", "ep2", "ep3", "ep4"};
-
-static void fotg210_disable_fifo_int(struct fotg210_ep *ep)
-{
-	u32 value = ioread32(ep->fotg210->reg + FOTG210_DMISGR1);
-
-	if (ep->dir_in)
-		value |= DMISGR1_MF_IN_INT(ep->epnum - 1);
-	else
-		value |= DMISGR1_MF_OUTSPK_INT(ep->epnum - 1);
-	iowrite32(value, ep->fotg210->reg + FOTG210_DMISGR1);
-}
-
-static void fotg210_enable_fifo_int(struct fotg210_ep *ep)
-{
-	u32 value = ioread32(ep->fotg210->reg + FOTG210_DMISGR1);
-
-	if (ep->dir_in)
-		value &= ~DMISGR1_MF_IN_INT(ep->epnum - 1);
-	else
-		value &= ~DMISGR1_MF_OUTSPK_INT(ep->epnum - 1);
-	iowrite32(value, ep->fotg210->reg + FOTG210_DMISGR1);
-}
-
-static void fotg210_set_cxdone(struct fotg210_udc *fotg210)
-{
-	u32 value = ioread32(fotg210->reg + FOTG210_DCFESR);
-
-	value |= DCFESR_CX_DONE;
-	iowrite32(value, fotg210->reg + FOTG210_DCFESR);
-}
-
-static void fotg210_done(struct fotg210_ep *ep, struct fotg210_request *req,
-			int status)
-{
-	list_del_init(&req->queue);
-
-	/* don't modify queue heads during completion callback */
-	if (ep->fotg210->gadget.speed == USB_SPEED_UNKNOWN)
-		req->req.status = -ESHUTDOWN;
-	else
-		req->req.status = status;
-
-	spin_unlock(&ep->fotg210->lock);
-	usb_gadget_giveback_request(&ep->ep, &req->req);
-	spin_lock(&ep->fotg210->lock);
-
-	if (ep->epnum) {
-		if (list_empty(&ep->queue))
-			fotg210_disable_fifo_int(ep);
-	} else {
-		fotg210_set_cxdone(ep->fotg210);
-	}
-}
-
-static void fotg210_fifo_ep_mapping(struct fotg210_ep *ep, u32 epnum,
-				u32 dir_in)
-{
-	struct fotg210_udc *fotg210 = ep->fotg210;
-	u32 val;
-
-	/* Driver should map an ep to a fifo and then map the fifo
-	 * to the ep. What a brain-damaged design!
-	 */
-
-	/* map a fifo to an ep */
-	val = ioread32(fotg210->reg + FOTG210_EPMAP);
-	val &= ~EPMAP_FIFONOMSK(epnum, dir_in);
-	val |= EPMAP_FIFONO(epnum, dir_in);
-	iowrite32(val, fotg210->reg + FOTG210_EPMAP);
-
-	/* map the ep to the fifo */
-	val = ioread32(fotg210->reg + FOTG210_FIFOMAP);
-	val &= ~FIFOMAP_EPNOMSK(epnum);
-	val |= FIFOMAP_EPNO(epnum);
-	iowrite32(val, fotg210->reg + FOTG210_FIFOMAP);
-
-	/* enable fifo */
-	val = ioread32(fotg210->reg + FOTG210_FIFOCF);
-	val |= FIFOCF_FIFO_EN(epnum - 1);
-	iowrite32(val, fotg210->reg + FOTG210_FIFOCF);
-}
-
-static void fotg210_set_fifo_dir(struct fotg210_ep *ep, u32 epnum, u32 dir_in)
-{
-	struct fotg210_udc *fotg210 = ep->fotg210;
-	u32 val;
-
-	val = ioread32(fotg210->reg + FOTG210_FIFOMAP);
-	val |= (dir_in ? FIFOMAP_DIRIN(epnum - 1) : FIFOMAP_DIROUT(epnum - 1));
-	iowrite32(val, fotg210->reg + FOTG210_FIFOMAP);
-}
-
-static void fotg210_set_tfrtype(struct fotg210_ep *ep, u32 epnum, u32 type)
-{
-	struct fotg210_udc *fotg210 = ep->fotg210;
-	u32 val;
-
-	val = ioread32(fotg210->reg + FOTG210_FIFOCF);
-	val |= FIFOCF_TYPE(type, epnum - 1);
-	iowrite32(val, fotg210->reg + FOTG210_FIFOCF);
-}
-
-static void fotg210_set_mps(struct fotg210_ep *ep, u32 epnum, u32 mps,
-				u32 dir_in)
-{
-	struct fotg210_udc *fotg210 = ep->fotg210;
-	u32 val;
-	u32 offset = dir_in ? FOTG210_INEPMPSR(epnum) :
-				FOTG210_OUTEPMPSR(epnum);
-
-	val = ioread32(fotg210->reg + offset);
-	val |= INOUTEPMPSR_MPS(mps);
-	iowrite32(val, fotg210->reg + offset);
-}
-
-static int fotg210_config_ep(struct fotg210_ep *ep,
-		     const struct usb_endpoint_descriptor *desc)
-{
-	struct fotg210_udc *fotg210 = ep->fotg210;
-
-	fotg210_set_fifo_dir(ep, ep->epnum, ep->dir_in);
-	fotg210_set_tfrtype(ep, ep->epnum, ep->type);
-	fotg210_set_mps(ep, ep->epnum, ep->ep.maxpacket, ep->dir_in);
-	fotg210_fifo_ep_mapping(ep, ep->epnum, ep->dir_in);
-
-	fotg210->ep[ep->epnum] = ep;
-
-	return 0;
-}
-
-static int fotg210_ep_enable(struct usb_ep *_ep,
-			  const struct usb_endpoint_descriptor *desc)
-{
-	struct fotg210_ep *ep;
-
-	ep = container_of(_ep, struct fotg210_ep, ep);
-
-	ep->desc = desc;
-	ep->epnum = usb_endpoint_num(desc);
-	ep->type = usb_endpoint_type(desc);
-	ep->dir_in = usb_endpoint_dir_in(desc);
-	ep->ep.maxpacket = usb_endpoint_maxp(desc);
-
-	return fotg210_config_ep(ep, desc);
-}
-
-static void fotg210_reset_tseq(struct fotg210_udc *fotg210, u8 epnum)
-{
-	struct fotg210_ep *ep = fotg210->ep[epnum];
-	u32 value;
-	void __iomem *reg;
-
-	reg = (ep->dir_in) ?
-		fotg210->reg + FOTG210_INEPMPSR(epnum) :
-		fotg210->reg + FOTG210_OUTEPMPSR(epnum);
-
-	/* Note: Driver needs to set and clear INOUTEPMPSR_RESET_TSEQ
-	 *	 bit. Controller wouldn't clear this bit. WTF!!!
-	 */
-
-	value = ioread32(reg);
-	value |= INOUTEPMPSR_RESET_TSEQ;
-	iowrite32(value, reg);
-
-	value = ioread32(reg);
-	value &= ~INOUTEPMPSR_RESET_TSEQ;
-	iowrite32(value, reg);
-}
-
-static int fotg210_ep_release(struct fotg210_ep *ep)
-{
-	if (!ep->epnum)
-		return 0;
-	ep->epnum = 0;
-	ep->stall = 0;
-	ep->wedged = 0;
-
-	fotg210_reset_tseq(ep->fotg210, ep->epnum);
-
-	return 0;
-}
-
-static int fotg210_ep_disable(struct usb_ep *_ep)
-{
-	struct fotg210_ep *ep;
-	struct fotg210_request *req;
-	unsigned long flags;
-
-	BUG_ON(!_ep);
-
-	ep = container_of(_ep, struct fotg210_ep, ep);
-
-	while (!list_empty(&ep->queue)) {
-		req = list_entry(ep->queue.next,
-			struct fotg210_request, queue);
-		spin_lock_irqsave(&ep->fotg210->lock, flags);
-		fotg210_done(ep, req, -ECONNRESET);
-		spin_unlock_irqrestore(&ep->fotg210->lock, flags);
-	}
-
-	return fotg210_ep_release(ep);
-}
-
-static struct usb_request *fotg210_ep_alloc_request(struct usb_ep *_ep,
-						gfp_t gfp_flags)
-{
-	struct fotg210_request *req;
-
-	req = kzalloc(sizeof(struct fotg210_request), gfp_flags);
-	if (!req)
-		return NULL;
-
-	INIT_LIST_HEAD(&req->queue);
-
-	return &req->req;
-}
-
-static void fotg210_ep_free_request(struct usb_ep *_ep,
-					struct usb_request *_req)
-{
-	struct fotg210_request *req;
-
-	req = container_of(_req, struct fotg210_request, req);
-	kfree(req);
-}
-
-static void fotg210_enable_dma(struct fotg210_ep *ep,
-			      dma_addr_t d, u32 len)
-{
-	u32 value;
-	struct fotg210_udc *fotg210 = ep->fotg210;
-
-	/* set transfer length and direction */
-	value = ioread32(fotg210->reg + FOTG210_DMACPSR1);
-	value &= ~(DMACPSR1_DMA_LEN(0xFFFF) | DMACPSR1_DMA_TYPE(1));
-	value |= DMACPSR1_DMA_LEN(len) | DMACPSR1_DMA_TYPE(ep->dir_in);
-	iowrite32(value, fotg210->reg + FOTG210_DMACPSR1);
-
-	/* set device DMA target FIFO number */
-	value = ioread32(fotg210->reg + FOTG210_DMATFNR);
-	if (ep->epnum)
-		value |= DMATFNR_ACC_FN(ep->epnum - 1);
-	else
-		value |= DMATFNR_ACC_CXF;
-	iowrite32(value, fotg210->reg + FOTG210_DMATFNR);
-
-	/* set DMA memory address */
-	iowrite32(d, fotg210->reg + FOTG210_DMACPSR2);
-
-	/* enable MDMA_EROR and MDMA_CMPLT interrupt */
-	value = ioread32(fotg210->reg + FOTG210_DMISGR2);
-	value &= ~(DMISGR2_MDMA_CMPLT | DMISGR2_MDMA_ERROR);
-	iowrite32(value, fotg210->reg + FOTG210_DMISGR2);
-
-	/* start DMA */
-	value = ioread32(fotg210->reg + FOTG210_DMACPSR1);
-	value |= DMACPSR1_DMA_START;
-	iowrite32(value, fotg210->reg + FOTG210_DMACPSR1);
-}
-
-static void fotg210_disable_dma(struct fotg210_ep *ep)
-{
-	iowrite32(DMATFNR_DISDMA, ep->fotg210->reg + FOTG210_DMATFNR);
-}
-
-static void fotg210_wait_dma_done(struct fotg210_ep *ep)
-{
-	u32 value;
-
-	do {
-		value = ioread32(ep->fotg210->reg + FOTG210_DISGR2);
-		if ((value & DISGR2_USBRST_INT) ||
-		    (value & DISGR2_DMA_ERROR))
-			goto dma_reset;
-	} while (!(value & DISGR2_DMA_CMPLT));
-
-	value &= ~DISGR2_DMA_CMPLT;
-	iowrite32(value, ep->fotg210->reg + FOTG210_DISGR2);
-	return;
-
-dma_reset:
-	value = ioread32(ep->fotg210->reg + FOTG210_DMACPSR1);
-	value |= DMACPSR1_DMA_ABORT;
-	iowrite32(value, ep->fotg210->reg + FOTG210_DMACPSR1);
-
-	/* reset fifo */
-	if (ep->epnum) {
-		value = ioread32(ep->fotg210->reg +
-				FOTG210_FIBCR(ep->epnum - 1));
-		value |= FIBCR_FFRST;
-		iowrite32(value, ep->fotg210->reg +
-				FOTG210_FIBCR(ep->epnum - 1));
-	} else {
-		value = ioread32(ep->fotg210->reg + FOTG210_DCFESR);
-		value |= DCFESR_CX_CLR;
-		iowrite32(value, ep->fotg210->reg + FOTG210_DCFESR);
-	}
-}
-
-static void fotg210_start_dma(struct fotg210_ep *ep,
-			struct fotg210_request *req)
-{
-	struct device *dev = &ep->fotg210->gadget.dev;
-	dma_addr_t d;
-	u8 *buffer;
-	u32 length;
-
-	if (ep->epnum) {
-		if (ep->dir_in) {
-			buffer = req->req.buf;
-			length = req->req.length;
-		} else {
-			buffer = req->req.buf + req->req.actual;
-			length = ioread32(ep->fotg210->reg +
-					FOTG210_FIBCR(ep->epnum - 1)) & FIBCR_BCFX;
-			if (length > req->req.length - req->req.actual)
-				length = req->req.length - req->req.actual;
-		}
-	} else {
-		buffer = req->req.buf + req->req.actual;
-		if (req->req.length - req->req.actual > ep->ep.maxpacket)
-			length = ep->ep.maxpacket;
-		else
-			length = req->req.length - req->req.actual;
-	}
-
-	d = dma_map_single(dev, buffer, length,
-			ep->dir_in ? DMA_TO_DEVICE : DMA_FROM_DEVICE);
-
-	if (dma_mapping_error(dev, d)) {
-		pr_err("dma_mapping_error\n");
-		return;
-	}
-
-	fotg210_enable_dma(ep, d, length);
-
-	/* check if dma is done */
-	fotg210_wait_dma_done(ep);
-
-	fotg210_disable_dma(ep);
-
-	/* update actual transfer length */
-	req->req.actual += length;
-
-	dma_unmap_single(dev, d, length, DMA_TO_DEVICE);
-}
-
-static void fotg210_ep0_queue(struct fotg210_ep *ep,
-				struct fotg210_request *req)
-{
-	if (!req->req.length) {
-		fotg210_done(ep, req, 0);
-		return;
-	}
-	if (ep->dir_in) { /* if IN */
-		fotg210_start_dma(ep, req);
-		if (req->req.length == req->req.actual)
-			fotg210_done(ep, req, 0);
-	} else { /* OUT */
-		u32 value = ioread32(ep->fotg210->reg + FOTG210_DMISGR0);
-
-		value &= ~DMISGR0_MCX_OUT_INT;
-		iowrite32(value, ep->fotg210->reg + FOTG210_DMISGR0);
-	}
-}
-
-static int fotg210_ep_queue(struct usb_ep *_ep, struct usb_request *_req,
-				gfp_t gfp_flags)
-{
-	struct fotg210_ep *ep;
-	struct fotg210_request *req;
-	unsigned long flags;
-	int request = 0;
-
-	ep = container_of(_ep, struct fotg210_ep, ep);
-	req = container_of(_req, struct fotg210_request, req);
-
-	if (ep->fotg210->gadget.speed == USB_SPEED_UNKNOWN)
-		return -ESHUTDOWN;
-
-	spin_lock_irqsave(&ep->fotg210->lock, flags);
-
-	if (list_empty(&ep->queue))
-		request = 1;
-
-	list_add_tail(&req->queue, &ep->queue);
-
-	req->req.actual = 0;
-	req->req.status = -EINPROGRESS;
-
-	if (!ep->epnum) /* ep0 */
-		fotg210_ep0_queue(ep, req);
-	else if (request && !ep->stall)
-		fotg210_enable_fifo_int(ep);
-
-	spin_unlock_irqrestore(&ep->fotg210->lock, flags);
-
-	return 0;
-}
-
-static int fotg210_ep_dequeue(struct usb_ep *_ep, struct usb_request *_req)
-{
-	struct fotg210_ep *ep;
-	struct fotg210_request *req;
-	unsigned long flags;
-
-	ep = container_of(_ep, struct fotg210_ep, ep);
-	req = container_of(_req, struct fotg210_request, req);
-
-	spin_lock_irqsave(&ep->fotg210->lock, flags);
-	if (!list_empty(&ep->queue))
-		fotg210_done(ep, req, -ECONNRESET);
-	spin_unlock_irqrestore(&ep->fotg210->lock, flags);
-
-	return 0;
-}
-
-static void fotg210_set_epnstall(struct fotg210_ep *ep)
-{
-	struct fotg210_udc *fotg210 = ep->fotg210;
-	u32 value;
-	void __iomem *reg;
-
-	/* check if IN FIFO is empty before stall */
-	if (ep->dir_in) {
-		do {
-			value = ioread32(fotg210->reg + FOTG210_DCFESR);
-		} while (!(value & DCFESR_FIFO_EMPTY(ep->epnum - 1)));
-	}
-
-	reg = (ep->dir_in) ?
-		fotg210->reg + FOTG210_INEPMPSR(ep->epnum) :
-		fotg210->reg + FOTG210_OUTEPMPSR(ep->epnum);
-	value = ioread32(reg);
-	value |= INOUTEPMPSR_STL_EP;
-	iowrite32(value, reg);
-}
-
-static void fotg210_clear_epnstall(struct fotg210_ep *ep)
-{
-	struct fotg210_udc *fotg210 = ep->fotg210;
-	u32 value;
-	void __iomem *reg;
-
-	reg = (ep->dir_in) ?
-		fotg210->reg + FOTG210_INEPMPSR(ep->epnum) :
-		fotg210->reg + FOTG210_OUTEPMPSR(ep->epnum);
-	value = ioread32(reg);
-	value &= ~INOUTEPMPSR_STL_EP;
-	iowrite32(value, reg);
-}
-
-static int fotg210_set_halt_and_wedge(struct usb_ep *_ep, int value, int wedge)
-{
-	struct fotg210_ep *ep;
-	struct fotg210_udc *fotg210;
-	unsigned long flags;
-
-	ep = container_of(_ep, struct fotg210_ep, ep);
-
-	fotg210 = ep->fotg210;
-
-	spin_lock_irqsave(&ep->fotg210->lock, flags);
-
-	if (value) {
-		fotg210_set_epnstall(ep);
-		ep->stall = 1;
-		if (wedge)
-			ep->wedged = 1;
-	} else {
-		fotg210_reset_tseq(fotg210, ep->epnum);
-		fotg210_clear_epnstall(ep);
-		ep->stall = 0;
-		ep->wedged = 0;
-		if (!list_empty(&ep->queue))
-			fotg210_enable_fifo_int(ep);
-	}
-
-	spin_unlock_irqrestore(&ep->fotg210->lock, flags);
-	return 0;
-}
-
-static int fotg210_ep_set_halt(struct usb_ep *_ep, int value)
-{
-	return fotg210_set_halt_and_wedge(_ep, value, 0);
-}
-
-static int fotg210_ep_set_wedge(struct usb_ep *_ep)
-{
-	return fotg210_set_halt_and_wedge(_ep, 1, 1);
-}
-
-static void fotg210_ep_fifo_flush(struct usb_ep *_ep)
-{
-}
-
-static const struct usb_ep_ops fotg210_ep_ops = {
-	.enable		= fotg210_ep_enable,
-	.disable	= fotg210_ep_disable,
-
-	.alloc_request	= fotg210_ep_alloc_request,
-	.free_request	= fotg210_ep_free_request,
-
-	.queue		= fotg210_ep_queue,
-	.dequeue	= fotg210_ep_dequeue,
-
-	.set_halt	= fotg210_ep_set_halt,
-	.fifo_flush	= fotg210_ep_fifo_flush,
-	.set_wedge	= fotg210_ep_set_wedge,
-};
-
-static void fotg210_clear_tx0byte(struct fotg210_udc *fotg210)
-{
-	u32 value = ioread32(fotg210->reg + FOTG210_TX0BYTE);
-
-	value &= ~(TX0BYTE_EP1 | TX0BYTE_EP2 | TX0BYTE_EP3
-		   | TX0BYTE_EP4);
-	iowrite32(value, fotg210->reg + FOTG210_TX0BYTE);
-}
-
-static void fotg210_clear_rx0byte(struct fotg210_udc *fotg210)
-{
-	u32 value = ioread32(fotg210->reg + FOTG210_RX0BYTE);
-
-	value &= ~(RX0BYTE_EP1 | RX0BYTE_EP2 | RX0BYTE_EP3
-		   | RX0BYTE_EP4);
-	iowrite32(value, fotg210->reg + FOTG210_RX0BYTE);
-}
-
-/* read 8-byte setup packet only */
-static void fotg210_rdsetupp(struct fotg210_udc *fotg210,
-		   u8 *buffer)
-{
-	int i = 0;
-	u8 *tmp = buffer;
-	u32 data;
-	u32 length = 8;
-
-	iowrite32(DMATFNR_ACC_CXF, fotg210->reg + FOTG210_DMATFNR);
-
-	for (i = (length >> 2); i > 0; i--) {
-		data = ioread32(fotg210->reg + FOTG210_CXPORT);
-		*tmp = data & 0xFF;
-		*(tmp + 1) = (data >> 8) & 0xFF;
-		*(tmp + 2) = (data >> 16) & 0xFF;
-		*(tmp + 3) = (data >> 24) & 0xFF;
-		tmp = tmp + 4;
-	}
-
-	switch (length % 4) {
-	case 1:
-		data = ioread32(fotg210->reg + FOTG210_CXPORT);
-		*tmp = data & 0xFF;
-		break;
-	case 2:
-		data = ioread32(fotg210->reg + FOTG210_CXPORT);
-		*tmp = data & 0xFF;
-		*(tmp + 1) = (data >> 8) & 0xFF;
-		break;
-	case 3:
-		data = ioread32(fotg210->reg + FOTG210_CXPORT);
-		*tmp = data & 0xFF;
-		*(tmp + 1) = (data >> 8) & 0xFF;
-		*(tmp + 2) = (data >> 16) & 0xFF;
-		break;
-	default:
-		break;
-	}
-
-	iowrite32(DMATFNR_DISDMA, fotg210->reg + FOTG210_DMATFNR);
-}
-
-static void fotg210_set_configuration(struct fotg210_udc *fotg210)
-{
-	u32 value = ioread32(fotg210->reg + FOTG210_DAR);
-
-	value |= DAR_AFT_CONF;
-	iowrite32(value, fotg210->reg + FOTG210_DAR);
-}
-
-static void fotg210_set_dev_addr(struct fotg210_udc *fotg210, u32 addr)
-{
-	u32 value = ioread32(fotg210->reg + FOTG210_DAR);
-
-	value |= (addr & 0x7F);
-	iowrite32(value, fotg210->reg + FOTG210_DAR);
-}
-
-static void fotg210_set_cxstall(struct fotg210_udc *fotg210)
-{
-	u32 value = ioread32(fotg210->reg + FOTG210_DCFESR);
-
-	value |= DCFESR_CX_STL;
-	iowrite32(value, fotg210->reg + FOTG210_DCFESR);
-}
-
-static void fotg210_request_error(struct fotg210_udc *fotg210)
-{
-	fotg210_set_cxstall(fotg210);
-	pr_err("request error!!\n");
-}
-
-static void fotg210_set_address(struct fotg210_udc *fotg210,
-				struct usb_ctrlrequest *ctrl)
-{
-	if (le16_to_cpu(ctrl->wValue) >= 0x0100) {
-		fotg210_request_error(fotg210);
-	} else {
-		fotg210_set_dev_addr(fotg210, le16_to_cpu(ctrl->wValue));
-		fotg210_set_cxdone(fotg210);
-	}
-}
-
-static void fotg210_set_feature(struct fotg210_udc *fotg210,
-				struct usb_ctrlrequest *ctrl)
-{
-	switch (ctrl->bRequestType & USB_RECIP_MASK) {
-	case USB_RECIP_DEVICE:
-		fotg210_set_cxdone(fotg210);
-		break;
-	case USB_RECIP_INTERFACE:
-		fotg210_set_cxdone(fotg210);
-		break;
-	case USB_RECIP_ENDPOINT: {
-		u8 epnum;
-		epnum = le16_to_cpu(ctrl->wIndex) & USB_ENDPOINT_NUMBER_MASK;
-		if (epnum)
-			fotg210_set_epnstall(fotg210->ep[epnum]);
-		else
-			fotg210_set_cxstall(fotg210);
-		fotg210_set_cxdone(fotg210);
-		}
-		break;
-	default:
-		fotg210_request_error(fotg210);
-		break;
-	}
-}
-
-static void fotg210_clear_feature(struct fotg210_udc *fotg210,
-				struct usb_ctrlrequest *ctrl)
-{
-	struct fotg210_ep *ep =
-		fotg210->ep[ctrl->wIndex & USB_ENDPOINT_NUMBER_MASK];
-
-	switch (ctrl->bRequestType & USB_RECIP_MASK) {
-	case USB_RECIP_DEVICE:
-		fotg210_set_cxdone(fotg210);
-		break;
-	case USB_RECIP_INTERFACE:
-		fotg210_set_cxdone(fotg210);
-		break;
-	case USB_RECIP_ENDPOINT:
-		if (ctrl->wIndex & USB_ENDPOINT_NUMBER_MASK) {
-			if (ep->wedged) {
-				fotg210_set_cxdone(fotg210);
-				break;
-			}
-			if (ep->stall)
-				fotg210_set_halt_and_wedge(&ep->ep, 0, 0);
-		}
-		fotg210_set_cxdone(fotg210);
-		break;
-	default:
-		fotg210_request_error(fotg210);
-		break;
-	}
-}
-
-static int fotg210_is_epnstall(struct fotg210_ep *ep)
-{
-	struct fotg210_udc *fotg210 = ep->fotg210;
-	u32 value;
-	void __iomem *reg;
-
-	reg = (ep->dir_in) ?
-		fotg210->reg + FOTG210_INEPMPSR(ep->epnum) :
-		fotg210->reg + FOTG210_OUTEPMPSR(ep->epnum);
-	value = ioread32(reg);
-	return value & INOUTEPMPSR_STL_EP ? 1 : 0;
-}
-
-/* For EP0 requests triggered by this driver (currently GET_STATUS response) */
-static void fotg210_ep0_complete(struct usb_ep *_ep, struct usb_request *req)
-{
-	struct fotg210_ep *ep;
-	struct fotg210_udc *fotg210;
-
-	ep = container_of(_ep, struct fotg210_ep, ep);
-	fotg210 = ep->fotg210;
-
-	if (req->status || req->actual != req->length) {
-		dev_warn(&fotg210->gadget.dev, "EP0 request failed: %d\n", req->status);
-	}
-}
-
-static void fotg210_get_status(struct fotg210_udc *fotg210,
-				struct usb_ctrlrequest *ctrl)
-{
-	u8 epnum;
-
-	switch (ctrl->bRequestType & USB_RECIP_MASK) {
-	case USB_RECIP_DEVICE:
-		fotg210->ep0_data = cpu_to_le16(1 << USB_DEVICE_SELF_POWERED);
-		break;
-	case USB_RECIP_INTERFACE:
-		fotg210->ep0_data = cpu_to_le16(0);
-		break;
-	case USB_RECIP_ENDPOINT:
-		epnum = ctrl->wIndex & USB_ENDPOINT_NUMBER_MASK;
-		if (epnum)
-			fotg210->ep0_data =
-				cpu_to_le16(fotg210_is_epnstall(fotg210->ep[epnum])
-					    << USB_ENDPOINT_HALT);
-		else
-			fotg210_request_error(fotg210);
-		break;
-
-	default:
-		fotg210_request_error(fotg210);
-		return;		/* exit */
-	}
-
-	fotg210->ep0_req->buf = &fotg210->ep0_data;
-	fotg210->ep0_req->length = 2;
-
-	spin_unlock(&fotg210->lock);
-	fotg210_ep_queue(fotg210->gadget.ep0, fotg210->ep0_req, GFP_ATOMIC);
-	spin_lock(&fotg210->lock);
-}
-
-static int fotg210_setup_packet(struct fotg210_udc *fotg210,
-				struct usb_ctrlrequest *ctrl)
-{
-	u8 *p = (u8 *)ctrl;
-	u8 ret = 0;
-
-	fotg210_rdsetupp(fotg210, p);
-
-	fotg210->ep[0]->dir_in = ctrl->bRequestType & USB_DIR_IN;
-
-	if (fotg210->gadget.speed == USB_SPEED_UNKNOWN) {
-		u32 value = ioread32(fotg210->reg + FOTG210_DMCR);
-		fotg210->gadget.speed = value & DMCR_HS_EN ?
-				USB_SPEED_HIGH : USB_SPEED_FULL;
-	}
-
-	/* check request */
-	if ((ctrl->bRequestType & USB_TYPE_MASK) == USB_TYPE_STANDARD) {
-		switch (ctrl->bRequest) {
-		case USB_REQ_GET_STATUS:
-			fotg210_get_status(fotg210, ctrl);
-			break;
-		case USB_REQ_CLEAR_FEATURE:
-			fotg210_clear_feature(fotg210, ctrl);
-			break;
-		case USB_REQ_SET_FEATURE:
-			fotg210_set_feature(fotg210, ctrl);
-			break;
-		case USB_REQ_SET_ADDRESS:
-			fotg210_set_address(fotg210, ctrl);
-			break;
-		case USB_REQ_SET_CONFIGURATION:
-			fotg210_set_configuration(fotg210);
-			ret = 1;
-			break;
-		default:
-			ret = 1;
-			break;
-		}
-	} else {
-		ret = 1;
-	}
-
-	return ret;
-}
-
-static void fotg210_ep0out(struct fotg210_udc *fotg210)
-{
-	struct fotg210_ep *ep = fotg210->ep[0];
-
-	if (!list_empty(&ep->queue) && !ep->dir_in) {
-		struct fotg210_request *req;
-
-		req = list_first_entry(&ep->queue,
-			struct fotg210_request, queue);
-
-		if (req->req.length)
-			fotg210_start_dma(ep, req);
-
-		if ((req->req.length - req->req.actual) < ep->ep.maxpacket)
-			fotg210_done(ep, req, 0);
-	} else {
-		pr_err("%s : empty queue\n", __func__);
-	}
-}
-
-static void fotg210_ep0in(struct fotg210_udc *fotg210)
-{
-	struct fotg210_ep *ep = fotg210->ep[0];
-
-	if ((!list_empty(&ep->queue)) && (ep->dir_in)) {
-		struct fotg210_request *req;
-
-		req = list_entry(ep->queue.next,
-				struct fotg210_request, queue);
-
-		if (req->req.length)
-			fotg210_start_dma(ep, req);
-
-		if (req->req.actual == req->req.length)
-			fotg210_done(ep, req, 0);
-	} else {
-		fotg210_set_cxdone(fotg210);
-	}
-}
-
-static void fotg210_clear_comabt_int(struct fotg210_udc *fotg210)
-{
-	u32 value = ioread32(fotg210->reg + FOTG210_DISGR0);
-
-	value &= ~DISGR0_CX_COMABT_INT;
-	iowrite32(value, fotg210->reg + FOTG210_DISGR0);
-}
-
-static void fotg210_in_fifo_handler(struct fotg210_ep *ep)
-{
-	struct fotg210_request *req = list_entry(ep->queue.next,
-					struct fotg210_request, queue);
-
-	if (req->req.length)
-		fotg210_start_dma(ep, req);
-	fotg210_done(ep, req, 0);
-}
-
-static void fotg210_out_fifo_handler(struct fotg210_ep *ep)
-{
-	struct fotg210_request *req = list_entry(ep->queue.next,
-						 struct fotg210_request, queue);
-	int disgr1 = ioread32(ep->fotg210->reg + FOTG210_DISGR1);
-
-	fotg210_start_dma(ep, req);
-
-	/* Complete the request when it's full or a short packet arrived.
-	 * Like other drivers, short_not_ok isn't handled.
-	 */
-
-	if (req->req.length == req->req.actual ||
-	    (disgr1 & DISGR1_SPK_INT(ep->epnum - 1)))
-		fotg210_done(ep, req, 0);
-}
-
-static irqreturn_t fotg210_irq(int irq, void *_fotg210)
-{
-	struct fotg210_udc *fotg210 = _fotg210;
-	u32 int_grp = ioread32(fotg210->reg + FOTG210_DIGR);
-	u32 int_msk = ioread32(fotg210->reg + FOTG210_DMIGR);
-
-	int_grp &= ~int_msk;
-
-	spin_lock(&fotg210->lock);
-
-	if (int_grp & DIGR_INT_G2) {
-		void __iomem *reg = fotg210->reg + FOTG210_DISGR2;
-		u32 int_grp2 = ioread32(reg);
-		u32 int_msk2 = ioread32(fotg210->reg + FOTG210_DMISGR2);
-		u32 value;
-
-		int_grp2 &= ~int_msk2;
-
-		if (int_grp2 & DISGR2_USBRST_INT) {
-			usb_gadget_udc_reset(&fotg210->gadget,
-					     fotg210->driver);
-			value = ioread32(reg);
-			value &= ~DISGR2_USBRST_INT;
-			iowrite32(value, reg);
-			pr_info("fotg210 udc reset\n");
-		}
-		if (int_grp2 & DISGR2_SUSP_INT) {
-			value = ioread32(reg);
-			value &= ~DISGR2_SUSP_INT;
-			iowrite32(value, reg);
-			pr_info("fotg210 udc suspend\n");
-		}
-		if (int_grp2 & DISGR2_RESM_INT) {
-			value = ioread32(reg);
-			value &= ~DISGR2_RESM_INT;
-			iowrite32(value, reg);
-			pr_info("fotg210 udc resume\n");
-		}
-		if (int_grp2 & DISGR2_ISO_SEQ_ERR_INT) {
-			value = ioread32(reg);
-			value &= ~DISGR2_ISO_SEQ_ERR_INT;
-			iowrite32(value, reg);
-			pr_info("fotg210 iso sequence error\n");
-		}
-		if (int_grp2 & DISGR2_ISO_SEQ_ABORT_INT) {
-			value = ioread32(reg);
-			value &= ~DISGR2_ISO_SEQ_ABORT_INT;
-			iowrite32(value, reg);
-			pr_info("fotg210 iso sequence abort\n");
-		}
-		if (int_grp2 & DISGR2_TX0BYTE_INT) {
-			fotg210_clear_tx0byte(fotg210);
-			value = ioread32(reg);
-			value &= ~DISGR2_TX0BYTE_INT;
-			iowrite32(value, reg);
-			pr_info("fotg210 transferred 0 byte\n");
-		}
-		if (int_grp2 & DISGR2_RX0BYTE_INT) {
-			fotg210_clear_rx0byte(fotg210);
-			value = ioread32(reg);
-			value &= ~DISGR2_RX0BYTE_INT;
-			iowrite32(value, reg);
-			pr_info("fotg210 received 0 byte\n");
-		}
-		if (int_grp2 & DISGR2_DMA_ERROR) {
-			value = ioread32(reg);
-			value &= ~DISGR2_DMA_ERROR;
-			iowrite32(value, reg);
-		}
-	}
-
-	if (int_grp & DIGR_INT_G0) {
-		void __iomem *reg = fotg210->reg + FOTG210_DISGR0;
-		u32 int_grp0 = ioread32(reg);
-		u32 int_msk0 = ioread32(fotg210->reg + FOTG210_DMISGR0);
-		struct usb_ctrlrequest ctrl;
-
-		int_grp0 &= ~int_msk0;
-
-		/* the highest priority in this source register */
-		if (int_grp0 & DISGR0_CX_COMABT_INT) {
-			fotg210_clear_comabt_int(fotg210);
-			pr_info("fotg210 CX command abort\n");
-		}
-
-		if (int_grp0 & DISGR0_CX_SETUP_INT) {
-			if (fotg210_setup_packet(fotg210, &ctrl)) {
-				spin_unlock(&fotg210->lock);
-				if (fotg210->driver->setup(&fotg210->gadget,
-							   &ctrl) < 0)
-					fotg210_set_cxstall(fotg210);
-				spin_lock(&fotg210->lock);
-			}
-		}
-		if (int_grp0 & DISGR0_CX_COMEND_INT)
-			pr_info("fotg210 cmd end\n");
-
-		if (int_grp0 & DISGR0_CX_IN_INT)
-			fotg210_ep0in(fotg210);
-
-		if (int_grp0 & DISGR0_CX_OUT_INT)
-			fotg210_ep0out(fotg210);
-
-		if (int_grp0 & DISGR0_CX_COMFAIL_INT) {
-			fotg210_set_cxstall(fotg210);
-			pr_info("fotg210 ep0 fail\n");
-		}
-	}
-
-	if (int_grp & DIGR_INT_G1) {
-		void __iomem *reg = fotg210->reg + FOTG210_DISGR1;
-		u32 int_grp1 = ioread32(reg);
-		u32 int_msk1 = ioread32(fotg210->reg + FOTG210_DMISGR1);
-		int fifo;
-
-		int_grp1 &= ~int_msk1;
-
-		for (fifo = 0; fifo < FOTG210_MAX_FIFO_NUM; fifo++) {
-			if (int_grp1 & DISGR1_IN_INT(fifo))
-				fotg210_in_fifo_handler(fotg210->ep[fifo + 1]);
-
-			if ((int_grp1 & DISGR1_OUT_INT(fifo)) ||
-			    (int_grp1 & DISGR1_SPK_INT(fifo)))
-				fotg210_out_fifo_handler(fotg210->ep[fifo + 1]);
-		}
-	}
-
-	spin_unlock(&fotg210->lock);
-
-	return IRQ_HANDLED;
-}
-
-static void fotg210_disable_unplug(struct fotg210_udc *fotg210)
-{
-	u32 reg = ioread32(fotg210->reg + FOTG210_PHYTMSR);
-
-	reg &= ~PHYTMSR_UNPLUG;
-	iowrite32(reg, fotg210->reg + FOTG210_PHYTMSR);
-}
-
-static int fotg210_udc_start(struct usb_gadget *g,
-		struct usb_gadget_driver *driver)
-{
-	struct fotg210_udc *fotg210 = gadget_to_fotg210(g);
-	u32 value;
-
-	/* hook up the driver */
-	fotg210->driver = driver;
-
-	/* enable device global interrupt */
-	value = ioread32(fotg210->reg + FOTG210_DMCR);
-	value |= DMCR_GLINT_EN;
-	iowrite32(value, fotg210->reg + FOTG210_DMCR);
-
-	return 0;
-}
-
-static void fotg210_init(struct fotg210_udc *fotg210)
-{
-	u32 value;
-
-	/* disable global interrupt and set int polarity to active high */
-	iowrite32(GMIR_MHC_INT | GMIR_MOTG_INT | GMIR_INT_POLARITY,
-		  fotg210->reg + FOTG210_GMIR);
-
-	/* disable device global interrupt */
-	value = ioread32(fotg210->reg + FOTG210_DMCR);
-	value &= ~DMCR_GLINT_EN;
-	iowrite32(value, fotg210->reg + FOTG210_DMCR);
-
-	/* enable only grp2 irqs we handle */
-	iowrite32(~(DISGR2_DMA_ERROR | DISGR2_RX0BYTE_INT | DISGR2_TX0BYTE_INT
-		    | DISGR2_ISO_SEQ_ABORT_INT | DISGR2_ISO_SEQ_ERR_INT
-		    | DISGR2_RESM_INT | DISGR2_SUSP_INT | DISGR2_USBRST_INT),
-		  fotg210->reg + FOTG210_DMISGR2);
-
-	/* disable all fifo interrupt */
-	iowrite32(~(u32)0, fotg210->reg + FOTG210_DMISGR1);
-
-	/* disable cmd end */
-	value = ioread32(fotg210->reg + FOTG210_DMISGR0);
-	value |= DMISGR0_MCX_COMEND;
-	iowrite32(value, fotg210->reg + FOTG210_DMISGR0);
-}
-
-static int fotg210_udc_stop(struct usb_gadget *g)
-{
-	struct fotg210_udc *fotg210 = gadget_to_fotg210(g);
-	unsigned long	flags;
-
-	spin_lock_irqsave(&fotg210->lock, flags);
-
-	fotg210_init(fotg210);
-	fotg210->driver = NULL;
-
-	spin_unlock_irqrestore(&fotg210->lock, flags);
-
-	return 0;
-}
-
-static const struct usb_gadget_ops fotg210_gadget_ops = {
-	.udc_start		= fotg210_udc_start,
-	.udc_stop		= fotg210_udc_stop,
-};
-
-static int fotg210_udc_remove(struct platform_device *pdev)
-{
-	struct fotg210_udc *fotg210 = platform_get_drvdata(pdev);
-	int i;
-
-	usb_del_gadget_udc(&fotg210->gadget);
-	iounmap(fotg210->reg);
-	free_irq(platform_get_irq(pdev, 0), fotg210);
-
-	fotg210_ep_free_request(&fotg210->ep[0]->ep, fotg210->ep0_req);
-	for (i = 0; i < FOTG210_MAX_NUM_EP; i++)
-		kfree(fotg210->ep[i]);
-	kfree(fotg210);
-
-	return 0;
-}
-
-static int fotg210_udc_probe(struct platform_device *pdev)
-{
-	struct resource *res, *ires;
-	struct fotg210_udc *fotg210 = NULL;
-	struct fotg210_ep *_ep[FOTG210_MAX_NUM_EP];
-	int ret = 0;
-	int i;
-
-	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
-	if (!res) {
-		pr_err("platform_get_resource error.\n");
-		return -ENODEV;
-	}
-
-	ires = platform_get_resource(pdev, IORESOURCE_IRQ, 0);
-	if (!ires) {
-		pr_err("platform_get_resource IORESOURCE_IRQ error.\n");
-		return -ENODEV;
-	}
-
-	ret = -ENOMEM;
-
-	/* initialize udc */
-	fotg210 = kzalloc(sizeof(struct fotg210_udc), GFP_KERNEL);
-	if (fotg210 == NULL)
-		goto err;
-
-	for (i = 0; i < FOTG210_MAX_NUM_EP; i++) {
-		_ep[i] = kzalloc(sizeof(struct fotg210_ep), GFP_KERNEL);
-		if (_ep[i] == NULL)
-			goto err_alloc;
-		fotg210->ep[i] = _ep[i];
-	}
-
-	fotg210->reg = ioremap(res->start, resource_size(res));
-	if (fotg210->reg == NULL) {
-		pr_err("ioremap error.\n");
-		goto err_alloc;
-	}
-
-	spin_lock_init(&fotg210->lock);
-
-	platform_set_drvdata(pdev, fotg210);
-
-	fotg210->gadget.ops = &fotg210_gadget_ops;
-
-	fotg210->gadget.max_speed = USB_SPEED_HIGH;
-	fotg210->gadget.dev.parent = &pdev->dev;
-	fotg210->gadget.dev.dma_mask = pdev->dev.dma_mask;
-	fotg210->gadget.name = udc_name;
-
-	INIT_LIST_HEAD(&fotg210->gadget.ep_list);
-
-	for (i = 0; i < FOTG210_MAX_NUM_EP; i++) {
-		struct fotg210_ep *ep = fotg210->ep[i];
-
-		if (i) {
-			INIT_LIST_HEAD(&fotg210->ep[i]->ep.ep_list);
-			list_add_tail(&fotg210->ep[i]->ep.ep_list,
-				      &fotg210->gadget.ep_list);
-		}
-		ep->fotg210 = fotg210;
-		INIT_LIST_HEAD(&ep->queue);
-		ep->ep.name = fotg210_ep_name[i];
-		ep->ep.ops = &fotg210_ep_ops;
-		usb_ep_set_maxpacket_limit(&ep->ep, (unsigned short) ~0);
-
-		if (i == 0) {
-			ep->ep.caps.type_control = true;
-		} else {
-			ep->ep.caps.type_iso = true;
-			ep->ep.caps.type_bulk = true;
-			ep->ep.caps.type_int = true;
-		}
-
-		ep->ep.caps.dir_in = true;
-		ep->ep.caps.dir_out = true;
-	}
-	usb_ep_set_maxpacket_limit(&fotg210->ep[0]->ep, 0x40);
-	fotg210->gadget.ep0 = &fotg210->ep[0]->ep;
-	INIT_LIST_HEAD(&fotg210->gadget.ep0->ep_list);
-
-	fotg210->ep0_req = fotg210_ep_alloc_request(&fotg210->ep[0]->ep,
-				GFP_KERNEL);
-	if (fotg210->ep0_req == NULL)
-		goto err_map;
-
-	fotg210->ep0_req->complete = fotg210_ep0_complete;
-
-	fotg210_init(fotg210);
-
-	fotg210_disable_unplug(fotg210);
-
-	ret = request_irq(ires->start, fotg210_irq, IRQF_SHARED,
-			  udc_name, fotg210);
-	if (ret < 0) {
-		pr_err("request_irq error (%d)\n", ret);
-		goto err_req;
-	}
-
-	ret = usb_add_gadget_udc(&pdev->dev, &fotg210->gadget);
-	if (ret)
-		goto err_add_udc;
-
-	dev_info(&pdev->dev, "version %s\n", DRIVER_VERSION);
-
-	return 0;
-
-err_add_udc:
-	free_irq(ires->start, fotg210);
-
-err_req:
-	fotg210_ep_free_request(&fotg210->ep[0]->ep, fotg210->ep0_req);
-
-err_map:
-	iounmap(fotg210->reg);
-
-err_alloc:
-	for (i = 0; i < FOTG210_MAX_NUM_EP; i++)
-		kfree(fotg210->ep[i]);
-	kfree(fotg210);
-
-err:
-	return ret;
-}
-
-static struct platform_driver fotg210_driver = {
-	.driver		= {
-		.name =	udc_name,
-	},
-	.probe		= fotg210_udc_probe,
-	.remove		= fotg210_udc_remove,
-};
-
-module_platform_driver(fotg210_driver);
-
-MODULE_AUTHOR("Yuan-Hsin Chen, Feng-Hsin Chiang <john453@faraday-tech.com>");
-MODULE_LICENSE("GPL");
-MODULE_DESCRIPTION(DRIVER_DESC);
--- /dev/null
+++ b/drivers/usb/fotg210/fotg210-udc.c
@@ -0,0 +1,1239 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * FOTG210 UDC Driver supports Bulk transfer so far
+ *
+ * Copyright (C) 2013 Faraday Technology Corporation
+ *
+ * Author : Yuan-Hsin Chen <yhchen@faraday-tech.com>
+ */
+
+#include <linux/dma-mapping.h>
+#include <linux/err.h>
+#include <linux/interrupt.h>
+#include <linux/io.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+#include <linux/usb/ch9.h>
+#include <linux/usb/gadget.h>
+
+#include "fotg210-udc.h"
+
+#define	DRIVER_DESC	"FOTG210 USB Device Controller Driver"
+#define	DRIVER_VERSION	"30-April-2013"
+
+static const char udc_name[] = "fotg210_udc";
+static const char * const fotg210_ep_name[] = {
+	"ep0", "ep1", "ep2", "ep3", "ep4"};
+
+static void fotg210_disable_fifo_int(struct fotg210_ep *ep)
+{
+	u32 value = ioread32(ep->fotg210->reg + FOTG210_DMISGR1);
+
+	if (ep->dir_in)
+		value |= DMISGR1_MF_IN_INT(ep->epnum - 1);
+	else
+		value |= DMISGR1_MF_OUTSPK_INT(ep->epnum - 1);
+	iowrite32(value, ep->fotg210->reg + FOTG210_DMISGR1);
+}
+
+static void fotg210_enable_fifo_int(struct fotg210_ep *ep)
+{
+	u32 value = ioread32(ep->fotg210->reg + FOTG210_DMISGR1);
+
+	if (ep->dir_in)
+		value &= ~DMISGR1_MF_IN_INT(ep->epnum - 1);
+	else
+		value &= ~DMISGR1_MF_OUTSPK_INT(ep->epnum - 1);
+	iowrite32(value, ep->fotg210->reg + FOTG210_DMISGR1);
+}
+
+static void fotg210_set_cxdone(struct fotg210_udc *fotg210)
+{
+	u32 value = ioread32(fotg210->reg + FOTG210_DCFESR);
+
+	value |= DCFESR_CX_DONE;
+	iowrite32(value, fotg210->reg + FOTG210_DCFESR);
+}
+
+static void fotg210_done(struct fotg210_ep *ep, struct fotg210_request *req,
+			int status)
+{
+	list_del_init(&req->queue);
+
+	/* don't modify queue heads during completion callback */
+	if (ep->fotg210->gadget.speed == USB_SPEED_UNKNOWN)
+		req->req.status = -ESHUTDOWN;
+	else
+		req->req.status = status;
+
+	spin_unlock(&ep->fotg210->lock);
+	usb_gadget_giveback_request(&ep->ep, &req->req);
+	spin_lock(&ep->fotg210->lock);
+
+	if (ep->epnum) {
+		if (list_empty(&ep->queue))
+			fotg210_disable_fifo_int(ep);
+	} else {
+		fotg210_set_cxdone(ep->fotg210);
+	}
+}
+
+static void fotg210_fifo_ep_mapping(struct fotg210_ep *ep, u32 epnum,
+				u32 dir_in)
+{
+	struct fotg210_udc *fotg210 = ep->fotg210;
+	u32 val;
+
+	/* Driver should map an ep to a fifo and then map the fifo
+	 * to the ep. What a brain-damaged design!
+	 */
+
+	/* map a fifo to an ep */
+	val = ioread32(fotg210->reg + FOTG210_EPMAP);
+	val &= ~EPMAP_FIFONOMSK(epnum, dir_in);
+	val |= EPMAP_FIFONO(epnum, dir_in);
+	iowrite32(val, fotg210->reg + FOTG210_EPMAP);
+
+	/* map the ep to the fifo */
+	val = ioread32(fotg210->reg + FOTG210_FIFOMAP);
+	val &= ~FIFOMAP_EPNOMSK(epnum);
+	val |= FIFOMAP_EPNO(epnum);
+	iowrite32(val, fotg210->reg + FOTG210_FIFOMAP);
+
+	/* enable fifo */
+	val = ioread32(fotg210->reg + FOTG210_FIFOCF);
+	val |= FIFOCF_FIFO_EN(epnum - 1);
+	iowrite32(val, fotg210->reg + FOTG210_FIFOCF);
+}
+
+static void fotg210_set_fifo_dir(struct fotg210_ep *ep, u32 epnum, u32 dir_in)
+{
+	struct fotg210_udc *fotg210 = ep->fotg210;
+	u32 val;
+
+	val = ioread32(fotg210->reg + FOTG210_FIFOMAP);
+	val |= (dir_in ? FIFOMAP_DIRIN(epnum - 1) : FIFOMAP_DIROUT(epnum - 1));
+	iowrite32(val, fotg210->reg + FOTG210_FIFOMAP);
+}
+
+static void fotg210_set_tfrtype(struct fotg210_ep *ep, u32 epnum, u32 type)
+{
+	struct fotg210_udc *fotg210 = ep->fotg210;
+	u32 val;
+
+	val = ioread32(fotg210->reg + FOTG210_FIFOCF);
+	val |= FIFOCF_TYPE(type, epnum - 1);
+	iowrite32(val, fotg210->reg + FOTG210_FIFOCF);
+}
+
+static void fotg210_set_mps(struct fotg210_ep *ep, u32 epnum, u32 mps,
+				u32 dir_in)
+{
+	struct fotg210_udc *fotg210 = ep->fotg210;
+	u32 val;
+	u32 offset = dir_in ? FOTG210_INEPMPSR(epnum) :
+				FOTG210_OUTEPMPSR(epnum);
+
+	val = ioread32(fotg210->reg + offset);
+	val |= INOUTEPMPSR_MPS(mps);
+	iowrite32(val, fotg210->reg + offset);
+}
+
+static int fotg210_config_ep(struct fotg210_ep *ep,
+		     const struct usb_endpoint_descriptor *desc)
+{
+	struct fotg210_udc *fotg210 = ep->fotg210;
+
+	fotg210_set_fifo_dir(ep, ep->epnum, ep->dir_in);
+	fotg210_set_tfrtype(ep, ep->epnum, ep->type);
+	fotg210_set_mps(ep, ep->epnum, ep->ep.maxpacket, ep->dir_in);
+	fotg210_fifo_ep_mapping(ep, ep->epnum, ep->dir_in);
+
+	fotg210->ep[ep->epnum] = ep;
+
+	return 0;
+}
+
+static int fotg210_ep_enable(struct usb_ep *_ep,
+			  const struct usb_endpoint_descriptor *desc)
+{
+	struct fotg210_ep *ep;
+
+	ep = container_of(_ep, struct fotg210_ep, ep);
+
+	ep->desc = desc;
+	ep->epnum = usb_endpoint_num(desc);
+	ep->type = usb_endpoint_type(desc);
+	ep->dir_in = usb_endpoint_dir_in(desc);
+	ep->ep.maxpacket = usb_endpoint_maxp(desc);
+
+	return fotg210_config_ep(ep, desc);
+}
+
+static void fotg210_reset_tseq(struct fotg210_udc *fotg210, u8 epnum)
+{
+	struct fotg210_ep *ep = fotg210->ep[epnum];
+	u32 value;
+	void __iomem *reg;
+
+	reg = (ep->dir_in) ?
+		fotg210->reg + FOTG210_INEPMPSR(epnum) :
+		fotg210->reg + FOTG210_OUTEPMPSR(epnum);
+
+	/* Note: Driver needs to set and clear INOUTEPMPSR_RESET_TSEQ
+	 *	 bit. Controller wouldn't clear this bit. WTF!!!
+	 */
+
+	value = ioread32(reg);
+	value |= INOUTEPMPSR_RESET_TSEQ;
+	iowrite32(value, reg);
+
+	value = ioread32(reg);
+	value &= ~INOUTEPMPSR_RESET_TSEQ;
+	iowrite32(value, reg);
+}
+
+static int fotg210_ep_release(struct fotg210_ep *ep)
+{
+	if (!ep->epnum)
+		return 0;
+	ep->epnum = 0;
+	ep->stall = 0;
+	ep->wedged = 0;
+
+	fotg210_reset_tseq(ep->fotg210, ep->epnum);
+
+	return 0;
+}
+
+static int fotg210_ep_disable(struct usb_ep *_ep)
+{
+	struct fotg210_ep *ep;
+	struct fotg210_request *req;
+	unsigned long flags;
+
+	BUG_ON(!_ep);
+
+	ep = container_of(_ep, struct fotg210_ep, ep);
+
+	while (!list_empty(&ep->queue)) {
+		req = list_entry(ep->queue.next,
+			struct fotg210_request, queue);
+		spin_lock_irqsave(&ep->fotg210->lock, flags);
+		fotg210_done(ep, req, -ECONNRESET);
+		spin_unlock_irqrestore(&ep->fotg210->lock, flags);
+	}
+
+	return fotg210_ep_release(ep);
+}
+
+static struct usb_request *fotg210_ep_alloc_request(struct usb_ep *_ep,
+						gfp_t gfp_flags)
+{
+	struct fotg210_request *req;
+
+	req = kzalloc(sizeof(struct fotg210_request), gfp_flags);
+	if (!req)
+		return NULL;
+
+	INIT_LIST_HEAD(&req->queue);
+
+	return &req->req;
+}
+
+static void fotg210_ep_free_request(struct usb_ep *_ep,
+					struct usb_request *_req)
+{
+	struct fotg210_request *req;
+
+	req = container_of(_req, struct fotg210_request, req);
+	kfree(req);
+}
+
+static void fotg210_enable_dma(struct fotg210_ep *ep,
+			      dma_addr_t d, u32 len)
+{
+	u32 value;
+	struct fotg210_udc *fotg210 = ep->fotg210;
+
+	/* set transfer length and direction */
+	value = ioread32(fotg210->reg + FOTG210_DMACPSR1);
+	value &= ~(DMACPSR1_DMA_LEN(0xFFFF) | DMACPSR1_DMA_TYPE(1));
+	value |= DMACPSR1_DMA_LEN(len) | DMACPSR1_DMA_TYPE(ep->dir_in);
+	iowrite32(value, fotg210->reg + FOTG210_DMACPSR1);
+
+	/* set device DMA target FIFO number */
+	value = ioread32(fotg210->reg + FOTG210_DMATFNR);
+	if (ep->epnum)
+		value |= DMATFNR_ACC_FN(ep->epnum - 1);
+	else
+		value |= DMATFNR_ACC_CXF;
+	iowrite32(value, fotg210->reg + FOTG210_DMATFNR);
+
+	/* set DMA memory address */
+	iowrite32(d, fotg210->reg + FOTG210_DMACPSR2);
+
+	/* enable MDMA_EROR and MDMA_CMPLT interrupt */
+	value = ioread32(fotg210->reg + FOTG210_DMISGR2);
+	value &= ~(DMISGR2_MDMA_CMPLT | DMISGR2_MDMA_ERROR);
+	iowrite32(value, fotg210->reg + FOTG210_DMISGR2);
+
+	/* start DMA */
+	value = ioread32(fotg210->reg + FOTG210_DMACPSR1);
+	value |= DMACPSR1_DMA_START;
+	iowrite32(value, fotg210->reg + FOTG210_DMACPSR1);
+}
+
+static void fotg210_disable_dma(struct fotg210_ep *ep)
+{
+	iowrite32(DMATFNR_DISDMA, ep->fotg210->reg + FOTG210_DMATFNR);
+}
+
+static void fotg210_wait_dma_done(struct fotg210_ep *ep)
+{
+	u32 value;
+
+	do {
+		value = ioread32(ep->fotg210->reg + FOTG210_DISGR2);
+		if ((value & DISGR2_USBRST_INT) ||
+		    (value & DISGR2_DMA_ERROR))
+			goto dma_reset;
+	} while (!(value & DISGR2_DMA_CMPLT));
+
+	value &= ~DISGR2_DMA_CMPLT;
+	iowrite32(value, ep->fotg210->reg + FOTG210_DISGR2);
+	return;
+
+dma_reset:
+	value = ioread32(ep->fotg210->reg + FOTG210_DMACPSR1);
+	value |= DMACPSR1_DMA_ABORT;
+	iowrite32(value, ep->fotg210->reg + FOTG210_DMACPSR1);
+
+	/* reset fifo */
+	if (ep->epnum) {
+		value = ioread32(ep->fotg210->reg +
+				FOTG210_FIBCR(ep->epnum - 1));
+		value |= FIBCR_FFRST;
+		iowrite32(value, ep->fotg210->reg +
+				FOTG210_FIBCR(ep->epnum - 1));
+	} else {
+		value = ioread32(ep->fotg210->reg + FOTG210_DCFESR);
+		value |= DCFESR_CX_CLR;
+		iowrite32(value, ep->fotg210->reg + FOTG210_DCFESR);
+	}
+}
+
+static void fotg210_start_dma(struct fotg210_ep *ep,
+			struct fotg210_request *req)
+{
+	struct device *dev = &ep->fotg210->gadget.dev;
+	dma_addr_t d;
+	u8 *buffer;
+	u32 length;
+
+	if (ep->epnum) {
+		if (ep->dir_in) {
+			buffer = req->req.buf;
+			length = req->req.length;
+		} else {
+			buffer = req->req.buf + req->req.actual;
+			length = ioread32(ep->fotg210->reg +
+					FOTG210_FIBCR(ep->epnum - 1)) & FIBCR_BCFX;
+			if (length > req->req.length - req->req.actual)
+				length = req->req.length - req->req.actual;
+		}
+	} else {
+		buffer = req->req.buf + req->req.actual;
+		if (req->req.length - req->req.actual > ep->ep.maxpacket)
+			length = ep->ep.maxpacket;
+		else
+			length = req->req.length - req->req.actual;
+	}
+
+	d = dma_map_single(dev, buffer, length,
+			ep->dir_in ? DMA_TO_DEVICE : DMA_FROM_DEVICE);
+
+	if (dma_mapping_error(dev, d)) {
+		pr_err("dma_mapping_error\n");
+		return;
+	}
+
+	fotg210_enable_dma(ep, d, length);
+
+	/* check if dma is done */
+	fotg210_wait_dma_done(ep);
+
+	fotg210_disable_dma(ep);
+
+	/* update actual transfer length */
+	req->req.actual += length;
+
+	dma_unmap_single(dev, d, length, DMA_TO_DEVICE);
+}
+
+static void fotg210_ep0_queue(struct fotg210_ep *ep,
+				struct fotg210_request *req)
+{
+	if (!req->req.length) {
+		fotg210_done(ep, req, 0);
+		return;
+	}
+	if (ep->dir_in) { /* if IN */
+		fotg210_start_dma(ep, req);
+		if (req->req.length == req->req.actual)
+			fotg210_done(ep, req, 0);
+	} else { /* OUT */
+		u32 value = ioread32(ep->fotg210->reg + FOTG210_DMISGR0);
+
+		value &= ~DMISGR0_MCX_OUT_INT;
+		iowrite32(value, ep->fotg210->reg + FOTG210_DMISGR0);
+	}
+}
+
+static int fotg210_ep_queue(struct usb_ep *_ep, struct usb_request *_req,
+				gfp_t gfp_flags)
+{
+	struct fotg210_ep *ep;
+	struct fotg210_request *req;
+	unsigned long flags;
+	int request = 0;
+
+	ep = container_of(_ep, struct fotg210_ep, ep);
+	req = container_of(_req, struct fotg210_request, req);
+
+	if (ep->fotg210->gadget.speed == USB_SPEED_UNKNOWN)
+		return -ESHUTDOWN;
+
+	spin_lock_irqsave(&ep->fotg210->lock, flags);
+
+	if (list_empty(&ep->queue))
+		request = 1;
+
+	list_add_tail(&req->queue, &ep->queue);
+
+	req->req.actual = 0;
+	req->req.status = -EINPROGRESS;
+
+	if (!ep->epnum) /* ep0 */
+		fotg210_ep0_queue(ep, req);
+	else if (request && !ep->stall)
+		fotg210_enable_fifo_int(ep);
+
+	spin_unlock_irqrestore(&ep->fotg210->lock, flags);
+
+	return 0;
+}
+
+static int fotg210_ep_dequeue(struct usb_ep *_ep, struct usb_request *_req)
+{
+	struct fotg210_ep *ep;
+	struct fotg210_request *req;
+	unsigned long flags;
+
+	ep = container_of(_ep, struct fotg210_ep, ep);
+	req = container_of(_req, struct fotg210_request, req);
+
+	spin_lock_irqsave(&ep->fotg210->lock, flags);
+	if (!list_empty(&ep->queue))
+		fotg210_done(ep, req, -ECONNRESET);
+	spin_unlock_irqrestore(&ep->fotg210->lock, flags);
+
+	return 0;
+}
+
+static void fotg210_set_epnstall(struct fotg210_ep *ep)
+{
+	struct fotg210_udc *fotg210 = ep->fotg210;
+	u32 value;
+	void __iomem *reg;
+
+	/* check if IN FIFO is empty before stall */
+	if (ep->dir_in) {
+		do {
+			value = ioread32(fotg210->reg + FOTG210_DCFESR);
+		} while (!(value & DCFESR_FIFO_EMPTY(ep->epnum - 1)));
+	}
+
+	reg = (ep->dir_in) ?
+		fotg210->reg + FOTG210_INEPMPSR(ep->epnum) :
+		fotg210->reg + FOTG210_OUTEPMPSR(ep->epnum);
+	value = ioread32(reg);
+	value |= INOUTEPMPSR_STL_EP;
+	iowrite32(value, reg);
+}
+
+static void fotg210_clear_epnstall(struct fotg210_ep *ep)
+{
+	struct fotg210_udc *fotg210 = ep->fotg210;
+	u32 value;
+	void __iomem *reg;
+
+	reg = (ep->dir_in) ?
+		fotg210->reg + FOTG210_INEPMPSR(ep->epnum) :
+		fotg210->reg + FOTG210_OUTEPMPSR(ep->epnum);
+	value = ioread32(reg);
+	value &= ~INOUTEPMPSR_STL_EP;
+	iowrite32(value, reg);
+}
+
+static int fotg210_set_halt_and_wedge(struct usb_ep *_ep, int value, int wedge)
+{
+	struct fotg210_ep *ep;
+	struct fotg210_udc *fotg210;
+	unsigned long flags;
+
+	ep = container_of(_ep, struct fotg210_ep, ep);
+
+	fotg210 = ep->fotg210;
+
+	spin_lock_irqsave(&ep->fotg210->lock, flags);
+
+	if (value) {
+		fotg210_set_epnstall(ep);
+		ep->stall = 1;
+		if (wedge)
+			ep->wedged = 1;
+	} else {
+		fotg210_reset_tseq(fotg210, ep->epnum);
+		fotg210_clear_epnstall(ep);
+		ep->stall = 0;
+		ep->wedged = 0;
+		if (!list_empty(&ep->queue))
+			fotg210_enable_fifo_int(ep);
+	}
+
+	spin_unlock_irqrestore(&ep->fotg210->lock, flags);
+	return 0;
+}
+
+static int fotg210_ep_set_halt(struct usb_ep *_ep, int value)
+{
+	return fotg210_set_halt_and_wedge(_ep, value, 0);
+}
+
+static int fotg210_ep_set_wedge(struct usb_ep *_ep)
+{
+	return fotg210_set_halt_and_wedge(_ep, 1, 1);
+}
+
+static void fotg210_ep_fifo_flush(struct usb_ep *_ep)
+{
+}
+
+static const struct usb_ep_ops fotg210_ep_ops = {
+	.enable		= fotg210_ep_enable,
+	.disable	= fotg210_ep_disable,
+
+	.alloc_request	= fotg210_ep_alloc_request,
+	.free_request	= fotg210_ep_free_request,
+
+	.queue		= fotg210_ep_queue,
+	.dequeue	= fotg210_ep_dequeue,
+
+	.set_halt	= fotg210_ep_set_halt,
+	.fifo_flush	= fotg210_ep_fifo_flush,
+	.set_wedge	= fotg210_ep_set_wedge,
+};
+
+static void fotg210_clear_tx0byte(struct fotg210_udc *fotg210)
+{
+	u32 value = ioread32(fotg210->reg + FOTG210_TX0BYTE);
+
+	value &= ~(TX0BYTE_EP1 | TX0BYTE_EP2 | TX0BYTE_EP3
+		   | TX0BYTE_EP4);
+	iowrite32(value, fotg210->reg + FOTG210_TX0BYTE);
+}
+
+static void fotg210_clear_rx0byte(struct fotg210_udc *fotg210)
+{
+	u32 value = ioread32(fotg210->reg + FOTG210_RX0BYTE);
+
+	value &= ~(RX0BYTE_EP1 | RX0BYTE_EP2 | RX0BYTE_EP3
+		   | RX0BYTE_EP4);
+	iowrite32(value, fotg210->reg + FOTG210_RX0BYTE);
+}
+
+/* read 8-byte setup packet only */
+static void fotg210_rdsetupp(struct fotg210_udc *fotg210,
+		   u8 *buffer)
+{
+	int i = 0;
+	u8 *tmp = buffer;
+	u32 data;
+	u32 length = 8;
+
+	iowrite32(DMATFNR_ACC_CXF, fotg210->reg + FOTG210_DMATFNR);
+
+	for (i = (length >> 2); i > 0; i--) {
+		data = ioread32(fotg210->reg + FOTG210_CXPORT);
+		*tmp = data & 0xFF;
+		*(tmp + 1) = (data >> 8) & 0xFF;
+		*(tmp + 2) = (data >> 16) & 0xFF;
+		*(tmp + 3) = (data >> 24) & 0xFF;
+		tmp = tmp + 4;
+	}
+
+	switch (length % 4) {
+	case 1:
+		data = ioread32(fotg210->reg + FOTG210_CXPORT);
+		*tmp = data & 0xFF;
+		break;
+	case 2:
+		data = ioread32(fotg210->reg + FOTG210_CXPORT);
+		*tmp = data & 0xFF;
+		*(tmp + 1) = (data >> 8) & 0xFF;
+		break;
+	case 3:
+		data = ioread32(fotg210->reg + FOTG210_CXPORT);
+		*tmp = data & 0xFF;
+		*(tmp + 1) = (data >> 8) & 0xFF;
+		*(tmp + 2) = (data >> 16) & 0xFF;
+		break;
+	default:
+		break;
+	}
+
+	iowrite32(DMATFNR_DISDMA, fotg210->reg + FOTG210_DMATFNR);
+}
+
+static void fotg210_set_configuration(struct fotg210_udc *fotg210)
+{
+	u32 value = ioread32(fotg210->reg + FOTG210_DAR);
+
+	value |= DAR_AFT_CONF;
+	iowrite32(value, fotg210->reg + FOTG210_DAR);
+}
+
+static void fotg210_set_dev_addr(struct fotg210_udc *fotg210, u32 addr)
+{
+	u32 value = ioread32(fotg210->reg + FOTG210_DAR);
+
+	value |= (addr & 0x7F);
+	iowrite32(value, fotg210->reg + FOTG210_DAR);
+}
+
+static void fotg210_set_cxstall(struct fotg210_udc *fotg210)
+{
+	u32 value = ioread32(fotg210->reg + FOTG210_DCFESR);
+
+	value |= DCFESR_CX_STL;
+	iowrite32(value, fotg210->reg + FOTG210_DCFESR);
+}
+
+static void fotg210_request_error(struct fotg210_udc *fotg210)
+{
+	fotg210_set_cxstall(fotg210);
+	pr_err("request error!!\n");
+}
+
+static void fotg210_set_address(struct fotg210_udc *fotg210,
+				struct usb_ctrlrequest *ctrl)
+{
+	if (le16_to_cpu(ctrl->wValue) >= 0x0100) {
+		fotg210_request_error(fotg210);
+	} else {
+		fotg210_set_dev_addr(fotg210, le16_to_cpu(ctrl->wValue));
+		fotg210_set_cxdone(fotg210);
+	}
+}
+
+static void fotg210_set_feature(struct fotg210_udc *fotg210,
+				struct usb_ctrlrequest *ctrl)
+{
+	switch (ctrl->bRequestType & USB_RECIP_MASK) {
+	case USB_RECIP_DEVICE:
+		fotg210_set_cxdone(fotg210);
+		break;
+	case USB_RECIP_INTERFACE:
+		fotg210_set_cxdone(fotg210);
+		break;
+	case USB_RECIP_ENDPOINT: {
+		u8 epnum;
+		epnum = le16_to_cpu(ctrl->wIndex) & USB_ENDPOINT_NUMBER_MASK;
+		if (epnum)
+			fotg210_set_epnstall(fotg210->ep[epnum]);
+		else
+			fotg210_set_cxstall(fotg210);
+		fotg210_set_cxdone(fotg210);
+		}
+		break;
+	default:
+		fotg210_request_error(fotg210);
+		break;
+	}
+}
+
+static void fotg210_clear_feature(struct fotg210_udc *fotg210,
+				struct usb_ctrlrequest *ctrl)
+{
+	struct fotg210_ep *ep =
+		fotg210->ep[ctrl->wIndex & USB_ENDPOINT_NUMBER_MASK];
+
+	switch (ctrl->bRequestType & USB_RECIP_MASK) {
+	case USB_RECIP_DEVICE:
+		fotg210_set_cxdone(fotg210);
+		break;
+	case USB_RECIP_INTERFACE:
+		fotg210_set_cxdone(fotg210);
+		break;
+	case USB_RECIP_ENDPOINT:
+		if (ctrl->wIndex & USB_ENDPOINT_NUMBER_MASK) {
+			if (ep->wedged) {
+				fotg210_set_cxdone(fotg210);
+				break;
+			}
+			if (ep->stall)
+				fotg210_set_halt_and_wedge(&ep->ep, 0, 0);
+		}
+		fotg210_set_cxdone(fotg210);
+		break;
+	default:
+		fotg210_request_error(fotg210);
+		break;
+	}
+}
+
+static int fotg210_is_epnstall(struct fotg210_ep *ep)
+{
+	struct fotg210_udc *fotg210 = ep->fotg210;
+	u32 value;
+	void __iomem *reg;
+
+	reg = (ep->dir_in) ?
+		fotg210->reg + FOTG210_INEPMPSR(ep->epnum) :
+		fotg210->reg + FOTG210_OUTEPMPSR(ep->epnum);
+	value = ioread32(reg);
+	return value & INOUTEPMPSR_STL_EP ? 1 : 0;
+}
+
+/* For EP0 requests triggered by this driver (currently GET_STATUS response) */
+static void fotg210_ep0_complete(struct usb_ep *_ep, struct usb_request *req)
+{
+	struct fotg210_ep *ep;
+	struct fotg210_udc *fotg210;
+
+	ep = container_of(_ep, struct fotg210_ep, ep);
+	fotg210 = ep->fotg210;
+
+	if (req->status || req->actual != req->length) {
+		dev_warn(&fotg210->gadget.dev, "EP0 request failed: %d\n", req->status);
+	}
+}
+
+static void fotg210_get_status(struct fotg210_udc *fotg210,
+				struct usb_ctrlrequest *ctrl)
+{
+	u8 epnum;
+
+	switch (ctrl->bRequestType & USB_RECIP_MASK) {
+	case USB_RECIP_DEVICE:
+		fotg210->ep0_data = cpu_to_le16(1 << USB_DEVICE_SELF_POWERED);
+		break;
+	case USB_RECIP_INTERFACE:
+		fotg210->ep0_data = cpu_to_le16(0);
+		break;
+	case USB_RECIP_ENDPOINT:
+		epnum = ctrl->wIndex & USB_ENDPOINT_NUMBER_MASK;
+		if (epnum)
+			fotg210->ep0_data =
+				cpu_to_le16(fotg210_is_epnstall(fotg210->ep[epnum])
+					    << USB_ENDPOINT_HALT);
+		else
+			fotg210_request_error(fotg210);
+		break;
+
+	default:
+		fotg210_request_error(fotg210);
+		return;		/* exit */
+	}
+
+	fotg210->ep0_req->buf = &fotg210->ep0_data;
+	fotg210->ep0_req->length = 2;
+
+	spin_unlock(&fotg210->lock);
+	fotg210_ep_queue(fotg210->gadget.ep0, fotg210->ep0_req, GFP_ATOMIC);
+	spin_lock(&fotg210->lock);
+}
+
+static int fotg210_setup_packet(struct fotg210_udc *fotg210,
+				struct usb_ctrlrequest *ctrl)
+{
+	u8 *p = (u8 *)ctrl;
+	u8 ret = 0;
+
+	fotg210_rdsetupp(fotg210, p);
+
+	fotg210->ep[0]->dir_in = ctrl->bRequestType & USB_DIR_IN;
+
+	if (fotg210->gadget.speed == USB_SPEED_UNKNOWN) {
+		u32 value = ioread32(fotg210->reg + FOTG210_DMCR);
+		fotg210->gadget.speed = value & DMCR_HS_EN ?
+				USB_SPEED_HIGH : USB_SPEED_FULL;
+	}
+
+	/* check request */
+	if ((ctrl->bRequestType & USB_TYPE_MASK) == USB_TYPE_STANDARD) {
+		switch (ctrl->bRequest) {
+		case USB_REQ_GET_STATUS:
+			fotg210_get_status(fotg210, ctrl);
+			break;
+		case USB_REQ_CLEAR_FEATURE:
+			fotg210_clear_feature(fotg210, ctrl);
+			break;
+		case USB_REQ_SET_FEATURE:
+			fotg210_set_feature(fotg210, ctrl);
+			break;
+		case USB_REQ_SET_ADDRESS:
+			fotg210_set_address(fotg210, ctrl);
+			break;
+		case USB_REQ_SET_CONFIGURATION:
+			fotg210_set_configuration(fotg210);
+			ret = 1;
+			break;
+		default:
+			ret = 1;
+			break;
+		}
+	} else {
+		ret = 1;
+	}
+
+	return ret;
+}
+
+static void fotg210_ep0out(struct fotg210_udc *fotg210)
+{
+	struct fotg210_ep *ep = fotg210->ep[0];
+
+	if (!list_empty(&ep->queue) && !ep->dir_in) {
+		struct fotg210_request *req;
+
+		req = list_first_entry(&ep->queue,
+			struct fotg210_request, queue);
+
+		if (req->req.length)
+			fotg210_start_dma(ep, req);
+
+		if ((req->req.length - req->req.actual) < ep->ep.maxpacket)
+			fotg210_done(ep, req, 0);
+	} else {
+		pr_err("%s : empty queue\n", __func__);
+	}
+}
+
+static void fotg210_ep0in(struct fotg210_udc *fotg210)
+{
+	struct fotg210_ep *ep = fotg210->ep[0];
+
+	if ((!list_empty(&ep->queue)) && (ep->dir_in)) {
+		struct fotg210_request *req;
+
+		req = list_entry(ep->queue.next,
+				struct fotg210_request, queue);
+
+		if (req->req.length)
+			fotg210_start_dma(ep, req);
+
+		if (req->req.actual == req->req.length)
+			fotg210_done(ep, req, 0);
+	} else {
+		fotg210_set_cxdone(fotg210);
+	}
+}
+
+static void fotg210_clear_comabt_int(struct fotg210_udc *fotg210)
+{
+	u32 value = ioread32(fotg210->reg + FOTG210_DISGR0);
+
+	value &= ~DISGR0_CX_COMABT_INT;
+	iowrite32(value, fotg210->reg + FOTG210_DISGR0);
+}
+
+static void fotg210_in_fifo_handler(struct fotg210_ep *ep)
+{
+	struct fotg210_request *req = list_entry(ep->queue.next,
+					struct fotg210_request, queue);
+
+	if (req->req.length)
+		fotg210_start_dma(ep, req);
+	fotg210_done(ep, req, 0);
+}
+
+static void fotg210_out_fifo_handler(struct fotg210_ep *ep)
+{
+	struct fotg210_request *req = list_entry(ep->queue.next,
+						 struct fotg210_request, queue);
+	int disgr1 = ioread32(ep->fotg210->reg + FOTG210_DISGR1);
+
+	fotg210_start_dma(ep, req);
+
+	/* Complete the request when it's full or a short packet arrived.
+	 * Like other drivers, short_not_ok isn't handled.
+	 */
+
+	if (req->req.length == req->req.actual ||
+	    (disgr1 & DISGR1_SPK_INT(ep->epnum - 1)))
+		fotg210_done(ep, req, 0);
+}
+
+static irqreturn_t fotg210_irq(int irq, void *_fotg210)
+{
+	struct fotg210_udc *fotg210 = _fotg210;
+	u32 int_grp = ioread32(fotg210->reg + FOTG210_DIGR);
+	u32 int_msk = ioread32(fotg210->reg + FOTG210_DMIGR);
+
+	int_grp &= ~int_msk;
+
+	spin_lock(&fotg210->lock);
+
+	if (int_grp & DIGR_INT_G2) {
+		void __iomem *reg = fotg210->reg + FOTG210_DISGR2;
+		u32 int_grp2 = ioread32(reg);
+		u32 int_msk2 = ioread32(fotg210->reg + FOTG210_DMISGR2);
+		u32 value;
+
+		int_grp2 &= ~int_msk2;
+
+		if (int_grp2 & DISGR2_USBRST_INT) {
+			usb_gadget_udc_reset(&fotg210->gadget,
+					     fotg210->driver);
+			value = ioread32(reg);
+			value &= ~DISGR2_USBRST_INT;
+			iowrite32(value, reg);
+			pr_info("fotg210 udc reset\n");
+		}
+		if (int_grp2 & DISGR2_SUSP_INT) {
+			value = ioread32(reg);
+			value &= ~DISGR2_SUSP_INT;
+			iowrite32(value, reg);
+			pr_info("fotg210 udc suspend\n");
+		}
+		if (int_grp2 & DISGR2_RESM_INT) {
+			value = ioread32(reg);
+			value &= ~DISGR2_RESM_INT;
+			iowrite32(value, reg);
+			pr_info("fotg210 udc resume\n");
+		}
+		if (int_grp2 & DISGR2_ISO_SEQ_ERR_INT) {
+			value = ioread32(reg);
+			value &= ~DISGR2_ISO_SEQ_ERR_INT;
+			iowrite32(value, reg);
+			pr_info("fotg210 iso sequence error\n");
+		}
+		if (int_grp2 & DISGR2_ISO_SEQ_ABORT_INT) {
+			value = ioread32(reg);
+			value &= ~DISGR2_ISO_SEQ_ABORT_INT;
+			iowrite32(value, reg);
+			pr_info("fotg210 iso sequence abort\n");
+		}
+		if (int_grp2 & DISGR2_TX0BYTE_INT) {
+			fotg210_clear_tx0byte(fotg210);
+			value = ioread32(reg);
+			value &= ~DISGR2_TX0BYTE_INT;
+			iowrite32(value, reg);
+			pr_info("fotg210 transferred 0 byte\n");
+		}
+		if (int_grp2 & DISGR2_RX0BYTE_INT) {
+			fotg210_clear_rx0byte(fotg210);
+			value = ioread32(reg);
+			value &= ~DISGR2_RX0BYTE_INT;
+			iowrite32(value, reg);
+			pr_info("fotg210 received 0 byte\n");
+		}
+		if (int_grp2 & DISGR2_DMA_ERROR) {
+			value = ioread32(reg);
+			value &= ~DISGR2_DMA_ERROR;
+			iowrite32(value, reg);
+		}
+	}
+
+	if (int_grp & DIGR_INT_G0) {
+		void __iomem *reg = fotg210->reg + FOTG210_DISGR0;
+		u32 int_grp0 = ioread32(reg);
+		u32 int_msk0 = ioread32(fotg210->reg + FOTG210_DMISGR0);
+		struct usb_ctrlrequest ctrl;
+
+		int_grp0 &= ~int_msk0;
+
+		/* the highest priority in this source register */
+		if (int_grp0 & DISGR0_CX_COMABT_INT) {
+			fotg210_clear_comabt_int(fotg210);
+			pr_info("fotg210 CX command abort\n");
+		}
+
+		if (int_grp0 & DISGR0_CX_SETUP_INT) {
+			if (fotg210_setup_packet(fotg210, &ctrl)) {
+				spin_unlock(&fotg210->lock);
+				if (fotg210->driver->setup(&fotg210->gadget,
+							   &ctrl) < 0)
+					fotg210_set_cxstall(fotg210);
+				spin_lock(&fotg210->lock);
+			}
+		}
+		if (int_grp0 & DISGR0_CX_COMEND_INT)
+			pr_info("fotg210 cmd end\n");
+
+		if (int_grp0 & DISGR0_CX_IN_INT)
+			fotg210_ep0in(fotg210);
+
+		if (int_grp0 & DISGR0_CX_OUT_INT)
+			fotg210_ep0out(fotg210);
+
+		if (int_grp0 & DISGR0_CX_COMFAIL_INT) {
+			fotg210_set_cxstall(fotg210);
+			pr_info("fotg210 ep0 fail\n");
+		}
+	}
+
+	if (int_grp & DIGR_INT_G1) {
+		void __iomem *reg = fotg210->reg + FOTG210_DISGR1;
+		u32 int_grp1 = ioread32(reg);
+		u32 int_msk1 = ioread32(fotg210->reg + FOTG210_DMISGR1);
+		int fifo;
+
+		int_grp1 &= ~int_msk1;
+
+		for (fifo = 0; fifo < FOTG210_MAX_FIFO_NUM; fifo++) {
+			if (int_grp1 & DISGR1_IN_INT(fifo))
+				fotg210_in_fifo_handler(fotg210->ep[fifo + 1]);
+
+			if ((int_grp1 & DISGR1_OUT_INT(fifo)) ||
+			    (int_grp1 & DISGR1_SPK_INT(fifo)))
+				fotg210_out_fifo_handler(fotg210->ep[fifo + 1]);
+		}
+	}
+
+	spin_unlock(&fotg210->lock);
+
+	return IRQ_HANDLED;
+}
+
+static void fotg210_disable_unplug(struct fotg210_udc *fotg210)
+{
+	u32 reg = ioread32(fotg210->reg + FOTG210_PHYTMSR);
+
+	reg &= ~PHYTMSR_UNPLUG;
+	iowrite32(reg, fotg210->reg + FOTG210_PHYTMSR);
+}
+
+static int fotg210_udc_start(struct usb_gadget *g,
+		struct usb_gadget_driver *driver)
+{
+	struct fotg210_udc *fotg210 = gadget_to_fotg210(g);
+	u32 value;
+
+	/* hook up the driver */
+	fotg210->driver = driver;
+
+	/* enable device global interrupt */
+	value = ioread32(fotg210->reg + FOTG210_DMCR);
+	value |= DMCR_GLINT_EN;
+	iowrite32(value, fotg210->reg + FOTG210_DMCR);
+
+	return 0;
+}
+
+static void fotg210_init(struct fotg210_udc *fotg210)
+{
+	u32 value;
+
+	/* disable global interrupt and set int polarity to active high */
+	iowrite32(GMIR_MHC_INT | GMIR_MOTG_INT | GMIR_INT_POLARITY,
+		  fotg210->reg + FOTG210_GMIR);
+
+	/* disable device global interrupt */
+	value = ioread32(fotg210->reg + FOTG210_DMCR);
+	value &= ~DMCR_GLINT_EN;
+	iowrite32(value, fotg210->reg + FOTG210_DMCR);
+
+	/* enable only grp2 irqs we handle */
+	iowrite32(~(DISGR2_DMA_ERROR | DISGR2_RX0BYTE_INT | DISGR2_TX0BYTE_INT
+		    | DISGR2_ISO_SEQ_ABORT_INT | DISGR2_ISO_SEQ_ERR_INT
+		    | DISGR2_RESM_INT | DISGR2_SUSP_INT | DISGR2_USBRST_INT),
+		  fotg210->reg + FOTG210_DMISGR2);
+
+	/* disable all fifo interrupt */
+	iowrite32(~(u32)0, fotg210->reg + FOTG210_DMISGR1);
+
+	/* disable cmd end */
+	value = ioread32(fotg210->reg + FOTG210_DMISGR0);
+	value |= DMISGR0_MCX_COMEND;
+	iowrite32(value, fotg210->reg + FOTG210_DMISGR0);
+}
+
+static int fotg210_udc_stop(struct usb_gadget *g)
+{
+	struct fotg210_udc *fotg210 = gadget_to_fotg210(g);
+	unsigned long	flags;
+
+	spin_lock_irqsave(&fotg210->lock, flags);
+
+	fotg210_init(fotg210);
+	fotg210->driver = NULL;
+
+	spin_unlock_irqrestore(&fotg210->lock, flags);
+
+	return 0;
+}
+
+static const struct usb_gadget_ops fotg210_gadget_ops = {
+	.udc_start		= fotg210_udc_start,
+	.udc_stop		= fotg210_udc_stop,
+};
+
+static int fotg210_udc_remove(struct platform_device *pdev)
+{
+	struct fotg210_udc *fotg210 = platform_get_drvdata(pdev);
+	int i;
+
+	usb_del_gadget_udc(&fotg210->gadget);
+	iounmap(fotg210->reg);
+	free_irq(platform_get_irq(pdev, 0), fotg210);
+
+	fotg210_ep_free_request(&fotg210->ep[0]->ep, fotg210->ep0_req);
+	for (i = 0; i < FOTG210_MAX_NUM_EP; i++)
+		kfree(fotg210->ep[i]);
+	kfree(fotg210);
+
+	return 0;
+}
+
+static int fotg210_udc_probe(struct platform_device *pdev)
+{
+	struct resource *res, *ires;
+	struct fotg210_udc *fotg210 = NULL;
+	struct fotg210_ep *_ep[FOTG210_MAX_NUM_EP];
+	int ret = 0;
+	int i;
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	if (!res) {
+		pr_err("platform_get_resource error.\n");
+		return -ENODEV;
+	}
+
+	ires = platform_get_resource(pdev, IORESOURCE_IRQ, 0);
+	if (!ires) {
+		pr_err("platform_get_resource IORESOURCE_IRQ error.\n");
+		return -ENODEV;
+	}
+
+	ret = -ENOMEM;
+
+	/* initialize udc */
+	fotg210 = kzalloc(sizeof(struct fotg210_udc), GFP_KERNEL);
+	if (fotg210 == NULL)
+		goto err;
+
+	for (i = 0; i < FOTG210_MAX_NUM_EP; i++) {
+		_ep[i] = kzalloc(sizeof(struct fotg210_ep), GFP_KERNEL);
+		if (_ep[i] == NULL)
+			goto err_alloc;
+		fotg210->ep[i] = _ep[i];
+	}
+
+	fotg210->reg = ioremap(res->start, resource_size(res));
+	if (fotg210->reg == NULL) {
+		pr_err("ioremap error.\n");
+		goto err_alloc;
+	}
+
+	spin_lock_init(&fotg210->lock);
+
+	platform_set_drvdata(pdev, fotg210);
+
+	fotg210->gadget.ops = &fotg210_gadget_ops;
+
+	fotg210->gadget.max_speed = USB_SPEED_HIGH;
+	fotg210->gadget.dev.parent = &pdev->dev;
+	fotg210->gadget.dev.dma_mask = pdev->dev.dma_mask;
+	fotg210->gadget.name = udc_name;
+
+	INIT_LIST_HEAD(&fotg210->gadget.ep_list);
+
+	for (i = 0; i < FOTG210_MAX_NUM_EP; i++) {
+		struct fotg210_ep *ep = fotg210->ep[i];
+
+		if (i) {
+			INIT_LIST_HEAD(&fotg210->ep[i]->ep.ep_list);
+			list_add_tail(&fotg210->ep[i]->ep.ep_list,
+				      &fotg210->gadget.ep_list);
+		}
+		ep->fotg210 = fotg210;
+		INIT_LIST_HEAD(&ep->queue);
+		ep->ep.name = fotg210_ep_name[i];
+		ep->ep.ops = &fotg210_ep_ops;
+		usb_ep_set_maxpacket_limit(&ep->ep, (unsigned short) ~0);
+
+		if (i == 0) {
+			ep->ep.caps.type_control = true;
+		} else {
+			ep->ep.caps.type_iso = true;
+			ep->ep.caps.type_bulk = true;
+			ep->ep.caps.type_int = true;
+		}
+
+		ep->ep.caps.dir_in = true;
+		ep->ep.caps.dir_out = true;
+	}
+	usb_ep_set_maxpacket_limit(&fotg210->ep[0]->ep, 0x40);
+	fotg210->gadget.ep0 = &fotg210->ep[0]->ep;
+	INIT_LIST_HEAD(&fotg210->gadget.ep0->ep_list);
+
+	fotg210->ep0_req = fotg210_ep_alloc_request(&fotg210->ep[0]->ep,
+				GFP_KERNEL);
+	if (fotg210->ep0_req == NULL)
+		goto err_map;
+
+	fotg210->ep0_req->complete = fotg210_ep0_complete;
+
+	fotg210_init(fotg210);
+
+	fotg210_disable_unplug(fotg210);
+
+	ret = request_irq(ires->start, fotg210_irq, IRQF_SHARED,
+			  udc_name, fotg210);
+	if (ret < 0) {
+		pr_err("request_irq error (%d)\n", ret);
+		goto err_req;
+	}
+
+	ret = usb_add_gadget_udc(&pdev->dev, &fotg210->gadget);
+	if (ret)
+		goto err_add_udc;
+
+	dev_info(&pdev->dev, "version %s\n", DRIVER_VERSION);
+
+	return 0;
+
+err_add_udc:
+	free_irq(ires->start, fotg210);
+
+err_req:
+	fotg210_ep_free_request(&fotg210->ep[0]->ep, fotg210->ep0_req);
+
+err_map:
+	iounmap(fotg210->reg);
+
+err_alloc:
+	for (i = 0; i < FOTG210_MAX_NUM_EP; i++)
+		kfree(fotg210->ep[i]);
+	kfree(fotg210);
+
+err:
+	return ret;
+}
+
+static struct platform_driver fotg210_driver = {
+	.driver		= {
+		.name =	udc_name,
+	},
+	.probe		= fotg210_udc_probe,
+	.remove		= fotg210_udc_remove,
+};
+
+module_platform_driver(fotg210_driver);
+
+MODULE_AUTHOR("Yuan-Hsin Chen, Feng-Hsin Chiang <john453@faraday-tech.com>");
+MODULE_LICENSE("GPL");
+MODULE_DESCRIPTION(DRIVER_DESC);
--- a/drivers/usb/gadget/udc/Kconfig
+++ b/drivers/usb/gadget/udc/Kconfig
@@ -108,17 +108,6 @@ config USB_FUSB300
 	help
 	   Faraday usb device controller FUSB300 driver
 
-config USB_FOTG210_UDC
-	depends on HAS_DMA
-	tristate "Faraday FOTG210 USB Peripheral Controller"
-	help
-	   Faraday USB2.0 OTG controller which can be configured as
-	   high speed or full speed USB device. This driver supppors
-	   Bulk Transfer so far.
-
-	   Say "y" to link the driver statically, or "m" to build a
-	   dynamically linked module called "fotg210_udc".
-
 config USB_GR_UDC
 	tristate "Aeroflex Gaisler GRUSBDC USB Peripheral Controller Driver"
 	depends on HAS_DMA
--- a/drivers/usb/gadget/udc/Makefile
+++ b/drivers/usb/gadget/udc/Makefile
@@ -34,7 +34,6 @@ obj-$(CONFIG_USB_EG20T)		+= pch_udc.o
 obj-$(CONFIG_USB_MV_UDC)	+= mv_udc.o
 mv_udc-y			:= mv_udc_core.o
 obj-$(CONFIG_USB_FUSB300)	+= fusb300_udc.o
-obj-$(CONFIG_USB_FOTG210_UDC)	+= fotg210-udc.o
 obj-$(CONFIG_USB_MV_U3D)	+= mv_u3d_core.o
 obj-$(CONFIG_USB_GR_UDC)	+= gr_udc.o
 obj-$(CONFIG_USB_GADGET_XILINX)	+= udc-xilinx.o
--- a/drivers/usb/host/Kconfig
+++ b/drivers/usb/host/Kconfig
@@ -389,17 +389,6 @@ config USB_ISP1362_HCD
 	  To compile this driver as a module, choose M here: the
 	  module will be called isp1362-hcd.
 
-config USB_FOTG210_HCD
-	tristate "FOTG210 HCD support"
-	depends on USB && HAS_DMA && HAS_IOMEM
-	help
-	  Faraday FOTG210 is an OTG controller which can be configured as
-	  an USB2.0 host. It is designed to meet USB2.0 EHCI specification
-	  with minor modification.
-
-	  To compile this driver as a module, choose M here: the
-	  module will be called fotg210-hcd.
-
 config USB_MAX3421_HCD
 	tristate "MAX3421 HCD (USB-over-SPI) support"
 	depends on USB && SPI
--- a/drivers/usb/host/Makefile
+++ b/drivers/usb/host/Makefile
@@ -84,6 +84,5 @@ obj-$(CONFIG_USB_EHCI_FSL)	+= ehci-fsl.o
 obj-$(CONFIG_USB_EHCI_MV)	+= ehci-mv.o
 obj-$(CONFIG_USB_HCD_BCMA)	+= bcma-hcd.o
 obj-$(CONFIG_USB_HCD_SSB)	+= ssb-hcd.o
-obj-$(CONFIG_USB_FOTG210_HCD)	+= fotg210-hcd.o
 obj-$(CONFIG_USB_MAX3421_HCD)	+= max3421-hcd.o
 obj-$(CONFIG_USB_XEN_HCD)	+= xen-hcd.o
--- /dev/null
+++ b/drivers/usb/fotg210/fotg210-hcd.h
@@ -0,0 +1,688 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+#ifndef __LINUX_FOTG210_H
+#define __LINUX_FOTG210_H
+
+#include <linux/usb/ehci-dbgp.h>
+
+/* definitions used for the EHCI driver */
+
+/*
+ * __hc32 and __hc16 are "Host Controller" types, they may be equivalent to
+ * __leXX (normally) or __beXX (given FOTG210_BIG_ENDIAN_DESC), depending on
+ * the host controller implementation.
+ *
+ * To facilitate the strongest possible byte-order checking from "sparse"
+ * and so on, we use __leXX unless that's not practical.
+ */
+#define __hc32	__le32
+#define __hc16	__le16
+
+/* statistics can be kept for tuning/monitoring */
+struct fotg210_stats {
+	/* irq usage */
+	unsigned long		normal;
+	unsigned long		error;
+	unsigned long		iaa;
+	unsigned long		lost_iaa;
+
+	/* termination of urbs from core */
+	unsigned long		complete;
+	unsigned long		unlink;
+};
+
+/* fotg210_hcd->lock guards shared data against other CPUs:
+ *   fotg210_hcd:	async, unlink, periodic (and shadow), ...
+ *   usb_host_endpoint: hcpriv
+ *   fotg210_qh:	qh_next, qtd_list
+ *   fotg210_qtd:	qtd_list
+ *
+ * Also, hold this lock when talking to HC registers or
+ * when updating hw_* fields in shared qh/qtd/... structures.
+ */
+
+#define	FOTG210_MAX_ROOT_PORTS	1		/* see HCS_N_PORTS */
+
+/*
+ * fotg210_rh_state values of FOTG210_RH_RUNNING or above mean that the
+ * controller may be doing DMA.  Lower values mean there's no DMA.
+ */
+enum fotg210_rh_state {
+	FOTG210_RH_HALTED,
+	FOTG210_RH_SUSPENDED,
+	FOTG210_RH_RUNNING,
+	FOTG210_RH_STOPPING
+};
+
+/*
+ * Timer events, ordered by increasing delay length.
+ * Always update event_delays_ns[] and event_handlers[] (defined in
+ * ehci-timer.c) in parallel with this list.
+ */
+enum fotg210_hrtimer_event {
+	FOTG210_HRTIMER_POLL_ASS,	/* Poll for async schedule off */
+	FOTG210_HRTIMER_POLL_PSS,	/* Poll for periodic schedule off */
+	FOTG210_HRTIMER_POLL_DEAD,	/* Wait for dead controller to stop */
+	FOTG210_HRTIMER_UNLINK_INTR,	/* Wait for interrupt QH unlink */
+	FOTG210_HRTIMER_FREE_ITDS,	/* Wait for unused iTDs and siTDs */
+	FOTG210_HRTIMER_ASYNC_UNLINKS,	/* Unlink empty async QHs */
+	FOTG210_HRTIMER_IAA_WATCHDOG,	/* Handle lost IAA interrupts */
+	FOTG210_HRTIMER_DISABLE_PERIODIC, /* Wait to disable periodic sched */
+	FOTG210_HRTIMER_DISABLE_ASYNC,	/* Wait to disable async sched */
+	FOTG210_HRTIMER_IO_WATCHDOG,	/* Check for missing IRQs */
+	FOTG210_HRTIMER_NUM_EVENTS	/* Must come last */
+};
+#define FOTG210_HRTIMER_NO_EVENT	99
+
+struct fotg210_hcd {			/* one per controller */
+	/* timing support */
+	enum fotg210_hrtimer_event	next_hrtimer_event;
+	unsigned		enabled_hrtimer_events;
+	ktime_t			hr_timeouts[FOTG210_HRTIMER_NUM_EVENTS];
+	struct hrtimer		hrtimer;
+
+	int			PSS_poll_count;
+	int			ASS_poll_count;
+	int			died_poll_count;
+
+	/* glue to PCI and HCD framework */
+	struct fotg210_caps __iomem *caps;
+	struct fotg210_regs __iomem *regs;
+	struct ehci_dbg_port __iomem *debug;
+
+	__u32			hcs_params;	/* cached register copy */
+	spinlock_t		lock;
+	enum fotg210_rh_state	rh_state;
+
+	/* general schedule support */
+	bool			scanning:1;
+	bool			need_rescan:1;
+	bool			intr_unlinking:1;
+	bool			async_unlinking:1;
+	bool			shutdown:1;
+	struct fotg210_qh		*qh_scan_next;
+
+	/* async schedule support */
+	struct fotg210_qh		*async;
+	struct fotg210_qh		*dummy;		/* For AMD quirk use */
+	struct fotg210_qh		*async_unlink;
+	struct fotg210_qh		*async_unlink_last;
+	struct fotg210_qh		*async_iaa;
+	unsigned		async_unlink_cycle;
+	unsigned		async_count;	/* async activity count */
+
+	/* periodic schedule support */
+#define	DEFAULT_I_TDPS		1024		/* some HCs can do less */
+	unsigned		periodic_size;
+	__hc32			*periodic;	/* hw periodic table */
+	dma_addr_t		periodic_dma;
+	struct list_head	intr_qh_list;
+	unsigned		i_thresh;	/* uframes HC might cache */
+
+	union fotg210_shadow	*pshadow;	/* mirror hw periodic table */
+	struct fotg210_qh		*intr_unlink;
+	struct fotg210_qh		*intr_unlink_last;
+	unsigned		intr_unlink_cycle;
+	unsigned		now_frame;	/* frame from HC hardware */
+	unsigned		next_frame;	/* scan periodic, start here */
+	unsigned		intr_count;	/* intr activity count */
+	unsigned		isoc_count;	/* isoc activity count */
+	unsigned		periodic_count;	/* periodic activity count */
+	/* max periodic time per uframe */
+	unsigned		uframe_periodic_max;
+
+
+	/* list of itds completed while now_frame was still active */
+	struct list_head	cached_itd_list;
+	struct fotg210_itd	*last_itd_to_free;
+
+	/* per root hub port */
+	unsigned long		reset_done[FOTG210_MAX_ROOT_PORTS];
+
+	/* bit vectors (one bit per port)
+	 * which ports were already suspended at the start of a bus suspend
+	 */
+	unsigned long		bus_suspended;
+
+	/* which ports are edicated to the companion controller */
+	unsigned long		companion_ports;
+
+	/* which ports are owned by the companion during a bus suspend */
+	unsigned long		owned_ports;
+
+	/* which ports have the change-suspend feature turned on */
+	unsigned long		port_c_suspend;
+
+	/* which ports are suspended */
+	unsigned long		suspended_ports;
+
+	/* which ports have started to resume */
+	unsigned long		resuming_ports;
+
+	/* per-HC memory pools (could be per-bus, but ...) */
+	struct dma_pool		*qh_pool;	/* qh per active urb */
+	struct dma_pool		*qtd_pool;	/* one or more per qh */
+	struct dma_pool		*itd_pool;	/* itd per iso urb */
+
+	unsigned		random_frame;
+	unsigned long		next_statechange;
+	ktime_t			last_periodic_enable;
+	u32			command;
+
+	/* SILICON QUIRKS */
+	unsigned		need_io_watchdog:1;
+	unsigned		fs_i_thresh:1;	/* Intel iso scheduling */
+
+	u8			sbrn;		/* packed release number */
+
+	/* irq statistics */
+#ifdef FOTG210_STATS
+	struct fotg210_stats	stats;
+#	define INCR(x) ((x)++)
+#else
+#	define INCR(x) do {} while (0)
+#endif
+
+	/* silicon clock */
+	struct clk		*pclk;
+};
+
+/* convert between an HCD pointer and the corresponding FOTG210_HCD */
+static inline struct fotg210_hcd *hcd_to_fotg210(struct usb_hcd *hcd)
+{
+	return (struct fotg210_hcd *)(hcd->hcd_priv);
+}
+static inline struct usb_hcd *fotg210_to_hcd(struct fotg210_hcd *fotg210)
+{
+	return container_of((void *) fotg210, struct usb_hcd, hcd_priv);
+}
+
+/*-------------------------------------------------------------------------*/
+
+/* EHCI register interface, corresponds to EHCI Revision 0.95 specification */
+
+/* Section 2.2 Host Controller Capability Registers */
+struct fotg210_caps {
+	/* these fields are specified as 8 and 16 bit registers,
+	 * but some hosts can't perform 8 or 16 bit PCI accesses.
+	 * some hosts treat caplength and hciversion as parts of a 32-bit
+	 * register, others treat them as two separate registers, this
+	 * affects the memory map for big endian controllers.
+	 */
+	u32		hc_capbase;
+#define HC_LENGTH(fotg210, p)	(0x00ff&((p) >> /* bits 7:0 / offset 00h */ \
+				(fotg210_big_endian_capbase(fotg210) ? 24 : 0)))
+#define HC_VERSION(fotg210, p)	(0xffff&((p) >> /* bits 31:16 / offset 02h */ \
+				(fotg210_big_endian_capbase(fotg210) ? 0 : 16)))
+	u32		hcs_params;     /* HCSPARAMS - offset 0x4 */
+#define HCS_N_PORTS(p)		(((p)>>0)&0xf)	/* bits 3:0, ports on HC */
+
+	u32		hcc_params;	/* HCCPARAMS - offset 0x8 */
+#define HCC_CANPARK(p)		((p)&(1 << 2))  /* true: can park on async qh */
+#define HCC_PGM_FRAMELISTLEN(p) ((p)&(1 << 1))  /* true: periodic_size changes*/
+	u8		portroute[8];	 /* nibbles for routing - offset 0xC */
+};
+
+
+/* Section 2.3 Host Controller Operational Registers */
+struct fotg210_regs {
+
+	/* USBCMD: offset 0x00 */
+	u32		command;
+
+/* EHCI 1.1 addendum */
+/* 23:16 is r/w intr rate, in microframes; default "8" == 1/msec */
+#define CMD_PARK	(1<<11)		/* enable "park" on async qh */
+#define CMD_PARK_CNT(c)	(((c)>>8)&3)	/* how many transfers to park for */
+#define CMD_IAAD	(1<<6)		/* "doorbell" interrupt async advance */
+#define CMD_ASE		(1<<5)		/* async schedule enable */
+#define CMD_PSE		(1<<4)		/* periodic schedule enable */
+/* 3:2 is periodic frame list size */
+#define CMD_RESET	(1<<1)		/* reset HC not bus */
+#define CMD_RUN		(1<<0)		/* start/stop HC */
+
+	/* USBSTS: offset 0x04 */
+	u32		status;
+#define STS_ASS		(1<<15)		/* Async Schedule Status */
+#define STS_PSS		(1<<14)		/* Periodic Schedule Status */
+#define STS_RECL	(1<<13)		/* Reclamation */
+#define STS_HALT	(1<<12)		/* Not running (any reason) */
+/* some bits reserved */
+	/* these STS_* flags are also intr_enable bits (USBINTR) */
+#define STS_IAA		(1<<5)		/* Interrupted on async advance */
+#define STS_FATAL	(1<<4)		/* such as some PCI access errors */
+#define STS_FLR		(1<<3)		/* frame list rolled over */
+#define STS_PCD		(1<<2)		/* port change detect */
+#define STS_ERR		(1<<1)		/* "error" completion (overflow, ...) */
+#define STS_INT		(1<<0)		/* "normal" completion (short, ...) */
+
+	/* USBINTR: offset 0x08 */
+	u32		intr_enable;
+
+	/* FRINDEX: offset 0x0C */
+	u32		frame_index;	/* current microframe number */
+	/* CTRLDSSEGMENT: offset 0x10 */
+	u32		segment;	/* address bits 63:32 if needed */
+	/* PERIODICLISTBASE: offset 0x14 */
+	u32		frame_list;	/* points to periodic list */
+	/* ASYNCLISTADDR: offset 0x18 */
+	u32		async_next;	/* address of next async queue head */
+
+	u32	reserved1;
+	/* PORTSC: offset 0x20 */
+	u32	port_status;
+/* 31:23 reserved */
+#define PORT_USB11(x) (((x)&(3<<10)) == (1<<10))	/* USB 1.1 device */
+#define PORT_RESET	(1<<8)		/* reset port */
+#define PORT_SUSPEND	(1<<7)		/* suspend port */
+#define PORT_RESUME	(1<<6)		/* resume it */
+#define PORT_PEC	(1<<3)		/* port enable change */
+#define PORT_PE		(1<<2)		/* port enable */
+#define PORT_CSC	(1<<1)		/* connect status change */
+#define PORT_CONNECT	(1<<0)		/* device connected */
+#define PORT_RWC_BITS   (PORT_CSC | PORT_PEC)
+	u32     reserved2[19];
+
+	/* OTGCSR: offet 0x70 */
+	u32     otgcsr;
+#define OTGCSR_HOST_SPD_TYP     (3 << 22)
+#define OTGCSR_A_BUS_DROP	(1 << 5)
+#define OTGCSR_A_BUS_REQ	(1 << 4)
+
+	/* OTGISR: offset 0x74 */
+	u32     otgisr;
+#define OTGISR_OVC	(1 << 10)
+
+	u32     reserved3[15];
+
+	/* GMIR: offset 0xB4 */
+	u32     gmir;
+#define GMIR_INT_POLARITY	(1 << 3) /*Active High*/
+#define GMIR_MHC_INT		(1 << 2)
+#define GMIR_MOTG_INT		(1 << 1)
+#define GMIR_MDEV_INT	(1 << 0)
+};
+
+/*-------------------------------------------------------------------------*/
+
+#define	QTD_NEXT(fotg210, dma)	cpu_to_hc32(fotg210, (u32)dma)
+
+/*
+ * EHCI Specification 0.95 Section 3.5
+ * QTD: describe data transfer components (buffer, direction, ...)
+ * See Fig 3-6 "Queue Element Transfer Descriptor Block Diagram".
+ *
+ * These are associated only with "QH" (Queue Head) structures,
+ * used with control, bulk, and interrupt transfers.
+ */
+struct fotg210_qtd {
+	/* first part defined by EHCI spec */
+	__hc32			hw_next;	/* see EHCI 3.5.1 */
+	__hc32			hw_alt_next;    /* see EHCI 3.5.2 */
+	__hc32			hw_token;	/* see EHCI 3.5.3 */
+#define	QTD_TOGGLE	(1 << 31)	/* data toggle */
+#define	QTD_LENGTH(tok)	(((tok)>>16) & 0x7fff)
+#define	QTD_IOC		(1 << 15)	/* interrupt on complete */
+#define	QTD_CERR(tok)	(((tok)>>10) & 0x3)
+#define	QTD_PID(tok)	(((tok)>>8) & 0x3)
+#define	QTD_STS_ACTIVE	(1 << 7)	/* HC may execute this */
+#define	QTD_STS_HALT	(1 << 6)	/* halted on error */
+#define	QTD_STS_DBE	(1 << 5)	/* data buffer error (in HC) */
+#define	QTD_STS_BABBLE	(1 << 4)	/* device was babbling (qtd halted) */
+#define	QTD_STS_XACT	(1 << 3)	/* device gave illegal response */
+#define	QTD_STS_MMF	(1 << 2)	/* incomplete split transaction */
+#define	QTD_STS_STS	(1 << 1)	/* split transaction state */
+#define	QTD_STS_PING	(1 << 0)	/* issue PING? */
+
+#define ACTIVE_BIT(fotg210)	cpu_to_hc32(fotg210, QTD_STS_ACTIVE)
+#define HALT_BIT(fotg210)		cpu_to_hc32(fotg210, QTD_STS_HALT)
+#define STATUS_BIT(fotg210)	cpu_to_hc32(fotg210, QTD_STS_STS)
+
+	__hc32			hw_buf[5];	/* see EHCI 3.5.4 */
+	__hc32			hw_buf_hi[5];	/* Appendix B */
+
+	/* the rest is HCD-private */
+	dma_addr_t		qtd_dma;		/* qtd address */
+	struct list_head	qtd_list;		/* sw qtd list */
+	struct urb		*urb;			/* qtd's urb */
+	size_t			length;			/* length of buffer */
+} __aligned(32);
+
+/* mask NakCnt+T in qh->hw_alt_next */
+#define QTD_MASK(fotg210)	cpu_to_hc32(fotg210, ~0x1f)
+
+#define IS_SHORT_READ(token) (QTD_LENGTH(token) != 0 && QTD_PID(token) == 1)
+
+/*-------------------------------------------------------------------------*/
+
+/* type tag from {qh,itd,fstn}->hw_next */
+#define Q_NEXT_TYPE(fotg210, dma)	((dma) & cpu_to_hc32(fotg210, 3 << 1))
+
+/*
+ * Now the following defines are not converted using the
+ * cpu_to_le32() macro anymore, since we have to support
+ * "dynamic" switching between be and le support, so that the driver
+ * can be used on one system with SoC EHCI controller using big-endian
+ * descriptors as well as a normal little-endian PCI EHCI controller.
+ */
+/* values for that type tag */
+#define Q_TYPE_ITD	(0 << 1)
+#define Q_TYPE_QH	(1 << 1)
+#define Q_TYPE_SITD	(2 << 1)
+#define Q_TYPE_FSTN	(3 << 1)
+
+/* next async queue entry, or pointer to interrupt/periodic QH */
+#define QH_NEXT(fotg210, dma) \
+	(cpu_to_hc32(fotg210, (((u32)dma)&~0x01f)|Q_TYPE_QH))
+
+/* for periodic/async schedules and qtd lists, mark end of list */
+#define FOTG210_LIST_END(fotg210) \
+	cpu_to_hc32(fotg210, 1) /* "null pointer" to hw */
+
+/*
+ * Entries in periodic shadow table are pointers to one of four kinds
+ * of data structure.  That's dictated by the hardware; a type tag is
+ * encoded in the low bits of the hardware's periodic schedule.  Use
+ * Q_NEXT_TYPE to get the tag.
+ *
+ * For entries in the async schedule, the type tag always says "qh".
+ */
+union fotg210_shadow {
+	struct fotg210_qh	*qh;		/* Q_TYPE_QH */
+	struct fotg210_itd	*itd;		/* Q_TYPE_ITD */
+	struct fotg210_fstn	*fstn;		/* Q_TYPE_FSTN */
+	__hc32			*hw_next;	/* (all types) */
+	void			*ptr;
+};
+
+/*-------------------------------------------------------------------------*/
+
+/*
+ * EHCI Specification 0.95 Section 3.6
+ * QH: describes control/bulk/interrupt endpoints
+ * See Fig 3-7 "Queue Head Structure Layout".
+ *
+ * These appear in both the async and (for interrupt) periodic schedules.
+ */
+
+/* first part defined by EHCI spec */
+struct fotg210_qh_hw {
+	__hc32			hw_next;	/* see EHCI 3.6.1 */
+	__hc32			hw_info1;	/* see EHCI 3.6.2 */
+#define	QH_CONTROL_EP	(1 << 27)	/* FS/LS control endpoint */
+#define	QH_HEAD		(1 << 15)	/* Head of async reclamation list */
+#define	QH_TOGGLE_CTL	(1 << 14)	/* Data toggle control */
+#define	QH_HIGH_SPEED	(2 << 12)	/* Endpoint speed */
+#define	QH_LOW_SPEED	(1 << 12)
+#define	QH_FULL_SPEED	(0 << 12)
+#define	QH_INACTIVATE	(1 << 7)	/* Inactivate on next transaction */
+	__hc32			hw_info2;	/* see EHCI 3.6.2 */
+#define	QH_SMASK	0x000000ff
+#define	QH_CMASK	0x0000ff00
+#define	QH_HUBADDR	0x007f0000
+#define	QH_HUBPORT	0x3f800000
+#define	QH_MULT		0xc0000000
+	__hc32			hw_current;	/* qtd list - see EHCI 3.6.4 */
+
+	/* qtd overlay (hardware parts of a struct fotg210_qtd) */
+	__hc32			hw_qtd_next;
+	__hc32			hw_alt_next;
+	__hc32			hw_token;
+	__hc32			hw_buf[5];
+	__hc32			hw_buf_hi[5];
+} __aligned(32);
+
+struct fotg210_qh {
+	struct fotg210_qh_hw	*hw;		/* Must come first */
+	/* the rest is HCD-private */
+	dma_addr_t		qh_dma;		/* address of qh */
+	union fotg210_shadow	qh_next;	/* ptr to qh; or periodic */
+	struct list_head	qtd_list;	/* sw qtd list */
+	struct list_head	intr_node;	/* list of intr QHs */
+	struct fotg210_qtd	*dummy;
+	struct fotg210_qh	*unlink_next;	/* next on unlink list */
+
+	unsigned		unlink_cycle;
+
+	u8			needs_rescan;	/* Dequeue during giveback */
+	u8			qh_state;
+#define	QH_STATE_LINKED		1		/* HC sees this */
+#define	QH_STATE_UNLINK		2		/* HC may still see this */
+#define	QH_STATE_IDLE		3		/* HC doesn't see this */
+#define	QH_STATE_UNLINK_WAIT	4		/* LINKED and on unlink q */
+#define	QH_STATE_COMPLETING	5		/* don't touch token.HALT */
+
+	u8			xacterrs;	/* XactErr retry counter */
+#define	QH_XACTERR_MAX		32		/* XactErr retry limit */
+
+	/* periodic schedule info */
+	u8			usecs;		/* intr bandwidth */
+	u8			gap_uf;		/* uframes split/csplit gap */
+	u8			c_usecs;	/* ... split completion bw */
+	u16			tt_usecs;	/* tt downstream bandwidth */
+	unsigned short		period;		/* polling interval */
+	unsigned short		start;		/* where polling starts */
+#define NO_FRAME ((unsigned short)~0)			/* pick new start */
+
+	struct usb_device	*dev;		/* access to TT */
+	unsigned		is_out:1;	/* bulk or intr OUT */
+	unsigned		clearing_tt:1;	/* Clear-TT-Buf in progress */
+};
+
+/*-------------------------------------------------------------------------*/
+
+/* description of one iso transaction (up to 3 KB data if highspeed) */
+struct fotg210_iso_packet {
+	/* These will be copied to iTD when scheduling */
+	u64			bufp;		/* itd->hw_bufp{,_hi}[pg] |= */
+	__hc32			transaction;	/* itd->hw_transaction[i] |= */
+	u8			cross;		/* buf crosses pages */
+	/* for full speed OUT splits */
+	u32			buf1;
+};
+
+/* temporary schedule data for packets from iso urbs (both speeds)
+ * each packet is one logical usb transaction to the device (not TT),
+ * beginning at stream->next_uframe
+ */
+struct fotg210_iso_sched {
+	struct list_head	td_list;
+	unsigned		span;
+	struct fotg210_iso_packet	packet[];
+};
+
+/*
+ * fotg210_iso_stream - groups all (s)itds for this endpoint.
+ * acts like a qh would, if EHCI had them for ISO.
+ */
+struct fotg210_iso_stream {
+	/* first field matches fotg210_hq, but is NULL */
+	struct fotg210_qh_hw	*hw;
+
+	u8			bEndpointAddress;
+	u8			highspeed;
+	struct list_head	td_list;	/* queued itds */
+	struct list_head	free_list;	/* list of unused itds */
+	struct usb_device	*udev;
+	struct usb_host_endpoint *ep;
+
+	/* output of (re)scheduling */
+	int			next_uframe;
+	__hc32			splits;
+
+	/* the rest is derived from the endpoint descriptor,
+	 * trusting urb->interval == f(epdesc->bInterval) and
+	 * including the extra info for hw_bufp[0..2]
+	 */
+	u8			usecs, c_usecs;
+	u16			interval;
+	u16			tt_usecs;
+	u16			maxp;
+	u16			raw_mask;
+	unsigned		bandwidth;
+
+	/* This is used to initialize iTD's hw_bufp fields */
+	__hc32			buf0;
+	__hc32			buf1;
+	__hc32			buf2;
+
+	/* this is used to initialize sITD's tt info */
+	__hc32			address;
+};
+
+/*-------------------------------------------------------------------------*/
+
+/*
+ * EHCI Specification 0.95 Section 3.3
+ * Fig 3-4 "Isochronous Transaction Descriptor (iTD)"
+ *
+ * Schedule records for high speed iso xfers
+ */
+struct fotg210_itd {
+	/* first part defined by EHCI spec */
+	__hc32			hw_next;	/* see EHCI 3.3.1 */
+	__hc32			hw_transaction[8]; /* see EHCI 3.3.2 */
+#define FOTG210_ISOC_ACTIVE	(1<<31)	/* activate transfer this slot */
+#define FOTG210_ISOC_BUF_ERR	(1<<30)	/* Data buffer error */
+#define FOTG210_ISOC_BABBLE	(1<<29)	/* babble detected */
+#define FOTG210_ISOC_XACTERR	(1<<28)	/* XactErr - transaction error */
+#define	FOTG210_ITD_LENGTH(tok)	(((tok)>>16) & 0x0fff)
+#define	FOTG210_ITD_IOC		(1 << 15)	/* interrupt on complete */
+
+#define ITD_ACTIVE(fotg210)	cpu_to_hc32(fotg210, FOTG210_ISOC_ACTIVE)
+
+	__hc32			hw_bufp[7];	/* see EHCI 3.3.3 */
+	__hc32			hw_bufp_hi[7];	/* Appendix B */
+
+	/* the rest is HCD-private */
+	dma_addr_t		itd_dma;	/* for this itd */
+	union fotg210_shadow	itd_next;	/* ptr to periodic q entry */
+
+	struct urb		*urb;
+	struct fotg210_iso_stream	*stream;	/* endpoint's queue */
+	struct list_head	itd_list;	/* list of stream's itds */
+
+	/* any/all hw_transactions here may be used by that urb */
+	unsigned		frame;		/* where scheduled */
+	unsigned		pg;
+	unsigned		index[8];	/* in urb->iso_frame_desc */
+} __aligned(32);
+
+/*-------------------------------------------------------------------------*/
+
+/*
+ * EHCI Specification 0.96 Section 3.7
+ * Periodic Frame Span Traversal Node (FSTN)
+ *
+ * Manages split interrupt transactions (using TT) that span frame boundaries
+ * into uframes 0/1; see 4.12.2.2.  In those uframes, a "save place" FSTN
+ * makes the HC jump (back) to a QH to scan for fs/ls QH completions until
+ * it hits a "restore" FSTN; then it returns to finish other uframe 0/1 work.
+ */
+struct fotg210_fstn {
+	__hc32			hw_next;	/* any periodic q entry */
+	__hc32			hw_prev;	/* qh or FOTG210_LIST_END */
+
+	/* the rest is HCD-private */
+	dma_addr_t		fstn_dma;
+	union fotg210_shadow	fstn_next;	/* ptr to periodic q entry */
+} __aligned(32);
+
+/*-------------------------------------------------------------------------*/
+
+/* Prepare the PORTSC wakeup flags during controller suspend/resume */
+
+#define fotg210_prepare_ports_for_controller_suspend(fotg210, do_wakeup) \
+		fotg210_adjust_port_wakeup_flags(fotg210, true, do_wakeup)
+
+#define fotg210_prepare_ports_for_controller_resume(fotg210)		\
+		fotg210_adjust_port_wakeup_flags(fotg210, false, false)
+
+/*-------------------------------------------------------------------------*/
+
+/*
+ * Some EHCI controllers have a Transaction Translator built into the
+ * root hub. This is a non-standard feature.  Each controller will need
+ * to add code to the following inline functions, and call them as
+ * needed (mostly in root hub code).
+ */
+
+static inline unsigned int
+fotg210_get_speed(struct fotg210_hcd *fotg210, unsigned int portsc)
+{
+	return (readl(&fotg210->regs->otgcsr)
+		& OTGCSR_HOST_SPD_TYP) >> 22;
+}
+
+/* Returns the speed of a device attached to a port on the root hub. */
+static inline unsigned int
+fotg210_port_speed(struct fotg210_hcd *fotg210, unsigned int portsc)
+{
+	switch (fotg210_get_speed(fotg210, portsc)) {
+	case 0:
+		return 0;
+	case 1:
+		return USB_PORT_STAT_LOW_SPEED;
+	case 2:
+	default:
+		return USB_PORT_STAT_HIGH_SPEED;
+	}
+}
+
+/*-------------------------------------------------------------------------*/
+
+#define	fotg210_has_fsl_portno_bug(e)		(0)
+
+/*
+ * While most USB host controllers implement their registers in
+ * little-endian format, a minority (celleb companion chip) implement
+ * them in big endian format.
+ *
+ * This attempts to support either format at compile time without a
+ * runtime penalty, or both formats with the additional overhead
+ * of checking a flag bit.
+ *
+ */
+
+#define fotg210_big_endian_mmio(e)	0
+#define fotg210_big_endian_capbase(e)	0
+
+static inline unsigned int fotg210_readl(const struct fotg210_hcd *fotg210,
+		__u32 __iomem *regs)
+{
+	return readl(regs);
+}
+
+static inline void fotg210_writel(const struct fotg210_hcd *fotg210,
+		const unsigned int val, __u32 __iomem *regs)
+{
+	writel(val, regs);
+}
+
+/* cpu to fotg210 */
+static inline __hc32 cpu_to_hc32(const struct fotg210_hcd *fotg210, const u32 x)
+{
+	return cpu_to_le32(x);
+}
+
+/* fotg210 to cpu */
+static inline u32 hc32_to_cpu(const struct fotg210_hcd *fotg210, const __hc32 x)
+{
+	return le32_to_cpu(x);
+}
+
+static inline u32 hc32_to_cpup(const struct fotg210_hcd *fotg210,
+			       const __hc32 *x)
+{
+	return le32_to_cpup(x);
+}
+
+/*-------------------------------------------------------------------------*/
+
+static inline unsigned fotg210_read_frame_index(struct fotg210_hcd *fotg210)
+{
+	return fotg210_readl(fotg210, &fotg210->regs->frame_index);
+}
+
+/*-------------------------------------------------------------------------*/
+
+#endif /* __LINUX_FOTG210_H */
--- /dev/null
+++ b/drivers/usb/fotg210/fotg210-udc.h
@@ -0,0 +1,249 @@
+// SPDX-License-Identifier: GPL-2.0+
+/*
+ * Faraday FOTG210 USB OTG controller
+ *
+ * Copyright (C) 2013 Faraday Technology Corporation
+ * Author: Yuan-Hsin Chen <yhchen@faraday-tech.com>
+ */
+
+#include <linux/kernel.h>
+
+#define FOTG210_MAX_NUM_EP	5 /* ep0...ep4 */
+#define FOTG210_MAX_FIFO_NUM	4 /* fifo0...fifo4 */
+
+/* Global Mask of HC/OTG/DEV interrupt Register(0xC4) */
+#define FOTG210_GMIR		0xC4
+#define GMIR_INT_POLARITY	0x8 /*Active High*/
+#define GMIR_MHC_INT		0x4
+#define GMIR_MOTG_INT		0x2
+#define GMIR_MDEV_INT		0x1
+
+/*  Device Main Control Register(0x100) */
+#define FOTG210_DMCR		0x100
+#define DMCR_HS_EN		(1 << 6)
+#define DMCR_CHIP_EN		(1 << 5)
+#define DMCR_SFRST		(1 << 4)
+#define DMCR_GOSUSP		(1 << 3)
+#define DMCR_GLINT_EN		(1 << 2)
+#define DMCR_HALF_SPEED		(1 << 1)
+#define DMCR_CAP_RMWAKUP	(1 << 0)
+
+/* Device Address Register(0x104) */
+#define FOTG210_DAR		0x104
+#define DAR_AFT_CONF		(1 << 7)
+
+/* Device Test Register(0x108) */
+#define FOTG210_DTR		0x108
+#define DTR_TST_CLRFF		(1 << 0)
+
+/* PHY Test Mode Selector register(0x114) */
+#define FOTG210_PHYTMSR		0x114
+#define PHYTMSR_TST_PKT		(1 << 4)
+#define PHYTMSR_TST_SE0NAK	(1 << 3)
+#define PHYTMSR_TST_KSTA	(1 << 2)
+#define PHYTMSR_TST_JSTA	(1 << 1)
+#define PHYTMSR_UNPLUG		(1 << 0)
+
+/* Cx configuration and FIFO Empty Status register(0x120) */
+#define FOTG210_DCFESR		0x120
+#define DCFESR_FIFO_EMPTY(fifo)	(1 << 8 << (fifo))
+#define DCFESR_CX_EMP		(1 << 5)
+#define DCFESR_CX_CLR		(1 << 3)
+#define DCFESR_CX_STL		(1 << 2)
+#define DCFESR_TST_PKDONE	(1 << 1)
+#define DCFESR_CX_DONE		(1 << 0)
+
+/* Device IDLE Counter Register(0x124) */
+#define FOTG210_DICR		0x124
+
+/* Device Mask of Interrupt Group Register (0x130) */
+#define FOTG210_DMIGR		0x130
+#define DMIGR_MINT_G0		(1 << 0)
+
+/* Device Mask of Interrupt Source Group 0(0x134) */
+#define FOTG210_DMISGR0		0x134
+#define DMISGR0_MCX_COMEND	(1 << 3)
+#define DMISGR0_MCX_OUT_INT	(1 << 2)
+#define DMISGR0_MCX_IN_INT	(1 << 1)
+#define DMISGR0_MCX_SETUP_INT	(1 << 0)
+
+/* Device Mask of Interrupt Source Group 1 Register(0x138)*/
+#define FOTG210_DMISGR1		0x138
+#define DMISGR1_MF3_IN_INT	(1 << 19)
+#define DMISGR1_MF2_IN_INT	(1 << 18)
+#define DMISGR1_MF1_IN_INT	(1 << 17)
+#define DMISGR1_MF0_IN_INT	(1 << 16)
+#define DMISGR1_MF_IN_INT(fifo)	(1 << (16 + (fifo)))
+#define DMISGR1_MF3_SPK_INT	(1 << 7)
+#define DMISGR1_MF3_OUT_INT	(1 << 6)
+#define DMISGR1_MF2_SPK_INT	(1 << 5)
+#define DMISGR1_MF2_OUT_INT	(1 << 4)
+#define DMISGR1_MF1_SPK_INT	(1 << 3)
+#define DMISGR1_MF1_OUT_INT	(1 << 2)
+#define DMISGR1_MF0_SPK_INT	(1 << 1)
+#define DMISGR1_MF0_OUT_INT	(1 << 0)
+#define DMISGR1_MF_OUTSPK_INT(fifo)	(0x3 << (fifo) * 2)
+
+/* Device Mask of Interrupt Source Group 2 Register (0x13C) */
+#define FOTG210_DMISGR2		0x13C
+#define DMISGR2_MDMA_ERROR	(1 << 8)
+#define DMISGR2_MDMA_CMPLT	(1 << 7)
+
+/* Device Interrupt group Register (0x140) */
+#define FOTG210_DIGR		0x140
+#define DIGR_INT_G2		(1 << 2)
+#define DIGR_INT_G1		(1 << 1)
+#define DIGR_INT_G0		(1 << 0)
+
+/* Device Interrupt Source Group 0 Register (0x144) */
+#define FOTG210_DISGR0		0x144
+#define DISGR0_CX_COMABT_INT	(1 << 5)
+#define DISGR0_CX_COMFAIL_INT	(1 << 4)
+#define DISGR0_CX_COMEND_INT	(1 << 3)
+#define DISGR0_CX_OUT_INT	(1 << 2)
+#define DISGR0_CX_IN_INT	(1 << 1)
+#define DISGR0_CX_SETUP_INT	(1 << 0)
+
+/* Device Interrupt Source Group 1 Register (0x148) */
+#define FOTG210_DISGR1		0x148
+#define DISGR1_OUT_INT(fifo)	(1 << ((fifo) * 2))
+#define DISGR1_SPK_INT(fifo)	(1 << 1 << ((fifo) * 2))
+#define DISGR1_IN_INT(fifo)	(1 << 16 << (fifo))
+
+/* Device Interrupt Source Group 2 Register (0x14C) */
+#define FOTG210_DISGR2		0x14C
+#define DISGR2_DMA_ERROR	(1 << 8)
+#define DISGR2_DMA_CMPLT	(1 << 7)
+#define DISGR2_RX0BYTE_INT	(1 << 6)
+#define DISGR2_TX0BYTE_INT	(1 << 5)
+#define DISGR2_ISO_SEQ_ABORT_INT	(1 << 4)
+#define DISGR2_ISO_SEQ_ERR_INT	(1 << 3)
+#define DISGR2_RESM_INT		(1 << 2)
+#define DISGR2_SUSP_INT		(1 << 1)
+#define DISGR2_USBRST_INT	(1 << 0)
+
+/* Device Receive Zero-Length Data Packet Register (0x150)*/
+#define FOTG210_RX0BYTE		0x150
+#define RX0BYTE_EP8		(1 << 7)
+#define RX0BYTE_EP7		(1 << 6)
+#define RX0BYTE_EP6		(1 << 5)
+#define RX0BYTE_EP5		(1 << 4)
+#define RX0BYTE_EP4		(1 << 3)
+#define RX0BYTE_EP3		(1 << 2)
+#define RX0BYTE_EP2		(1 << 1)
+#define RX0BYTE_EP1		(1 << 0)
+
+/* Device Transfer Zero-Length Data Packet Register (0x154)*/
+#define FOTG210_TX0BYTE		0x154
+#define TX0BYTE_EP8		(1 << 7)
+#define TX0BYTE_EP7		(1 << 6)
+#define TX0BYTE_EP6		(1 << 5)
+#define TX0BYTE_EP5		(1 << 4)
+#define TX0BYTE_EP4		(1 << 3)
+#define TX0BYTE_EP3		(1 << 2)
+#define TX0BYTE_EP2		(1 << 1)
+#define TX0BYTE_EP1		(1 << 0)
+
+/* Device IN Endpoint x MaxPacketSize Register(0x160+4*(x-1)) */
+#define FOTG210_INEPMPSR(ep)	(0x160 + 4 * ((ep) - 1))
+#define INOUTEPMPSR_MPS(mps)	((mps) & 0x2FF)
+#define INOUTEPMPSR_STL_EP	(1 << 11)
+#define INOUTEPMPSR_RESET_TSEQ	(1 << 12)
+
+/* Device OUT Endpoint x MaxPacketSize Register(0x180+4*(x-1)) */
+#define FOTG210_OUTEPMPSR(ep)	(0x180 + 4 * ((ep) - 1))
+
+/* Device Endpoint 1~4 Map Register (0x1A0) */
+#define FOTG210_EPMAP		0x1A0
+#define EPMAP_FIFONO(ep, dir)		\
+	((((ep) - 1) << ((ep) - 1) * 8) << ((dir) ? 0 : 4))
+#define EPMAP_FIFONOMSK(ep, dir)	\
+	((3 << ((ep) - 1) * 8) << ((dir) ? 0 : 4))
+
+/* Device FIFO Map Register (0x1A8) */
+#define FOTG210_FIFOMAP		0x1A8
+#define FIFOMAP_DIROUT(fifo)	(0x0 << 4 << (fifo) * 8)
+#define FIFOMAP_DIRIN(fifo)	(0x1 << 4 << (fifo) * 8)
+#define FIFOMAP_BIDIR(fifo)	(0x2 << 4 << (fifo) * 8)
+#define FIFOMAP_NA(fifo)	(0x3 << 4 << (fifo) * 8)
+#define FIFOMAP_EPNO(ep)	((ep) << ((ep) - 1) * 8)
+#define FIFOMAP_EPNOMSK(ep)	(0xF << ((ep) - 1) * 8)
+
+/* Device FIFO Confuguration Register (0x1AC) */
+#define FOTG210_FIFOCF		0x1AC
+#define FIFOCF_TYPE(type, fifo)	((type) << (fifo) * 8)
+#define FIFOCF_BLK_SIN(fifo)	(0x0 << (fifo) * 8 << 2)
+#define FIFOCF_BLK_DUB(fifo)	(0x1 << (fifo) * 8 << 2)
+#define FIFOCF_BLK_TRI(fifo)	(0x2 << (fifo) * 8 << 2)
+#define FIFOCF_BLKSZ_512(fifo)	(0x0 << (fifo) * 8 << 4)
+#define FIFOCF_BLKSZ_1024(fifo)	(0x1 << (fifo) * 8 << 4)
+#define FIFOCF_FIFO_EN(fifo)	(0x1 << (fifo) * 8 << 5)
+
+/* Device FIFO n Instruction and Byte Count Register (0x1B0+4*n) */
+#define FOTG210_FIBCR(fifo)	(0x1B0 + (fifo) * 4)
+#define FIBCR_BCFX		0x7FF
+#define FIBCR_FFRST		(1 << 12)
+
+/* Device DMA Target FIFO Number Register (0x1C0) */
+#define FOTG210_DMATFNR		0x1C0
+#define DMATFNR_ACC_CXF		(1 << 4)
+#define DMATFNR_ACC_F3		(1 << 3)
+#define DMATFNR_ACC_F2		(1 << 2)
+#define DMATFNR_ACC_F1		(1 << 1)
+#define DMATFNR_ACC_F0		(1 << 0)
+#define DMATFNR_ACC_FN(fifo)	(1 << (fifo))
+#define DMATFNR_DISDMA		0
+
+/* Device DMA Controller Parameter setting 1 Register (0x1C8) */
+#define FOTG210_DMACPSR1	0x1C8
+#define DMACPSR1_DMA_LEN(len)	(((len) & 0xFFFF) << 8)
+#define DMACPSR1_DMA_ABORT	(1 << 3)
+#define DMACPSR1_DMA_TYPE(dir_in)	(((dir_in) ? 1 : 0) << 1)
+#define DMACPSR1_DMA_START	(1 << 0)
+
+/* Device DMA Controller Parameter setting 2 Register (0x1CC) */
+#define FOTG210_DMACPSR2	0x1CC
+
+/* Device DMA Controller Parameter setting 3 Register (0x1CC) */
+#define FOTG210_CXPORT		0x1D0
+
+struct fotg210_request {
+	struct usb_request	req;
+	struct list_head	queue;
+};
+
+struct fotg210_ep {
+	struct usb_ep		ep;
+	struct fotg210_udc	*fotg210;
+
+	struct list_head	queue;
+	unsigned		stall:1;
+	unsigned		wedged:1;
+	unsigned		use_dma:1;
+
+	unsigned char		epnum;
+	unsigned char		type;
+	unsigned char		dir_in;
+	unsigned int		maxp;
+	const struct usb_endpoint_descriptor	*desc;
+};
+
+struct fotg210_udc {
+	spinlock_t		lock; /* protect the struct */
+	void __iomem		*reg;
+
+	unsigned long		irq_trigger;
+
+	struct usb_gadget		gadget;
+	struct usb_gadget_driver	*driver;
+
+	struct fotg210_ep	*ep[FOTG210_MAX_NUM_EP];
+
+	struct usb_request	*ep0_req;	/* for internal request */
+	__le16			ep0_data;
+	u8			ep0_dir;	/* 0/0x80  out/in */
+
+	u8			reenum;		/* if re-enumeration */
+};
+
+#define gadget_to_fotg210(g)	container_of((g), struct fotg210_udc, gadget)
--- a/drivers/usb/gadget/udc/fotg210.h
+++ /dev/null
@@ -1,249 +0,0 @@
-// SPDX-License-Identifier: GPL-2.0+
-/*
- * Faraday FOTG210 USB OTG controller
- *
- * Copyright (C) 2013 Faraday Technology Corporation
- * Author: Yuan-Hsin Chen <yhchen@faraday-tech.com>
- */
-
-#include <linux/kernel.h>
-
-#define FOTG210_MAX_NUM_EP	5 /* ep0...ep4 */
-#define FOTG210_MAX_FIFO_NUM	4 /* fifo0...fifo4 */
-
-/* Global Mask of HC/OTG/DEV interrupt Register(0xC4) */
-#define FOTG210_GMIR		0xC4
-#define GMIR_INT_POLARITY	0x8 /*Active High*/
-#define GMIR_MHC_INT		0x4
-#define GMIR_MOTG_INT		0x2
-#define GMIR_MDEV_INT		0x1
-
-/*  Device Main Control Register(0x100) */
-#define FOTG210_DMCR		0x100
-#define DMCR_HS_EN		(1 << 6)
-#define DMCR_CHIP_EN		(1 << 5)
-#define DMCR_SFRST		(1 << 4)
-#define DMCR_GOSUSP		(1 << 3)
-#define DMCR_GLINT_EN		(1 << 2)
-#define DMCR_HALF_SPEED		(1 << 1)
-#define DMCR_CAP_RMWAKUP	(1 << 0)
-
-/* Device Address Register(0x104) */
-#define FOTG210_DAR		0x104
-#define DAR_AFT_CONF		(1 << 7)
-
-/* Device Test Register(0x108) */
-#define FOTG210_DTR		0x108
-#define DTR_TST_CLRFF		(1 << 0)
-
-/* PHY Test Mode Selector register(0x114) */
-#define FOTG210_PHYTMSR		0x114
-#define PHYTMSR_TST_PKT		(1 << 4)
-#define PHYTMSR_TST_SE0NAK	(1 << 3)
-#define PHYTMSR_TST_KSTA	(1 << 2)
-#define PHYTMSR_TST_JSTA	(1 << 1)
-#define PHYTMSR_UNPLUG		(1 << 0)
-
-/* Cx configuration and FIFO Empty Status register(0x120) */
-#define FOTG210_DCFESR		0x120
-#define DCFESR_FIFO_EMPTY(fifo)	(1 << 8 << (fifo))
-#define DCFESR_CX_EMP		(1 << 5)
-#define DCFESR_CX_CLR		(1 << 3)
-#define DCFESR_CX_STL		(1 << 2)
-#define DCFESR_TST_PKDONE	(1 << 1)
-#define DCFESR_CX_DONE		(1 << 0)
-
-/* Device IDLE Counter Register(0x124) */
-#define FOTG210_DICR		0x124
-
-/* Device Mask of Interrupt Group Register (0x130) */
-#define FOTG210_DMIGR		0x130
-#define DMIGR_MINT_G0		(1 << 0)
-
-/* Device Mask of Interrupt Source Group 0(0x134) */
-#define FOTG210_DMISGR0		0x134
-#define DMISGR0_MCX_COMEND	(1 << 3)
-#define DMISGR0_MCX_OUT_INT	(1 << 2)
-#define DMISGR0_MCX_IN_INT	(1 << 1)
-#define DMISGR0_MCX_SETUP_INT	(1 << 0)
-
-/* Device Mask of Interrupt Source Group 1 Register(0x138)*/
-#define FOTG210_DMISGR1		0x138
-#define DMISGR1_MF3_IN_INT	(1 << 19)
-#define DMISGR1_MF2_IN_INT	(1 << 18)
-#define DMISGR1_MF1_IN_INT	(1 << 17)
-#define DMISGR1_MF0_IN_INT	(1 << 16)
-#define DMISGR1_MF_IN_INT(fifo)	(1 << (16 + (fifo)))
-#define DMISGR1_MF3_SPK_INT	(1 << 7)
-#define DMISGR1_MF3_OUT_INT	(1 << 6)
-#define DMISGR1_MF2_SPK_INT	(1 << 5)
-#define DMISGR1_MF2_OUT_INT	(1 << 4)
-#define DMISGR1_MF1_SPK_INT	(1 << 3)
-#define DMISGR1_MF1_OUT_INT	(1 << 2)
-#define DMISGR1_MF0_SPK_INT	(1 << 1)
-#define DMISGR1_MF0_OUT_INT	(1 << 0)
-#define DMISGR1_MF_OUTSPK_INT(fifo)	(0x3 << (fifo) * 2)
-
-/* Device Mask of Interrupt Source Group 2 Register (0x13C) */
-#define FOTG210_DMISGR2		0x13C
-#define DMISGR2_MDMA_ERROR	(1 << 8)
-#define DMISGR2_MDMA_CMPLT	(1 << 7)
-
-/* Device Interrupt group Register (0x140) */
-#define FOTG210_DIGR		0x140
-#define DIGR_INT_G2		(1 << 2)
-#define DIGR_INT_G1		(1 << 1)
-#define DIGR_INT_G0		(1 << 0)
-
-/* Device Interrupt Source Group 0 Register (0x144) */
-#define FOTG210_DISGR0		0x144
-#define DISGR0_CX_COMABT_INT	(1 << 5)
-#define DISGR0_CX_COMFAIL_INT	(1 << 4)
-#define DISGR0_CX_COMEND_INT	(1 << 3)
-#define DISGR0_CX_OUT_INT	(1 << 2)
-#define DISGR0_CX_IN_INT	(1 << 1)
-#define DISGR0_CX_SETUP_INT	(1 << 0)
-
-/* Device Interrupt Source Group 1 Register (0x148) */
-#define FOTG210_DISGR1		0x148
-#define DISGR1_OUT_INT(fifo)	(1 << ((fifo) * 2))
-#define DISGR1_SPK_INT(fifo)	(1 << 1 << ((fifo) * 2))
-#define DISGR1_IN_INT(fifo)	(1 << 16 << (fifo))
-
-/* Device Interrupt Source Group 2 Register (0x14C) */
-#define FOTG210_DISGR2		0x14C
-#define DISGR2_DMA_ERROR	(1 << 8)
-#define DISGR2_DMA_CMPLT	(1 << 7)
-#define DISGR2_RX0BYTE_INT	(1 << 6)
-#define DISGR2_TX0BYTE_INT	(1 << 5)
-#define DISGR2_ISO_SEQ_ABORT_INT	(1 << 4)
-#define DISGR2_ISO_SEQ_ERR_INT	(1 << 3)
-#define DISGR2_RESM_INT		(1 << 2)
-#define DISGR2_SUSP_INT		(1 << 1)
-#define DISGR2_USBRST_INT	(1 << 0)
-
-/* Device Receive Zero-Length Data Packet Register (0x150)*/
-#define FOTG210_RX0BYTE		0x150
-#define RX0BYTE_EP8		(1 << 7)
-#define RX0BYTE_EP7		(1 << 6)
-#define RX0BYTE_EP6		(1 << 5)
-#define RX0BYTE_EP5		(1 << 4)
-#define RX0BYTE_EP4		(1 << 3)
-#define RX0BYTE_EP3		(1 << 2)
-#define RX0BYTE_EP2		(1 << 1)
-#define RX0BYTE_EP1		(1 << 0)
-
-/* Device Transfer Zero-Length Data Packet Register (0x154)*/
-#define FOTG210_TX0BYTE		0x154
-#define TX0BYTE_EP8		(1 << 7)
-#define TX0BYTE_EP7		(1 << 6)
-#define TX0BYTE_EP6		(1 << 5)
-#define TX0BYTE_EP5		(1 << 4)
-#define TX0BYTE_EP4		(1 << 3)
-#define TX0BYTE_EP3		(1 << 2)
-#define TX0BYTE_EP2		(1 << 1)
-#define TX0BYTE_EP1		(1 << 0)
-
-/* Device IN Endpoint x MaxPacketSize Register(0x160+4*(x-1)) */
-#define FOTG210_INEPMPSR(ep)	(0x160 + 4 * ((ep) - 1))
-#define INOUTEPMPSR_MPS(mps)	((mps) & 0x2FF)
-#define INOUTEPMPSR_STL_EP	(1 << 11)
-#define INOUTEPMPSR_RESET_TSEQ	(1 << 12)
-
-/* Device OUT Endpoint x MaxPacketSize Register(0x180+4*(x-1)) */
-#define FOTG210_OUTEPMPSR(ep)	(0x180 + 4 * ((ep) - 1))
-
-/* Device Endpoint 1~4 Map Register (0x1A0) */
-#define FOTG210_EPMAP		0x1A0
-#define EPMAP_FIFONO(ep, dir)		\
-	((((ep) - 1) << ((ep) - 1) * 8) << ((dir) ? 0 : 4))
-#define EPMAP_FIFONOMSK(ep, dir)	\
-	((3 << ((ep) - 1) * 8) << ((dir) ? 0 : 4))
-
-/* Device FIFO Map Register (0x1A8) */
-#define FOTG210_FIFOMAP		0x1A8
-#define FIFOMAP_DIROUT(fifo)	(0x0 << 4 << (fifo) * 8)
-#define FIFOMAP_DIRIN(fifo)	(0x1 << 4 << (fifo) * 8)
-#define FIFOMAP_BIDIR(fifo)	(0x2 << 4 << (fifo) * 8)
-#define FIFOMAP_NA(fifo)	(0x3 << 4 << (fifo) * 8)
-#define FIFOMAP_EPNO(ep)	((ep) << ((ep) - 1) * 8)
-#define FIFOMAP_EPNOMSK(ep)	(0xF << ((ep) - 1) * 8)
-
-/* Device FIFO Confuguration Register (0x1AC) */
-#define FOTG210_FIFOCF		0x1AC
-#define FIFOCF_TYPE(type, fifo)	((type) << (fifo) * 8)
-#define FIFOCF_BLK_SIN(fifo)	(0x0 << (fifo) * 8 << 2)
-#define FIFOCF_BLK_DUB(fifo)	(0x1 << (fifo) * 8 << 2)
-#define FIFOCF_BLK_TRI(fifo)	(0x2 << (fifo) * 8 << 2)
-#define FIFOCF_BLKSZ_512(fifo)	(0x0 << (fifo) * 8 << 4)
-#define FIFOCF_BLKSZ_1024(fifo)	(0x1 << (fifo) * 8 << 4)
-#define FIFOCF_FIFO_EN(fifo)	(0x1 << (fifo) * 8 << 5)
-
-/* Device FIFO n Instruction and Byte Count Register (0x1B0+4*n) */
-#define FOTG210_FIBCR(fifo)	(0x1B0 + (fifo) * 4)
-#define FIBCR_BCFX		0x7FF
-#define FIBCR_FFRST		(1 << 12)
-
-/* Device DMA Target FIFO Number Register (0x1C0) */
-#define FOTG210_DMATFNR		0x1C0
-#define DMATFNR_ACC_CXF		(1 << 4)
-#define DMATFNR_ACC_F3		(1 << 3)
-#define DMATFNR_ACC_F2		(1 << 2)
-#define DMATFNR_ACC_F1		(1 << 1)
-#define DMATFNR_ACC_F0		(1 << 0)
-#define DMATFNR_ACC_FN(fifo)	(1 << (fifo))
-#define DMATFNR_DISDMA		0
-
-/* Device DMA Controller Parameter setting 1 Register (0x1C8) */
-#define FOTG210_DMACPSR1	0x1C8
-#define DMACPSR1_DMA_LEN(len)	(((len) & 0xFFFF) << 8)
-#define DMACPSR1_DMA_ABORT	(1 << 3)
-#define DMACPSR1_DMA_TYPE(dir_in)	(((dir_in) ? 1 : 0) << 1)
-#define DMACPSR1_DMA_START	(1 << 0)
-
-/* Device DMA Controller Parameter setting 2 Register (0x1CC) */
-#define FOTG210_DMACPSR2	0x1CC
-
-/* Device DMA Controller Parameter setting 3 Register (0x1CC) */
-#define FOTG210_CXPORT		0x1D0
-
-struct fotg210_request {
-	struct usb_request	req;
-	struct list_head	queue;
-};
-
-struct fotg210_ep {
-	struct usb_ep		ep;
-	struct fotg210_udc	*fotg210;
-
-	struct list_head	queue;
-	unsigned		stall:1;
-	unsigned		wedged:1;
-	unsigned		use_dma:1;
-
-	unsigned char		epnum;
-	unsigned char		type;
-	unsigned char		dir_in;
-	unsigned int		maxp;
-	const struct usb_endpoint_descriptor	*desc;
-};
-
-struct fotg210_udc {
-	spinlock_t		lock; /* protect the struct */
-	void __iomem		*reg;
-
-	unsigned long		irq_trigger;
-
-	struct usb_gadget		gadget;
-	struct usb_gadget_driver	*driver;
-
-	struct fotg210_ep	*ep[FOTG210_MAX_NUM_EP];
-
-	struct usb_request	*ep0_req;	/* for internal request */
-	__le16			ep0_data;
-	u8			ep0_dir;	/* 0/0x80  out/in */
-
-	u8			reenum;		/* if re-enumeration */
-};
-
-#define gadget_to_fotg210(g)	container_of((g), struct fotg210_udc, gadget)
--- a/drivers/usb/host/fotg210.h
+++ /dev/null
@@ -1,688 +0,0 @@
-/* SPDX-License-Identifier: GPL-2.0 */
-#ifndef __LINUX_FOTG210_H
-#define __LINUX_FOTG210_H
-
-#include <linux/usb/ehci-dbgp.h>
-
-/* definitions used for the EHCI driver */
-
-/*
- * __hc32 and __hc16 are "Host Controller" types, they may be equivalent to
- * __leXX (normally) or __beXX (given FOTG210_BIG_ENDIAN_DESC), depending on
- * the host controller implementation.
- *
- * To facilitate the strongest possible byte-order checking from "sparse"
- * and so on, we use __leXX unless that's not practical.
- */
-#define __hc32	__le32
-#define __hc16	__le16
-
-/* statistics can be kept for tuning/monitoring */
-struct fotg210_stats {
-	/* irq usage */
-	unsigned long		normal;
-	unsigned long		error;
-	unsigned long		iaa;
-	unsigned long		lost_iaa;
-
-	/* termination of urbs from core */
-	unsigned long		complete;
-	unsigned long		unlink;
-};
-
-/* fotg210_hcd->lock guards shared data against other CPUs:
- *   fotg210_hcd:	async, unlink, periodic (and shadow), ...
- *   usb_host_endpoint: hcpriv
- *   fotg210_qh:	qh_next, qtd_list
- *   fotg210_qtd:	qtd_list
- *
- * Also, hold this lock when talking to HC registers or
- * when updating hw_* fields in shared qh/qtd/... structures.
- */
-
-#define	FOTG210_MAX_ROOT_PORTS	1		/* see HCS_N_PORTS */
-
-/*
- * fotg210_rh_state values of FOTG210_RH_RUNNING or above mean that the
- * controller may be doing DMA.  Lower values mean there's no DMA.
- */
-enum fotg210_rh_state {
-	FOTG210_RH_HALTED,
-	FOTG210_RH_SUSPENDED,
-	FOTG210_RH_RUNNING,
-	FOTG210_RH_STOPPING
-};
-
-/*
- * Timer events, ordered by increasing delay length.
- * Always update event_delays_ns[] and event_handlers[] (defined in
- * ehci-timer.c) in parallel with this list.
- */
-enum fotg210_hrtimer_event {
-	FOTG210_HRTIMER_POLL_ASS,	/* Poll for async schedule off */
-	FOTG210_HRTIMER_POLL_PSS,	/* Poll for periodic schedule off */
-	FOTG210_HRTIMER_POLL_DEAD,	/* Wait for dead controller to stop */
-	FOTG210_HRTIMER_UNLINK_INTR,	/* Wait for interrupt QH unlink */
-	FOTG210_HRTIMER_FREE_ITDS,	/* Wait for unused iTDs and siTDs */
-	FOTG210_HRTIMER_ASYNC_UNLINKS,	/* Unlink empty async QHs */
-	FOTG210_HRTIMER_IAA_WATCHDOG,	/* Handle lost IAA interrupts */
-	FOTG210_HRTIMER_DISABLE_PERIODIC, /* Wait to disable periodic sched */
-	FOTG210_HRTIMER_DISABLE_ASYNC,	/* Wait to disable async sched */
-	FOTG210_HRTIMER_IO_WATCHDOG,	/* Check for missing IRQs */
-	FOTG210_HRTIMER_NUM_EVENTS	/* Must come last */
-};
-#define FOTG210_HRTIMER_NO_EVENT	99
-
-struct fotg210_hcd {			/* one per controller */
-	/* timing support */
-	enum fotg210_hrtimer_event	next_hrtimer_event;
-	unsigned		enabled_hrtimer_events;
-	ktime_t			hr_timeouts[FOTG210_HRTIMER_NUM_EVENTS];
-	struct hrtimer		hrtimer;
-
-	int			PSS_poll_count;
-	int			ASS_poll_count;
-	int			died_poll_count;
-
-	/* glue to PCI and HCD framework */
-	struct fotg210_caps __iomem *caps;
-	struct fotg210_regs __iomem *regs;
-	struct ehci_dbg_port __iomem *debug;
-
-	__u32			hcs_params;	/* cached register copy */
-	spinlock_t		lock;
-	enum fotg210_rh_state	rh_state;
-
-	/* general schedule support */
-	bool			scanning:1;
-	bool			need_rescan:1;
-	bool			intr_unlinking:1;
-	bool			async_unlinking:1;
-	bool			shutdown:1;
-	struct fotg210_qh		*qh_scan_next;
-
-	/* async schedule support */
-	struct fotg210_qh		*async;
-	struct fotg210_qh		*dummy;		/* For AMD quirk use */
-	struct fotg210_qh		*async_unlink;
-	struct fotg210_qh		*async_unlink_last;
-	struct fotg210_qh		*async_iaa;
-	unsigned		async_unlink_cycle;
-	unsigned		async_count;	/* async activity count */
-
-	/* periodic schedule support */
-#define	DEFAULT_I_TDPS		1024		/* some HCs can do less */
-	unsigned		periodic_size;
-	__hc32			*periodic;	/* hw periodic table */
-	dma_addr_t		periodic_dma;
-	struct list_head	intr_qh_list;
-	unsigned		i_thresh;	/* uframes HC might cache */
-
-	union fotg210_shadow	*pshadow;	/* mirror hw periodic table */
-	struct fotg210_qh		*intr_unlink;
-	struct fotg210_qh		*intr_unlink_last;
-	unsigned		intr_unlink_cycle;
-	unsigned		now_frame;	/* frame from HC hardware */
-	unsigned		next_frame;	/* scan periodic, start here */
-	unsigned		intr_count;	/* intr activity count */
-	unsigned		isoc_count;	/* isoc activity count */
-	unsigned		periodic_count;	/* periodic activity count */
-	/* max periodic time per uframe */
-	unsigned		uframe_periodic_max;
-
-
-	/* list of itds completed while now_frame was still active */
-	struct list_head	cached_itd_list;
-	struct fotg210_itd	*last_itd_to_free;
-
-	/* per root hub port */
-	unsigned long		reset_done[FOTG210_MAX_ROOT_PORTS];
-
-	/* bit vectors (one bit per port)
-	 * which ports were already suspended at the start of a bus suspend
-	 */
-	unsigned long		bus_suspended;
-
-	/* which ports are edicated to the companion controller */
-	unsigned long		companion_ports;
-
-	/* which ports are owned by the companion during a bus suspend */
-	unsigned long		owned_ports;
-
-	/* which ports have the change-suspend feature turned on */
-	unsigned long		port_c_suspend;
-
-	/* which ports are suspended */
-	unsigned long		suspended_ports;
-
-	/* which ports have started to resume */
-	unsigned long		resuming_ports;
-
-	/* per-HC memory pools (could be per-bus, but ...) */
-	struct dma_pool		*qh_pool;	/* qh per active urb */
-	struct dma_pool		*qtd_pool;	/* one or more per qh */
-	struct dma_pool		*itd_pool;	/* itd per iso urb */
-
-	unsigned		random_frame;
-	unsigned long		next_statechange;
-	ktime_t			last_periodic_enable;
-	u32			command;
-
-	/* SILICON QUIRKS */
-	unsigned		need_io_watchdog:1;
-	unsigned		fs_i_thresh:1;	/* Intel iso scheduling */
-
-	u8			sbrn;		/* packed release number */
-
-	/* irq statistics */
-#ifdef FOTG210_STATS
-	struct fotg210_stats	stats;
-#	define INCR(x) ((x)++)
-#else
-#	define INCR(x) do {} while (0)
-#endif
-
-	/* silicon clock */
-	struct clk		*pclk;
-};
-
-/* convert between an HCD pointer and the corresponding FOTG210_HCD */
-static inline struct fotg210_hcd *hcd_to_fotg210(struct usb_hcd *hcd)
-{
-	return (struct fotg210_hcd *)(hcd->hcd_priv);
-}
-static inline struct usb_hcd *fotg210_to_hcd(struct fotg210_hcd *fotg210)
-{
-	return container_of((void *) fotg210, struct usb_hcd, hcd_priv);
-}
-
-/*-------------------------------------------------------------------------*/
-
-/* EHCI register interface, corresponds to EHCI Revision 0.95 specification */
-
-/* Section 2.2 Host Controller Capability Registers */
-struct fotg210_caps {
-	/* these fields are specified as 8 and 16 bit registers,
-	 * but some hosts can't perform 8 or 16 bit PCI accesses.
-	 * some hosts treat caplength and hciversion as parts of a 32-bit
-	 * register, others treat them as two separate registers, this
-	 * affects the memory map for big endian controllers.
-	 */
-	u32		hc_capbase;
-#define HC_LENGTH(fotg210, p)	(0x00ff&((p) >> /* bits 7:0 / offset 00h */ \
-				(fotg210_big_endian_capbase(fotg210) ? 24 : 0)))
-#define HC_VERSION(fotg210, p)	(0xffff&((p) >> /* bits 31:16 / offset 02h */ \
-				(fotg210_big_endian_capbase(fotg210) ? 0 : 16)))
-	u32		hcs_params;     /* HCSPARAMS - offset 0x4 */
-#define HCS_N_PORTS(p)		(((p)>>0)&0xf)	/* bits 3:0, ports on HC */
-
-	u32		hcc_params;	/* HCCPARAMS - offset 0x8 */
-#define HCC_CANPARK(p)		((p)&(1 << 2))  /* true: can park on async qh */
-#define HCC_PGM_FRAMELISTLEN(p) ((p)&(1 << 1))  /* true: periodic_size changes*/
-	u8		portroute[8];	 /* nibbles for routing - offset 0xC */
-};
-
-
-/* Section 2.3 Host Controller Operational Registers */
-struct fotg210_regs {
-
-	/* USBCMD: offset 0x00 */
-	u32		command;
-
-/* EHCI 1.1 addendum */
-/* 23:16 is r/w intr rate, in microframes; default "8" == 1/msec */
-#define CMD_PARK	(1<<11)		/* enable "park" on async qh */
-#define CMD_PARK_CNT(c)	(((c)>>8)&3)	/* how many transfers to park for */
-#define CMD_IAAD	(1<<6)		/* "doorbell" interrupt async advance */
-#define CMD_ASE		(1<<5)		/* async schedule enable */
-#define CMD_PSE		(1<<4)		/* periodic schedule enable */
-/* 3:2 is periodic frame list size */
-#define CMD_RESET	(1<<1)		/* reset HC not bus */
-#define CMD_RUN		(1<<0)		/* start/stop HC */
-
-	/* USBSTS: offset 0x04 */
-	u32		status;
-#define STS_ASS		(1<<15)		/* Async Schedule Status */
-#define STS_PSS		(1<<14)		/* Periodic Schedule Status */
-#define STS_RECL	(1<<13)		/* Reclamation */
-#define STS_HALT	(1<<12)		/* Not running (any reason) */
-/* some bits reserved */
-	/* these STS_* flags are also intr_enable bits (USBINTR) */
-#define STS_IAA		(1<<5)		/* Interrupted on async advance */
-#define STS_FATAL	(1<<4)		/* such as some PCI access errors */
-#define STS_FLR		(1<<3)		/* frame list rolled over */
-#define STS_PCD		(1<<2)		/* port change detect */
-#define STS_ERR		(1<<1)		/* "error" completion (overflow, ...) */
-#define STS_INT		(1<<0)		/* "normal" completion (short, ...) */
-
-	/* USBINTR: offset 0x08 */
-	u32		intr_enable;
-
-	/* FRINDEX: offset 0x0C */
-	u32		frame_index;	/* current microframe number */
-	/* CTRLDSSEGMENT: offset 0x10 */
-	u32		segment;	/* address bits 63:32 if needed */
-	/* PERIODICLISTBASE: offset 0x14 */
-	u32		frame_list;	/* points to periodic list */
-	/* ASYNCLISTADDR: offset 0x18 */
-	u32		async_next;	/* address of next async queue head */
-
-	u32	reserved1;
-	/* PORTSC: offset 0x20 */
-	u32	port_status;
-/* 31:23 reserved */
-#define PORT_USB11(x) (((x)&(3<<10)) == (1<<10))	/* USB 1.1 device */
-#define PORT_RESET	(1<<8)		/* reset port */
-#define PORT_SUSPEND	(1<<7)		/* suspend port */
-#define PORT_RESUME	(1<<6)		/* resume it */
-#define PORT_PEC	(1<<3)		/* port enable change */
-#define PORT_PE		(1<<2)		/* port enable */
-#define PORT_CSC	(1<<1)		/* connect status change */
-#define PORT_CONNECT	(1<<0)		/* device connected */
-#define PORT_RWC_BITS   (PORT_CSC | PORT_PEC)
-	u32     reserved2[19];
-
-	/* OTGCSR: offet 0x70 */
-	u32     otgcsr;
-#define OTGCSR_HOST_SPD_TYP     (3 << 22)
-#define OTGCSR_A_BUS_DROP	(1 << 5)
-#define OTGCSR_A_BUS_REQ	(1 << 4)
-
-	/* OTGISR: offset 0x74 */
-	u32     otgisr;
-#define OTGISR_OVC	(1 << 10)
-
-	u32     reserved3[15];
-
-	/* GMIR: offset 0xB4 */
-	u32     gmir;
-#define GMIR_INT_POLARITY	(1 << 3) /*Active High*/
-#define GMIR_MHC_INT		(1 << 2)
-#define GMIR_MOTG_INT		(1 << 1)
-#define GMIR_MDEV_INT	(1 << 0)
-};
-
-/*-------------------------------------------------------------------------*/
-
-#define	QTD_NEXT(fotg210, dma)	cpu_to_hc32(fotg210, (u32)dma)
-
-/*
- * EHCI Specification 0.95 Section 3.5
- * QTD: describe data transfer components (buffer, direction, ...)
- * See Fig 3-6 "Queue Element Transfer Descriptor Block Diagram".
- *
- * These are associated only with "QH" (Queue Head) structures,
- * used with control, bulk, and interrupt transfers.
- */
-struct fotg210_qtd {
-	/* first part defined by EHCI spec */
-	__hc32			hw_next;	/* see EHCI 3.5.1 */
-	__hc32			hw_alt_next;    /* see EHCI 3.5.2 */
-	__hc32			hw_token;	/* see EHCI 3.5.3 */
-#define	QTD_TOGGLE	(1 << 31)	/* data toggle */
-#define	QTD_LENGTH(tok)	(((tok)>>16) & 0x7fff)
-#define	QTD_IOC		(1 << 15)	/* interrupt on complete */
-#define	QTD_CERR(tok)	(((tok)>>10) & 0x3)
-#define	QTD_PID(tok)	(((tok)>>8) & 0x3)
-#define	QTD_STS_ACTIVE	(1 << 7)	/* HC may execute this */
-#define	QTD_STS_HALT	(1 << 6)	/* halted on error */
-#define	QTD_STS_DBE	(1 << 5)	/* data buffer error (in HC) */
-#define	QTD_STS_BABBLE	(1 << 4)	/* device was babbling (qtd halted) */
-#define	QTD_STS_XACT	(1 << 3)	/* device gave illegal response */
-#define	QTD_STS_MMF	(1 << 2)	/* incomplete split transaction */
-#define	QTD_STS_STS	(1 << 1)	/* split transaction state */
-#define	QTD_STS_PING	(1 << 0)	/* issue PING? */
-
-#define ACTIVE_BIT(fotg210)	cpu_to_hc32(fotg210, QTD_STS_ACTIVE)
-#define HALT_BIT(fotg210)		cpu_to_hc32(fotg210, QTD_STS_HALT)
-#define STATUS_BIT(fotg210)	cpu_to_hc32(fotg210, QTD_STS_STS)
-
-	__hc32			hw_buf[5];	/* see EHCI 3.5.4 */
-	__hc32			hw_buf_hi[5];	/* Appendix B */
-
-	/* the rest is HCD-private */
-	dma_addr_t		qtd_dma;		/* qtd address */
-	struct list_head	qtd_list;		/* sw qtd list */
-	struct urb		*urb;			/* qtd's urb */
-	size_t			length;			/* length of buffer */
-} __aligned(32);
-
-/* mask NakCnt+T in qh->hw_alt_next */
-#define QTD_MASK(fotg210)	cpu_to_hc32(fotg210, ~0x1f)
-
-#define IS_SHORT_READ(token) (QTD_LENGTH(token) != 0 && QTD_PID(token) == 1)
-
-/*-------------------------------------------------------------------------*/
-
-/* type tag from {qh,itd,fstn}->hw_next */
-#define Q_NEXT_TYPE(fotg210, dma)	((dma) & cpu_to_hc32(fotg210, 3 << 1))
-
-/*
- * Now the following defines are not converted using the
- * cpu_to_le32() macro anymore, since we have to support
- * "dynamic" switching between be and le support, so that the driver
- * can be used on one system with SoC EHCI controller using big-endian
- * descriptors as well as a normal little-endian PCI EHCI controller.
- */
-/* values for that type tag */
-#define Q_TYPE_ITD	(0 << 1)
-#define Q_TYPE_QH	(1 << 1)
-#define Q_TYPE_SITD	(2 << 1)
-#define Q_TYPE_FSTN	(3 << 1)
-
-/* next async queue entry, or pointer to interrupt/periodic QH */
-#define QH_NEXT(fotg210, dma) \
-	(cpu_to_hc32(fotg210, (((u32)dma)&~0x01f)|Q_TYPE_QH))
-
-/* for periodic/async schedules and qtd lists, mark end of list */
-#define FOTG210_LIST_END(fotg210) \
-	cpu_to_hc32(fotg210, 1) /* "null pointer" to hw */
-
-/*
- * Entries in periodic shadow table are pointers to one of four kinds
- * of data structure.  That's dictated by the hardware; a type tag is
- * encoded in the low bits of the hardware's periodic schedule.  Use
- * Q_NEXT_TYPE to get the tag.
- *
- * For entries in the async schedule, the type tag always says "qh".
- */
-union fotg210_shadow {
-	struct fotg210_qh	*qh;		/* Q_TYPE_QH */
-	struct fotg210_itd	*itd;		/* Q_TYPE_ITD */
-	struct fotg210_fstn	*fstn;		/* Q_TYPE_FSTN */
-	__hc32			*hw_next;	/* (all types) */
-	void			*ptr;
-};
-
-/*-------------------------------------------------------------------------*/
-
-/*
- * EHCI Specification 0.95 Section 3.6
- * QH: describes control/bulk/interrupt endpoints
- * See Fig 3-7 "Queue Head Structure Layout".
- *
- * These appear in both the async and (for interrupt) periodic schedules.
- */
-
-/* first part defined by EHCI spec */
-struct fotg210_qh_hw {
-	__hc32			hw_next;	/* see EHCI 3.6.1 */
-	__hc32			hw_info1;	/* see EHCI 3.6.2 */
-#define	QH_CONTROL_EP	(1 << 27)	/* FS/LS control endpoint */
-#define	QH_HEAD		(1 << 15)	/* Head of async reclamation list */
-#define	QH_TOGGLE_CTL	(1 << 14)	/* Data toggle control */
-#define	QH_HIGH_SPEED	(2 << 12)	/* Endpoint speed */
-#define	QH_LOW_SPEED	(1 << 12)
-#define	QH_FULL_SPEED	(0 << 12)
-#define	QH_INACTIVATE	(1 << 7)	/* Inactivate on next transaction */
-	__hc32			hw_info2;	/* see EHCI 3.6.2 */
-#define	QH_SMASK	0x000000ff
-#define	QH_CMASK	0x0000ff00
-#define	QH_HUBADDR	0x007f0000
-#define	QH_HUBPORT	0x3f800000
-#define	QH_MULT		0xc0000000
-	__hc32			hw_current;	/* qtd list - see EHCI 3.6.4 */
-
-	/* qtd overlay (hardware parts of a struct fotg210_qtd) */
-	__hc32			hw_qtd_next;
-	__hc32			hw_alt_next;
-	__hc32			hw_token;
-	__hc32			hw_buf[5];
-	__hc32			hw_buf_hi[5];
-} __aligned(32);
-
-struct fotg210_qh {
-	struct fotg210_qh_hw	*hw;		/* Must come first */
-	/* the rest is HCD-private */
-	dma_addr_t		qh_dma;		/* address of qh */
-	union fotg210_shadow	qh_next;	/* ptr to qh; or periodic */
-	struct list_head	qtd_list;	/* sw qtd list */
-	struct list_head	intr_node;	/* list of intr QHs */
-	struct fotg210_qtd	*dummy;
-	struct fotg210_qh	*unlink_next;	/* next on unlink list */
-
-	unsigned		unlink_cycle;
-
-	u8			needs_rescan;	/* Dequeue during giveback */
-	u8			qh_state;
-#define	QH_STATE_LINKED		1		/* HC sees this */
-#define	QH_STATE_UNLINK		2		/* HC may still see this */
-#define	QH_STATE_IDLE		3		/* HC doesn't see this */
-#define	QH_STATE_UNLINK_WAIT	4		/* LINKED and on unlink q */
-#define	QH_STATE_COMPLETING	5		/* don't touch token.HALT */
-
-	u8			xacterrs;	/* XactErr retry counter */
-#define	QH_XACTERR_MAX		32		/* XactErr retry limit */
-
-	/* periodic schedule info */
-	u8			usecs;		/* intr bandwidth */
-	u8			gap_uf;		/* uframes split/csplit gap */
-	u8			c_usecs;	/* ... split completion bw */
-	u16			tt_usecs;	/* tt downstream bandwidth */
-	unsigned short		period;		/* polling interval */
-	unsigned short		start;		/* where polling starts */
-#define NO_FRAME ((unsigned short)~0)			/* pick new start */
-
-	struct usb_device	*dev;		/* access to TT */
-	unsigned		is_out:1;	/* bulk or intr OUT */
-	unsigned		clearing_tt:1;	/* Clear-TT-Buf in progress */
-};
-
-/*-------------------------------------------------------------------------*/
-
-/* description of one iso transaction (up to 3 KB data if highspeed) */
-struct fotg210_iso_packet {
-	/* These will be copied to iTD when scheduling */
-	u64			bufp;		/* itd->hw_bufp{,_hi}[pg] |= */
-	__hc32			transaction;	/* itd->hw_transaction[i] |= */
-	u8			cross;		/* buf crosses pages */
-	/* for full speed OUT splits */
-	u32			buf1;
-};
-
-/* temporary schedule data for packets from iso urbs (both speeds)
- * each packet is one logical usb transaction to the device (not TT),
- * beginning at stream->next_uframe
- */
-struct fotg210_iso_sched {
-	struct list_head	td_list;
-	unsigned		span;
-	struct fotg210_iso_packet	packet[];
-};
-
-/*
- * fotg210_iso_stream - groups all (s)itds for this endpoint.
- * acts like a qh would, if EHCI had them for ISO.
- */
-struct fotg210_iso_stream {
-	/* first field matches fotg210_hq, but is NULL */
-	struct fotg210_qh_hw	*hw;
-
-	u8			bEndpointAddress;
-	u8			highspeed;
-	struct list_head	td_list;	/* queued itds */
-	struct list_head	free_list;	/* list of unused itds */
-	struct usb_device	*udev;
-	struct usb_host_endpoint *ep;
-
-	/* output of (re)scheduling */
-	int			next_uframe;
-	__hc32			splits;
-
-	/* the rest is derived from the endpoint descriptor,
-	 * trusting urb->interval == f(epdesc->bInterval) and
-	 * including the extra info for hw_bufp[0..2]
-	 */
-	u8			usecs, c_usecs;
-	u16			interval;
-	u16			tt_usecs;
-	u16			maxp;
-	u16			raw_mask;
-	unsigned		bandwidth;
-
-	/* This is used to initialize iTD's hw_bufp fields */
-	__hc32			buf0;
-	__hc32			buf1;
-	__hc32			buf2;
-
-	/* this is used to initialize sITD's tt info */
-	__hc32			address;
-};
-
-/*-------------------------------------------------------------------------*/
-
-/*
- * EHCI Specification 0.95 Section 3.3
- * Fig 3-4 "Isochronous Transaction Descriptor (iTD)"
- *
- * Schedule records for high speed iso xfers
- */
-struct fotg210_itd {
-	/* first part defined by EHCI spec */
-	__hc32			hw_next;	/* see EHCI 3.3.1 */
-	__hc32			hw_transaction[8]; /* see EHCI 3.3.2 */
-#define FOTG210_ISOC_ACTIVE	(1<<31)	/* activate transfer this slot */
-#define FOTG210_ISOC_BUF_ERR	(1<<30)	/* Data buffer error */
-#define FOTG210_ISOC_BABBLE	(1<<29)	/* babble detected */
-#define FOTG210_ISOC_XACTERR	(1<<28)	/* XactErr - transaction error */
-#define	FOTG210_ITD_LENGTH(tok)	(((tok)>>16) & 0x0fff)
-#define	FOTG210_ITD_IOC		(1 << 15)	/* interrupt on complete */
-
-#define ITD_ACTIVE(fotg210)	cpu_to_hc32(fotg210, FOTG210_ISOC_ACTIVE)
-
-	__hc32			hw_bufp[7];	/* see EHCI 3.3.3 */
-	__hc32			hw_bufp_hi[7];	/* Appendix B */
-
-	/* the rest is HCD-private */
-	dma_addr_t		itd_dma;	/* for this itd */
-	union fotg210_shadow	itd_next;	/* ptr to periodic q entry */
-
-	struct urb		*urb;
-	struct fotg210_iso_stream	*stream;	/* endpoint's queue */
-	struct list_head	itd_list;	/* list of stream's itds */
-
-	/* any/all hw_transactions here may be used by that urb */
-	unsigned		frame;		/* where scheduled */
-	unsigned		pg;
-	unsigned		index[8];	/* in urb->iso_frame_desc */
-} __aligned(32);
-
-/*-------------------------------------------------------------------------*/
-
-/*
- * EHCI Specification 0.96 Section 3.7
- * Periodic Frame Span Traversal Node (FSTN)
- *
- * Manages split interrupt transactions (using TT) that span frame boundaries
- * into uframes 0/1; see 4.12.2.2.  In those uframes, a "save place" FSTN
- * makes the HC jump (back) to a QH to scan for fs/ls QH completions until
- * it hits a "restore" FSTN; then it returns to finish other uframe 0/1 work.
- */
-struct fotg210_fstn {
-	__hc32			hw_next;	/* any periodic q entry */
-	__hc32			hw_prev;	/* qh or FOTG210_LIST_END */
-
-	/* the rest is HCD-private */
-	dma_addr_t		fstn_dma;
-	union fotg210_shadow	fstn_next;	/* ptr to periodic q entry */
-} __aligned(32);
-
-/*-------------------------------------------------------------------------*/
-
-/* Prepare the PORTSC wakeup flags during controller suspend/resume */
-
-#define fotg210_prepare_ports_for_controller_suspend(fotg210, do_wakeup) \
-		fotg210_adjust_port_wakeup_flags(fotg210, true, do_wakeup)
-
-#define fotg210_prepare_ports_for_controller_resume(fotg210)		\
-		fotg210_adjust_port_wakeup_flags(fotg210, false, false)
-
-/*-------------------------------------------------------------------------*/
-
-/*
- * Some EHCI controllers have a Transaction Translator built into the
- * root hub. This is a non-standard feature.  Each controller will need
- * to add code to the following inline functions, and call them as
- * needed (mostly in root hub code).
- */
-
-static inline unsigned int
-fotg210_get_speed(struct fotg210_hcd *fotg210, unsigned int portsc)
-{
-	return (readl(&fotg210->regs->otgcsr)
-		& OTGCSR_HOST_SPD_TYP) >> 22;
-}
-
-/* Returns the speed of a device attached to a port on the root hub. */
-static inline unsigned int
-fotg210_port_speed(struct fotg210_hcd *fotg210, unsigned int portsc)
-{
-	switch (fotg210_get_speed(fotg210, portsc)) {
-	case 0:
-		return 0;
-	case 1:
-		return USB_PORT_STAT_LOW_SPEED;
-	case 2:
-	default:
-		return USB_PORT_STAT_HIGH_SPEED;
-	}
-}
-
-/*-------------------------------------------------------------------------*/
-
-#define	fotg210_has_fsl_portno_bug(e)		(0)
-
-/*
- * While most USB host controllers implement their registers in
- * little-endian format, a minority (celleb companion chip) implement
- * them in big endian format.
- *
- * This attempts to support either format at compile time without a
- * runtime penalty, or both formats with the additional overhead
- * of checking a flag bit.
- *
- */
-
-#define fotg210_big_endian_mmio(e)	0
-#define fotg210_big_endian_capbase(e)	0
-
-static inline unsigned int fotg210_readl(const struct fotg210_hcd *fotg210,
-		__u32 __iomem *regs)
-{
-	return readl(regs);
-}
-
-static inline void fotg210_writel(const struct fotg210_hcd *fotg210,
-		const unsigned int val, __u32 __iomem *regs)
-{
-	writel(val, regs);
-}
-
-/* cpu to fotg210 */
-static inline __hc32 cpu_to_hc32(const struct fotg210_hcd *fotg210, const u32 x)
-{
-	return cpu_to_le32(x);
-}
-
-/* fotg210 to cpu */
-static inline u32 hc32_to_cpu(const struct fotg210_hcd *fotg210, const __hc32 x)
-{
-	return le32_to_cpu(x);
-}
-
-static inline u32 hc32_to_cpup(const struct fotg210_hcd *fotg210,
-			       const __hc32 *x)
-{
-	return le32_to_cpup(x);
-}
-
-/*-------------------------------------------------------------------------*/
-
-static inline unsigned fotg210_read_frame_index(struct fotg210_hcd *fotg210)
-{
-	return fotg210_readl(fotg210, &fotg210->regs->frame_index);
-}
-
-/*-------------------------------------------------------------------------*/
-
-#endif /* __LINUX_FOTG210_H */
