// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "dlink,dap-x1860-a1", "mediatek,mt7621-soc";
	model = "D-Link DAP-X1860 A1";

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	aliases {
		label-mac-device = &gmac0;
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_red;
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power_green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		led_power_red: power_red {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
		};

		power_orange {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_ORANGE>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		rssihigh {
			label = "green:rssihigh";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		rssimedium {
			label = "green:rssimedium";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
		};

		rssilow_orange {
			label = "orange:rssilow";
			gpios = <&gpio 26 GPIO_ACTIVE_LOW>;
		};

		rssilow_green {
			label = "green:rssilow";
			gpios = <&gpio 27 GPIO_ACTIVE_LOW>;
		};
	};

	virtual_flash {
		compatible = "mtd-concat";

		devices = <&fwconcat0 &fwconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "ubi";
				reg = <0x0 0x0>;
			};
		};
	};
};

&nand {
	status = "okay";

	mediatek,nmbm;
	/* rsvd = Remapping Range / NAND Erase-Size */
	/* rsvd = 0x800000 / 0x20000 */
	mediatek,bmt-max-reserved-blocks = <64>;
	/* Remapping should include raw-nand we operate upon without UBI layer. */
	/* This includes (at least) the kernel which has to be loaded by U-Boot.*/
	mediatek,bmt-remap-range =
		<0x0 0x980000>;

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "bootloader";
			reg = <0x0 0x80000>;
			read-only;
		};

		partition@80000 {
			label = "config";
			reg = <0x80000 0x80000>;
			read-only;
		};

		partition@100000 {
			label = "factory";
			reg = <0x100000 0x80000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				eeprom_factory_0: eeprom@0 {
					reg = <0x0 0xe00>;
				};

				macaddr_factory_4: macaddr@4 {
					reg = <0x4 0x6>;
				};

				precal_factory_e10: precal@e10 {
					reg = <0xe10 0x19c10>;
				};
			};
		};

		partition@180000 {
			label = "kernel";
			reg = <0x180000 0x0800000>;
		};

		fwconcat0: partition@980000 {
			label = "fwconcat0";
			reg = <0x980000 0x2c00000>;
		};

		partition@3580000 {
			label = "manufacture";
			reg = <0x3580000 0x400000>;
			read-only;
		};

		partition@3980000 {
			label = "storage";
			reg = <0x3980000 0x680000>;
			read-only;
		};

		fwconcat1: partition@4000000 {
			label = "fwconcat1";
			reg = <0x4000000 0x3800000>;
		};
	};
};

&pcie {
	status = "okay";
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_0>, <&precal_factory_e10>;
		nvmem-cell-names = "eeprom", "precal";
		mediatek,disable-radar-background;
	};
};

&ethernet {
	pinctrl-0 = <&mdio_pins>, <&rgmii1_pins>;
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_4>;
	nvmem-cell-names = "mac-address";
};

&switch0 {
	gpio-controller;
	#gpio-cells = <2>;

	ports {
		port@0 {
			status = "okay";
			label = "lan";
		};
	};
};

&state_default {
	gpio {
		groups = "uart2";
		function = "gpio";
	};
};
