From 96cf10a8e7297065459473c081a6fb6432a22312 Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Sun, 26 Sep 2021 00:59:25 +0200
Subject: [PATCH 02/11] net: dsa: rtl8366: Drop custom VLAN set-up
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This hacky default VLAN setup was done in order to direct
packets to the right ports and provide port isolation, both
which we now support properly using custom tags and proper
bridge port isolation.

We can drop the custom VLAN code and leave all VLAN handling
alone, as users expect things to be. We can also drop
ds->configure_vlan_while_not_filtering = false; and let
the core deal with any VLANs it wants.

Cc: Mauri Sandberg <sandberg@mailfence.com>
Cc: DENG Qingfang <dqfext@gmail.com>
Reviewed-by: Vladimir Oltean <olteanv@gmail.com>
Reviewed-by: Alvin Šipraga <alsi@bang-olufsen.dk>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/dsa/realtek-smi-core.h |  1 -
 drivers/net/dsa/rtl8366.c          | 48 ------------------------------
 drivers/net/dsa/rtl8366rb.c        |  4 +--
 3 files changed, 1 insertion(+), 52 deletions(-)

--- a/drivers/net/dsa/realtek-smi-core.h
+++ b/drivers/net/dsa/realtek-smi-core.h
@@ -129,7 +129,6 @@ int rtl8366_set_pvid(struct realtek_smi
 int rtl8366_enable_vlan4k(struct realtek_smi *smi, bool enable);
 int rtl8366_enable_vlan(struct realtek_smi *smi, bool enable);
 int rtl8366_reset_vlan(struct realtek_smi *smi);
-int rtl8366_init_vlan(struct realtek_smi *smi);
 int rtl8366_vlan_filtering(struct dsa_switch *ds, int port, bool vlan_filtering,
 			   struct netlink_ext_ack *extack);
 int rtl8366_vlan_add(struct dsa_switch *ds, int port,
--- a/drivers/net/dsa/rtl8366.c
+++ b/drivers/net/dsa/rtl8366.c
@@ -292,54 +292,6 @@ int rtl8366_reset_vlan(struct realtek_sm
 }
 EXPORT_SYMBOL_GPL(rtl8366_reset_vlan);
 
-int rtl8366_init_vlan(struct realtek_smi *smi)
-{
-	int port;
-	int ret;
-
-	ret = rtl8366_reset_vlan(smi);
-	if (ret)
-		return ret;
-
-	/* Loop over the available ports, for each port, associate
-	 * it with the VLAN (port+1)
-	 */
-	for (port = 0; port < smi->num_ports; port++) {
-		u32 mask;
-
-		if (port == smi->cpu_port)
-			/* For the CPU port, make all ports members of this
-			 * VLAN.
-			 */
-			mask = GENMASK((int)smi->num_ports - 1, 0);
-		else
-			/* For all other ports, enable itself plus the
-			 * CPU port.
-			 */
-			mask = BIT(port) | BIT(smi->cpu_port);
-
-		/* For each port, set the port as member of VLAN (port+1)
-		 * and untagged, except for the CPU port: the CPU port (5) is
-		 * member of VLAN 6 and so are ALL the other ports as well.
-		 * Use filter 0 (no filter).
-		 */
-		dev_info(smi->dev, "VLAN%d port mask for port %d, %08x\n",
-			 (port + 1), port, mask);
-		ret = rtl8366_set_vlan(smi, (port + 1), mask, mask, 0);
-		if (ret)
-			return ret;
-
-		dev_info(smi->dev, "VLAN%d port %d, PVID set to %d\n",
-			 (port + 1), port, (port + 1));
-		ret = rtl8366_set_pvid(smi, port, (port + 1));
-		if (ret)
-			return ret;
-	}
-
-	return rtl8366_enable_vlan(smi, true);
-}
-EXPORT_SYMBOL_GPL(rtl8366_init_vlan);
-
 int rtl8366_vlan_filtering(struct dsa_switch *ds, int port, bool vlan_filtering,
 			   struct netlink_ext_ack *extack)
 {
--- a/drivers/net/dsa/rtl8366rb.c
+++ b/drivers/net/dsa/rtl8366rb.c
@@ -985,7 +985,7 @@ static int rtl8366rb_setup(struct dsa_sw
 			return ret;
 	}
 
-	ret = rtl8366_init_vlan(smi);
+	ret = rtl8366_reset_vlan(smi);
 	if (ret)
 		return ret;
 
@@ -999,8 +999,6 @@ static int rtl8366rb_setup(struct dsa_sw
 		return -ENODEV;
 	}
 
-	ds->configure_vlan_while_not_filtering = false;
-
 	return 0;
 }
 
