From 3684d32820cdf7f9ca10a1cfd6236bfcaaf1c6bd Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Tue, 19 May 2020 11:46:47 +0100
Subject: [PATCH] media: bcm2835-unicam: Retain packing information on
 G_FMT

The change to retrieve the pixel format always on g_fmt didn't
check whether the native or unpacked version of the format
had been requested, and always returned the packed one.
Correct this so that the packing setting is retained whereever
possible.

Fixes "9d59e89 media: bcm2835-unicam: Re-fetch mbus code from subdev
on a g_fmt call"

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 .../media/platform/bcm2835/bcm2835-unicam.c   | 19 +++++++++++++++++--
 1 file changed, 17 insertions(+), 2 deletions(-)

--- a/drivers/media/platform/bcm2835/bcm2835-unicam.c
+++ b/drivers/media/platform/bcm2835/bcm2835-unicam.c
@@ -982,8 +982,23 @@ static int unicam_g_fmt_vid_cap(struct f
 	if (!fmt)
 		return -EINVAL;
 
-	node->fmt = fmt;
-	node->v_fmt.fmt.pix.pixelformat = fmt->fourcc;
+	if (node->fmt != fmt) {
+		/*
+		 * The sensor format has changed so the pixelformat needs to
+		 * be updated. Try and retain the packed/unpacked choice if
+		 * at all possible.
+		 */
+		if (node->fmt->repacked_fourcc ==
+						node->v_fmt.fmt.pix.pixelformat)
+			/* Using the repacked format */
+			node->v_fmt.fmt.pix.pixelformat = fmt->repacked_fourcc;
+		else
+			/* Using the native format */
+			node->v_fmt.fmt.pix.pixelformat = fmt->fourcc;
+
+		node->fmt = fmt;
+	}
+
 	*f = node->v_fmt;
 
 	return 0;
