From 2b8634d1468ff498cc91b6adf993c27ae6fa079d Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Fri, 26 May 2023 22:48:01 +0200
Subject: [PATCH] cpufreq: qcom-nvmem: use SoC ID-s from bindings

SMEM SoC ID-s are now stored in DT bindings so lets use those instead of
defining them in the driver again.

Signed-off-by: Robert Marko <robimarko@gmail.com>
Reviewed-by: Konrad Dybcio <konrad.dybcio@linaro.org>
Reviewed-by: Bjorn Andersson <bjorn.andersson@linaro.org>
Acked-by: Viresh Kumar <viresh.kumar@linaro.org>
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
Link: https://lore.kernel.org/r/20230526204802.3081168-4-robimarko@gmail.com
---
 drivers/cpufreq/qcom-cpufreq-nvmem.c | 15 +++++----------
 1 file changed, 5 insertions(+), 10 deletions(-)

--- a/drivers/cpufreq/qcom-cpufreq-nvmem.c
+++ b/drivers/cpufreq/qcom-cpufreq-nvmem.c
@@ -31,12 +31,7 @@
 
 #define MSM_ID_SMEM	137
 
-enum _msm_id {
-	MSM8996V3 = 0xF6ul,
-	APQ8096V3 = 0x123ul,
-	MSM8996SG = 0x131ul,
-	APQ8096SG = 0x138ul,
-};
+#include <dt-bindings/arm/qcom,ids.h>
 
 enum _msm8996_version {
 	MSM8996_V3,
@@ -154,12 +149,12 @@ static enum _msm8996_version qcom_cpufre
 	msm_id++;
 
 	switch ((enum _msm_id)*msm_id) {
-	case MSM8996V3:
-	case APQ8096V3:
+	case QCOM_ID_MSM8996:
+	case QCOM_ID_APQ8096:
 		version = MSM8996_V3;
 		break;
-	case MSM8996SG:
-	case APQ8096SG:
+	case QCOM_ID_MSM8996SG:
+	case QCOM_ID_APQ8096SG:
 		version = MSM8996_SG;
 		break;
 	default:
