From 56d3067cb694ba60d654e7f5ef231b6fabc4697f Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Wed, 7 Jun 2023 20:44:48 +0200
Subject: [PATCH] arm64: dts: qcom: ipq8074: add critical thermal trips

According to bindings, thermal zones must have associated trips as well.
Since we currently dont have CPUFreq support and thus no passive cooling
lets start by defining critical trips to protect the devices against
severe overheating.

Signed-off-by: Robert Marko <robimarko@gmail.com>
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
Link: https://lore.kernel.org/r/20230607184448.2512179-1-robimarko@gmail.com
---
 arch/arm64/boot/dts/qcom/ipq8074.dtsi | 96 +++++++++++++++++++++++++++
 1 file changed, 96 insertions(+)

--- a/arch/arm64/boot/dts/qcom/ipq8074.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq8074.dtsi
@@ -899,6 +899,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 4>;
+
+			trips {
+				nss-top-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 
 		nss0-thermal {
@@ -906,6 +914,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 5>;
+
+			trips {
+				nss-0-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 
 		nss1-thermal {
@@ -913,6 +929,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 6>;
+
+			trips {
+				nss-1-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 
 		wcss-phya0-thermal {
@@ -920,6 +944,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 7>;
+
+			trips {
+				wcss-phya0-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 
 		wcss-phya1-thermal {
@@ -927,6 +959,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 8>;
+
+			trips {
+				wcss-phya1-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 
 		cpu0_thermal: cpu0-thermal {
@@ -934,6 +974,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 9>;
+
+			trips {
+				cpu0-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 
 		cpu1_thermal: cpu1-thermal {
@@ -941,6 +989,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 10>;
+
+			trips {
+				cpu1-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 
 		cpu2_thermal: cpu2-thermal {
@@ -948,6 +1004,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 11>;
+
+			trips {
+				cpu2-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 
 		cpu3_thermal: cpu3-thermal {
@@ -955,6 +1019,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 12>;
+
+			trips {
+				cpu3-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 
 		cluster_thermal: cluster-thermal {
@@ -962,6 +1034,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 13>;
+
+			trips {
+				cluster-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 
 		wcss-phyb0-thermal {
@@ -969,6 +1049,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 14>;
+
+			trips {
+				wcss-phyb0-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 
 		wcss-phyb1-thermal {
@@ -976,6 +1064,14 @@
 			polling-delay = <1000>;
 
 			thermal-sensors = <&tsens 15>;
+
+			trips {
+				wcss-phyb1-crit {
+					temperature = <110000>;
+					hysteresis = <1000>;
+					type = "critical";
+				};
+			};
 		};
 	};
 };
