// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "vr9.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/mips/lantiq_rcu_gphy.h>

/ {
	compatible = "avm,fritz7430", "lantiq,xway", "lantiq,vr9";
	model = "AVM FRITZ!Box 7430";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_info_red;
		led-running = &led_power;
		led-upgrade = &led_info_green;

		led-dsl = &led_info_green;
		led-wifi = &led_wifi;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x8000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		dect {
			label = "dect";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_PHONE>;
		};

		wifi {
			label = "wifi";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 31 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};

		led_info_green: info_green {
			label = "green:info";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		led_info_red: info_red {
			label = "red:info";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		led_wifi: wifi {
			label = "green:wifi";
			gpios = <&gpio 34 GPIO_ACTIVE_LOW>;
		};

		dect {
			label = "green:dect";
			gpios = <&gpio 35 GPIO_ACTIVE_LOW>;
		};

		fon {
			label = "green:fon";
			gpios = <&gpio 36 GPIO_ACTIVE_LOW>;
		};
	};

	usb0_vbus: regulator-usb0-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB0_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpio = <&gpio 5 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&localbus {
	flash@0 {
		compatible = "lantiq,nand-xway";
		bank-width = <2>;
		reg = <0 0x0 0x8000000>;
		lantiq,cs = <1>;

		pinctrl-0 = <&nand_pins>, <&nand_cs1_pins>;
		pinctrl-names = "default";

		nand-use-soft-ecc-engine;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "urlader";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "nand-tffs";
				reg = <0x40000 0x400000>;
				read-only;
			};

			partition@440000 {
				label = "kernel";
				reg = <0x440000 0x400000>;
			};

			partition@840000 {
				label = "ubi";
				reg = <0x840000 0x3000000>;
			};

			partition@3840000 {
				label = "reserved-kernel";
				reg = <0x3840000 0x400000>;
				read-only;
			};

			partition@3c40000 {
				label = "reserved-filesystem";
				reg = <0x3c40000 0x3000000>;
				read-only;
			};

			partition@6c40000 {
				label = "config";
				reg = <0x6c40000 0x200000>;
				read-only;
			};

			partition@6e40000 {
				label = "nand-filesystem";
				reg = <0x6e40000 0x11c0000>;
				read-only;
			};
		};
	};
};

&pcie0 {
	status = "okay";

	gpio-reset = <&gpio 11 GPIO_ACTIVE_LOW>;

	pcie@0 {
		reg = <0 0 0 0 0>;
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		device_type = "pci";

		wifi@168c,abcd {
			compatible = "pci168c,abcd";
			reg = <0 0 0 0 0>;
			qca,no-eeprom; /* load from ath9k-eeprom-pci-0000:01:00.0.bin */
		};
	};
};

&gphy0 {
	lantiq,gphy-mode = <GPHY_MODE_FE>;
};

&gphy1 {
	lantiq,gphy-mode = <GPHY_MODE_FE>;
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		pcie-rst {
			lantiq,pins = "io11";
			lantiq,open-drain = <1>;
			lantiq,output = <1>;
		};
	};
};

&gswip_mdio {
	phy11: ethernet-phy@11 {
		reg = <0x11>;
	};
	phy12: ethernet-phy@12 {
		reg = <0x12>;
	};
	phy13: ethernet-phy@13 {
		reg = <0x13>;
	};
	phy14: ethernet-phy@14 {
		reg = <0x14>;
	};
};

&gswip_ports {
	port@2 {
		reg = <2>;
		label = "lan3";
		phy-mode = "internal";
		phy-handle = <&phy11>;
	};
	port@3 {
		reg = <3>;
		label = "lan4";
		phy-mode = "internal";
		phy-handle = <&phy12>;
	};
	port@4 {
		reg = <4>;
		label = "lan1";
		phy-mode = "internal";
		phy-handle = <&phy13>;
	};
	port@5 {
		reg = <5>;
		label = "lan2";
		phy-mode = "internal";
		phy-handle = <&phy14>;
	};
};

&usb_phy0 {
	status = "okay";
};

&usb0 {
	status = "okay";

	vbus-supply = <&usb0_vbus>;
};
