// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "tplink,ex220-v1", "mediatek,mt7621-soc";
	model = "TP-Link EX220 v1";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		label-mac-device = &gmac0;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	keys {
		compatible = "gpio-keys";

		button-wps {
			label = "rfkill";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};

		button-reset {
			label = "reset";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led-wps {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WPS;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		led-lan {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		led-wan-orange {
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_WAN;
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		led-wan-green {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WAN;
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		led-wifi5g {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <5>;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		led-wifi2g {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <2>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led_power: led-power {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_POWER;
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "boot";
				reg = <0x00 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "config";
				reg = <0x50000 0x10000>;
				read-only;
			};

			partition@60000 {
				label = "isp_config";
				reg = <0x60000 0x10000>;
				read-only;
			};

			partition@70000 {
				label = "rom_file";
				reg = <0x70000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_rom_file_f100: macaddr@f100 {
						compatible = "mac-base";
						reg = <0xf100 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@80000 {
				label = "cloud";
				reg = <0x80000 0x10000>;
				read-only;
			};

			partition@90000 {
				label = "radio";
				reg = <0x90000 0x20000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					eeprom_radio_0: eeprom@0 {
						reg = <0x0 0xe00>;
					};

					precal_radio_e10: precal@e10 {
						reg = <0xe10 0x19c10>;
					};
				};
			};

			partition@b0000 {
				label = "config_bak";
				reg = <0xb0000 0x10000>;
				read-only;
			};

			partition@c0000 {
				compatible = "denx,fit";
				label = "firmware";
				reg = <0xc0000 0xf30000>;
			};
		};
	};
};

&pcie {
	status = "okay";
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_radio_0>, <&precal_radio_e10>, <&macaddr_rom_file_f100 0>;
		nvmem-cell-names = "eeprom", "precal", "mac-address";
		mediatek,disable-radar-background;
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_rom_file_f100 0>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy4>;

	nvmem-cells = <&macaddr_rom_file_f100 1>;
	nvmem-cell-names = "mac-address";
};

&mdio {
	ethphy4: ethernet-phy@4 {
		reg = <4>;
	};
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "lan1";
		};

		port@1 {
			status = "okay";
			label = "lan2";
		};

		port@2 {
			status = "okay";
			label = "lan3";
		};

		port@3 {
			status = "okay";
			label = "lan4";
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "uart3", "jtag", "wdt";
		function = "gpio";
	};
};
