From 8857b0ab6a562c473c5bded0efda9390b82a84d4 Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Tue, 27 Sep 2022 22:12:17 +0200
Subject: [PATCH] arm64: dts: qcom: ipq6018: fix NAND node name

Per schema it should be nand-controller@79b0000 instead of nand@79b0000.
Fix it to match nand-controller.yaml requirements.

Signed-off-by: Robert Marko <robimarko@gmail.com>
Reviewed-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Reviewed-by: Neil Armstrong <neil.armstrong@linaro.org>
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
Link: https://lore.kernel.org/r/20220927201218.1264506-1-robimarko@gmail.com
---
 arch/arm64/boot/dts/qcom/ipq6018.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/qcom/ipq6018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq6018.dtsi
@@ -348,7 +348,7 @@
 			status = "disabled";
 		};
 
-		qpic_nand: nand@79b0000 {
+		qpic_nand: nand-controller@79b0000 {
 			compatible = "qcom,ipq6018-nand";
 			reg = <0x0 0x079b0000 0x0 0x10000>;
 			#address-cells = <1>;
