From 04f6ec35cbb9794bb185f58d15c7d8f326374618 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Mon, 21 Nov 2022 13:33:37 +0100
Subject: [PATCH] drm/tests: helpers: Switch to a platform_device
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The device managed resources are ran if the device has bus, which is not
the case of a root_device.

Let's use a platform_device instead.

Reviewed-by: Javier Martinez Canillas <javierm@redhat.com>
Reviewed-by: Maíra Canal <mcanal@igalia.com>
Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 drivers/gpu/drm/tests/drm_kunit_helpers.c | 16 ++++++++++++++--
 1 file changed, 14 insertions(+), 2 deletions(-)

--- a/drivers/gpu/drm/tests/drm_kunit_helpers.c
+++ b/drivers/gpu/drm/tests/drm_kunit_helpers.c
@@ -7,6 +7,7 @@
 #include <kunit/resource.h>
 
 #include <linux/device.h>
+#include <linux/platform_device.h>
 
 #define KUNIT_DEVICE_NAME	"drm-kunit-mock-device"
 
@@ -32,7 +33,16 @@ static const struct drm_mode_config_func
  */
 struct device *drm_kunit_helper_alloc_device(struct kunit *test)
 {
-	return root_device_register(KUNIT_DEVICE_NAME);
+	struct platform_device *pdev;
+	int ret;
+
+	pdev = platform_device_alloc(KUNIT_DEVICE_NAME, PLATFORM_DEVID_NONE);
+	KUNIT_ASSERT_NOT_ERR_OR_NULL(test, pdev);
+
+	ret = platform_device_add(pdev);
+	KUNIT_ASSERT_EQ(test, ret, 0);
+
+	return &pdev->dev;
 }
 EXPORT_SYMBOL_GPL(drm_kunit_helper_alloc_device);
 
@@ -45,7 +55,9 @@ EXPORT_SYMBOL_GPL(drm_kunit_helper_alloc
  */
 void drm_kunit_helper_free_device(struct kunit *test, struct device *dev)
 {
-	root_device_unregister(dev);
+	struct platform_device *pdev = to_platform_device(dev);
+
+	platform_device_unregister(pdev);
 }
 EXPORT_SYMBOL_GPL(drm_kunit_helper_free_device);
 
