// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "wavlink,wl-wn573hx1", "mediatek,mt7621-soc";
	model = "WAVLINK WL-WN573HX1";

	aliases {
		led-boot = &led_status_blue;
		led-failsafe = &led_status_blue;
		led-running = &led_status_blue;
		led-upgrade = &led_status_blue;
		label-mac-device = &gmac0;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_status_blue:status_led {
			label = "blue:status_led";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_3fff4>;
	nvmem-cell-names = "mac-address";
};

&mdio {
	ethphy4: ethernet-phy@4 {
		reg = <4>;
	};
};

&pcie {
	status = "okay";
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_0>, <&precal_factory_e10>;
		nvmem-cell-names = "eeprom", "precal";
	};
};

&spi0 {
	status = "okay";
	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <14000000>;
		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x00000 0x30000>;
			};

			partition@30000 {
				label = "config";
				reg = <0x30000 0x10000>;
			};

			partition@50000 {
				label = "factory";
				reg = <0x50000 0x40000>;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					eeprom_factory_0: eeprom@0 {
						reg = <0x0 0xe00>;
					};

					precal_factory_e10: precal@e10 {
						reg = <0xe10 0x19c10>;
					};

					macaddr_factory_3fff4: macaddr@3fff4 {
						reg = <0x3fff4 0x6>;
					};
				};
			};

			partition@90000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x90000 0xf70000>;
			};
		};
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_3fff4>;
	nvmem-cell-names = "mac-address";
};

&mdio {
	ethphy4: ethernet-phy@4 {
		reg = <4>;
	};
};

&switch0 {
	ports {
		port@3 {
			status = "okay";
			label = "lan";
		};
	};
};
