From 038ba1dc4e54d51d953f5618d8eb5dd39bd9de25 Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Tue, 13 Feb 2024 14:35:51 +0100
Subject: [PATCH] net: phy: aquantia: add AQR111 and AQR111B0 PHY ID

Add Aquantia AQR111 and AQR111B0 PHY ID. These PHY advertise 10G speed
but actually supports up to 5G speed, hence some manual fixup is needed.

The Aquantia AQR111B0 PHY is just a variant of the AQR111 with smaller
chip size.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Link: https://lore.kernel.org/r/20240213133558.1836-1-ansuelsmth@gmail.com
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---
 drivers/net/phy/aquantia/aquantia_main.c | 52 ++++++++++++++++++++++++
 1 file changed, 52 insertions(+)

--- a/drivers/net/phy/aquantia/aquantia_main.c
+++ b/drivers/net/phy/aquantia/aquantia_main.c
@@ -22,6 +22,8 @@
 #define PHY_ID_AQR107	0x03a1b4e0
 #define PHY_ID_AQCS109	0x03a1b5c2
 #define PHY_ID_AQR405	0x03a1b4b0
+#define PHY_ID_AQR111	0x03a1b610
+#define PHY_ID_AQR111B0	0x03a1b612
 #define PHY_ID_AQR113C	0x31c31c12
 
 #define MDIO_PHYXS_VEND_IF_STATUS		0xe812
@@ -672,6 +674,16 @@ static int aqr107_probe(struct phy_devic
 	return aqr_hwmon_probe(phydev);
 }
 
+static int aqr111_config_init(struct phy_device *phydev)
+{
+	/* AQR111 reports supporting speed up to 10G,
+	 * however only speeds up to 5G are supported.
+	 */
+	phy_set_max_speed(phydev, SPEED_5000);
+
+	return aqr107_config_init(phydev);
+}
+
 static struct phy_driver aqr_driver[] = {
 {
 	PHY_ID_MATCH_MODEL(PHY_ID_AQ1202),
@@ -746,6 +758,42 @@ static struct phy_driver aqr_driver[] =
 	.link_change_notify = aqr107_link_change_notify,
 },
 {
+	PHY_ID_MATCH_MODEL(PHY_ID_AQR111),
+	.name		= "Aquantia AQR111",
+	.probe		= aqr107_probe,
+	.config_init	= aqr111_config_init,
+	.config_aneg    = aqr_config_aneg,
+	.config_intr	= aqr_config_intr,
+	.handle_interrupt = aqr_handle_interrupt,
+	.read_status	= aqr107_read_status,
+	.get_tunable    = aqr107_get_tunable,
+	.set_tunable    = aqr107_set_tunable,
+	.suspend	= aqr107_suspend,
+	.resume		= aqr107_resume,
+	.get_sset_count	= aqr107_get_sset_count,
+	.get_strings	= aqr107_get_strings,
+	.get_stats	= aqr107_get_stats,
+	.link_change_notify = aqr107_link_change_notify,
+},
+{
+	PHY_ID_MATCH_MODEL(PHY_ID_AQR111B0),
+	.name		= "Aquantia AQR111B0",
+	.probe		= aqr107_probe,
+	.config_init	= aqr111_config_init,
+	.config_aneg    = aqr_config_aneg,
+	.config_intr	= aqr_config_intr,
+	.handle_interrupt = aqr_handle_interrupt,
+	.read_status	= aqr107_read_status,
+	.get_tunable    = aqr107_get_tunable,
+	.set_tunable    = aqr107_set_tunable,
+	.suspend	= aqr107_suspend,
+	.resume		= aqr107_resume,
+	.get_sset_count	= aqr107_get_sset_count,
+	.get_strings	= aqr107_get_strings,
+	.get_stats	= aqr107_get_stats,
+	.link_change_notify = aqr107_link_change_notify,
+},
+{
 	PHY_ID_MATCH_MODEL(PHY_ID_AQR405),
 	.name		= "Aquantia AQR405",
 	.config_aneg    = aqr_config_aneg,
@@ -784,6 +832,8 @@ static struct mdio_device_id __maybe_unu
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR107) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQCS109) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR405) },
+	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR111) },
+	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR111B0) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR113C) },
 	{ }
 };
