// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "bcm6328.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "ADB P.DG A4101N A-000-1A1-AE";
	compatible = "adb,pdg-a4101n-a-000-1a1-ae", "brcm,bcm6328";

	aliases {
		led-boot = &led_dsl_green;
		led-failsafe = &led_dsl_green;
		led-upgrade = &led_dsl_green;
	};

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		wifi {
			label = "wifi";
			gpios = <&pinctrl 12 1>;
			linux,code = <KEY_WLAN>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&pinctrl 23 1>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			gpios = <&pinctrl 24 1>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led@31 {
			label = "green:tel";
			gpios = <&pinctrl 31 1>;
		};
	};
};

&leds {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_leds>;

	led_dsl_green: led@3 {
		reg = <3>;
		active-low;
		label = "green:dsl";
	};

	led@9 {
		reg = <9>;
		active-low;
		function = LED_FUNCTION_WPS;
		color = <LED_COLOR_ID_GREEN>;
	};

	led@10 {
		reg = <10>;
		active-low;
		function = LED_FUNCTION_USB;
		color = <LED_COLOR_ID_GREEN>;
	};

	led@11 {
		reg = <11>;
		active-low;
		label = "green:internet";
	};
};

&hsspi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <16666667>;
		spi-tx-bus-width = <2>;
		spi-rx-bus-width = <2>;
		reg = <0>;

		#address-cells = <1>;
		#size-cells = <1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				reg = <0x000000 0x010000>;
				label = "cfe";
				read-only;
			};

			partition@10000 {
				reg = <0x010000 0xff0000>;
				label = "linux";
				compatible = "brcm,bcm963xx-imagetag";
			};
		};
	};
};

&pinctrl {
	pinctrl_leds: leds {
		function = "led";
		pins = "gpio3", "gpio9", "gpio10",
		       "gpio11";
	};

	green_internet_switch {
		gpio-hog;
		gpios = <2 1>;
		output-low;
		line-name = "green:internet-switch";
	};
};

&uart0 {
	status = "okay";
};
