From d387e34fec407f881fdf165b5d7ec128ebff362f Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Tue, 19 Sep 2023 14:47:20 +0200
Subject: [PATCH] net: sfp: add quirk for Fiberstone GPON-ONU-34-20BI

Fiberstone GPON-ONU-34-20B can operate at 2500base-X, but report 1.2GBd
NRZ in their EEPROM.

The module also require the ignore tx fault fixup similar to Huawei MA5671A
as it gets disabled on error messages with serial redirection enabled.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
Link: https://lore.kernel.org/r/20230919124720.8210-1-ansuelsmth@gmail.com
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---
 drivers/net/phy/sfp.c | 5 +++++
 1 file changed, 5 insertions(+)

--- a/drivers/net/phy/sfp.c
+++ b/drivers/net/phy/sfp.c
@@ -393,6 +393,11 @@ static const struct sfp_quirk sfp_quirks
 	SFP_QUIRK("ALCATELLUCENT", "3FE46541AA", sfp_quirk_2500basex,
 		  sfp_fixup_long_startup),
 
+	// Fiberstore GPON-ONU-34-20BI can operate at 2500base-X, but report 1.2GBd
+	// NRZ in their EEPROM
+	SFP_QUIRK("FS", "GPON-ONU-34-20BI", sfp_quirk_2500basex,
+		  sfp_fixup_ignore_tx_fault),
+
 	SFP_QUIRK_F("HALNy", "HL-GSFP", sfp_fixup_halny_gsfp),
 
 	// HG MXPD-483II-F 2.5G supports 2500Base-X, but incorrectly reports
