From 1fbe96ec05c41b313b4e7cc4b39b191b4a3f7540 Mon Sep 17 00:00:00 2001
From: Samuel Holland <samuel@sholland.org>
Date: Sat, 7 May 2022 18:38:34 -0500
Subject: [PATCH 012/117] irqchip/sifive-plic: Enable oneshot-safe threaded
 EOIs

Signed-off-by: Samuel Holland <samuel@sholland.org>
---
 drivers/irqchip/irq-sifive-plic.c | 4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

--- a/drivers/irqchip/irq-sifive-plic.c
+++ b/drivers/irqchip/irq-sifive-plic.c
@@ -201,7 +201,9 @@ static struct irq_chip plic_chip = {
 	.irq_set_affinity = plic_set_affinity,
 #endif
 	.irq_set_type	= plic_irq_set_type,
-	.flags		= IRQCHIP_AFFINITY_PRE_STARTUP,
+	.flags		= IRQCHIP_ONESHOT_SAFE |
+			  IRQCHIP_EOI_THREADED |
+			  IRQCHIP_AFFINITY_PRE_STARTUP,
 };
 
 static int plic_irq_set_type(struct irq_data *d, unsigned int type)
