This prevents the options from being delete with make kernel_oldconfig.
---
 drivers/ssb/Kconfig |    2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/bcma/Kconfig
+++ b/drivers/bcma/Kconfig
@@ -36,6 +36,7 @@ config BCMA_HOST_PCI
 config BCMA_HOST_SOC
 	bool "Support for BCMA in a SoC"
 	depends on HAS_IOMEM
+	select USB_HCD_BCMA if USB_EHCI_HCD || USB_OHCI_HCD
 	help
 	  Host interface for a Broadcom AIX bus directly mapped into
 	  the memory. This only works with the Broadcom SoCs from the
--- a/drivers/ssb/Kconfig
+++ b/drivers/ssb/Kconfig
@@ -141,6 +141,7 @@ config SSB_SFLASH
 config SSB_EMBEDDED
 	bool
 	depends on SSB_DRIVER_MIPS && SSB_PCICORE_HOSTMODE
+	select USB_HCD_SSB if USB_EHCI_HCD || USB_OHCI_HCD
 	default y
 
 config SSB_DRIVER_EXTIF
