// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/mtd/partitions/uimage.h>

/ {
	compatible = "dlink,covr-p2500-a1", "qca,qca9563";
	model = "D-Link COVR-P2500 A1";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_red;
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins>;

		lan {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};

		led_power_green: power_green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan5g {
			label = "green:wlan5g";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0radio";
		};

		led_power_red: power_red {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "green:wlan2g";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1radio";
		};
	};

	virtual_flash {
		compatible = "mtd-concat";

		devices = <&fwconcat0 &fwconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				compatible = "openwrt,uimage", "denx,uimage";
				openwrt,ih-magic = <0x68737173>;
				label = "firmware";
				reg = <0x0 0x0>;
			};
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x40000 0x10000>;
				read-only;
			};

			fwconcat0: partition@50000 {
				label = "fwconcat0";
				reg = <0x50000 0xe30000>;
			};

			partition@e80000 {
				label = "loader";
				reg = <0xe80000 0x10000>;
				read-only;
			};

			fwconcat1: partition@e90000 {
				label = "fwconcat1";
				reg = <0xe90000 0x160000>;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					calibration_ath9k: calibration@1000 {
						reg = <0x1000 0x440>;
					};

					precalibration_ath10k: pre-calibration@5000 {
						reg = <0x5000 0x2f20>;
					};
				};
			};
		};
	};
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0 0 0 0 0>;

		nvmem-cells = <&precalibration_ath10k>;
		nvmem-cell-names = "pre-calibration";
	};
};

&gpio {
	phy-reset {
		gpio-hog;
		gpios = <11 GPIO_ACTIVE_LOW>;
		output-low;
		line-name = "phy-reset";
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "sgmii";
		qca,mib-poll-interval = <500>;

		qca,ar8327-initvals = <
			0x04 0x00080080 /* PORT0 PAD MODE CTRL */
			0x10 0x81000080 /* POWER_ON_STRAP */
			0x50 0xcc35cc35 /* LED_CTRL0 */
			0x54 0xcb37cb37 /* LED_CTRL1 */
			0x58 0x00000000 /* LED_CTRL2 */
			0x5c 0x00f3cf00 /* LED_CTRL3 */
			0x7c 0x0000007e /* PORT0_STATUS */
			>;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x03000101 0x00000101 0x00001919>;

	phy-mode = "sgmii";
	phy-handle = <&phy0>;
};

&wmac {
	status = "okay";

	nvmem-cells = <&calibration_ath9k>;
	nvmem-cell-names = "calibration";
};
