From 9e8e24ab716098e617195ce29b88e84608bf2108 Mon Sep 17 00:00:00 2001
From: Sam Shih <sam.shih@mediatek.com>
Date: Fri, 6 Jan 2023 16:28:42 +0100
Subject: [PATCH 07/19] arm64: dts: mt7986: add usb related device nodes

This patch adds USB support for MT7986.

Signed-off-by: Sam Shih <sam.shih@mediatek.com>
Signed-off-by: Frank Wunderlich <frank-w@public-files.de>
Reviewed-by: Chunfeng Yun <chunfeng.yun@mediatek.com>
Link: https://lore.kernel.org/r/20230106152845.88717-3-linux@fw-web.de
Signed-off-by: Matthias Brugger <matthias.bgg@gmail.com>
---
 arch/arm64/boot/dts/mediatek/mt7986a-rfb.dts |  8 +++
 arch/arm64/boot/dts/mediatek/mt7986a.dtsi    | 55 ++++++++++++++++++++
 arch/arm64/boot/dts/mediatek/mt7986b-rfb.dts |  8 +++
 3 files changed, 71 insertions(+)

--- a/arch/arm64/boot/dts/mediatek/mt7986a-rfb.dts
+++ b/arch/arm64/boot/dts/mediatek/mt7986a-rfb.dts
@@ -140,6 +140,10 @@
 	status = "okay";
 };
 
+&ssusb {
+	status = "okay";
+};
+
 &switch {
 	ports {
 		#address-cells = <1>;
@@ -201,6 +205,10 @@
 	status = "okay";
 };
 
+&usb_phy {
+	status = "okay";
+};
+
 &wifi {
 	status = "okay";
 	pinctrl-names = "default", "dbdc";
--- a/arch/arm64/boot/dts/mediatek/mt7986a.dtsi
+++ b/arch/arm64/boot/dts/mediatek/mt7986a.dtsi
@@ -322,6 +322,61 @@
 			status = "disabled";
 		};
 
+		ssusb: usb@11200000 {
+			compatible = "mediatek,mt7986-xhci",
+				     "mediatek,mtk-xhci";
+			reg = <0 0x11200000 0 0x2e00>,
+			      <0 0x11203e00 0 0x0100>;
+			reg-names = "mac", "ippc";
+			interrupts = <GIC_SPI 173 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&infracfg CLK_INFRA_IUSB_SYS_CK>,
+				 <&infracfg CLK_INFRA_IUSB_CK>,
+				 <&infracfg CLK_INFRA_IUSB_133_CK>,
+				 <&infracfg CLK_INFRA_IUSB_66M_CK>,
+				 <&topckgen CLK_TOP_U2U3_XHCI_SEL>;
+			clock-names = "sys_ck",
+				      "ref_ck",
+				      "mcu_ck",
+				      "dma_ck",
+				      "xhci_ck";
+			phys = <&u2port0 PHY_TYPE_USB2>,
+			       <&u3port0 PHY_TYPE_USB3>,
+			       <&u2port1 PHY_TYPE_USB2>;
+			status = "disabled";
+		};
+
+		usb_phy: t-phy@11e10000 {
+			compatible = "mediatek,mt7986-tphy",
+				     "mediatek,generic-tphy-v2";
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0 0 0x11e10000 0x1700>;
+			status = "disabled";
+
+			u2port0: usb-phy@0 {
+				reg = <0x0 0x700>;
+				clocks = <&topckgen CLK_TOP_DA_U2_REFSEL>,
+					 <&topckgen CLK_TOP_DA_U2_CK_1P_SEL>;
+				clock-names = "ref", "da_ref";
+				#phy-cells = <1>;
+			};
+
+			u3port0: usb-phy@700 {
+				reg = <0x700 0x900>;
+				clocks = <&topckgen CLK_TOP_USB3_PHY_SEL>;
+				clock-names = "ref";
+				#phy-cells = <1>;
+			};
+
+			u2port1: usb-phy@1000 {
+				reg = <0x1000 0x700>;
+				clocks = <&topckgen CLK_TOP_DA_U2_REFSEL>,
+					 <&topckgen CLK_TOP_DA_U2_CK_1P_SEL>;
+				clock-names = "ref", "da_ref";
+				#phy-cells = <1>;
+			};
+		};
+
 		ethsys: syscon@15000000 {
 			 #address-cells = <1>;
 			 #size-cells = <1>;
--- a/arch/arm64/boot/dts/mediatek/mt7986b-rfb.dts
+++ b/arch/arm64/boot/dts/mediatek/mt7986b-rfb.dts
@@ -167,10 +167,18 @@
 	status = "okay";
 };
 
+&ssusb {
+	status = "okay";
+};
+
 &uart0 {
 	status = "okay";
 };
 
+&usb_phy {
+	status = "okay";
+};
+
 &wifi {
 	status = "okay";
 	pinctrl-names = "default", "dbdc";
