From 4973056cceacc70966396039fae99867dfafd796 Mon Sep 17 00:00:00 2001
From: Sean Anderson <sean.anderson@seco.com>
Date: Fri, 22 Oct 2021 18:41:04 -0400
Subject: [PATCH] net: convert users of bitmap_foo() to linkmode_foo()

This converts instances of
	bitmap_foo(args..., __ETHTOOL_LINK_MODE_MASK_NBITS)
to
	linkmode_foo(args...)

I manually fixed up some lines to prevent them from being excessively
long. Otherwise, this change was generated with the following semantic
patch:

// Generated with
// echo linux/linkmode.h > includes
// git grep -Flf includes include/ | cut -f 2- -d / | cat includes - \
// | sort | uniq | tee new_includes | wc -l && mv new_includes includes
// and repeating until the number stopped going up
@i@
@@

(
 #include <linux/acpi_mdio.h>
|
 #include <linux/brcmphy.h>
|
 #include <linux/dsa/loop.h>
|
 #include <linux/dsa/sja1105.h>
|
 #include <linux/ethtool.h>
|
 #include <linux/ethtool_netlink.h>
|
 #include <linux/fec.h>
|
 #include <linux/fs_enet_pd.h>
|
 #include <linux/fsl/enetc_mdio.h>
|
 #include <linux/fwnode_mdio.h>
|
 #include <linux/linkmode.h>
|
 #include <linux/lsm_audit.h>
|
 #include <linux/mdio-bitbang.h>
|
 #include <linux/mdio.h>
|
 #include <linux/mdio-mux.h>
|
 #include <linux/mii.h>
|
 #include <linux/mii_timestamper.h>
|
 #include <linux/mlx5/accel.h>
|
 #include <linux/mlx5/cq.h>
|
 #include <linux/mlx5/device.h>
|
 #include <linux/mlx5/driver.h>
|
 #include <linux/mlx5/eswitch.h>
|
 #include <linux/mlx5/fs.h>
|
 #include <linux/mlx5/port.h>
|
 #include <linux/mlx5/qp.h>
|
 #include <linux/mlx5/rsc_dump.h>
|
 #include <linux/mlx5/transobj.h>
|
 #include <linux/mlx5/vport.h>
|
 #include <linux/of_mdio.h>
|
 #include <linux/of_net.h>
|
 #include <linux/pcs-lynx.h>
|
 #include <linux/pcs/pcs-xpcs.h>
|
 #include <linux/phy.h>
|
 #include <linux/phy_led_triggers.h>
|
 #include <linux/phylink.h>
|
 #include <linux/platform_data/bcmgenet.h>
|
 #include <linux/platform_data/xilinx-ll-temac.h>
|
 #include <linux/pxa168_eth.h>
|
 #include <linux/qed/qed_eth_if.h>
|
 #include <linux/qed/qed_fcoe_if.h>
|
 #include <linux/qed/qed_if.h>
|
 #include <linux/qed/qed_iov_if.h>
|
 #include <linux/qed/qed_iscsi_if.h>
|
 #include <linux/qed/qed_ll2_if.h>
|
 #include <linux/qed/qed_nvmetcp_if.h>
|
 #include <linux/qed/qed_rdma_if.h>
|
 #include <linux/sfp.h>
|
 #include <linux/sh_eth.h>
|
 #include <linux/smsc911x.h>
|
 #include <linux/soc/nxp/lpc32xx-misc.h>
|
 #include <linux/stmmac.h>
|
 #include <linux/sunrpc/svc_rdma.h>
|
 #include <linux/sxgbe_platform.h>
|
 #include <net/cfg80211.h>
|
 #include <net/dsa.h>
|
 #include <net/mac80211.h>
|
 #include <net/selftests.h>
|
 #include <rdma/ib_addr.h>
|
 #include <rdma/ib_cache.h>
|
 #include <rdma/ib_cm.h>
|
 #include <rdma/ib_hdrs.h>
|
 #include <rdma/ib_mad.h>
|
 #include <rdma/ib_marshall.h>
|
 #include <rdma/ib_pack.h>
|
 #include <rdma/ib_pma.h>
|
 #include <rdma/ib_sa.h>
|
 #include <rdma/ib_smi.h>
|
 #include <rdma/ib_umem.h>
|
 #include <rdma/ib_umem_odp.h>
|
 #include <rdma/ib_verbs.h>
|
 #include <rdma/iw_cm.h>
|
 #include <rdma/mr_pool.h>
|
 #include <rdma/opa_addr.h>
|
 #include <rdma/opa_port_info.h>
|
 #include <rdma/opa_smi.h>
|
 #include <rdma/opa_vnic.h>
|
 #include <rdma/rdma_cm.h>
|
 #include <rdma/rdma_cm_ib.h>
|
 #include <rdma/rdmavt_cq.h>
|
 #include <rdma/rdma_vt.h>
|
 #include <rdma/rdmavt_qp.h>
|
 #include <rdma/rw.h>
|
 #include <rdma/tid_rdma_defs.h>
|
 #include <rdma/uverbs_ioctl.h>
|
 #include <rdma/uverbs_named_ioctl.h>
|
 #include <rdma/uverbs_std_types.h>
|
 #include <rdma/uverbs_types.h>
|
 #include <soc/mscc/ocelot.h>
|
 #include <soc/mscc/ocelot_ptp.h>
|
 #include <soc/mscc/ocelot_vcap.h>
|
 #include <trace/events/ib_mad.h>
|
 #include <trace/events/rdma_core.h>
|
 #include <trace/events/rdma.h>
|
 #include <trace/events/rpcrdma.h>
|
 #include <uapi/linux/ethtool.h>
|
 #include <uapi/linux/ethtool_netlink.h>
|
 #include <uapi/linux/mdio.h>
|
 #include <uapi/linux/mii.h>
)

@depends on i@
expression list args;
@@

(
- bitmap_zero(args, __ETHTOOL_LINK_MODE_MASK_NBITS)
+ linkmode_zero(args)
|
- bitmap_copy(args, __ETHTOOL_LINK_MODE_MASK_NBITS)
+ linkmode_copy(args)
|
- bitmap_and(args, __ETHTOOL_LINK_MODE_MASK_NBITS)
+ linkmode_and(args)
|
- bitmap_or(args, __ETHTOOL_LINK_MODE_MASK_NBITS)
+ linkmode_or(args)
|
- bitmap_empty(args, ETHTOOL_LINK_MODE_MASK_NBITS)
+ linkmode_empty(args)
|
- bitmap_andnot(args, __ETHTOOL_LINK_MODE_MASK_NBITS)
+ linkmode_andnot(args)
|
- bitmap_equal(args, __ETHTOOL_LINK_MODE_MASK_NBITS)
+ linkmode_equal(args)
|
- bitmap_intersects(args, __ETHTOOL_LINK_MODE_MASK_NBITS)
+ linkmode_intersects(args)
|
- bitmap_subset(args, __ETHTOOL_LINK_MODE_MASK_NBITS)
+ linkmode_subset(args)
)

Add missing linux/mii.h include to mellanox. -DaveM

Signed-off-by: Sean Anderson <sean.anderson@seco.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/dsa/b53/b53_common.c              |  6 ++----
 drivers/net/dsa/bcm_sf2.c                     |  8 +++----
 drivers/net/dsa/hirschmann/hellcreek.c        |  6 ++----
 drivers/net/dsa/lantiq_gswip.c                | 14 ++++++-------
 drivers/net/dsa/microchip/ksz8795.c           |  8 +++----
 drivers/net/dsa/mv88e6xxx/chip.c              |  5 ++---
 drivers/net/dsa/ocelot/felix_vsc9959.c        |  8 +++----
 drivers/net/dsa/ocelot/seville_vsc9953.c      |  8 +++----
 drivers/net/dsa/qca/ar9331.c                  | 10 ++++-----
 drivers/net/dsa/sja1105/sja1105_main.c        |  7 +++----
 drivers/net/dsa/xrs700x/xrs700x.c             |  8 +++----
 drivers/net/ethernet/amd/xgbe/xgbe-ethtool.c  |  8 +++----
 drivers/net/ethernet/atheros/ag71xx.c         |  8 +++----
 drivers/net/ethernet/cadence/macb_main.c      | 11 +++++-----
 .../net/ethernet/freescale/enetc/enetc_pf.c   |  8 +++----
 .../net/ethernet/huawei/hinic/hinic_ethtool.c | 10 ++++-----
 .../net/ethernet/intel/ixgbe/ixgbe_ethtool.c  |  5 ++---
 drivers/net/ethernet/marvell/mvneta.c         | 10 ++++-----
 .../net/ethernet/marvell/mvpp2/mvpp2_main.c   |  7 +++----
 .../marvell/octeontx2/nic/otx2_ethtool.c      |  5 ++---
 drivers/net/ethernet/marvell/pxa168_eth.c     |  3 +--
 .../net/ethernet/mellanox/mlx4/en_ethtool.c   | 21 +++++++------------
 .../microchip/sparx5/sparx5_phylink.c         |  7 +++----
 drivers/net/ethernet/mscc/ocelot_net.c        |  7 +++----
 .../ethernet/pensando/ionic/ionic_ethtool.c   |  3 +--
 .../net/ethernet/xilinx/xilinx_axienet_main.c |  8 +++----
 drivers/net/pcs/pcs-xpcs.c                    |  2 +-
 drivers/net/phy/sfp-bus.c                     |  2 +-
 net/ethtool/ioctl.c                           |  7 +++----
 29 files changed, 87 insertions(+), 133 deletions(-)

--- a/drivers/net/dsa/b53/b53_common.c
+++ b/drivers/net/dsa/b53/b53_common.c
@@ -1349,10 +1349,8 @@ void b53_phylink_validate(struct dsa_swi
 		phylink_set(mask, 100baseT_Full);
 	}
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 
 	phylink_helper_basex_speed(state);
 }
--- a/drivers/net/dsa/bcm_sf2.c
+++ b/drivers/net/dsa/bcm_sf2.c
@@ -692,7 +692,7 @@ static void bcm_sf2_sw_validate(struct d
 	    state->interface != PHY_INTERFACE_MODE_GMII &&
 	    state->interface != PHY_INTERFACE_MODE_INTERNAL &&
 	    state->interface != PHY_INTERFACE_MODE_MOCA) {
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		if (port != core_readl(priv, CORE_IMP0_PRT_ID))
 			dev_err(ds->dev,
 				"Unsupported interface: %d for port %d\n",
@@ -720,10 +720,8 @@ static void bcm_sf2_sw_validate(struct d
 	phylink_set(mask, 100baseT_Half);
 	phylink_set(mask, 100baseT_Full);
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static void bcm_sf2_sw_mac_config(struct dsa_switch *ds, int port,
--- a/drivers/net/dsa/hirschmann/hellcreek.c
+++ b/drivers/net/dsa/hirschmann/hellcreek.c
@@ -1476,10 +1476,8 @@ static void hellcreek_phylink_validate(s
 	else
 		phylink_set(mask, 1000baseT_Full);
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static int
--- a/drivers/net/dsa/lantiq_gswip.c
+++ b/drivers/net/dsa/lantiq_gswip.c
@@ -1452,10 +1452,8 @@ static void gswip_phylink_set_capab(unsi
 	phylink_set(mask, 100baseT_Half);
 	phylink_set(mask, 100baseT_Full);
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static void gswip_xrx200_phylink_validate(struct dsa_switch *ds, int port,
@@ -1483,7 +1481,7 @@ static void gswip_xrx200_phylink_validat
 			goto unsupported;
 		break;
 	default:
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		dev_err(ds->dev, "Unsupported port: %i\n", port);
 		return;
 	}
@@ -1493,7 +1491,7 @@ static void gswip_xrx200_phylink_validat
 	return;
 
 unsupported:
-	bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_zero(supported);
 	dev_err(ds->dev, "Unsupported interface '%s' for port %d\n",
 		phy_modes(state->interface), port);
 }
@@ -1523,7 +1521,7 @@ static void gswip_xrx300_phylink_validat
 			goto unsupported;
 		break;
 	default:
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		dev_err(ds->dev, "Unsupported port: %i\n", port);
 		return;
 	}
@@ -1533,7 +1531,7 @@ static void gswip_xrx300_phylink_validat
 	return;
 
 unsupported:
-	bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_zero(supported);
 	dev_err(ds->dev, "Unsupported interface '%s' for port %d\n",
 		phy_modes(state->interface), port);
 }
--- a/drivers/net/dsa/microchip/ksz8795.c
+++ b/drivers/net/dsa/microchip/ksz8795.c
@@ -1542,15 +1542,13 @@ static void ksz8_validate(struct dsa_swi
 	phylink_set(mask, 100baseT_Half);
 	phylink_set(mask, 100baseT_Full);
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 
 	return;
 
 unsupported:
-	bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_zero(supported);
 	dev_err(ds->dev, "Unsupported interface: %s, port: %d\n",
 		phy_modes(state->interface), port);
 }
--- a/drivers/net/dsa/mv88e6xxx/chip.c
+++ b/drivers/net/dsa/mv88e6xxx/chip.c
@@ -683,9 +683,8 @@ static void mv88e6xxx_validate(struct ds
 	if (chip->info->ops->phylink_validate)
 		chip->info->ops->phylink_validate(chip, port, mask, state);
 
-	bitmap_and(supported, supported, mask, __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 
 	/* We can only operate at 2500BaseX or 1000BaseX.  If requested
 	 * to advertise both, only report advertising at 2500BaseX.
--- a/drivers/net/dsa/ocelot/felix_vsc9959.c
+++ b/drivers/net/dsa/ocelot/felix_vsc9959.c
@@ -944,7 +944,7 @@ static void vsc9959_phylink_validate(str
 
 	if (state->interface != PHY_INTERFACE_MODE_NA &&
 	    state->interface != ocelot_port->phy_mode) {
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		return;
 	}
 
@@ -966,10 +966,8 @@ static void vsc9959_phylink_validate(str
 		phylink_set(mask, 2500baseX_Full);
 	}
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static int vsc9959_prevalidate_phy_mode(struct ocelot *ocelot, int port,
--- a/drivers/net/dsa/ocelot/seville_vsc9953.c
+++ b/drivers/net/dsa/ocelot/seville_vsc9953.c
@@ -1000,7 +1000,7 @@ static void vsc9953_phylink_validate(str
 
 	if (state->interface != PHY_INTERFACE_MODE_NA &&
 	    state->interface != ocelot_port->phy_mode) {
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		return;
 	}
 
@@ -1019,10 +1019,8 @@ static void vsc9953_phylink_validate(str
 		phylink_set(mask, 2500baseX_Full);
 	}
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static int vsc9953_prevalidate_phy_mode(struct ocelot *ocelot, int port,
--- a/drivers/net/dsa/qca/ar9331.c
+++ b/drivers/net/dsa/qca/ar9331.c
@@ -522,7 +522,7 @@ static void ar9331_sw_phylink_validate(s
 			goto unsupported;
 		break;
 	default:
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		dev_err(ds->dev, "Unsupported port: %i\n", port);
 		return;
 	}
@@ -536,15 +536,13 @@ static void ar9331_sw_phylink_validate(s
 	phylink_set(mask, 100baseT_Half);
 	phylink_set(mask, 100baseT_Full);
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 
 	return;
 
 unsupported:
-	bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_zero(supported);
 	dev_err(ds->dev, "Unsupported interface: %d, port: %d\n",
 		state->interface, port);
 }
--- a/drivers/net/dsa/sja1105/sja1105_main.c
+++ b/drivers/net/dsa/sja1105/sja1105_main.c
@@ -1360,7 +1360,7 @@ static void sja1105_phylink_validate(str
 	 */
 	if (state->interface != PHY_INTERFACE_MODE_NA &&
 	    sja1105_phy_mode_mismatch(priv, port, state->interface)) {
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		return;
 	}
 
@@ -1380,9 +1380,8 @@ static void sja1105_phylink_validate(str
 		phylink_set(mask, 2500baseX_Full);
 	}
 
-	bitmap_and(supported, supported, mask, __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static int
--- a/drivers/net/dsa/xrs700x/xrs700x.c
+++ b/drivers/net/dsa/xrs700x/xrs700x.c
@@ -457,7 +457,7 @@ static void xrs700x_phylink_validate(str
 		phylink_set(mask, 1000baseT_Full);
 		break;
 	default:
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		dev_err(ds->dev, "Unsupported port: %i\n", port);
 		return;
 	}
@@ -468,10 +468,8 @@ static void xrs700x_phylink_validate(str
 	phylink_set(mask, 10baseT_Full);
 	phylink_set(mask, 100baseT_Full);
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static void xrs700x_mac_link_up(struct dsa_switch *ds, int port,
--- a/drivers/net/ethernet/amd/xgbe/xgbe-ethtool.c
+++ b/drivers/net/ethernet/amd/xgbe/xgbe-ethtool.c
@@ -374,9 +374,8 @@ static int xgbe_set_link_ksettings(struc
 		  __ETHTOOL_LINK_MODE_MASK_NBITS, cmd->link_modes.advertising,
 		  __ETHTOOL_LINK_MODE_MASK_NBITS, lks->link_modes.supported);
 
-	bitmap_and(advertising,
-		   cmd->link_modes.advertising, lks->link_modes.supported,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(advertising, cmd->link_modes.advertising,
+		     lks->link_modes.supported);
 
 	if ((cmd->base.autoneg == AUTONEG_ENABLE) &&
 	    bitmap_empty(advertising, __ETHTOOL_LINK_MODE_MASK_NBITS)) {
@@ -389,8 +388,7 @@ static int xgbe_set_link_ksettings(struc
 	pdata->phy.autoneg = cmd->base.autoneg;
 	pdata->phy.speed = speed;
 	pdata->phy.duplex = cmd->base.duplex;
-	bitmap_copy(lks->link_modes.advertising, advertising,
-		    __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_copy(lks->link_modes.advertising, advertising);
 
 	if (cmd->base.autoneg == AUTONEG_ENABLE)
 		XGBE_SET_ADV(lks, Autoneg);
--- a/drivers/net/ethernet/atheros/ag71xx.c
+++ b/drivers/net/ethernet/atheros/ag71xx.c
@@ -1082,14 +1082,12 @@ static void ag71xx_mac_validate(struct p
 		phylink_set(mask, 1000baseX_Full);
 	}
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 
 	return;
 unsupported:
-	bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_zero(supported);
 }
 
 static void ag71xx_mac_pcs_get_state(struct phylink_config *config,
--- a/drivers/net/ethernet/cadence/macb_main.c
+++ b/drivers/net/ethernet/cadence/macb_main.c
@@ -523,21 +523,21 @@ static void macb_validate(struct phylink
 	    state->interface != PHY_INTERFACE_MODE_SGMII &&
 	    state->interface != PHY_INTERFACE_MODE_10GBASER &&
 	    !phy_interface_mode_is_rgmii(state->interface)) {
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		return;
 	}
 
 	if (!macb_is_gem(bp) &&
 	    (state->interface == PHY_INTERFACE_MODE_GMII ||
 	     phy_interface_mode_is_rgmii(state->interface))) {
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		return;
 	}
 
 	if (state->interface == PHY_INTERFACE_MODE_10GBASER &&
 	    !(bp->caps & MACB_CAPS_HIGH_SPEED &&
 	      bp->caps & MACB_CAPS_PCS)) {
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		return;
 	}
 
@@ -576,9 +576,8 @@ static void macb_validate(struct phylink
 			phylink_set(mask, 1000baseT_Half);
 	}
 out:
-	bitmap_and(supported, supported, mask, __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static void macb_usx_pcs_link_up(struct phylink_pcs *pcs, unsigned int mode,
--- a/drivers/net/ethernet/freescale/enetc/enetc_pf.c
+++ b/drivers/net/ethernet/freescale/enetc/enetc_pf.c
@@ -965,7 +965,7 @@ static void enetc_pl_mac_validate(struct
 	    state->interface != PHY_INTERFACE_MODE_2500BASEX &&
 	    state->interface != PHY_INTERFACE_MODE_USXGMII &&
 	    !phy_interface_mode_is_rgmii(state->interface)) {
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		return;
 	}
 
@@ -988,10 +988,8 @@ static void enetc_pl_mac_validate(struct
 		phylink_set(mask, 2500baseX_Full);
 	}
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static void enetc_pl_mac_config(struct phylink_config *config,
--- a/drivers/net/ethernet/huawei/hinic/hinic_ethtool.c
+++ b/drivers/net/ethernet/huawei/hinic/hinic_ethtool.c
@@ -322,12 +322,10 @@ static int hinic_get_link_ksettings(stru
 		}
 	}
 
-	bitmap_copy(link_ksettings->link_modes.supported,
-		    (unsigned long *)&settings.supported,
-		    __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_copy(link_ksettings->link_modes.advertising,
-		    (unsigned long *)&settings.advertising,
-		    __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_copy(link_ksettings->link_modes.supported,
+		      (unsigned long *)&settings.supported);
+	linkmode_copy(link_ksettings->link_modes.advertising,
+		      (unsigned long *)&settings.advertising);
 
 	return 0;
 }
--- a/drivers/net/ethernet/intel/ixgbe/ixgbe_ethtool.c
+++ b/drivers/net/ethernet/intel/ixgbe/ixgbe_ethtool.c
@@ -467,9 +467,8 @@ static int ixgbe_set_link_ksettings(stru
 		 * this function does not support duplex forcing, but can
 		 * limit the advertising of the adapter to the specified speed
 		 */
-		if (!bitmap_subset(cmd->link_modes.advertising,
-				   cmd->link_modes.supported,
-				   __ETHTOOL_LINK_MODE_MASK_NBITS))
+		if (!linkmode_subset(cmd->link_modes.advertising,
+				     cmd->link_modes.supported))
 			return -EINVAL;
 
 		/* only allow one speed at a time if no autoneg */
--- a/drivers/net/ethernet/marvell/mvneta.c
+++ b/drivers/net/ethernet/marvell/mvneta.c
@@ -3835,14 +3835,14 @@ static void mvneta_validate(struct phyli
 	 */
 	if (phy_interface_mode_is_8023z(state->interface)) {
 		if (!phylink_test(state->advertising, Autoneg)) {
-			bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+			linkmode_zero(supported);
 			return;
 		}
 	} else if (state->interface != PHY_INTERFACE_MODE_NA &&
 		   state->interface != PHY_INTERFACE_MODE_QSGMII &&
 		   state->interface != PHY_INTERFACE_MODE_SGMII &&
 		   !phy_interface_mode_is_rgmii(state->interface)) {
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		return;
 	}
 
@@ -3871,10 +3871,8 @@ static void mvneta_validate(struct phyli
 		phylink_set(mask, 100baseT_Full);
 	}
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 
 	/* We can only operate at 2500BaseX or 1000BaseX.  If requested
 	 * to advertise both, only report advertising at 2500BaseX.
--- a/drivers/net/ethernet/marvell/mvpp2/mvpp2_main.c
+++ b/drivers/net/ethernet/marvell/mvpp2/mvpp2_main.c
@@ -6352,15 +6352,14 @@ static void mvpp2_phylink_validate(struc
 		goto empty_set;
 	}
 
-	bitmap_and(supported, supported, mask, __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 
 	phylink_helper_basex_speed(state);
 	return;
 
 empty_set:
-	bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_zero(supported);
 }
 
 static void mvpp2_xlg_config(struct mvpp2_port *port, unsigned int mode,
--- a/drivers/net/ethernet/marvell/octeontx2/nic/otx2_ethtool.c
+++ b/drivers/net/ethernet/marvell/octeontx2/nic/otx2_ethtool.c
@@ -1172,9 +1172,8 @@ static int otx2_set_link_ksettings(struc
 	otx2_get_link_ksettings(netdev, &cur_ks);
 
 	/* Check requested modes against supported modes by hardware */
-	if (!bitmap_subset(cmd->link_modes.advertising,
-			   cur_ks.link_modes.supported,
-			   __ETHTOOL_LINK_MODE_MASK_NBITS))
+	if (!linkmode_subset(cmd->link_modes.advertising,
+			     cur_ks.link_modes.supported))
 		return -EINVAL;
 
 	mutex_lock(&mbox->lock);
--- a/drivers/net/ethernet/marvell/pxa168_eth.c
+++ b/drivers/net/ethernet/marvell/pxa168_eth.c
@@ -977,8 +977,7 @@ static int pxa168_init_phy(struct net_de
 	cmd.base.phy_address = pep->phy_addr;
 	cmd.base.speed = pep->phy_speed;
 	cmd.base.duplex = pep->phy_duplex;
-	bitmap_copy(cmd.link_modes.advertising, PHY_BASIC_FEATURES,
-		    __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_copy(cmd.link_modes.advertising, PHY_BASIC_FEATURES);
 	cmd.base.autoneg = AUTONEG_ENABLE;
 
 	if (cmd.base.speed != 0)
--- a/drivers/net/ethernet/mellanox/mlx4/en_ethtool.c
+++ b/drivers/net/ethernet/mellanox/mlx4/en_ethtool.c
@@ -39,6 +39,7 @@
 #include <linux/in.h>
 #include <net/ip.h>
 #include <linux/bitmap.h>
+#include <linux/mii.h>
 
 #include "mlx4_en.h"
 #include "en_port.h"
@@ -643,10 +644,8 @@ static unsigned long *ptys2ethtool_link_
 		unsigned int i;						\
 		cfg = &ptys2ethtool_map[reg_];				\
 		cfg->speed = speed_;					\
-		bitmap_zero(cfg->supported,				\
-			    __ETHTOOL_LINK_MODE_MASK_NBITS);		\
-		bitmap_zero(cfg->advertised,				\
-			    __ETHTOOL_LINK_MODE_MASK_NBITS);		\
+		linkmode_zero(cfg->supported);				\
+		linkmode_zero(cfg->advertised);				\
 		for (i = 0 ; i < ARRAY_SIZE(modes) ; ++i) {		\
 			__set_bit(modes[i], cfg->supported);		\
 			__set_bit(modes[i], cfg->advertised);		\
@@ -702,10 +701,8 @@ static void ptys2ethtool_update_link_mod
 	int i;
 	for (i = 0; i < MLX4_LINK_MODES_SZ; i++) {
 		if (eth_proto & MLX4_PROT_MASK(i))
-			bitmap_or(link_modes, link_modes,
-				  ptys2ethtool_link_mode(&ptys2ethtool_map[i],
-							 report),
-				  __ETHTOOL_LINK_MODE_MASK_NBITS);
+			linkmode_or(link_modes, link_modes,
+				    ptys2ethtool_link_mode(&ptys2ethtool_map[i], report));
 	}
 }
 
@@ -716,11 +713,9 @@ static u32 ethtool2ptys_link_modes(const
 	u32 ptys_modes = 0;
 
 	for (i = 0; i < MLX4_LINK_MODES_SZ; i++) {
-		if (bitmap_intersects(
-			    ptys2ethtool_link_mode(&ptys2ethtool_map[i],
-						   report),
-			    link_modes,
-			    __ETHTOOL_LINK_MODE_MASK_NBITS))
+		ulong *map_mode = ptys2ethtool_link_mode(&ptys2ethtool_map[i],
+							 report);
+		if (linkmode_intersects(map_mode, link_modes))
 			ptys_modes |= 1 << i;
 	}
 	return ptys_modes;
--- a/drivers/net/ethernet/microchip/sparx5/sparx5_phylink.c
+++ b/drivers/net/ethernet/microchip/sparx5/sparx5_phylink.c
@@ -92,12 +92,11 @@ static void sparx5_phylink_validate(stru
 		}
 		break;
 	default:
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		return;
 	}
-	bitmap_and(supported, supported, mask, __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static void sparx5_phylink_mac_config(struct phylink_config *config,
--- a/drivers/net/ethernet/mscc/ocelot_net.c
+++ b/drivers/net/ethernet/mscc/ocelot_net.c
@@ -1509,7 +1509,7 @@ static void vsc7514_phylink_validate(str
 
 	if (state->interface != PHY_INTERFACE_MODE_NA &&
 	    state->interface != ocelot_port->phy_mode) {
-		bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(supported);
 		return;
 	}
 
@@ -1528,9 +1528,8 @@ static void vsc7514_phylink_validate(str
 	phylink_set(mask, 2500baseT_Full);
 	phylink_set(mask, 2500baseX_Full);
 
-	bitmap_and(supported, supported, mask, __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static void vsc7514_phylink_mac_config(struct phylink_config *config,
--- a/drivers/net/ethernet/pensando/ionic/ionic_ethtool.c
+++ b/drivers/net/ethernet/pensando/ionic/ionic_ethtool.c
@@ -228,8 +228,7 @@ static int ionic_get_link_ksettings(stru
 		break;
 	}
 
-	bitmap_copy(ks->link_modes.advertising, ks->link_modes.supported,
-		    __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_copy(ks->link_modes.advertising, ks->link_modes.supported);
 
 	ethtool_link_ksettings_add_link_mode(ks, supported, FEC_BASER);
 	ethtool_link_ksettings_add_link_mode(ks, supported, FEC_RS);
--- a/drivers/net/ethernet/xilinx/xilinx_axienet_main.c
+++ b/drivers/net/ethernet/xilinx/xilinx_axienet_main.c
@@ -1565,7 +1565,7 @@ static void axienet_validate(struct phyl
 			netdev_warn(ndev, "Cannot use PHY mode %s, supported: %s\n",
 				    phy_modes(state->interface),
 				    phy_modes(lp->phy_mode));
-			bitmap_zero(supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+			linkmode_zero(supported);
 			return;
 		}
 	}
@@ -1598,10 +1598,8 @@ static void axienet_validate(struct phyl
 		break;
 	}
 
-	bitmap_and(supported, supported, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
-	bitmap_and(state->advertising, state->advertising, mask,
-		   __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_and(supported, supported, mask);
+	linkmode_and(state->advertising, state->advertising, mask);
 }
 
 static void axienet_mac_pcs_get_state(struct phylink_config *config,
--- a/drivers/net/pcs/pcs-xpcs.c
+++ b/drivers/net/pcs/pcs-xpcs.c
@@ -637,7 +637,7 @@ void xpcs_validate(struct dw_xpcs *xpcs,
 	if (state->interface == PHY_INTERFACE_MODE_NA)
 		return;
 
-	bitmap_zero(xpcs_supported, __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_zero(xpcs_supported);
 
 	compat = xpcs_find_compat(xpcs->id, state->interface);
 
--- a/drivers/net/phy/sfp-bus.c
+++ b/drivers/net/phy/sfp-bus.c
@@ -379,7 +379,7 @@ void sfp_parse_support(struct sfp_bus *b
 	if (bus->sfp_quirk)
 		bus->sfp_quirk->modes(id, modes);
 
-	bitmap_or(support, support, modes, __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_or(support, support, modes);
 
 	phylink_set(support, Autoneg);
 	phylink_set(support, Pause);
--- a/net/ethtool/ioctl.c
+++ b/net/ethtool/ioctl.c
@@ -335,7 +335,7 @@ EXPORT_SYMBOL(ethtool_intersect_link_mas
 void ethtool_convert_legacy_u32_to_link_mode(unsigned long *dst,
 					     u32 legacy_u32)
 {
-	bitmap_zero(dst, __ETHTOOL_LINK_MODE_MASK_NBITS);
+	linkmode_zero(dst);
 	dst[0] = legacy_u32;
 }
 EXPORT_SYMBOL(ethtool_convert_legacy_u32_to_link_mode);
@@ -350,11 +350,10 @@ bool ethtool_convert_link_mode_to_legacy
 	if (__ETHTOOL_LINK_MODE_MASK_NBITS > 32) {
 		__ETHTOOL_DECLARE_LINK_MODE_MASK(ext);
 
-		bitmap_zero(ext, __ETHTOOL_LINK_MODE_MASK_NBITS);
+		linkmode_zero(ext);
 		bitmap_fill(ext, 32);
 		bitmap_complement(ext, ext, __ETHTOOL_LINK_MODE_MASK_NBITS);
-		if (bitmap_intersects(ext, src,
-				      __ETHTOOL_LINK_MODE_MASK_NBITS)) {
+		if (linkmode_intersects(ext, src)) {
 			/* src mask goes beyond bit 31 */
 			retval = false;
 		}
