// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm6368.dtsi"

/ {
	model = "Comtrend VR-3025un";
	compatible = "comtrend,vr-3025un", "brcm,bcm6368";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_red;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 34 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led@2 {
			label = "green:dsl";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};

		led@5 {
			label = "green:internet";
			gpios = <&gpio 5 GPIO_ACTIVE_HIGH>;
		};

		led_power_green: led@22 {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 22 GPIO_ACTIVE_HIGH>;
		};

		led_power_red: led@24 {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpio 24 GPIO_ACTIVE_HIGH>;
			panic-indicator;
		};

		led@31 {
			label = "red:internet";
			gpios = <&gpio 31 GPIO_ACTIVE_HIGH>;
		};
	};

	bcm43222-sprom {
		compatible = "brcm,ssb-sprom";

		pci-bus = <0>;
		pci-dev = <1>;

		nvmem-cells = <&macaddr_cfe_6a0 1>;
		nvmem-cell-names = "mac-address";

		brcm,sprom = "brcm/bcm43222-sprom.bin";
		brcm,sprom-fixups = <97 0xfeb3>,
				    <98 0x1618>,
				    <99 0xfab0>,
				    <113 0xfed1>,
				    <114 0x1609>,
				    <115 0xfad9>;
	};
};

&ehci {
	status = "okay";
};

&ethernet {
	status = "okay";

	nvmem-cells = <&macaddr_cfe_6a0 0>;
	nvmem-cell-names = "mac-address";
};

&ohci {
	status = "okay";
};

&pci {
	status = "okay";
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "CFE";
			reg = <0x000000 0x010000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_cfe_6a0: macaddr@6a0 {
					compatible = "mac-base";
					reg = <0x6a0 0x6>;
					#nvmem-cell-cells = <1>;
				};
			};
		};

		partition@20000 {
			compatible = "brcm,bcm963xx-imagetag";
			label = "firmware";
			reg = <0x010000 0x7e0000>;
		};

		partition@1fe0000 {
			label = "nvram";
			reg = <0x7f0000 0x010000>;
		};
	};
};

&pinctrl {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_ephy0_led &pinctrl_ephy1_led
		     &pinctrl_ephy2_led &pinctrl_ephy3_led>;
};

&switch0 {
	ports {
		port@0 {
			reg = <0>;
			label = "lan1";

			phy-handle = <&phy1>;
			phy-mode = "mii";
		};

		port@1 {
			reg = <1>;
			label = "lan2";

			phy-handle = <&phy2>;
			phy-mode = "mii";
		};

		port@2 {
			reg = <2>;
			label = "lan3";

			phy-handle = <&phy3>;
			phy-mode = "mii";
		};

		port@3 {
			reg = <3>;
			label = "iptv";

			phy-handle = <&phy4>;
			phy-mode = "mii";
		};
	};
};

&uart0 {
	status = "okay";
};

&usbh {
	status = "okay";
};
