From c3552d3f85f06cf4b4818bd84c4fcc09d8d45165 Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Mon, 3 Apr 2023 02:17:19 +0100
Subject: [PATCH 01/13] net: dsa: mt7530: make some noise if register read
 fails

Simply returning the negative error value instead of the read value
doesn't seem like a good idea. Return 0 instead and add WARN_ON_ONCE(1)
so this kind of error will not go unnoticed.

Suggested-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/dsa/mt7530.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/net/dsa/mt7530.c
+++ b/drivers/net/dsa/mt7530.c
@@ -224,9 +224,10 @@ mt7530_mii_read(struct mt7530_priv *priv
 	/* MT7530 uses 31 as the pseudo port */
 	ret = bus->write(bus, 0x1f, 0x1f, page);
 	if (ret < 0) {
+		WARN_ON_ONCE(1);
 		dev_err(&bus->dev,
 			"failed to read mt7530 register\n");
-		return ret;
+		return 0;
 	}
 
 	lo = bus->read(bus, 0x1f, r);
