#!/bin/sh

[ -e /lib/firmware/$FIRMWARE ] && exit 0

. /lib/functions/caldata.sh

board=$(board_name)

case "$FIRMWARE" in
"ath11k/IPQ8074/hw2.0/cal-ahb-c000000.wifi.bin")
	case "$board" in
	arcadyan,aw1000|\
	buffalo,wxr-5950ax12|\
	cmcc,rm2-6|\
	compex,wpq873|\
	dynalink,dl-wrx36|\
	edgecore,eap102|\
	edimax,cax1800|\
	linksys,mx4200v1|\
	linksys,mx4200v2|\
	linksys,mx5300|\
	netgear,rax120v2|\
	netgear,wax218|\
	netgear,wax620|\
	netgear,wax630|\
	qnap,301w|\
	redmi,ax6|\
	xiaomi,ax3600|\
	xiaomi,ax9000|\
	yuncore,ax880|\
	zte,mf269|\
	zyxel,nbg7815)
		caldata_extract "0:art" 0x1000 0x20000
		;;
	prpl,haze)
		caldata_extract_mmc "0:ART" 0x1000 0x20000
		;;
	esac
	;;
"ath11k/QCN9074/hw1.0/cal-pci-0000:01:00.0.bin"|\
"ath11k/QCN9074/hw1.0/cal-pci-0001:01:00.0.bin")
	case "$board" in
	prpl,haze)
		caldata_extract_mmc "0:ART" 0x26800 0x20000
		;;
	xiaomi,ax9000)
		caldata_extract "0:art" 0x26800 0x20000
		;;
	esac
	;;
*)
	exit 1
	;;
esac
