// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7240.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "D-Link DIR-615 E4";
	compatible = "dlink,dir-615-e4", "qca,ar7240";

	aliases {
		led-boot = &led_power_amber;
		led-failsafe = &led_power_amber;
		led-running = &led_power_green;
		led-upgrade = &led_power_amber;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&switch_led_pins>;

		led_power_green: power_green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 6 GPIO_ACTIVE_HIGH>;
		};

		led_power_amber: power_amber {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
		};

		wps {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		lan1 {
			label = "green:lan1";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		lan2 {
			label = "green:lan2";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		lan3 {
			label = "green:lan3";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		lan4 {
			label = "green:lan4";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		wan_amber {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
		};

		wan_green {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wlan {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&ath9k 1 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <33000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				reg = <0x0 0x30000>;
				label = "u-boot";
				read-only;
			};

			partition@30000 {
				reg = <0x30000 0x10000>;
				label = "nvram";
				read-only;
			};

			partition@40000 {
				compatible = "denx,uimage";
				reg = <0x40000 0x3b0000>;
				label = "firmware";
			};

			partition@3f0000 {
				reg = <0x3f0000 0x10000>;
				label = "art";
				read-only;
			};
		};
	};
};

&eth1 {
	status = "okay";
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		compatible = "pci168c,002b";
		reg = <0x0000 0 0 0 0>;
		qca,no-eeprom;
		#gpio-cells = <2>;
		gpio-controller;
	};
};

&pinmux {
	switch_led_pins: pinmux_switch_led_pins {
		pinctrl-single,bits = <0x0 0x0 0xf8>;
	};
};
