From 49502408007b77ff290ce62e6218cefaeedcb31a Mon Sep 17 00:00:00 2001
From: Vasily Khoruzhick <anarsoul@gmail.com>
Date: Thu, 9 Mar 2023 17:03:49 -0800
Subject: [PATCH] mmc: sdhci-of-dwcmshc: properly determine max clock on
 Rockchip

Currently .get_max_clock returns the current clock rate for cclk_emmc
on rk35xx, thus max clock gets set to whatever bootloader set it to.

In case of u-boot, it is intentionally reset to 50 MHz if it boots
from eMMC, see mmc_deinit() in u-boot sources. As a result, HS200 and
HS400 modes are never selected by Linux, because dwcmshc_rk35xx_postinit
clears appropriate caps if host->mmc->f_max is < 52MHz

cclk_emmc is not a fixed clock on rk35xx, so using
sdhci_pltfm_clk_get_max_clock is not appropriate here.

Implement rk35xx_get_max_clock that returns actual max clock for cclk_emmc.

Signed-off-by: Vasily Khoruzhick <anarsoul@gmail.com>
Acked-by: Adrian Hunter <adrian.hunter@intel.com>
Link: https://lore.kernel.org/r/20230310010349.509132-1-anarsoul@gmail.com
Signed-off-by: Ulf Hansson <ulf.hansson@linaro.org>
---
 drivers/mmc/host/sdhci-of-dwcmshc.c | 9 ++++++++-
 1 file changed, 8 insertions(+), 1 deletion(-)

--- a/drivers/mmc/host/sdhci-of-dwcmshc.c
+++ b/drivers/mmc/host/sdhci-of-dwcmshc.c
@@ -126,6 +126,13 @@ static unsigned int dwcmshc_get_max_cloc
 		return pltfm_host->clock;
 }
 
+static unsigned int rk35xx_get_max_clock(struct sdhci_host *host)
+{
+	struct sdhci_pltfm_host *pltfm_host = sdhci_priv(host);
+
+	return clk_round_rate(pltfm_host->clk, ULONG_MAX);
+}
+
 static void dwcmshc_check_auto_cmd23(struct mmc_host *mmc,
 				     struct mmc_request *mrq)
 {
@@ -343,7 +350,7 @@ static const struct sdhci_ops sdhci_dwcm
 	.set_clock		= dwcmshc_rk3568_set_clock,
 	.set_bus_width		= sdhci_set_bus_width,
 	.set_uhs_signaling	= dwcmshc_set_uhs_signaling,
-	.get_max_clock		= sdhci_pltfm_clk_get_max_clock,
+	.get_max_clock		= rk35xx_get_max_clock,
 	.reset			= rk35xx_sdhci_reset,
 	.adma_write_desc	= dwcmshc_adma_write_desc,
 };
