From 52811174f534824f5e5bcdb681f0c508aa335244 Mon Sep 17 00:00:00 2001
From: Naushir Patuck <naush@raspberrypi.com>
Date: Wed, 4 Oct 2023 11:09:10 +0100
Subject: [PATCH] media: i2c: Move Kconfig entry for IMX477 to the camera
 sensor section

It was accidentally placed in the audio decoder section.

Signed-off-by: Naushir Patuck <naush@raspberrypi.com>
---
 drivers/media/i2c/Kconfig | 22 +++++++++++-----------
 1 file changed, 11 insertions(+), 11 deletions(-)

--- a/drivers/media/i2c/Kconfig
+++ b/drivers/media/i2c/Kconfig
@@ -270,6 +270,17 @@ config VIDEO_IMX412
 	  To compile this driver as a module, choose M here: the
 	  module will be called imx412.
 
+config VIDEO_IMX477
+	tristate "Sony IMX477 sensor support"
+	depends on I2C && VIDEO_DEV
+	select VIDEO_V4L2_SUBDEV_API
+	help
+	  This is a Video4Linux2 sensor driver for the Sony
+	  IMX477 camera. Also supports the Sony IMX378.
+
+	  To compile this driver as a module, choose M here: the
+	  module will be called imx477.
+
 config VIDEO_IMX519
 	tristate "Arducam IMX519 sensor support"
 	depends on I2C && VIDEO_DEV
@@ -1106,17 +1117,6 @@ config VIDEO_UDA1342
 	  To compile this driver as a module, choose M here: the
 	  module will be called uda1342.
 
-config VIDEO_IMX477
-	tristate "Sony IMX477 sensor support"
-	depends on I2C && VIDEO_DEV
-	select VIDEO_V4L2_SUBDEV_API
-	help
-	  This is a Video4Linux2 sensor driver for the Sony
-	  IMX477 camera. Also supports the Sony IMX378.
-
-	  To compile this driver as a module, choose M here: the
-	  module will be called imx477.
-
 config VIDEO_VP27SMPX
 	tristate "Panasonic VP27's internal MPX"
 	depends on VIDEO_DEV && I2C
