From 0b5ed6065e35da3e27a6ade1682ce0ba0fbc4ec0 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Thu, 6 Apr 2023 10:38:40 +0100
Subject: [PATCH] Bluetooth: hci_bcm: Add more invalid BDADDRs

The kernel needs to recognise the default BDADDRs used by the Bluetooth
modems, so add a few more that we care about.

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 drivers/bluetooth/btbcm.c | 8 ++++++++
 1 file changed, 8 insertions(+)

--- a/drivers/bluetooth/btbcm.c
+++ b/drivers/bluetooth/btbcm.c
@@ -24,11 +24,15 @@
 #define BDADDR_BCM20702A1 (&(bdaddr_t) {{0x00, 0x00, 0xa0, 0x02, 0x70, 0x20}})
 #define BDADDR_BCM2076B1 (&(bdaddr_t) {{0x79, 0x56, 0x00, 0xa0, 0x76, 0x20}})
 #define BDADDR_BCM43430A0 (&(bdaddr_t) {{0xac, 0x1f, 0x12, 0xa0, 0x43, 0x43}})
+#define BDADDR_BCM43430A1 (&(bdaddr_t) {{0xac, 0x1f, 0x12, 0xa1, 0x43, 0x43}})
+#define BDADDR_BCM43430B0 (&(bdaddr_t) {{0xac, 0x1f, 0x37, 0xb0, 0x43, 0x43}})
 #define BDADDR_BCM4324B3 (&(bdaddr_t) {{0x00, 0x00, 0x00, 0xb3, 0x24, 0x43}})
 #define BDADDR_BCM4330B1 (&(bdaddr_t) {{0x00, 0x00, 0x00, 0xb1, 0x30, 0x43}})
 #define BDADDR_BCM4334B0 (&(bdaddr_t) {{0x00, 0x00, 0x00, 0xb0, 0x34, 0x43}})
+#define BDADDR_BCM4345C0 (&(bdaddr_t) {{0xac, 0x1f, 0x00, 0xc0, 0x45, 0x43}})
 #define BDADDR_BCM4345C5 (&(bdaddr_t) {{0xac, 0x1f, 0x00, 0xc5, 0x45, 0x43}})
 #define BDADDR_BCM43341B (&(bdaddr_t) {{0xac, 0x1f, 0x00, 0x1b, 0x34, 0x43}})
+#define BDADDR_BCM43438 (&(bdaddr_t) {{0xaa, 0xaa, 0xaa, 0xaa, 0xaa, 0xaa}})
 
 #define BCM_FW_NAME_LEN			64
 #define BCM_FW_NAME_COUNT_MAX		4
@@ -122,8 +126,12 @@ int btbcm_check_bdaddr(struct hci_dev *h
 	    !bacmp(&bda->bdaddr, BDADDR_BCM4324B3) ||
 	    !bacmp(&bda->bdaddr, BDADDR_BCM4330B1) ||
 	    !bacmp(&bda->bdaddr, BDADDR_BCM4334B0) ||
+	    !bacmp(&bda->bdaddr, BDADDR_BCM4345C0) ||
 	    !bacmp(&bda->bdaddr, BDADDR_BCM4345C5) ||
 	    !bacmp(&bda->bdaddr, BDADDR_BCM43430A0) ||
+	    !bacmp(&bda->bdaddr, BDADDR_BCM43430A1) ||
+	    !bacmp(&bda->bdaddr, BDADDR_BCM43430B0) ||
+	    !bacmp(&bda->bdaddr, BDADDR_BCM43438) ||
 	    !bacmp(&bda->bdaddr, BDADDR_BCM43341B)) {
 		/* Try falling back to BDADDR EFI variable */
 		if (btbcm_set_bdaddr_from_efi(hdev) != 0) {
