From 2f5a75f9687553d6e91fcc09b233f5f6176b3681 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Fri, 17 Feb 2023 13:36:14 +0100
Subject: [PATCH] dt-bindings: display: Add BCM2712 HVS bindings

The BCM2712 has a completely different HVS than the previous
generations, so let's add a new compatible for it.

Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 .../devicetree/bindings/display/brcm,bcm2835-hvs.yaml        | 5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

--- a/Documentation/devicetree/bindings/display/brcm,bcm2835-hvs.yaml
+++ b/Documentation/devicetree/bindings/display/brcm,bcm2835-hvs.yaml
@@ -13,6 +13,7 @@ properties:
   compatible:
     enum:
       - brcm,bcm2711-hvs
+      - brcm,bcm2712-hvs
       - brcm,bcm2835-hvs
 
   reg:
@@ -36,7 +37,9 @@ if:
   properties:
     compatible:
       contains:
-        const: brcm,bcm2711-hvs
+        enum:
+          - brcm,bcm2711-hvs
+          - brcm,bcm2712-hvs
 
 then:
   required:
