// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "wavlink,ws-wn572hp3-4g", "mediatek,mt7621-soc";
	model = "Wavlink WS-WN572HP3 4G";

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	aliases {
		label-mac-device = &wifi1;
		led-boot = &led_status_blue;
		led-failsafe = &led_status_blue;
		led-running = &led_status_blue;
		led-upgrade = &led_status_blue;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset Button";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		rssihigh {
			label = "blue:rssihigh";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		rssimedium {
			label = "blue:rssimedium";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};

		rssilow {
			label = "blue:rssilow";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		led_status_blue: status_blue {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		// gpio 15 would be Quectels PWRKEY if used
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <40000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "config";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					eeprom_factory_0: eeprom@0 {
						reg = <0x0 0x400>;
					};

					eeprom_factory_8000: eeprom@8000 {
						reg = <0x8000 0x4da8>;
					};

					macaddr_factory_e000: macaddr@e000 {
						reg = <0xe000 0x6>;
					};

					macaddr_factory_e006: macaddr@e006 {
						reg = <0xe006 0x6>;
					};
				};
			};

			partition@50000 {
				compatible = "denx,fit";
				label = "firmware";
				reg = <0x50000 0xf30000>;
			};

			partition@f00000 {
				label = "vendor";
				reg = <0xf80000 0x80000>;
				read-only;
			};
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	mt76@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		ieee80211-freq-limit = <2400000 2500000>;
		nvmem-cells = <&eeprom_factory_0>;
		nvmem-cell-names = "eeprom";
	};
};

&pcie1 {
	wifi1: mt76@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		ieee80211-freq-limit = <5000000 6000000>;
		nvmem-cells = <&eeprom_factory_8000>;
		nvmem-cell-names = "eeprom";
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_e000>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy4>;

	nvmem-cells = <&macaddr_factory_e006>;
	nvmem-cell-names = "mac-address";
};

&mdio {
	ethphy4: ethernet-phy@4 {
		reg = <4>;
	};
};

&switch0 {
	ports {
		port@1 {
			status = "okay";
			label = "lan";
		};
	};
};

&state_default {
	gpio {
		groups = "wdt";
		function = "gpio";
	};
};
