From 6c94e0184e56f9e9f1f5d5f54b20758433e498d2 Mon Sep 17 00:00:00 2001
From: Christian 'Ansuel' Marangi <ansuelsmth@gmail.com>
Date: Wed, 15 Jun 2022 16:47:09 +0200
Subject: [PATCH 1/2] ARM: dts: qcom: fix wrong nad_pins definition for ipq806x

Fix wrong nand_pings definition for bias-disable pins.

Signed-off-by: Christian 'Ansuel' Marangi <ansuelsmth@gmail.com>
---
 arch/arm/boot/dts/qcom-ipq8064.dtsi | 7 ++-----
 1 file changed, 2 insertions(+), 5 deletions(-)

--- a/arch/arm/boot/dts/qcom-ipq8064.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq8064.dtsi
@@ -599,12 +599,9 @@
 			};
 
 			nand_pins: nand_pins {
-				mux {
+				disable {
 					pins = "gpio34", "gpio35", "gpio36",
-					       "gpio37", "gpio38", "gpio39",
-					       "gpio40", "gpio41", "gpio42",
-					       "gpio43", "gpio44", "gpio45",
-					       "gpio46", "gpio47";
+					       "gpio37", "gpio38";
 					function = "nand";
 					drive-strength = <10>;
 					bias-disable;
