--- /dev/null
+++ b/drivers/net/wireless/rt2x00/rt2x00eeprom.c
@@ -0,0 +1,98 @@
+/*
+	Copyright (C) 2004 - 2009 Ivo van Doorn <IvDoorn@gmail.com>
+	Copyright (C) 2004 - 2009 Gertjan van Wingerde <gwingerde@gmail.com>
+	<http://rt2x00.serialmonkey.com>
+
+	This program is free software; you can redistribute it and/or modify
+	it under the terms of the GNU General Public License as published by
+	the Free Software Foundation; either version 2 of the License, or
+	(at your option) any later version.
+
+	This program is distributed in the hope that it will be useful,
+	but WITHOUT ANY WARRANTY; without even the implied warranty of
+	MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
+	GNU General Public License for more details.
+
+	You should have received a copy of the GNU General Public License
+	along with this program; if not, write to the
+	Free Software Foundation, Inc.,
+	59 Temple Place - Suite 330, Boston, MA 02111-1307, USA.
+ */
+
+/*
+	Module: rt2x00lib
+	Abstract: rt2x00 eeprom file loading routines.
+ */
+
+#include <linux/kernel.h>
+#include <linux/module.h>
+
+#include "rt2x00.h"
+#include "rt2x00lib.h"
+
+static int rt2x00lib_request_eeprom_file(struct rt2x00_dev *rt2x00dev)
+{
+	const struct firmware *ee;
+	char *ee_name;
+	int retval;
+
+	ee_name = rt2x00dev->ops->lib->get_eeprom_file_name(rt2x00dev);
+	if (!ee_name) {
+		ERROR(rt2x00dev,
+		      "Invalid EEPROM filename.\n"
+		      "Please file bug report to %s.\n", DRV_PROJECT);
+		return -EINVAL;
+	}
+
+	INFO(rt2x00dev, "Loading EEPROM data from '%s'.\n", ee_name);
+
+	retval = request_firmware(&ee, ee_name, rt2x00dev->dev);
+	if (retval) {
+		ERROR(rt2x00dev, "Failed to request EEPROM.\n");
+		return retval;
+	}
+
+	if (!ee || !ee->size || !ee->data) {
+		ERROR(rt2x00dev, "Failed to read EEPROM file.\n");
+		retval = -ENOENT;
+		goto err_exit;
+	}
+
+	if (ee->size != rt2x00dev->ops->eeprom_size) {
+		ERROR(rt2x00dev,
+		      "EEPROM file size is invalid, it should be %d bytes\n",
+		      rt2x00dev->ops->eeprom_size);
+		retval = -EINVAL;
+		goto err_release_ee;
+	}
+
+	rt2x00dev->eeprom_file = ee;
+	return 0;
+
+err_release_ee:
+	release_firmware(ee);
+err_exit:
+	return retval;
+}
+
+int rt2x00lib_load_eeprom_file(struct rt2x00_dev *rt2x00dev)
+{
+	int retval;
+
+	if (!test_bit(REQUIRE_EEPROM_FILE, &rt2x00dev->cap_flags))
+		return 0;
+
+	if (!rt2x00dev->eeprom_file) {
+		retval = rt2x00lib_request_eeprom_file(rt2x00dev);
+		if (retval)
+			return retval;
+	}
+
+	return 0;
+}
+
+void rt2x00lib_free_eeprom_file(struct rt2x00_dev *rt2x00dev)
+{
+	release_firmware(rt2x00dev->eeprom_file);
+	rt2x00dev->eeprom_file = NULL;
+}
--- a/drivers/net/wireless/rt2x00/rt2x00.h
+++ b/drivers/net/wireless/rt2x00/rt2x00.h
@@ -560,6 +560,7 @@ struct rt2x00lib_ops {
 			       const u8 *data, const size_t len);
 	int (*load_firmware) (struct rt2x00_dev *rt2x00dev,
 			      const u8 *data, const size_t len);
+	char *(*get_eeprom_file_name) (struct rt2x00_dev *rt2x00dev);
 
 	/*
 	 * Device initialization/deinitialization handlers.
@@ -721,6 +722,7 @@ enum rt2x00_capability_flags {
 	REQUIRE_SW_SEQNO,
 	REQUIRE_HT_TX_DESC,
 	REQUIRE_PS_AUTOWAKE,
+	REQUIRE_EEPROM_FILE,
 
 	/*
 	 * Capabilities
@@ -976,6 +978,11 @@ struct rt2x00_dev {
 	const struct firmware *fw;
 
 	/*
+	 * EEPROM image.
+	 */
+	const struct firmware *eeprom_file;
+
+	/*
 	 * FIFO for storing tx status reports between isr and tasklet.
 	 */
 	DECLARE_KFIFO_PTR(txstatus_fifo, u32);
--- a/drivers/net/wireless/rt2x00/rt2x00lib.h
+++ b/drivers/net/wireless/rt2x00/rt2x00lib.h
@@ -322,6 +322,22 @@ static inline void rt2x00lib_free_firmwa
 #endif /* CONFIG_RT2X00_LIB_FIRMWARE */
 
 /*
+ * EEPROM file handlers.
+ */
+#ifdef CONFIG_RT2X00_LIB_EEPROM
+int rt2x00lib_load_eeprom_file(struct rt2x00_dev *rt2x00dev);
+void rt2x00lib_free_eeprom_file(struct rt2x00_dev *rt2x00dev);
+#else
+static inline int rt2x00lib_load_eeprom_file(struct rt2x00_dev *rt2x00dev)
+{
+	return 0;
+}
+static inline void rt2x00lib_free_eeprom_file(struct rt2x00_dev *rt2x00dev)
+{
+}
+#endif /* CONFIG_RT2X00_LIB_EEPROM_FILE */
+
+/*
  * Debugfs handlers.
  */
 #ifdef CONFIG_RT2X00_LIB_DEBUGFS
--- a/drivers/net/wireless/rt2x00/Kconfig
+++ b/drivers/net/wireless/rt2x00/Kconfig
@@ -60,6 +60,7 @@ config RT2800PCI
 	select RT2X00_LIB_PCI if PCI
 	select RT2X00_LIB_SOC if RALINK_RT288X || RALINK_RT305X
 	select RT2X00_LIB_FIRMWARE
+	select RT2X00_LIB_EEPROM
 	select RT2X00_LIB_CRYPTO
 	select CRC_CCITT
 	select EEPROM_93CX6
@@ -212,6 +213,9 @@ config RT2X00_LIB_FIRMWARE
 config RT2X00_LIB_CRYPTO
 	boolean
 
+config RT2X00_LIB_EEPROM
+	boolean
+
 config RT2X00_LIB_LEDS
 	boolean
 	default y if (RT2X00_LIB=y && LEDS_CLASS=y) || (RT2X00_LIB=m && LEDS_CLASS!=n)
--- a/drivers/net/wireless/rt2x00/Makefile
+++ b/drivers/net/wireless/rt2x00/Makefile
@@ -7,6 +7,7 @@ rt2x00lib-$(CONFIG_RT2X00_LIB_DEBUGFS)	+
 rt2x00lib-$(CONFIG_RT2X00_LIB_CRYPTO)	+= rt2x00crypto.o
 rt2x00lib-$(CONFIG_RT2X00_LIB_FIRMWARE)	+= rt2x00firmware.o
 rt2x00lib-$(CONFIG_RT2X00_LIB_LEDS)	+= rt2x00leds.o
+rt2x00lib-$(CONFIG_RT2X00_LIB_EEPROM)	+= rt2x00eeprom.o
 
 obj-$(CONFIG_RT2X00_LIB)		+= rt2x00lib.o
 obj-$(CONFIG_RT2X00_LIB_PCI)		+= rt2x00pci.o
--- a/drivers/net/wireless/rt2x00/rt2800pci.c
+++ b/drivers/net/wireless/rt2x00/rt2800pci.c
@@ -84,20 +84,10 @@ static void rt2800pci_mcu_status(struct 
 	rt2x00pci_register_write(rt2x00dev, H2M_MAILBOX_CID, ~0);
 }
 
-#if defined(CONFIG_RALINK_RT288X) || defined(CONFIG_RALINK_RT305X)
 static void rt2800pci_read_eeprom_soc(struct rt2x00_dev *rt2x00dev)
 {
-	void __iomem *base_addr = ioremap(0x1F040000, EEPROM_SIZE);
-
-	memcpy_fromio(rt2x00dev->eeprom, base_addr, EEPROM_SIZE);
-
-	iounmap(base_addr);
+	memcpy(rt2x00dev->eeprom, rt2x00dev->eeprom_file->data, EEPROM_SIZE);
 }
-#else
-static inline void rt2800pci_read_eeprom_soc(struct rt2x00_dev *rt2x00dev)
-{
-}
-#endif /* CONFIG_RALINK_RT288X || CONFIG_RALINK_RT305X */
 
 #ifdef CONFIG_PCI
 static void rt2800pci_eepromregister_read(struct eeprom_93cx6 *eeprom)
@@ -317,6 +307,20 @@ static int rt2800pci_write_firmware(stru
 }
 
 /*
+ * EEPROM file functions.
+ */
+static char *rt2800pci_get_eeprom_file_name(struct rt2x00_dev *rt2x00dev)
+{
+	struct rt2x00_platform_data *pdata;
+
+	pdata = rt2x00dev->dev->platform_data;
+	if (pdata)
+		return pdata->eeprom_file_name;
+
+	return NULL;
+}
+
+/*
  * Initialization functions.
  */
 static bool rt2800pci_get_entry_state(struct queue_entry *entry)
@@ -1159,6 +1163,7 @@ static const struct rt2x00lib_ops rt2800
 	.get_firmware_name	= rt2800pci_get_firmware_name,
 	.check_firmware		= rt2800_check_firmware,
 	.load_firmware		= rt2800_load_firmware,
+	.get_eeprom_file_name   = rt2800pci_get_eeprom_file_name,
 	.initialize		= rt2x00pci_initialize,
 	.uninitialize		= rt2x00pci_uninitialize,
 	.get_entry_state	= rt2800pci_get_entry_state,
--- a/drivers/net/wireless/rt2x00/rt2x00dev.c
+++ b/drivers/net/wireless/rt2x00/rt2x00dev.c
@@ -1163,6 +1163,10 @@ int rt2x00lib_probe_dev(struct rt2x00_de
 
 	rt2x00dev->hw->wiphy->flags |= WIPHY_FLAG_IBSS_RSN;
 
+	retval = rt2x00lib_load_eeprom_file(rt2x00dev);
+	if (retval)
+		goto exit;
+
 	/*
 	 * Initialize work.
 	 */
@@ -1287,6 +1291,11 @@ void rt2x00lib_remove_dev(struct rt2x00_
 	 */
 	if (rt2x00dev->drv_data)
 		kfree(rt2x00dev->drv_data);
+
+	/*
+	 * Free EEPROM image.
+	 */
+	rt2x00lib_free_eeprom_file(rt2x00dev);
 }
 EXPORT_SYMBOL_GPL(rt2x00lib_remove_dev);
 
--- a/drivers/net/wireless/rt2x00/rt2x00soc.c
+++ b/drivers/net/wireless/rt2x00/rt2x00soc.c
@@ -94,6 +94,7 @@ int rt2x00soc_probe(struct platform_devi
 	rt2x00dev->hw = hw;
 	rt2x00dev->irq = platform_get_irq(pdev, 0);
 	rt2x00dev->name = pdev->dev.driver->name;
+	set_bit(REQUIRE_EEPROM_FILE, &rt2x00dev->cap_flags);
 
 	rt2x00_set_chip_intf(rt2x00dev, RT2X00_CHIP_INTF_SOC);
 
