From 68368e80b4db83afe39664a7d43c8b5c7b8ac3b4 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Sun, 24 Jun 2012 13:49:33 +0200
Subject: [PATCH 21/34] MIPS: ath79: add QCA955X specific glue to ath79_device_reset_{set,clear}

---
 arch/mips/ath79/common.c |    6 ++++--
 1 files changed, 4 insertions(+), 2 deletions(-)

--- a/arch/mips/ath79/common.c
+++ b/arch/mips/ath79/common.c
@@ -70,7 +70,8 @@ void ath79_device_reset_set(u32 mask)
 		reg = AR913X_RESET_REG_RESET_MODULE;
 	else if (soc_is_ar933x())
 		reg = AR933X_RESET_REG_RESET_MODULE;
-	else if (soc_is_ar934x())
+	else if (soc_is_ar934x() ||
+		 soc_is_qca955x())
 		reg = AR934X_RESET_REG_RESET_MODULE;
 	else
 		BUG();
@@ -96,7 +97,8 @@ void ath79_device_reset_clear(u32 mask)
 		reg = AR913X_RESET_REG_RESET_MODULE;
 	else if (soc_is_ar933x())
 		reg = AR933X_RESET_REG_RESET_MODULE;
-	else if (soc_is_ar934x())
+	else if (soc_is_ar934x() ||
+		 soc_is_qca955x())
 		reg = AR934X_RESET_REG_RESET_MODULE;
 	else
 		BUG();
