From 41ee87b6ddd525fab54e21ede506f2084bcabed3 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <florian@openwrt.org>
Date: Wed, 25 Jan 2012 17:39:52 +0100
Subject: [PATCH 14/63] MIPS: BCM63XX: fix BCM6368 IPSec clock bit

The IPsec clock bit is 18 and not 17.

Signed-off-by: Florian Fainelli <florian@openwrt.org>
---
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h
@@ -99,7 +99,7 @@
 #define CKCTL_6368_USBH_EN		(1 << 15)
 #define CKCTL_6368_DISABLE_GLESS_EN	(1 << 16)
 #define CKCTL_6368_NAND_EN		(1 << 17)
-#define CKCTL_6368_IPSEC_EN		(1 << 17)
+#define CKCTL_6368_IPSEC_EN		(1 << 18)
 
 #define CKCTL_6368_ALL_SAFE_EN		(CKCTL_6368_SWPKT_USB_EN |	\
 					CKCTL_6368_SWPKT_SAR_EN |	\
