From 6d5c5bb13db3fd8e3dd0b82742b3957f41a4a3ac Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Thu, 24 May 2012 20:38:58 +0200
Subject: [PATCH] bcm63xx_enet: reset port link state in bcm_enetsw_open

bcm_enetsw_open disables all ports, but does not reset their link state.
This results in connected ports staying disabled after a ifdown/ifup
cycle, since bcm_enetsw_phy_poll only enables them if their current state
is different from the stored link state.

Fix this by also resetting the port link state.

Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
---
 drivers/net/ethernet/broadcom/bcm63xx_enet.c |    2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/net/ethernet/broadcom/bcm63xx_enet.c
+++ b/drivers/net/ethernet/broadcom/bcm63xx_enet.c
@@ -2214,6 +2214,8 @@ static int bcm_enetsw_open(struct net_de
 		enetsw_writeb(priv, ENETSW_PTCTRL_RXDIS_MASK |
 			      ENETSW_PTCTRL_TXDIS_MASK,
 			      ENETSW_PTCTRL_REG(i));
+
+		priv->sw_port_link[i] = 0;
 	}
 
 	/* reset mib */
