From 5d0de52f8e36916485a61b820916b71b5d918e6f Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Sun, 24 Jun 2012 13:44:23 +0200
Subject: [PATCH 19/34] MIPS: ath79: add IRQ handling code for the QCA955X SoCs

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 arch/mips/ath79/irq.c                          |  110 ++++++++++++++++++++++--
 arch/mips/include/asm/mach-ath79/ar71xx_regs.h |   32 +++++++
 arch/mips/include/asm/mach-ath79/irq.h         |    9 ++-
 3 files changed, 142 insertions(+), 9 deletions(-)

--- a/arch/mips/ath79/irq.c
+++ b/arch/mips/ath79/irq.c
@@ -130,7 +130,10 @@ static void __init ath79_misc_irq_init(v
 
 	if (soc_is_ar71xx() || soc_is_ar913x())
 		ath79_misc_irq_chip.irq_mask_ack = ar71xx_misc_irq_mask;
-	else if (soc_is_ar724x() || soc_is_ar933x() || soc_is_ar934x())
+	else if (soc_is_ar724x() ||
+		 soc_is_ar933x() ||
+		 soc_is_ar934x() ||
+		 soc_is_qca955x())
 		ath79_misc_irq_chip.irq_ack = ar724x_misc_irq_ack;
 	else
 		BUG();
@@ -177,6 +180,88 @@ static void ar934x_ip2_irq_init(void)
 	irq_set_chained_handler(ATH79_CPU_IRQ_IP2, ar934x_ip2_irq_dispatch);
 }
 
+static void qca955x_ip2_irq_dispatch(unsigned int irq, struct irq_desc *desc)
+{
+	u32 status;
+
+	disable_irq_nosync(irq);
+
+	status = ath79_reset_rr(QCA955X_RESET_REG_EXT_INT_STATUS);
+	status &= QCA955X_EXT_INT_PCIE_RC1_ALL | QCA955X_EXT_INT_WMAC_ALL;
+
+	if (status == 0) {
+		spurious_interrupt();
+		goto enable;
+	}
+
+	if (status & QCA955X_EXT_INT_PCIE_RC1_ALL) {
+		/* TODO: flush DDR? */
+		generic_handle_irq(ATH79_IP2_IRQ(0));
+	}
+
+	if (status & QCA955X_EXT_INT_WMAC_ALL) {
+		/* TODO: flsuh DDR? */
+		generic_handle_irq(ATH79_IP2_IRQ(1));
+	}
+
+enable:
+	enable_irq(irq);
+}
+
+static void qca955x_ip3_irq_dispatch(unsigned int irq, struct irq_desc *desc)
+{
+	u32 status;
+
+	disable_irq_nosync(irq);
+
+	status = ath79_reset_rr(QCA955X_RESET_REG_EXT_INT_STATUS);
+	status &= QCA955X_EXT_INT_PCIE_RC2_ALL |
+		  QCA955X_EXT_INT_USB1 |
+		  QCA955X_EXT_INT_USB2;
+
+	if (status == 0) {
+		spurious_interrupt();
+		goto enable;
+	}
+
+	if (status & QCA955X_EXT_INT_USB1) {
+		/* TODO: flush DDR? */
+		generic_handle_irq(ATH79_IP3_IRQ(0));
+	}
+
+	if (status & QCA955X_EXT_INT_USB2) {
+		/* TODO: flsuh DDR? */
+		generic_handle_irq(ATH79_IP3_IRQ(1));
+	}
+
+	if (status & QCA955X_EXT_INT_PCIE_RC2_ALL) {
+		/* TODO: flush DDR? */
+		generic_handle_irq(ATH79_IP3_IRQ(2));
+	}
+
+enable:
+	enable_irq(irq);
+}
+
+static void qca955x_irq_init(void)
+{
+	int i;
+
+	for (i = ATH79_IP2_IRQ_BASE;
+	     i < ATH79_IP2_IRQ_BASE + ATH79_IP2_IRQ_COUNT; i++)
+		irq_set_chip_and_handler(i, &dummy_irq_chip,
+					 handle_level_irq);
+
+	irq_set_chained_handler(ATH79_CPU_IRQ_IP2, qca955x_ip2_irq_dispatch);
+
+	for (i = ATH79_IP3_IRQ_BASE;
+	     i < ATH79_IP3_IRQ_BASE + ATH79_IP3_IRQ_COUNT; i++)
+		irq_set_chip_and_handler(i, &dummy_irq_chip,
+					 handle_level_irq);
+
+	irq_set_chained_handler(ATH79_CPU_IRQ_IP3, qca955x_ip3_irq_dispatch);
+}
+
 asmlinkage void plat_irq_dispatch(void)
 {
 	unsigned long pending;
@@ -212,6 +297,17 @@ asmlinkage void plat_irq_dispatch(void)
  * Issue a flush in the handlers to ensure that the driver sees
  * the update.
  */
+
+static void ath79_default_ip2_handler(void)
+{
+	do_IRQ(ATH79_CPU_IRQ_IP2);
+}
+
+static void ath79_default_ip3_handler(void)
+{
+	do_IRQ(ATH79_CPU_IRQ_USB);
+}
+
 static void ar71xx_ip2_handler(void)
 {
 	ath79_ddr_wb_flush(AR71XX_DDR_REG_FLUSH_PCI);
@@ -236,11 +332,6 @@ static void ar933x_ip2_handler(void)
 	do_IRQ(ATH79_CPU_IRQ_IP2);
 }
 
-static void ar934x_ip2_handler(void)
-{
-	do_IRQ(ATH79_CPU_IRQ_IP2);
-}
-
 static void ar71xx_ip3_handler(void)
 {
 	ath79_ddr_wb_flush(AR71XX_DDR_REG_FLUSH_USB);
@@ -286,8 +377,11 @@ void __init arch_init_irq(void)
 		ath79_ip2_handler = ar933x_ip2_handler;
 		ath79_ip3_handler = ar933x_ip3_handler;
 	} else if (soc_is_ar934x()) {
-		ath79_ip2_handler = ar934x_ip2_handler;
+		ath79_ip2_handler = ath79_default_ip2_handler;
 		ath79_ip3_handler = ar934x_ip3_handler;
+	} else if (soc_is_qca955x()) {
+		ath79_ip2_handler = ath79_default_ip2_handler;
+		ath79_ip3_handler = ath79_default_ip3_handler;
 	} else {
 		BUG();
 	}
@@ -298,4 +392,6 @@ void __init arch_init_irq(void)
 
 	if (soc_is_ar934x())
 		ar934x_ip2_irq_init();
+	else if (soc_is_qca955x())
+		qca955x_irq_init();
 }
--- a/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
+++ b/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
@@ -298,6 +298,7 @@
 #define AR934X_RESET_REG_PCIE_WMAC_INT_STATUS	0xac
 
 #define QCA955X_RESET_REG_BOOTSTRAP		0xb0
+#define QCA955X_RESET_REG_EXT_INT_STATUS	0xac
 
 #define MISC_INT_ETHSW			BIT(12)
 #define MISC_INT_TIMER4			BIT(10)
@@ -396,6 +397,37 @@
 	 AR934X_PCIE_WMAC_INT_PCIE_RC1 | AR934X_PCIE_WMAC_INT_PCIE_RC2 | \
 	 AR934X_PCIE_WMAC_INT_PCIE_RC3)
 
+#define QCA955X_EXT_INT_WMAC_MISC		BIT(0)
+#define QCA955X_EXT_INT_WMAC_TX			BIT(1)
+#define QCA955X_EXT_INT_WMAC_RXLP		BIT(2)
+#define QCA955X_EXT_INT_WMAC_RXHP		BIT(3)
+#define QCA955X_EXT_INT_PCIE_RC1		BIT(4)
+#define QCA955X_EXT_INT_PCIE_RC1_INT0		BIT(5)
+#define QCA955X_EXT_INT_PCIE_RC1_INT1		BIT(6)
+#define QCA955X_EXT_INT_PCIE_RC1_INT2		BIT(7)
+#define QCA955X_EXT_INT_PCIE_RC1_INT3		BIT(8)
+#define QCA955X_EXT_INT_PCIE_RC2		BIT(12)
+#define QCA955X_EXT_INT_PCIE_RC2_INT0		BIT(13)
+#define QCA955X_EXT_INT_PCIE_RC2_INT1		BIT(14)
+#define QCA955X_EXT_INT_PCIE_RC2_INT2		BIT(15)
+#define QCA955X_EXT_INT_PCIE_RC2_INT3		BIT(16)
+#define QCA955X_EXT_INT_USB1			BIT(24)
+#define QCA955X_EXT_INT_USB2			BIT(28)
+
+#define QCA955X_EXT_INT_WMAC_ALL \
+	(QCA955X_EXT_INT_WMAC_MISC | QCA955X_EXT_INT_WMAC_TX | \
+	 QCA955X_EXT_INT_WMAC_RXLP | QCA955X_EXT_INT_WMAC_RXHP)
+
+#define QCA955X_EXT_INT_PCIE_RC1_ALL \
+	(QCA955X_EXT_INT_PCIE_RC1 | QCA955X_EXT_INT_PCIE_RC1_INT0 | \
+	 QCA955X_EXT_INT_PCIE_RC1_INT1 | QCA955X_EXT_INT_PCIE_RC1_INT2 | \
+	 QCA955X_EXT_INT_PCIE_RC1_INT3)
+
+#define QCA955X_EXT_INT_PCIE_RC2_ALL \
+	(QCA955X_EXT_INT_PCIE_RC2 | QCA955X_EXT_INT_PCIE_RC2_INT0 | \
+	 QCA955X_EXT_INT_PCIE_RC2_INT1 | QCA955X_EXT_INT_PCIE_RC2_INT2 | \
+	 QCA955X_EXT_INT_PCIE_RC2_INT3)
+
 #define REV_ID_MAJOR_MASK		0xfff0
 #define REV_ID_MAJOR_AR71XX		0x00a0
 #define REV_ID_MAJOR_AR913X		0x00b0
--- a/arch/mips/include/asm/mach-ath79/irq.h
+++ b/arch/mips/include/asm/mach-ath79/irq.h
@@ -10,7 +10,7 @@
 #define __ASM_MACH_ATH79_IRQ_H
 
 #define MIPS_CPU_IRQ_BASE	0
-#define NR_IRQS			48
+#define NR_IRQS			51
 
 #define ATH79_MISC_IRQ_BASE	8
 #define ATH79_MISC_IRQ_COUNT	32
@@ -23,8 +23,13 @@
 #define ATH79_IP2_IRQ_COUNT	2
 #define ATH79_IP2_IRQ(_x)	(ATH79_IP2_IRQ_BASE + (_x))
 
+#define ATH79_IP3_IRQ_BASE	(ATH79_IP2_IRQ_BASE + ATH79_IP2_IRQ_COUNT)
+#define ATH79_IP3_IRQ_COUNT     3
+#define ATH79_IP3_IRQ(_x)       (ATH79_IP3_IRQ_BASE + (_x))
+
 #define ATH79_CPU_IRQ_IP2	(MIPS_CPU_IRQ_BASE + 2)
-#define ATH79_CPU_IRQ_USB	(MIPS_CPU_IRQ_BASE + 3)
+#define ATH79_CPU_IRQ_IP3	(MIPS_CPU_IRQ_BASE + 3)
+#define ATH79_CPU_IRQ_USB	ATH79_CPU_IRQ_IP3
 #define ATH79_CPU_IRQ_GE0	(MIPS_CPU_IRQ_BASE + 4)
 #define ATH79_CPU_IRQ_GE1	(MIPS_CPU_IRQ_BASE + 5)
 #define ATH79_CPU_IRQ_MISC	(MIPS_CPU_IRQ_BASE + 6)
