--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -308,4 +308,11 @@ config LEDS_TRIGGER_MORSE
 	tristate "LED Morse Trigger"
 	depends on LEDS_TRIGGERS
 
+config LEDS_TRIGGER_NETDEV
+	tristate "LED Netdev Trigger"
+	depends on NET && LEDS_TRIGGERS
+	help
+	  This allows LEDs to be controlled by network device activity.
+	  If unsure, say Y.
+
 endif # NEW_LEDS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -41,3 +41,4 @@ obj-$(CONFIG_LEDS_TRIGGER_BACKLIGHT)	+=
 obj-$(CONFIG_LEDS_TRIGGER_GPIO)		+= ledtrig-gpio.o
 obj-$(CONFIG_LEDS_TRIGGER_DEFAULT_ON)	+= ledtrig-default-on.o
 obj-$(CONFIG_LEDS_TRIGGER_MORSE)	+= ledtrig-morse.o
+obj-$(CONFIG_LEDS_TRIGGER_NETDEV)	+= ledtrig-netdev.o
