--- a/drivers/net/phy/Kconfig
+++ b/drivers/net/phy/Kconfig
@@ -13,6 +13,16 @@ menuconfig PHYLIB
 
 if PHYLIB
 
+config SWCONFIG
+	tristate "Switch configuration API"
+	---help---
+	  Switch configuration API using netlink. This allows
+	  you to configure the VLAN features of certain switches.
+
+config SWCONFIG_LEDS
+	bool "Switch LED trigger support"
+	depends on (SWCONFIG && LEDS_TRIGGERS)
+
 comment "MII PHY device drivers"
 
 config MARVELL_PHY
--- a/drivers/net/phy/Makefile
+++ b/drivers/net/phy/Makefile
@@ -3,6 +3,7 @@
 libphy-objs			:= phy.o phy_device.o mdio_bus.o
 
 obj-$(CONFIG_PHYLIB)		+= libphy.o
+obj-$(CONFIG_SWCONFIG)		+= swconfig.o
 obj-$(CONFIG_MARVELL_PHY)	+= marvell.o
 obj-$(CONFIG_DAVICOM_PHY)	+= davicom.o
 obj-$(CONFIG_CICADA_PHY)	+= cicada.o
