--- a/drivers/ssb/b43_pci_bridge.c
+++ b/drivers/ssb/b43_pci_bridge.c
@@ -5,12 +5,13 @@
  * because of its small size we include it in the SSB core
  * instead of creating a standalone module.
  *
- * Copyright 2007  Michael Buesch <mb@bu3sch.de>
+ * Copyright 2007  Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
 
 #include <linux/pci.h>
+#include <linux/module.h>
 #include <linux/ssb/ssb.h>
 
 #include "ssb_private.h"
--- a/drivers/ssb/driver_chipcommon.c
+++ b/drivers/ssb/driver_chipcommon.c
@@ -3,7 +3,7 @@
  * Broadcom ChipCommon core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
--- a/drivers/ssb/driver_chipcommon_pmu.c
+++ b/drivers/ssb/driver_chipcommon_pmu.c
@@ -2,7 +2,7 @@
  * Sonics Silicon Backplane
  * Broadcom ChipCommon Power Management Unit driver
  *
- * Copyright 2009, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2009, Michael Buesch <m@bues.ch>
  * Copyright 2007, Broadcom Corporation
  *
  * Licensed under the GNU/GPL. See COPYING for details.
@@ -12,6 +12,9 @@
 #include <linux/ssb/ssb_regs.h>
 #include <linux/ssb/ssb_driver_chipcommon.h>
 #include <linux/delay.h>
+#ifdef CONFIG_BCM47XX
+#include <asm/mach-bcm47xx/nvram.h>
+#endif
 
 #include "ssb_private.h"
 
@@ -91,10 +94,6 @@ static void ssb_pmu0_pllinit_r0(struct s
 	u32 pmuctl, tmp, pllctl;
 	unsigned int i;
 
-	if ((bus->chip_id == 0x5354) && !crystalfreq) {
-		/* The 5354 crystal freq is 25MHz */
-		crystalfreq = 25000;
-	}
 	if (crystalfreq)
 		e = pmu0_plltab_find_entry(crystalfreq);
 	if (!e)
@@ -320,7 +319,11 @@ static void ssb_pmu_pll_init(struct ssb_
 	u32 crystalfreq = 0; /* in kHz. 0 = keep default freq. */
 
 	if (bus->bustype == SSB_BUSTYPE_SSB) {
-		/* TODO: The user may override the crystal frequency. */
+#ifdef CONFIG_BCM47XX
+		char buf[20];
+		if (nvram_getenv("xtalfreq", buf, sizeof(buf)) >= 0)
+			crystalfreq = simple_strtoul(buf, NULL, 0);
+#endif
 	}
 
 	switch (bus->chip_id) {
@@ -329,7 +332,11 @@ static void ssb_pmu_pll_init(struct ssb_
 		ssb_pmu1_pllinit_r0(cc, crystalfreq);
 		break;
 	case 0x4328:
+		ssb_pmu0_pllinit_r0(cc, crystalfreq);
+		break;
 	case 0x5354:
+		if (crystalfreq == 0)
+			crystalfreq = 25000;
 		ssb_pmu0_pllinit_r0(cc, crystalfreq);
 		break;
 	case 0x4322:
@@ -417,9 +424,9 @@ static void ssb_pmu_resources_init(struc
 	u32 min_msk = 0, max_msk = 0;
 	unsigned int i;
 	const struct pmu_res_updown_tab_entry *updown_tab = NULL;
-	unsigned int updown_tab_size;
+	unsigned int updown_tab_size = 0;
 	const struct pmu_res_depend_tab_entry *depend_tab = NULL;
-	unsigned int depend_tab_size;
+	unsigned int depend_tab_size = 0;
 
 	switch (bus->chip_id) {
 	case 0x4312:
@@ -606,3 +613,34 @@ void ssb_pmu_set_ldo_paref(struct ssb_ch
 
 EXPORT_SYMBOL(ssb_pmu_set_ldo_voltage);
 EXPORT_SYMBOL(ssb_pmu_set_ldo_paref);
+
+u32 ssb_pmu_get_cpu_clock(struct ssb_chipcommon *cc)
+{
+	struct ssb_bus *bus = cc->dev->bus;
+
+	switch (bus->chip_id) {
+	case 0x5354:
+		/* 5354 chip uses a non programmable PLL of frequency 240MHz */
+		return 240000000;
+	default:
+		ssb_printk(KERN_ERR PFX
+			   "ERROR: PMU cpu clock unknown for device %04X\n",
+			   bus->chip_id);
+		return 0;
+	}
+}
+
+u32 ssb_pmu_get_controlclock(struct ssb_chipcommon *cc)
+{
+	struct ssb_bus *bus = cc->dev->bus;
+
+	switch (bus->chip_id) {
+	case 0x5354:
+		return 120000000;
+	default:
+		ssb_printk(KERN_ERR PFX
+			   "ERROR: PMU controlclock unknown for device %04X\n",
+			   bus->chip_id);
+		return 0;
+	}
+}
--- a/drivers/ssb/driver_extif.c
+++ b/drivers/ssb/driver_extif.c
@@ -3,7 +3,7 @@
  * Broadcom EXTIF core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  * Copyright 2006, 2007, Felix Fietkau <nbd@openwrt.org>
  * Copyright 2007, Aurelien Jarno <aurelien@aurel32.net>
  *
--- a/drivers/ssb/driver_gige.c
+++ b/drivers/ssb/driver_gige.c
@@ -3,7 +3,7 @@
  * Broadcom Gigabit Ethernet core driver
  *
  * Copyright 2008, Broadcom Corporation
- * Copyright 2008, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2008, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -106,8 +106,9 @@ void gige_pcicfg_write32(struct ssb_gige
 	gige_write32(dev, SSB_GIGE_PCICFG + offset, value);
 }
 
-static int ssb_gige_pci_read_config(struct pci_bus *bus, unsigned int devfn,
-				    int reg, int size, u32 *val)
+static int __devinit ssb_gige_pci_read_config(struct pci_bus *bus,
+					      unsigned int devfn, int reg,
+					      int size, u32 *val)
 {
 	struct ssb_gige *dev = container_of(bus->ops, struct ssb_gige, pci_ops);
 	unsigned long flags;
@@ -136,8 +137,9 @@ static int ssb_gige_pci_read_config(stru
 	return PCIBIOS_SUCCESSFUL;
 }
 
-static int ssb_gige_pci_write_config(struct pci_bus *bus, unsigned int devfn,
-				     int reg, int size, u32 val)
+static int __devinit ssb_gige_pci_write_config(struct pci_bus *bus,
+					       unsigned int devfn, int reg,
+					       int size, u32 val)
 {
 	struct ssb_gige *dev = container_of(bus->ops, struct ssb_gige, pci_ops);
 	unsigned long flags;
@@ -166,7 +168,8 @@ static int ssb_gige_pci_write_config(str
 	return PCIBIOS_SUCCESSFUL;
 }
 
-static int ssb_gige_probe(struct ssb_device *sdev, const struct ssb_device_id *id)
+static int __devinit ssb_gige_probe(struct ssb_device *sdev,
+				    const struct ssb_device_id *id)
 {
 	struct ssb_gige *dev;
 	u32 base, tmslow, tmshigh;
--- a/drivers/ssb/driver_mipscore.c
+++ b/drivers/ssb/driver_mipscore.c
@@ -3,7 +3,7 @@
  * Broadcom MIPS core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -208,6 +208,9 @@ u32 ssb_cpu_clock(struct ssb_mipscore *m
 	struct ssb_bus *bus = mcore->dev->bus;
 	u32 pll_type, n, m, rate = 0;
 
+	if (bus->chipco.capabilities & SSB_CHIPCO_CAP_PMU)
+		return ssb_pmu_get_cpu_clock(&bus->chipco);
+
 	if (bus->extif.dev) {
 		ssb_extif_get_clockcontrol(&bus->extif, &pll_type, &n, &m);
 	} else if (bus->chipco.dev) {
--- a/drivers/ssb/driver_pcicore.c
+++ b/drivers/ssb/driver_pcicore.c
@@ -3,7 +3,7 @@
  * Broadcom PCI-core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -74,7 +74,7 @@ static u32 get_cfgspace_addr(struct ssb_
 	u32 tmp;
 
 	/* We do only have one cardbus device behind the bridge. */
-	if (pc->cardbusmode && (dev >= 1))
+	if (pc->cardbusmode && (dev > 1))
 		goto out;
 
 	if (bus == 0) {
@@ -314,7 +314,7 @@ int ssb_pcicore_pcibios_map_irq(const st
 	return ssb_mips_irq(extpci_core->dev) + 2;
 }
 
-static void ssb_pcicore_init_hostmode(struct ssb_pcicore *pc)
+static void __devinit ssb_pcicore_init_hostmode(struct ssb_pcicore *pc)
 {
 	u32 val;
 
@@ -379,7 +379,7 @@ static void ssb_pcicore_init_hostmode(st
 	register_pci_controller(&ssb_pcicore_controller);
 }
 
-static int pcicore_is_in_hostmode(struct ssb_pcicore *pc)
+static int __devinit pcicore_is_in_hostmode(struct ssb_pcicore *pc)
 {
 	struct ssb_bus *bus = pc->dev->bus;
 	u16 chipid_top;
@@ -412,7 +412,7 @@ static int pcicore_is_in_hostmode(struct
  * Workarounds.
  **************************************************/
 
-static void ssb_pcicore_fix_sprom_core_index(struct ssb_pcicore *pc)
+static void __devinit ssb_pcicore_fix_sprom_core_index(struct ssb_pcicore *pc)
 {
 	u16 tmp = pcicore_read16(pc, SSB_PCICORE_SPROM(0));
 	if (((tmp & 0xF000) >> 12) != pc->dev->core_index) {
@@ -514,7 +514,7 @@ static void ssb_pcicore_pcie_setup_worka
  * Generic and Clientmode operation code.
  **************************************************/
 
-static void ssb_pcicore_init_clientmode(struct ssb_pcicore *pc)
+static void __devinit ssb_pcicore_init_clientmode(struct ssb_pcicore *pc)
 {
 	struct ssb_device *pdev = pc->dev;
 	struct ssb_bus *bus = pdev->bus;
--- a/drivers/ssb/embedded.c
+++ b/drivers/ssb/embedded.c
@@ -3,7 +3,7 @@
  * Embedded systems support code
  *
  * Copyright 2005-2008, Broadcom Corporation
- * Copyright 2006-2008, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006-2008, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
--- a/drivers/ssb/main.c
+++ b/drivers/ssb/main.c
@@ -3,7 +3,7 @@
  * Subsystem core
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -12,6 +12,7 @@
 
 #include <linux/delay.h>
 #include <linux/io.h>
+#include <linux/module.h>
 #include <linux/ssb/ssb.h>
 #include <linux/ssb/ssb_regs.h>
 #include <linux/ssb/ssb_driver_gige.h>
@@ -139,19 +140,6 @@ static void ssb_device_put(struct ssb_de
 		put_device(dev->dev);
 }
 
-static inline struct ssb_driver *ssb_driver_get(struct ssb_driver *drv)
-{
-	if (drv)
-		get_driver(&drv->drv);
-	return drv;
-}
-
-static inline void ssb_driver_put(struct ssb_driver *drv)
-{
-	if (drv)
-		put_driver(&drv->drv);
-}
-
 static int ssb_device_resume(struct device *dev)
 {
 	struct ssb_device *ssb_dev = dev_to_ssb_dev(dev);
@@ -249,11 +237,9 @@ int ssb_devices_freeze(struct ssb_bus *b
 			ssb_device_put(sdev);
 			continue;
 		}
-		sdrv = ssb_driver_get(drv_to_ssb_drv(sdev->dev->driver));
-		if (!sdrv || SSB_WARN_ON(!sdrv->remove)) {
-			ssb_device_put(sdev);
+		sdrv = drv_to_ssb_drv(sdev->dev->driver);
+		if (SSB_WARN_ON(!sdrv->remove))
 			continue;
-		}
 		sdrv->remove(sdev);
 		ctx->device_frozen[i] = 1;
 	}
@@ -292,7 +278,6 @@ int ssb_devices_thaw(struct ssb_freeze_c
 				   dev_name(sdev->dev));
 			result = err;
 		}
-		ssb_driver_put(sdrv);
 		ssb_device_put(sdev);
 	}
 
@@ -557,7 +542,7 @@ error:
 }
 
 /* Needs ssb_buses_lock() */
-static int ssb_attach_queued_buses(void)
+static int __devinit ssb_attach_queued_buses(void)
 {
 	struct ssb_bus *bus, *n;
 	int err = 0;
@@ -768,9 +753,9 @@ out:
 	return err;
 }
 
-static int ssb_bus_register(struct ssb_bus *bus,
-			    ssb_invariants_func_t get_invariants,
-			    unsigned long baseaddr)
+static int __devinit ssb_bus_register(struct ssb_bus *bus,
+				      ssb_invariants_func_t get_invariants,
+				      unsigned long baseaddr)
 {
 	int err;
 
@@ -851,8 +836,8 @@ err_disable_xtal:
 }
 
 #ifdef CONFIG_SSB_PCIHOST
-int ssb_bus_pcibus_register(struct ssb_bus *bus,
-			    struct pci_dev *host_pci)
+int __devinit ssb_bus_pcibus_register(struct ssb_bus *bus,
+				      struct pci_dev *host_pci)
 {
 	int err;
 
@@ -875,9 +860,9 @@ EXPORT_SYMBOL(ssb_bus_pcibus_register);
 #endif /* CONFIG_SSB_PCIHOST */
 
 #ifdef CONFIG_SSB_PCMCIAHOST
-int ssb_bus_pcmciabus_register(struct ssb_bus *bus,
-			       struct pcmcia_device *pcmcia_dev,
-			       unsigned long baseaddr)
+int __devinit ssb_bus_pcmciabus_register(struct ssb_bus *bus,
+					 struct pcmcia_device *pcmcia_dev,
+					 unsigned long baseaddr)
 {
 	int err;
 
@@ -897,8 +882,9 @@ EXPORT_SYMBOL(ssb_bus_pcmciabus_register
 #endif /* CONFIG_SSB_PCMCIAHOST */
 
 #ifdef CONFIG_SSB_SDIOHOST
-int ssb_bus_sdiobus_register(struct ssb_bus *bus, struct sdio_func *func,
-			     unsigned int quirks)
+int __devinit ssb_bus_sdiobus_register(struct ssb_bus *bus,
+				       struct sdio_func *func,
+				       unsigned int quirks)
 {
 	int err;
 
@@ -918,9 +904,9 @@ int ssb_bus_sdiobus_register(struct ssb_
 EXPORT_SYMBOL(ssb_bus_sdiobus_register);
 #endif /* CONFIG_SSB_PCMCIAHOST */
 
-int ssb_bus_ssbbus_register(struct ssb_bus *bus,
-			    unsigned long baseaddr,
-			    ssb_invariants_func_t get_invariants)
+int __devinit ssb_bus_ssbbus_register(struct ssb_bus *bus,
+				      unsigned long baseaddr,
+				      ssb_invariants_func_t get_invariants)
 {
 	int err;
 
@@ -1001,8 +987,8 @@ u32 ssb_calc_clock_rate(u32 plltype, u32
 	switch (plltype) {
 	case SSB_PLLTYPE_6: /* 100/200 or 120/240 only */
 		if (m & SSB_CHIPCO_CLK_T6_MMASK)
-			return SSB_CHIPCO_CLK_T6_M0;
-		return SSB_CHIPCO_CLK_T6_M1;
+			return SSB_CHIPCO_CLK_T6_M1;
+		return SSB_CHIPCO_CLK_T6_M0;
 	case SSB_PLLTYPE_1: /* 48Mhz base, 3 dividers */
 	case SSB_PLLTYPE_3: /* 25Mhz, 2 dividers */
 	case SSB_PLLTYPE_4: /* 48Mhz, 4 dividers */
@@ -1092,6 +1078,9 @@ u32 ssb_clockspeed(struct ssb_bus *bus)
 	u32 plltype;
 	u32 clkctl_n, clkctl_m;
 
+	if (bus->chipco.capabilities & SSB_CHIPCO_CAP_PMU)
+		return ssb_pmu_get_controlclock(&bus->chipco);
+
 	if (ssb_extif_available(&bus->extif))
 		ssb_extif_get_clockcontrol(&bus->extif, &plltype,
 					   &clkctl_n, &clkctl_m);
@@ -1259,13 +1248,34 @@ void ssb_device_disable(struct ssb_devic
 }
 EXPORT_SYMBOL(ssb_device_disable);
 
+/* Some chipsets need routing known for PCIe and 64-bit DMA */
+static bool ssb_dma_translation_special_bit(struct ssb_device *dev)
+{
+	u16 chip_id = dev->bus->chip_id;
+
+	if (dev->id.coreid == SSB_DEV_80211) {
+		return (chip_id == 0x4322 || chip_id == 43221 ||
+			chip_id == 43231 || chip_id == 43222);
+	}
+
+	return 0;
+}
+
 u32 ssb_dma_translation(struct ssb_device *dev)
 {
 	switch (dev->bus->bustype) {
 	case SSB_BUSTYPE_SSB:
 		return 0;
 	case SSB_BUSTYPE_PCI:
-		return SSB_PCI_DMA;
+		if (pci_is_pcie(dev->bus->host_pci) &&
+		    ssb_read32(dev, SSB_TMSHIGH) & SSB_TMSHIGH_DMA64) {
+			return SSB_PCIE_DMA_H32;
+		} else {
+			if (ssb_dma_translation_special_bit(dev))
+				return SSB_PCIE_DMA_H32;
+			else
+				return SSB_PCI_DMA;
+		}
 	default:
 		__ssb_dma_not_implemented(dev);
 	}
--- a/drivers/ssb/pci.c
+++ b/drivers/ssb/pci.c
@@ -1,7 +1,7 @@
 /*
  * Sonics Silicon Backplane PCI-Hostbus related functions.
  *
- * Copyright (C) 2005-2006 Michael Buesch <mb@bu3sch.de>
+ * Copyright (C) 2005-2006 Michael Buesch <m@bues.ch>
  * Copyright (C) 2005 Martin Langer <martin-langer@gmx.de>
  * Copyright (C) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (C) 2005 Danny van Dyk <kugelfang@gentoo.org>
@@ -331,7 +331,6 @@ static void sprom_extract_r123(struct ss
 {
 	int i;
 	u16 v;
-	s8 gain;
 	u16 loc[3];
 
 	if (out->revision == 3)			/* rev 3 moved MAC */
@@ -390,20 +389,12 @@ static void sprom_extract_r123(struct ss
 		SPEX(boardflags_hi, SSB_SPROM2_BFLHI, 0xFFFF, 0);
 
 	/* Extract the antenna gain values. */
-	gain = r123_extract_antgain(out->revision, in,
-				    SSB_SPROM1_AGAIN_BG,
-				    SSB_SPROM1_AGAIN_BG_SHIFT);
-	out->antenna_gain.ghz24.a0 = gain;
-	out->antenna_gain.ghz24.a1 = gain;
-	out->antenna_gain.ghz24.a2 = gain;
-	out->antenna_gain.ghz24.a3 = gain;
-	gain = r123_extract_antgain(out->revision, in,
-				    SSB_SPROM1_AGAIN_A,
-				    SSB_SPROM1_AGAIN_A_SHIFT);
-	out->antenna_gain.ghz5.a0 = gain;
-	out->antenna_gain.ghz5.a1 = gain;
-	out->antenna_gain.ghz5.a2 = gain;
-	out->antenna_gain.ghz5.a3 = gain;
+	out->antenna_gain.a0 = r123_extract_antgain(out->revision, in,
+						    SSB_SPROM1_AGAIN_BG,
+						    SSB_SPROM1_AGAIN_BG_SHIFT);
+	out->antenna_gain.a1 = r123_extract_antgain(out->revision, in,
+						    SSB_SPROM1_AGAIN_A,
+						    SSB_SPROM1_AGAIN_A_SHIFT);
 }
 
 /* Revs 4 5 and 8 have partially shared layout */
@@ -504,16 +495,14 @@ static void sprom_extract_r45(struct ssb
 	}
 
 	/* Extract the antenna gain values. */
-	SPEX(antenna_gain.ghz24.a0, SSB_SPROM4_AGAIN01,
+	SPEX(antenna_gain.a0, SSB_SPROM4_AGAIN01,
 	     SSB_SPROM4_AGAIN0, SSB_SPROM4_AGAIN0_SHIFT);
-	SPEX(antenna_gain.ghz24.a1, SSB_SPROM4_AGAIN01,
+	SPEX(antenna_gain.a1, SSB_SPROM4_AGAIN01,
 	     SSB_SPROM4_AGAIN1, SSB_SPROM4_AGAIN1_SHIFT);
-	SPEX(antenna_gain.ghz24.a2, SSB_SPROM4_AGAIN23,
+	SPEX(antenna_gain.a2, SSB_SPROM4_AGAIN23,
 	     SSB_SPROM4_AGAIN2, SSB_SPROM4_AGAIN2_SHIFT);
-	SPEX(antenna_gain.ghz24.a3, SSB_SPROM4_AGAIN23,
+	SPEX(antenna_gain.a3, SSB_SPROM4_AGAIN23,
 	     SSB_SPROM4_AGAIN3, SSB_SPROM4_AGAIN3_SHIFT);
-	memcpy(&out->antenna_gain.ghz5, &out->antenna_gain.ghz24,
-	       sizeof(out->antenna_gain.ghz5));
 
 	sprom_extract_r458(out, in);
 
@@ -523,7 +512,13 @@ static void sprom_extract_r45(struct ssb
 static void sprom_extract_r8(struct ssb_sprom *out, const u16 *in)
 {
 	int i;
-	u16 v;
+	u16 v, o;
+	u16 pwr_info_offset[] = {
+		SSB_SROM8_PWR_INFO_CORE0, SSB_SROM8_PWR_INFO_CORE1,
+		SSB_SROM8_PWR_INFO_CORE2, SSB_SROM8_PWR_INFO_CORE3
+	};
+	BUILD_BUG_ON(ARRAY_SIZE(pwr_info_offset) !=
+			ARRAY_SIZE(out->core_pwr_info));
 
 	/* extract the MAC address */
 	for (i = 0; i < 3; i++) {
@@ -596,16 +591,69 @@ static void sprom_extract_r8(struct ssb_
 	SPEX32(ofdm5ghpo, SSB_SPROM8_OFDM5GHPO, 0xFFFFFFFF, 0);
 
 	/* Extract the antenna gain values. */
-	SPEX(antenna_gain.ghz24.a0, SSB_SPROM8_AGAIN01,
+	SPEX(antenna_gain.a0, SSB_SPROM8_AGAIN01,
 	     SSB_SPROM8_AGAIN0, SSB_SPROM8_AGAIN0_SHIFT);
-	SPEX(antenna_gain.ghz24.a1, SSB_SPROM8_AGAIN01,
+	SPEX(antenna_gain.a1, SSB_SPROM8_AGAIN01,
 	     SSB_SPROM8_AGAIN1, SSB_SPROM8_AGAIN1_SHIFT);
-	SPEX(antenna_gain.ghz24.a2, SSB_SPROM8_AGAIN23,
+	SPEX(antenna_gain.a2, SSB_SPROM8_AGAIN23,
 	     SSB_SPROM8_AGAIN2, SSB_SPROM8_AGAIN2_SHIFT);
-	SPEX(antenna_gain.ghz24.a3, SSB_SPROM8_AGAIN23,
+	SPEX(antenna_gain.a3, SSB_SPROM8_AGAIN23,
 	     SSB_SPROM8_AGAIN3, SSB_SPROM8_AGAIN3_SHIFT);
-	memcpy(&out->antenna_gain.ghz5, &out->antenna_gain.ghz24,
-	       sizeof(out->antenna_gain.ghz5));
+
+	/* Extract cores power info info */
+	for (i = 0; i < ARRAY_SIZE(pwr_info_offset); i++) {
+		o = pwr_info_offset[i];
+		SPEX(core_pwr_info[i].itssi_2g, o + SSB_SROM8_2G_MAXP_ITSSI,
+			SSB_SPROM8_2G_ITSSI, SSB_SPROM8_2G_ITSSI_SHIFT);
+		SPEX(core_pwr_info[i].maxpwr_2g, o + SSB_SROM8_2G_MAXP_ITSSI,
+			SSB_SPROM8_2G_MAXP, 0);
+
+		SPEX(core_pwr_info[i].pa_2g[0], o + SSB_SROM8_2G_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_2g[1], o + SSB_SROM8_2G_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_2g[2], o + SSB_SROM8_2G_PA_2, ~0, 0);
+
+		SPEX(core_pwr_info[i].itssi_5g, o + SSB_SROM8_5G_MAXP_ITSSI,
+			SSB_SPROM8_5G_ITSSI, SSB_SPROM8_5G_ITSSI_SHIFT);
+		SPEX(core_pwr_info[i].maxpwr_5g, o + SSB_SROM8_5G_MAXP_ITSSI,
+			SSB_SPROM8_5G_MAXP, 0);
+		SPEX(core_pwr_info[i].maxpwr_5gh, o + SSB_SPROM8_5GHL_MAXP,
+			SSB_SPROM8_5GH_MAXP, 0);
+		SPEX(core_pwr_info[i].maxpwr_5gl, o + SSB_SPROM8_5GHL_MAXP,
+			SSB_SPROM8_5GL_MAXP, SSB_SPROM8_5GL_MAXP_SHIFT);
+
+		SPEX(core_pwr_info[i].pa_5gl[0], o + SSB_SROM8_5GL_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gl[1], o + SSB_SROM8_5GL_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gl[2], o + SSB_SROM8_5GL_PA_2, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[0], o + SSB_SROM8_5G_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[1], o + SSB_SROM8_5G_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[2], o + SSB_SROM8_5G_PA_2, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[0], o + SSB_SROM8_5GH_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[1], o + SSB_SROM8_5GH_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[2], o + SSB_SROM8_5GH_PA_2, ~0, 0);
+	}
+
+	/* Extract FEM info */
+	SPEX(fem.ghz2.tssipos, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_TSSIPOS, SSB_SROM8_FEM_TSSIPOS_SHIFT);
+	SPEX(fem.ghz2.extpa_gain, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_EXTPA_GAIN, SSB_SROM8_FEM_EXTPA_GAIN_SHIFT);
+	SPEX(fem.ghz2.pdet_range, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_PDET_RANGE, SSB_SROM8_FEM_PDET_RANGE_SHIFT);
+	SPEX(fem.ghz2.tr_iso, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_TR_ISO, SSB_SROM8_FEM_TR_ISO_SHIFT);
+	SPEX(fem.ghz2.antswlut, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_ANTSWLUT, SSB_SROM8_FEM_ANTSWLUT_SHIFT);
+
+	SPEX(fem.ghz5.tssipos, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_TSSIPOS, SSB_SROM8_FEM_TSSIPOS_SHIFT);
+	SPEX(fem.ghz5.extpa_gain, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_EXTPA_GAIN, SSB_SROM8_FEM_EXTPA_GAIN_SHIFT);
+	SPEX(fem.ghz5.pdet_range, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_PDET_RANGE, SSB_SROM8_FEM_PDET_RANGE_SHIFT);
+	SPEX(fem.ghz5.tr_iso, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_TR_ISO, SSB_SROM8_FEM_TR_ISO_SHIFT);
+	SPEX(fem.ghz5.antswlut, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_ANTSWLUT, SSB_SROM8_FEM_ANTSWLUT_SHIFT);
 
 	sprom_extract_r458(out, in);
 
@@ -734,12 +782,9 @@ out_free:
 static void ssb_pci_get_boardinfo(struct ssb_bus *bus,
 				  struct ssb_boardinfo *bi)
 {
-	pci_read_config_word(bus->host_pci, PCI_SUBSYSTEM_VENDOR_ID,
-			     &bi->vendor);
-	pci_read_config_word(bus->host_pci, PCI_SUBSYSTEM_ID,
-			     &bi->type);
-	pci_read_config_word(bus->host_pci, PCI_REVISION_ID,
-			     &bi->rev);
+	bi->vendor = bus->host_pci->subsystem_vendor;
+	bi->type = bus->host_pci->subsystem_device;
+	bi->rev = bus->host_pci->revision;
 }
 
 int ssb_pci_get_invariants(struct ssb_bus *bus,
--- a/drivers/ssb/pcihost_wrapper.c
+++ b/drivers/ssb/pcihost_wrapper.c
@@ -6,7 +6,7 @@
  * Copyright (c) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (c) 2005 Danny van Dyk <kugelfang@gentoo.org>
  * Copyright (c) 2005 Andreas Jaggi <andreas.jaggi@waterwave.ch>
- * Copyright (c) 2005-2007 Michael Buesch <mbuesch@freenet.de>
+ * Copyright (c) 2005-2007 Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -53,8 +53,8 @@ static int ssb_pcihost_resume(struct pci
 # define ssb_pcihost_resume	NULL
 #endif /* CONFIG_PM */
 
-static int ssb_pcihost_probe(struct pci_dev *dev,
-			     const struct pci_device_id *id)
+static int __devinit ssb_pcihost_probe(struct pci_dev *dev,
+				       const struct pci_device_id *id)
 {
 	struct ssb_bus *ssb;
 	int err = -ENOMEM;
@@ -110,7 +110,7 @@ static void ssb_pcihost_remove(struct pc
 	pci_set_drvdata(dev, NULL);
 }
 
-int ssb_pcihost_register(struct pci_driver *driver)
+int __devinit ssb_pcihost_register(struct pci_driver *driver)
 {
 	driver->probe = ssb_pcihost_probe;
 	driver->remove = ssb_pcihost_remove;
--- a/drivers/ssb/pcmcia.c
+++ b/drivers/ssb/pcmcia.c
@@ -3,7 +3,7 @@
  * PCMCIA-Hostbus related functions
  *
  * Copyright 2006 Johannes Berg <johannes@sipsolutions.net>
- * Copyright 2007-2008 Michael Buesch <mb@bu3sch.de>
+ * Copyright 2007-2008 Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -676,14 +676,10 @@ static int ssb_pcmcia_do_get_invariants(
 	case SSB_PCMCIA_CIS_ANTGAIN:
 		GOTO_ERROR_ON(tuple->TupleDataLen != 2,
 			"antg tpl size");
-		sprom->antenna_gain.ghz24.a0 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz24.a1 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz24.a2 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz24.a3 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz5.a0 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz5.a1 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz5.a2 = tuple->TupleData[1];
-		sprom->antenna_gain.ghz5.a3 = tuple->TupleData[1];
+		sprom->antenna_gain.a0 = tuple->TupleData[1];
+		sprom->antenna_gain.a1 = tuple->TupleData[1];
+		sprom->antenna_gain.a2 = tuple->TupleData[1];
+		sprom->antenna_gain.a3 = tuple->TupleData[1];
 		break;
 	case SSB_PCMCIA_CIS_BFLAGS:
 		GOTO_ERROR_ON((tuple->TupleDataLen != 3) &&
--- a/drivers/ssb/scan.c
+++ b/drivers/ssb/scan.c
@@ -2,7 +2,7 @@
  * Sonics Silicon Backplane
  * Bus scanning
  *
- * Copyright (C) 2005-2007 Michael Buesch <mb@bu3sch.de>
+ * Copyright (C) 2005-2007 Michael Buesch <m@bues.ch>
  * Copyright (C) 2005 Martin Langer <martin-langer@gmx.de>
  * Copyright (C) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (C) 2005 Danny van Dyk <kugelfang@gentoo.org>
@@ -310,8 +310,7 @@ int ssb_bus_scan(struct ssb_bus *bus,
 	} else {
 		if (bus->bustype == SSB_BUSTYPE_PCI) {
 			bus->chip_id = pcidev_to_chipid(bus->host_pci);
-			pci_read_config_byte(bus->host_pci, PCI_REVISION_ID,
-					     &bus->chip_rev);
+			bus->chip_rev = bus->host_pci->revision;
 			bus->chip_package = 0;
 		} else {
 			bus->chip_id = 0x4710;
@@ -319,6 +318,9 @@ int ssb_bus_scan(struct ssb_bus *bus,
 			bus->chip_package = 0;
 		}
 	}
+	ssb_printk(KERN_INFO PFX "Found chip with id 0x%04X, rev 0x%02X and "
+		   "package 0x%02X\n", bus->chip_id, bus->chip_rev,
+		   bus->chip_package);
 	if (!bus->nr_devices)
 		bus->nr_devices = chipid_to_nrcores(bus->chip_id);
 	if (bus->nr_devices > ARRAY_SIZE(bus->devices)) {
--- a/drivers/ssb/sdio.c
+++ b/drivers/ssb/sdio.c
@@ -6,7 +6,7 @@
  *
  * Based on drivers/ssb/pcmcia.c
  * Copyright 2006 Johannes Berg <johannes@sipsolutions.net>
- * Copyright 2007-2008 Michael Buesch <mb@bu3sch.de>
+ * Copyright 2007-2008 Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  *
@@ -551,14 +551,10 @@ int ssb_sdio_get_invariants(struct ssb_b
 			case SSB_SDIO_CIS_ANTGAIN:
 				GOTO_ERROR_ON(tuple->size != 2,
 					      "antg tpl size");
-				sprom->antenna_gain.ghz24.a0 = tuple->data[1];
-				sprom->antenna_gain.ghz24.a1 = tuple->data[1];
-				sprom->antenna_gain.ghz24.a2 = tuple->data[1];
-				sprom->antenna_gain.ghz24.a3 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a0 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a1 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a2 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a3 = tuple->data[1];
+				sprom->antenna_gain.a0 = tuple->data[1];
+				sprom->antenna_gain.a1 = tuple->data[1];
+				sprom->antenna_gain.a2 = tuple->data[1];
+				sprom->antenna_gain.a3 = tuple->data[1];
 				break;
 			case SSB_SDIO_CIS_BFLAGS:
 				GOTO_ERROR_ON((tuple->size != 3) &&
--- a/drivers/ssb/sprom.c
+++ b/drivers/ssb/sprom.c
@@ -2,7 +2,7 @@
  * Sonics Silicon Backplane
  * Common SPROM support routines
  *
- * Copyright (C) 2005-2008 Michael Buesch <mb@bu3sch.de>
+ * Copyright (C) 2005-2008 Michael Buesch <m@bues.ch>
  * Copyright (C) 2005 Martin Langer <martin-langer@gmx.de>
  * Copyright (C) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (C) 2005 Danny van Dyk <kugelfang@gentoo.org>
--- a/include/linux/ssb/ssb.h
+++ b/include/linux/ssb/ssb.h
@@ -16,6 +16,12 @@ struct pcmcia_device;
 struct ssb_bus;
 struct ssb_driver;
 
+struct ssb_sprom_core_pwr_info {
+	u8 itssi_2g, itssi_5g;
+	u8 maxpwr_2g, maxpwr_5gl, maxpwr_5g, maxpwr_5gh;
+	u16 pa_2g[4], pa_5gl[4], pa_5g[4], pa_5gh[4];
+};
+
 struct ssb_sprom {
 	u8 revision;
 	u8 il0mac[6];		/* MAC address for 802.11b/g */
@@ -25,8 +31,13 @@ struct ssb_sprom {
 	u8 et1phyaddr;		/* MII address for enet1 */
 	u8 et0mdcport;		/* MDIO for enet0 */
 	u8 et1mdcport;		/* MDIO for enet1 */
-	u8 board_rev;		/* Board revision number from SPROM. */
+	u16 board_rev;		/* Board revision number from SPROM. */
+	u16 board_num;		/* Board number from SPROM. */
+	u16 board_type;		/* Board type from SPROM. */
 	u8 country_code;	/* Country Code */
+	char alpha2[2];		/* Country Code as two chars like EU or US */
+	u8 leddc_on_time;	/* LED Powersave Duty Cycle On Count */
+	u8 leddc_off_time;	/* LED Powersave Duty Cycle Off Count */
 	u8 ant_available_a;	/* 2GHz antenna available bits (up to 4) */
 	u8 ant_available_bg;	/* 5GHz antenna available bits (up to 4) */
 	u16 pa0b0;
@@ -45,10 +56,10 @@ struct ssb_sprom {
 	u8 gpio1;		/* GPIO pin 1 */
 	u8 gpio2;		/* GPIO pin 2 */
 	u8 gpio3;		/* GPIO pin 3 */
-	u16 maxpwr_bg;		/* 2.4GHz Amplifier Max Power (in dBm Q5.2) */
-	u16 maxpwr_al;		/* 5.2GHz Amplifier Max Power (in dBm Q5.2) */
-	u16 maxpwr_a;		/* 5.3GHz Amplifier Max Power (in dBm Q5.2) */
-	u16 maxpwr_ah;		/* 5.8GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_bg;		/* 2.4GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_al;		/* 5.2GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_a;		/* 5.3GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_ah;		/* 5.8GHz Amplifier Max Power (in dBm Q5.2) */
 	u8 itssi_a;		/* Idle TSSI Target for A-PHY */
 	u8 itssi_bg;		/* Idle TSSI Target for B/G-PHY */
 	u8 tri2g;		/* 2.4GHz TX isolation */
@@ -59,8 +70,8 @@ struct ssb_sprom {
 	u8 txpid5gl[4];		/* 4.9 - 5.1GHz TX power index */
 	u8 txpid5g[4];		/* 5.1 - 5.5GHz TX power index */
 	u8 txpid5gh[4];		/* 5.5 - ...GHz TX power index */
-	u8 rxpo2g;		/* 2GHz RX power offset */
-	u8 rxpo5g;		/* 5GHz RX power offset */
+	s8 rxpo2g;		/* 2GHz RX power offset */
+	s8 rxpo5g;		/* 5GHz RX power offset */
 	u8 rssisav2g;		/* 2GHz RSSI params */
 	u8 rssismc2g;
 	u8 rssismf2g;
@@ -80,26 +91,104 @@ struct ssb_sprom {
 	u16 boardflags2_hi;	/* Board flags (bits 48-63) */
 	/* TODO store board flags in a single u64 */
 
+	struct ssb_sprom_core_pwr_info core_pwr_info[4];
+
 	/* Antenna gain values for up to 4 antennas
 	 * on each band. Values in dBm/4 (Q5.2). Negative gain means the
 	 * loss in the connectors is bigger than the gain. */
 	struct {
-		struct {
-			s8 a0, a1, a2, a3;
-		} ghz24;	/* 2.4GHz band */
-		struct {
-			s8 a0, a1, a2, a3;
-		} ghz5;		/* 5GHz band */
+		s8 a0, a1, a2, a3;
 	} antenna_gain;
 
-	/* TODO - add any parameters needed from rev 2, 3, 4, 5 or 8 SPROMs */
+	struct {
+		struct {
+			u8 tssipos, extpa_gain, pdet_range, tr_iso, antswlut;
+		} ghz2;
+		struct {
+			u8 tssipos, extpa_gain, pdet_range, tr_iso, antswlut;
+		} ghz5;
+	} fem;
+
+	u16 mcs2gpo[8];
+	u16 mcs5gpo[8];
+	u16 mcs5glpo[8];
+	u16 mcs5ghpo[8];
+	u8 opo;
+
+	u8 rxgainerr2ga[3];
+	u8 rxgainerr5gla[3];
+	u8 rxgainerr5gma[3];
+	u8 rxgainerr5gha[3];
+	u8 rxgainerr5gua[3];
+
+	u8 noiselvl2ga[3];
+	u8 noiselvl5gla[3];
+	u8 noiselvl5gma[3];
+	u8 noiselvl5gha[3];
+	u8 noiselvl5gua[3];
+
+	u8 regrev;
+	u8 txchain;
+	u8 rxchain;
+	u8 antswitch;
+	u16 cddpo;
+	u16 stbcpo;
+	u16 bw40po;
+	u16 bwduppo;
+
+	u8 tempthresh;
+	u8 tempoffset;
+	u16 rawtempsense;
+	u8 measpower;
+	u8 tempsense_slope;
+	u8 tempcorrx;
+	u8 tempsense_option;
+	u8 freqoffset_corr;
+	u8 iqcal_swp_dis;
+	u8 hw_iqcal_en;
+	u8 elna2g;
+	u8 elna5g;
+	u8 phycal_tempdelta;
+	u8 temps_period;
+	u8 temps_hysteresis;
+	u8 measpower1;
+	u8 measpower2;
+	u8 pcieingress_war;
+
+	/* power per rate from sromrev 9 */
+	u16 cckbw202gpo;
+	u16 cckbw20ul2gpo;
+	u32 legofdmbw202gpo;
+	u32 legofdmbw20ul2gpo;
+	u32 legofdmbw205glpo;
+	u32 legofdmbw20ul5glpo;
+	u32 legofdmbw205gmpo;
+	u32 legofdmbw20ul5gmpo;
+	u32 legofdmbw205ghpo;
+	u32 legofdmbw20ul5ghpo;
+	u32 mcsbw202gpo;
+	u32 mcsbw20ul2gpo;
+	u32 mcsbw402gpo;
+	u32 mcsbw205glpo;
+	u32 mcsbw20ul5glpo;
+	u32 mcsbw405glpo;
+	u32 mcsbw205gmpo;
+	u32 mcsbw20ul5gmpo;
+	u32 mcsbw405gmpo;
+	u32 mcsbw205ghpo;
+	u32 mcsbw20ul5ghpo;
+	u32 mcsbw405ghpo;
+	u16 mcs32po;
+	u16 legofdm40duppo;
+	u8 sar2g;
+	u8 sar5g;
 };
 
 /* Information about the PCB the circuitry is soldered on. */
 struct ssb_boardinfo {
 	u16 vendor;
 	u16 type;
-	u16 rev;
+	u8  rev;
 };
 
 
@@ -229,10 +318,9 @@ struct ssb_driver {
 #define drv_to_ssb_drv(_drv) container_of(_drv, struct ssb_driver, drv)
 
 extern int __ssb_driver_register(struct ssb_driver *drv, struct module *owner);
-static inline int ssb_driver_register(struct ssb_driver *drv)
-{
-	return __ssb_driver_register(drv, THIS_MODULE);
-}
+#define ssb_driver_register(drv) \
+	__ssb_driver_register(drv, THIS_MODULE)
+
 extern void ssb_driver_unregister(struct ssb_driver *drv);
 
 
--- a/include/linux/ssb/ssb_driver_chipcommon.h
+++ b/include/linux/ssb/ssb_driver_chipcommon.h
@@ -8,7 +8,7 @@
  * gpio interface, extbus, and support for serial and parallel flashes.
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GPL version 2. See COPYING for details.
  */
--- a/include/linux/ssb/ssb_regs.h
+++ b/include/linux/ssb/ssb_regs.h
@@ -432,6 +432,56 @@
 #define  SSB_SPROM8_RXPO2G		0x00FF	/* 2GHz RX power offset */
 #define  SSB_SPROM8_RXPO5G		0xFF00	/* 5GHz RX power offset */
 #define  SSB_SPROM8_RXPO5G_SHIFT	8
+#define SSB_SPROM8_FEM2G		0x00AE
+#define SSB_SPROM8_FEM5G		0x00B0
+#define  SSB_SROM8_FEM_TSSIPOS		0x0001
+#define  SSB_SROM8_FEM_TSSIPOS_SHIFT	0
+#define  SSB_SROM8_FEM_EXTPA_GAIN	0x0006
+#define  SSB_SROM8_FEM_EXTPA_GAIN_SHIFT	1
+#define  SSB_SROM8_FEM_PDET_RANGE	0x00F8
+#define  SSB_SROM8_FEM_PDET_RANGE_SHIFT	3
+#define  SSB_SROM8_FEM_TR_ISO		0x0700
+#define  SSB_SROM8_FEM_TR_ISO_SHIFT	8
+#define  SSB_SROM8_FEM_ANTSWLUT		0xF800
+#define  SSB_SROM8_FEM_ANTSWLUT_SHIFT	11
+#define SSB_SPROM8_THERMAL		0x00B2
+#define SSB_SPROM8_MPWR_RAWTS		0x00B4
+#define SSB_SPROM8_TS_SLP_OPT_CORRX	0x00B6
+#define SSB_SPROM8_FOC_HWIQ_IQSWP	0x00B8
+#define SSB_SPROM8_PHYCAL_TEMPDELTA	0x00BA
+
+/* There are 4 blocks with power info sharing the same layout */
+#define SSB_SROM8_PWR_INFO_CORE0	0x00C0
+#define SSB_SROM8_PWR_INFO_CORE1	0x00E0
+#define SSB_SROM8_PWR_INFO_CORE2	0x0100
+#define SSB_SROM8_PWR_INFO_CORE3	0x0120
+
+#define SSB_SROM8_2G_MAXP_ITSSI		0x00
+#define  SSB_SPROM8_2G_MAXP		0x00FF
+#define  SSB_SPROM8_2G_ITSSI		0xFF00
+#define  SSB_SPROM8_2G_ITSSI_SHIFT	8
+#define SSB_SROM8_2G_PA_0		0x02	/* 2GHz power amp settings */
+#define SSB_SROM8_2G_PA_1		0x04
+#define SSB_SROM8_2G_PA_2		0x06
+#define SSB_SROM8_5G_MAXP_ITSSI		0x08	/* 5GHz ITSSI and 5.3GHz Max Power */
+#define  SSB_SPROM8_5G_MAXP		0x00FF
+#define  SSB_SPROM8_5G_ITSSI		0xFF00
+#define  SSB_SPROM8_5G_ITSSI_SHIFT	8
+#define SSB_SPROM8_5GHL_MAXP		0x0A	/* 5.2GHz and 5.8GHz Max Power */
+#define  SSB_SPROM8_5GH_MAXP		0x00FF
+#define  SSB_SPROM8_5GL_MAXP		0xFF00
+#define  SSB_SPROM8_5GL_MAXP_SHIFT	8
+#define SSB_SROM8_5G_PA_0		0x0C	/* 5.3GHz power amp settings */
+#define SSB_SROM8_5G_PA_1		0x0E
+#define SSB_SROM8_5G_PA_2		0x10
+#define SSB_SROM8_5GL_PA_0		0x12	/* 5.2GHz power amp settings */
+#define SSB_SROM8_5GL_PA_1		0x14
+#define SSB_SROM8_5GL_PA_2		0x16
+#define SSB_SROM8_5GH_PA_0		0x18	/* 5.8GHz power amp settings */
+#define SSB_SROM8_5GH_PA_1		0x1A
+#define SSB_SROM8_5GH_PA_2		0x1C
+
+/* TODO: Make it deprecated */
 #define SSB_SPROM8_MAXP_BG		0x00C0  /* Max Power 2GHz in path 1 */
 #define  SSB_SPROM8_MAXP_BG_MASK	0x00FF  /* Mask for Max Power 2GHz */
 #define  SSB_SPROM8_ITSSI_BG		0xFF00	/* Mask for path 1 itssi_bg */
@@ -456,12 +506,53 @@
 #define SSB_SPROM8_PA1HIB0		0x00D8	/* 5.8GHz power amp settings */
 #define SSB_SPROM8_PA1HIB1		0x00DA
 #define SSB_SPROM8_PA1HIB2		0x00DC
+
 #define SSB_SPROM8_CCK2GPO		0x0140	/* CCK power offset */
 #define SSB_SPROM8_OFDM2GPO		0x0142	/* 2.4GHz OFDM power offset */
 #define SSB_SPROM8_OFDM5GPO		0x0146	/* 5.3GHz OFDM power offset */
 #define SSB_SPROM8_OFDM5GLPO		0x014A	/* 5.2GHz OFDM power offset */
 #define SSB_SPROM8_OFDM5GHPO		0x014E	/* 5.8GHz OFDM power offset */
 
+/* Values for boardflags_lo read from SPROM */
+#define SSB_BFL_BTCOEXIST		0x0001	/* implements Bluetooth coexistance */
+#define SSB_BFL_PACTRL			0x0002	/* GPIO 9 controlling the PA */
+#define SSB_BFL_AIRLINEMODE		0x0004	/* implements GPIO 13 radio disable indication */
+#define SSB_BFL_RSSI			0x0008	/* software calculates nrssi slope. */
+#define SSB_BFL_ENETSPI			0x0010	/* has ephy roboswitch spi */
+#define SSB_BFL_XTAL_NOSLOW		0x0020	/* no slow clock available */
+#define SSB_BFL_CCKHIPWR		0x0040	/* can do high power CCK transmission */
+#define SSB_BFL_ENETADM			0x0080	/* has ADMtek switch */
+#define SSB_BFL_ENETVLAN		0x0100	/* can do vlan */
+#define SSB_BFL_AFTERBURNER		0x0200	/* supports Afterburner mode */
+#define SSB_BFL_NOPCI			0x0400	/* board leaves PCI floating */
+#define SSB_BFL_FEM			0x0800	/* supports the Front End Module */
+#define SSB_BFL_EXTLNA			0x1000	/* has an external LNA */
+#define SSB_BFL_HGPA			0x2000	/* had high gain PA */
+#define SSB_BFL_BTCMOD			0x4000	/* BFL_BTCOEXIST is given in alternate GPIOs */
+#define SSB_BFL_ALTIQ			0x8000	/* alternate I/Q settings */
+
+/* Values for boardflags_hi read from SPROM */
+#define SSB_BFH_NOPA			0x0001	/* has no PA */
+#define SSB_BFH_RSSIINV			0x0002	/* RSSI uses positive slope (not TSSI) */
+#define SSB_BFH_PAREF			0x0004	/* uses the PARef LDO */
+#define SSB_BFH_3TSWITCH		0x0008	/* uses a triple throw switch shared with bluetooth */
+#define SSB_BFH_PHASESHIFT		0x0010	/* can support phase shifter */
+#define SSB_BFH_BUCKBOOST		0x0020	/* has buck/booster */
+#define SSB_BFH_FEM_BT			0x0040	/* has FEM and switch to share antenna with bluetooth */
+
+/* Values for boardflags2_lo read from SPROM */
+#define SSB_BFL2_RXBB_INT_REG_DIS	0x0001	/* external RX BB regulator present */
+#define SSB_BFL2_APLL_WAR		0x0002	/* alternative A-band PLL settings implemented */
+#define SSB_BFL2_TXPWRCTRL_EN 		0x0004	/* permits enabling TX Power Control */
+#define SSB_BFL2_2X4_DIV		0x0008	/* 2x4 diversity switch */
+#define SSB_BFL2_5G_PWRGAIN		0x0010	/* supports 5G band power gain */
+#define SSB_BFL2_PCIEWAR_OVR		0x0020	/* overrides ASPM and Clkreq settings */
+#define SSB_BFL2_CAESERS_BRD		0x0040	/* is Caesers board (unused) */
+#define SSB_BFL2_BTC3WIRE		0x0080	/* used 3-wire bluetooth coexist */
+#define SSB_BFL2_SKWRKFEM_BRD		0x0100	/* 4321mcm93 uses Skyworks FEM */
+#define SSB_BFL2_SPUR_WAR		0x0200	/* has a workaround for clock-harmonic spurs */
+#define SSB_BFL2_GPLL_WAR		0x0400	/* altenative G-band PLL settings implemented */
+
 /* Values for SSB_SPROM1_BINF_CCODE */
 enum {
 	SSB_SPROM1CCODE_WORLD = 0,
--- a/drivers/ssb/ssb_private.h
+++ b/drivers/ssb/ssb_private.h
@@ -207,4 +207,8 @@ static inline void b43_pci_ssb_bridge_ex
 }
 #endif /* CONFIG_SSB_B43_PCI_BRIDGE */
 
+/* driver_chipcommon_pmu.c */
+extern u32 ssb_pmu_get_cpu_clock(struct ssb_chipcommon *cc);
+extern u32 ssb_pmu_get_controlclock(struct ssb_chipcommon *cc);
+
 #endif /* LINUX_SSB_PRIVATE_H_ */
--- a/include/linux/ssb/ssb_driver_gige.h
+++ b/include/linux/ssb/ssb_driver_gige.h
@@ -2,6 +2,7 @@
 #define LINUX_SSB_DRIVER_GIGE_H_
 
 #include <linux/ssb/ssb.h>
+#include <linux/bug.h>
 #include <linux/pci.h>
 #include <linux/spinlock.h>
 
