--- a/drivers/ssb/driver_chipcommon.c
+++ b/drivers/ssb/driver_chipcommon.c
@@ -3,7 +3,7 @@
  * Broadcom ChipCommon core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -46,40 +46,66 @@ void ssb_chipco_set_clockmode(struct ssb
 	if (!ccdev)
 		return;
 	bus = ccdev->bus;
+
+	/* We support SLOW only on 6..9 */
+	if (ccdev->id.revision >= 10 && mode == SSB_CLKMODE_SLOW)
+		mode = SSB_CLKMODE_DYNAMIC;
+
+	if (cc->capabilities & SSB_CHIPCO_CAP_PMU)
+		return; /* PMU controls clockmode, separated function needed */
+	SSB_WARN_ON(ccdev->id.revision >= 20);
+
 	/* chipcommon cores prior to rev6 don't support dynamic clock control */
 	if (ccdev->id.revision < 6)
 		return;
-	/* chipcommon cores rev10 are a whole new ball game */
+
+	/* ChipCommon cores rev10+ need testing */
 	if (ccdev->id.revision >= 10)
 		return;
+
 	if (!(cc->capabilities & SSB_CHIPCO_CAP_PCTL))
 		return;
 
 	switch (mode) {
-	case SSB_CLKMODE_SLOW:
+	case SSB_CLKMODE_SLOW: /* For revs 6..9 only */
 		tmp = chipco_read32(cc, SSB_CHIPCO_SLOWCLKCTL);
 		tmp |= SSB_CHIPCO_SLOWCLKCTL_FSLOW;
 		chipco_write32(cc, SSB_CHIPCO_SLOWCLKCTL, tmp);
 		break;
 	case SSB_CLKMODE_FAST:
-		ssb_pci_xtal(bus, SSB_GPIO_XTAL, 1); /* Force crystal on */
-		tmp = chipco_read32(cc, SSB_CHIPCO_SLOWCLKCTL);
-		tmp &= ~SSB_CHIPCO_SLOWCLKCTL_FSLOW;
-		tmp |= SSB_CHIPCO_SLOWCLKCTL_IPLL;
-		chipco_write32(cc, SSB_CHIPCO_SLOWCLKCTL, tmp);
+		if (ccdev->id.revision < 10) {
+			ssb_pci_xtal(bus, SSB_GPIO_XTAL, 1); /* Force crystal on */
+			tmp = chipco_read32(cc, SSB_CHIPCO_SLOWCLKCTL);
+			tmp &= ~SSB_CHIPCO_SLOWCLKCTL_FSLOW;
+			tmp |= SSB_CHIPCO_SLOWCLKCTL_IPLL;
+			chipco_write32(cc, SSB_CHIPCO_SLOWCLKCTL, tmp);
+		} else {
+			chipco_write32(cc, SSB_CHIPCO_SYSCLKCTL,
+				(chipco_read32(cc, SSB_CHIPCO_SYSCLKCTL) |
+				 SSB_CHIPCO_SYSCLKCTL_FORCEHT));
+			/* udelay(150); TODO: not available in early init */
+		}
 		break;
 	case SSB_CLKMODE_DYNAMIC:
-		tmp = chipco_read32(cc, SSB_CHIPCO_SLOWCLKCTL);
-		tmp &= ~SSB_CHIPCO_SLOWCLKCTL_FSLOW;
-		tmp &= ~SSB_CHIPCO_SLOWCLKCTL_IPLL;
-		tmp &= ~SSB_CHIPCO_SLOWCLKCTL_ENXTAL;
-		if ((tmp & SSB_CHIPCO_SLOWCLKCTL_SRC) != SSB_CHIPCO_SLOWCLKCTL_SRC_XTAL)
-			tmp |= SSB_CHIPCO_SLOWCLKCTL_ENXTAL;
-		chipco_write32(cc, SSB_CHIPCO_SLOWCLKCTL, tmp);
-
-		/* for dynamic control, we have to release our xtal_pu "force on" */
-		if (tmp & SSB_CHIPCO_SLOWCLKCTL_ENXTAL)
-			ssb_pci_xtal(bus, SSB_GPIO_XTAL, 0);
+		if (ccdev->id.revision < 10) {
+			tmp = chipco_read32(cc, SSB_CHIPCO_SLOWCLKCTL);
+			tmp &= ~SSB_CHIPCO_SLOWCLKCTL_FSLOW;
+			tmp &= ~SSB_CHIPCO_SLOWCLKCTL_IPLL;
+			tmp &= ~SSB_CHIPCO_SLOWCLKCTL_ENXTAL;
+			if ((tmp & SSB_CHIPCO_SLOWCLKCTL_SRC) !=
+			    SSB_CHIPCO_SLOWCLKCTL_SRC_XTAL)
+				tmp |= SSB_CHIPCO_SLOWCLKCTL_ENXTAL;
+			chipco_write32(cc, SSB_CHIPCO_SLOWCLKCTL, tmp);
+
+			/* For dynamic control, we have to release our xtal_pu
+			 * "force on" */
+			if (tmp & SSB_CHIPCO_SLOWCLKCTL_ENXTAL)
+				ssb_pci_xtal(bus, SSB_GPIO_XTAL, 0);
+		} else {
+			chipco_write32(cc, SSB_CHIPCO_SYSCLKCTL,
+				(chipco_read32(cc, SSB_CHIPCO_SYSCLKCTL) &
+				 ~SSB_CHIPCO_SYSCLKCTL_FORCEHT));
+		}
 		break;
 	default:
 		SSB_WARN_ON(1);
@@ -209,6 +235,24 @@ static void chipco_powercontrol_init(str
 	}
 }
 
+/* http://bcm-v4.sipsolutions.net/802.11/PmuFastPwrupDelay */
+static u16 pmu_fast_powerup_delay(struct ssb_chipcommon *cc)
+{
+	struct ssb_bus *bus = cc->dev->bus;
+
+	switch (bus->chip_id) {
+	case 0x4312:
+	case 0x4322:
+	case 0x4328:
+		return 7000;
+	case 0x4325:
+		/* TODO: */
+	default:
+		return 15000;
+	}
+}
+
+/* http://bcm-v4.sipsolutions.net/802.11/ClkctlFastPwrupDelay */
 static void calc_fast_powerup_delay(struct ssb_chipcommon *cc)
 {
 	struct ssb_bus *bus = cc->dev->bus;
@@ -218,6 +262,12 @@ static void calc_fast_powerup_delay(stru
 
 	if (bus->bustype != SSB_BUSTYPE_PCI)
 		return;
+
+	if (cc->capabilities & SSB_CHIPCO_CAP_PMU) {
+		cc->fast_pwrup_delay = pmu_fast_powerup_delay(cc);
+		return;
+	}
+
 	if (!(cc->capabilities & SSB_CHIPCO_CAP_PCTL))
 		return;
 
@@ -236,6 +286,12 @@ void ssb_chipcommon_init(struct ssb_chip
 	if (cc->dev->id.revision >= 11)
 		cc->status = chipco_read32(cc, SSB_CHIPCO_CHIPSTAT);
 	ssb_dprintk(KERN_INFO PFX "chipcommon status is 0x%x\n", cc->status);
+
+	if (cc->dev->id.revision >= 20) {
+		chipco_write32(cc, SSB_CHIPCO_GPIOPULLUP, 0);
+		chipco_write32(cc, SSB_CHIPCO_GPIOPULLDOWN, 0);
+	}
+
 	ssb_pmu_init(cc);
 	chipco_powercontrol_init(cc);
 	ssb_chipco_set_clockmode(cc, SSB_CLKMODE_FAST);
@@ -373,6 +429,7 @@ u32 ssb_chipco_gpio_control(struct ssb_c
 {
 	return chipco_write32_masked(cc, SSB_CHIPCO_GPIOCTL, mask, value);
 }
+EXPORT_SYMBOL(ssb_chipco_gpio_control);
 
 u32 ssb_chipco_gpio_intmask(struct ssb_chipcommon *cc, u32 mask, u32 value)
 {
--- a/drivers/ssb/driver_chipcommon_pmu.c
+++ b/drivers/ssb/driver_chipcommon_pmu.c
@@ -2,7 +2,7 @@
  * Sonics Silicon Backplane
  * Broadcom ChipCommon Power Management Unit driver
  *
- * Copyright 2009, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2009, Michael Buesch <m@bues.ch>
  * Copyright 2007, Broadcom Corporation
  *
  * Licensed under the GNU/GPL. See COPYING for details.
@@ -12,6 +12,9 @@
 #include <linux/ssb/ssb_regs.h>
 #include <linux/ssb/ssb_driver_chipcommon.h>
 #include <linux/delay.h>
+#ifdef CONFIG_BCM47XX
+#include <asm/mach-bcm47xx/nvram.h>
+#endif
 
 #include "ssb_private.h"
 
@@ -91,10 +94,6 @@ static void ssb_pmu0_pllinit_r0(struct s
 	u32 pmuctl, tmp, pllctl;
 	unsigned int i;
 
-	if ((bus->chip_id == 0x5354) && !crystalfreq) {
-		/* The 5354 crystal freq is 25MHz */
-		crystalfreq = 25000;
-	}
 	if (crystalfreq)
 		e = pmu0_plltab_find_entry(crystalfreq);
 	if (!e)
@@ -320,7 +319,11 @@ static void ssb_pmu_pll_init(struct ssb_
 	u32 crystalfreq = 0; /* in kHz. 0 = keep default freq. */
 
 	if (bus->bustype == SSB_BUSTYPE_SSB) {
-		/* TODO: The user may override the crystal frequency. */
+#ifdef CONFIG_BCM47XX
+		char buf[20];
+		if (nvram_getenv("xtalfreq", buf, sizeof(buf)) >= 0)
+			crystalfreq = simple_strtoul(buf, NULL, 0);
+#endif
 	}
 
 	switch (bus->chip_id) {
@@ -329,9 +332,19 @@ static void ssb_pmu_pll_init(struct ssb_
 		ssb_pmu1_pllinit_r0(cc, crystalfreq);
 		break;
 	case 0x4328:
+		ssb_pmu0_pllinit_r0(cc, crystalfreq);
+		break;
 	case 0x5354:
+		if (crystalfreq == 0)
+			crystalfreq = 25000;
 		ssb_pmu0_pllinit_r0(cc, crystalfreq);
 		break;
+	case 0x4322:
+		if (cc->pmu.rev == 2) {
+			chipco_write32(cc, SSB_CHIPCO_PLLCTL_ADDR, 0x0000000A);
+			chipco_write32(cc, SSB_CHIPCO_PLLCTL_DATA, 0x380005C0);
+		}
+		break;
 	default:
 		ssb_printk(KERN_ERR PFX
 			   "ERROR: PLL init unknown for device %04X\n",
@@ -411,12 +424,15 @@ static void ssb_pmu_resources_init(struc
 	u32 min_msk = 0, max_msk = 0;
 	unsigned int i;
 	const struct pmu_res_updown_tab_entry *updown_tab = NULL;
-	unsigned int updown_tab_size;
+	unsigned int updown_tab_size = 0;
 	const struct pmu_res_depend_tab_entry *depend_tab = NULL;
-	unsigned int depend_tab_size;
+	unsigned int depend_tab_size = 0;
 
 	switch (bus->chip_id) {
 	case 0x4312:
+		 min_msk = 0xCBB;
+		 break;
+	case 0x4322:
 		/* We keep the default settings:
 		 * min_msk = 0xCBB
 		 * max_msk = 0x7FFFF
@@ -495,9 +511,9 @@ static void ssb_pmu_resources_init(struc
 		chipco_write32(cc, SSB_CHIPCO_PMU_MAXRES_MSK, max_msk);
 }
 
+/* http://bcm-v4.sipsolutions.net/802.11/SSB/PmuInit */
 void ssb_pmu_init(struct ssb_chipcommon *cc)
 {
-	struct ssb_bus *bus = cc->dev->bus;
 	u32 pmucap;
 
 	if (!(cc->capabilities & SSB_CHIPCO_CAP_PMU))
@@ -509,15 +525,12 @@ void ssb_pmu_init(struct ssb_chipcommon
 	ssb_dprintk(KERN_DEBUG PFX "Found rev %u PMU (capabilities 0x%08X)\n",
 		    cc->pmu.rev, pmucap);
 
-	if (cc->pmu.rev >= 1) {
-		if ((bus->chip_id == 0x4325) && (bus->chip_rev < 2)) {
-			chipco_mask32(cc, SSB_CHIPCO_PMU_CTL,
-				      ~SSB_CHIPCO_PMU_CTL_NOILPONW);
-		} else {
-			chipco_set32(cc, SSB_CHIPCO_PMU_CTL,
-				     SSB_CHIPCO_PMU_CTL_NOILPONW);
-		}
-	}
+	if (cc->pmu.rev == 1)
+		chipco_mask32(cc, SSB_CHIPCO_PMU_CTL,
+			      ~SSB_CHIPCO_PMU_CTL_NOILPONW);
+	else
+		chipco_set32(cc, SSB_CHIPCO_PMU_CTL,
+			     SSB_CHIPCO_PMU_CTL_NOILPONW);
 	ssb_pmu_pll_init(cc);
 	ssb_pmu_resources_init(cc);
 }
@@ -600,3 +613,34 @@ void ssb_pmu_set_ldo_paref(struct ssb_ch
 
 EXPORT_SYMBOL(ssb_pmu_set_ldo_voltage);
 EXPORT_SYMBOL(ssb_pmu_set_ldo_paref);
+
+u32 ssb_pmu_get_cpu_clock(struct ssb_chipcommon *cc)
+{
+	struct ssb_bus *bus = cc->dev->bus;
+
+	switch (bus->chip_id) {
+	case 0x5354:
+		/* 5354 chip uses a non programmable PLL of frequency 240MHz */
+		return 240000000;
+	default:
+		ssb_printk(KERN_ERR PFX
+			   "ERROR: PMU cpu clock unknown for device %04X\n",
+			   bus->chip_id);
+		return 0;
+	}
+}
+
+u32 ssb_pmu_get_controlclock(struct ssb_chipcommon *cc)
+{
+	struct ssb_bus *bus = cc->dev->bus;
+
+	switch (bus->chip_id) {
+	case 0x5354:
+		return 120000000;
+	default:
+		ssb_printk(KERN_ERR PFX
+			   "ERROR: PMU controlclock unknown for device %04X\n",
+			   bus->chip_id);
+		return 0;
+	}
+}
--- a/drivers/ssb/driver_gige.c
+++ b/drivers/ssb/driver_gige.c
@@ -3,7 +3,7 @@
  * Broadcom Gigabit Ethernet core driver
  *
  * Copyright 2008, Broadcom Corporation
- * Copyright 2008, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2008, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -12,6 +12,7 @@
 #include <linux/ssb/ssb_driver_gige.h>
 #include <linux/pci.h>
 #include <linux/pci_regs.h>
+#include <linux/slab.h>
 
 
 /*
@@ -105,8 +106,9 @@ void gige_pcicfg_write32(struct ssb_gige
 	gige_write32(dev, SSB_GIGE_PCICFG + offset, value);
 }
 
-static int ssb_gige_pci_read_config(struct pci_bus *bus, unsigned int devfn,
-				    int reg, int size, u32 *val)
+static int __devinit ssb_gige_pci_read_config(struct pci_bus *bus,
+					      unsigned int devfn, int reg,
+					      int size, u32 *val)
 {
 	struct ssb_gige *dev = container_of(bus->ops, struct ssb_gige, pci_ops);
 	unsigned long flags;
@@ -135,8 +137,9 @@ static int ssb_gige_pci_read_config(stru
 	return PCIBIOS_SUCCESSFUL;
 }
 
-static int ssb_gige_pci_write_config(struct pci_bus *bus, unsigned int devfn,
-				     int reg, int size, u32 val)
+static int __devinit ssb_gige_pci_write_config(struct pci_bus *bus,
+					       unsigned int devfn, int reg,
+					       int size, u32 val)
 {
 	struct ssb_gige *dev = container_of(bus->ops, struct ssb_gige, pci_ops);
 	unsigned long flags;
@@ -165,7 +168,8 @@ static int ssb_gige_pci_write_config(str
 	return PCIBIOS_SUCCESSFUL;
 }
 
-static int ssb_gige_probe(struct ssb_device *sdev, const struct ssb_device_id *id)
+static int __devinit ssb_gige_probe(struct ssb_device *sdev,
+				    const struct ssb_device_id *id)
 {
 	struct ssb_gige *dev;
 	u32 base, tmslow, tmshigh;
--- a/drivers/ssb/driver_mipscore.c
+++ b/drivers/ssb/driver_mipscore.c
@@ -3,7 +3,7 @@
  * Broadcom MIPS core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -208,6 +208,9 @@ u32 ssb_cpu_clock(struct ssb_mipscore *m
 	struct ssb_bus *bus = mcore->dev->bus;
 	u32 pll_type, n, m, rate = 0;
 
+	if (bus->chipco.capabilities & SSB_CHIPCO_CAP_PMU)
+		return ssb_pmu_get_cpu_clock(&bus->chipco);
+
 	if (bus->extif.dev) {
 		ssb_extif_get_clockcontrol(&bus->extif, &pll_type, &n, &m);
 	} else if (bus->chipco.dev) {
@@ -270,7 +273,6 @@ void ssb_mipscore_init(struct ssb_mipsco
 				set_irq(dev, irq++);
 			}
 			break;
-			/* fallthrough */
 		case SSB_DEV_PCI:
 		case SSB_DEV_ETHERNET:
 		case SSB_DEV_ETHERNET_GBIT:
@@ -281,6 +283,10 @@ void ssb_mipscore_init(struct ssb_mipsco
 				set_irq(dev, irq++);
 				break;
 			}
+			/* fallthrough */
+		case SSB_DEV_EXTIF:
+			set_irq(dev, 0);
+			break;
 		}
 	}
 	ssb_dprintk(KERN_INFO PFX "after irq reconfiguration\n");
--- a/drivers/ssb/driver_pcicore.c
+++ b/drivers/ssb/driver_pcicore.c
@@ -3,7 +3,7 @@
  * Broadcom PCI-core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -15,6 +15,11 @@
 
 #include "ssb_private.h"
 
+static u32 ssb_pcie_read(struct ssb_pcicore *pc, u32 address);
+static void ssb_pcie_write(struct ssb_pcicore *pc, u32 address, u32 data);
+static u16 ssb_pcie_mdio_read(struct ssb_pcicore *pc, u8 device, u8 address);
+static void ssb_pcie_mdio_write(struct ssb_pcicore *pc, u8 device,
+				u8 address, u16 data);
 
 static inline
 u32 pcicore_read32(struct ssb_pcicore *pc, u16 offset)
@@ -69,7 +74,7 @@ static u32 get_cfgspace_addr(struct ssb_
 	u32 tmp;
 
 	/* We do only have one cardbus device behind the bridge. */
-	if (pc->cardbusmode && (dev >= 1))
+	if (pc->cardbusmode && (dev > 1))
 		goto out;
 
 	if (bus == 0) {
@@ -246,20 +251,12 @@ static struct pci_controller ssb_pcicore
 	.pci_ops	= &ssb_pcicore_pciops,
 	.io_resource	= &ssb_pcicore_io_resource,
 	.mem_resource	= &ssb_pcicore_mem_resource,
-	.mem_offset	= 0x24000000,
 };
 
-static u32 ssb_pcicore_pcibus_iobase = 0x100;
-static u32 ssb_pcicore_pcibus_membase = SSB_PCI_DMA;
-
 /* This function is called when doing a pci_enable_device().
  * We must first check if the device is a device on the PCI-core bridge. */
 int ssb_pcicore_plat_dev_init(struct pci_dev *d)
 {
-	struct resource *res;
-	int pos, size;
-	u32 *base;
-
 	if (d->bus->ops != &ssb_pcicore_pciops) {
 		/* This is not a device on the PCI-core bridge. */
 		return -ENODEV;
@@ -268,27 +265,6 @@ int ssb_pcicore_plat_dev_init(struct pci
 	ssb_printk(KERN_INFO "PCI: Fixing up device %s\n",
 		   pci_name(d));
 
-	/* Fix up resource bases */
-	for (pos = 0; pos < 6; pos++) {
-		res = &d->resource[pos];
-		if (res->flags & IORESOURCE_IO)
-			base = &ssb_pcicore_pcibus_iobase;
-		else
-			base = &ssb_pcicore_pcibus_membase;
-		res->flags |= IORESOURCE_PCI_FIXED;
-		if (res->end) {
-			size = res->end - res->start + 1;
-			if (*base & (size - 1))
-				*base = (*base + size) & ~(size - 1);
-			res->start = *base;
-			res->end = res->start + size - 1;
-			*base += size;
-			pci_write_config_dword(d, PCI_BASE_ADDRESS_0 + (pos << 2), res->start);
-		}
-		/* Fix up PCI bridge BAR0 only */
-		if (d->bus->number == 0 && PCI_SLOT(d->devfn) == 0)
-			break;
-	}
 	/* Fix up interrupt lines */
 	d->irq = ssb_mips_irq(extpci_core->dev) + 2;
 	pci_write_config_byte(d, PCI_INTERRUPT_LINE, d->irq);
@@ -338,7 +314,7 @@ int ssb_pcicore_pcibios_map_irq(const st
 	return ssb_mips_irq(extpci_core->dev) + 2;
 }
 
-static void ssb_pcicore_init_hostmode(struct ssb_pcicore *pc)
+static void __devinit ssb_pcicore_init_hostmode(struct ssb_pcicore *pc)
 {
 	u32 val;
 
@@ -403,7 +379,7 @@ static void ssb_pcicore_init_hostmode(st
 	register_pci_controller(&ssb_pcicore_controller);
 }
 
-static int pcicore_is_in_hostmode(struct ssb_pcicore *pc)
+static int __devinit pcicore_is_in_hostmode(struct ssb_pcicore *pc)
 {
 	struct ssb_bus *bus = pc->dev->bus;
 	u16 chipid_top;
@@ -432,25 +408,137 @@ static int pcicore_is_in_hostmode(struct
 }
 #endif /* CONFIG_SSB_PCICORE_HOSTMODE */
 
+/**************************************************
+ * Workarounds.
+ **************************************************/
+
+static void __devinit ssb_pcicore_fix_sprom_core_index(struct ssb_pcicore *pc)
+{
+	u16 tmp = pcicore_read16(pc, SSB_PCICORE_SPROM(0));
+	if (((tmp & 0xF000) >> 12) != pc->dev->core_index) {
+		tmp &= ~0xF000;
+		tmp |= (pc->dev->core_index << 12);
+		pcicore_write16(pc, SSB_PCICORE_SPROM(0), tmp);
+	}
+}
+
+static u8 ssb_pcicore_polarity_workaround(struct ssb_pcicore *pc)
+{
+	return (ssb_pcie_read(pc, 0x204) & 0x10) ? 0xC0 : 0x80;
+}
+
+static void ssb_pcicore_serdes_workaround(struct ssb_pcicore *pc)
+{
+	const u8 serdes_pll_device = 0x1D;
+	const u8 serdes_rx_device = 0x1F;
+	u16 tmp;
+
+	ssb_pcie_mdio_write(pc, serdes_rx_device, 1 /* Control */,
+			    ssb_pcicore_polarity_workaround(pc));
+	tmp = ssb_pcie_mdio_read(pc, serdes_pll_device, 1 /* Control */);
+	if (tmp & 0x4000)
+		ssb_pcie_mdio_write(pc, serdes_pll_device, 1, tmp & ~0x4000);
+}
+
+static void ssb_pcicore_pci_setup_workarounds(struct ssb_pcicore *pc)
+{
+	struct ssb_device *pdev = pc->dev;
+	struct ssb_bus *bus = pdev->bus;
+	u32 tmp;
+
+	tmp = pcicore_read32(pc, SSB_PCICORE_SBTOPCI2);
+	tmp |= SSB_PCICORE_SBTOPCI_PREF;
+	tmp |= SSB_PCICORE_SBTOPCI_BURST;
+	pcicore_write32(pc, SSB_PCICORE_SBTOPCI2, tmp);
+
+	if (pdev->id.revision < 5) {
+		tmp = ssb_read32(pdev, SSB_IMCFGLO);
+		tmp &= ~SSB_IMCFGLO_SERTO;
+		tmp |= 2;
+		tmp &= ~SSB_IMCFGLO_REQTO;
+		tmp |= 3 << SSB_IMCFGLO_REQTO_SHIFT;
+		ssb_write32(pdev, SSB_IMCFGLO, tmp);
+		ssb_commit_settings(bus);
+	} else if (pdev->id.revision >= 11) {
+		tmp = pcicore_read32(pc, SSB_PCICORE_SBTOPCI2);
+		tmp |= SSB_PCICORE_SBTOPCI_MRM;
+		pcicore_write32(pc, SSB_PCICORE_SBTOPCI2, tmp);
+	}
+}
+
+static void ssb_pcicore_pcie_setup_workarounds(struct ssb_pcicore *pc)
+{
+	u32 tmp;
+	u8 rev = pc->dev->id.revision;
+
+	if (rev == 0 || rev == 1) {
+		/* TLP Workaround register. */
+		tmp = ssb_pcie_read(pc, 0x4);
+		tmp |= 0x8;
+		ssb_pcie_write(pc, 0x4, tmp);
+	}
+	if (rev == 1) {
+		/* DLLP Link Control register. */
+		tmp = ssb_pcie_read(pc, 0x100);
+		tmp |= 0x40;
+		ssb_pcie_write(pc, 0x100, tmp);
+	}
+
+	if (rev == 0) {
+		const u8 serdes_rx_device = 0x1F;
+
+		ssb_pcie_mdio_write(pc, serdes_rx_device,
+					2 /* Timer */, 0x8128);
+		ssb_pcie_mdio_write(pc, serdes_rx_device,
+					6 /* CDR */, 0x0100);
+		ssb_pcie_mdio_write(pc, serdes_rx_device,
+					7 /* CDR BW */, 0x1466);
+	} else if (rev == 3 || rev == 4 || rev == 5) {
+		/* TODO: DLLP Power Management Threshold */
+		ssb_pcicore_serdes_workaround(pc);
+		/* TODO: ASPM */
+	} else if (rev == 7) {
+		/* TODO: No PLL down */
+	}
+
+	if (rev >= 6) {
+		/* Miscellaneous Configuration Fixup */
+		tmp = pcicore_read16(pc, SSB_PCICORE_SPROM(5));
+		if (!(tmp & 0x8000))
+			pcicore_write16(pc, SSB_PCICORE_SPROM(5),
+					tmp | 0x8000);
+	}
+}
 
 /**************************************************
  * Generic and Clientmode operation code.
  **************************************************/
 
-static void ssb_pcicore_init_clientmode(struct ssb_pcicore *pc)
+static void __devinit ssb_pcicore_init_clientmode(struct ssb_pcicore *pc)
 {
+	struct ssb_device *pdev = pc->dev;
+	struct ssb_bus *bus = pdev->bus;
+
+	if (bus->bustype == SSB_BUSTYPE_PCI)
+		ssb_pcicore_fix_sprom_core_index(pc);
+
 	/* Disable PCI interrupts. */
-	ssb_write32(pc->dev, SSB_INTVEC, 0);
+	ssb_write32(pdev, SSB_INTVEC, 0);
+
+	/* Additional PCIe always once-executed workarounds */
+	if (pc->dev->id.coreid == SSB_DEV_PCIE) {
+		ssb_pcicore_serdes_workaround(pc);
+		/* TODO: ASPM */
+		/* TODO: Clock Request Update */
+	}
 }
 
-void ssb_pcicore_init(struct ssb_pcicore *pc)
+void __devinit ssb_pcicore_init(struct ssb_pcicore *pc)
 {
 	struct ssb_device *dev = pc->dev;
-	struct ssb_bus *bus;
 
 	if (!dev)
 		return;
-	bus = dev->bus;
 	if (!ssb_device_is_enabled(dev))
 		ssb_device_enable(dev, 0);
 
@@ -475,58 +563,104 @@ static void ssb_pcie_write(struct ssb_pc
 	pcicore_write32(pc, 0x134, data);
 }
 
-static void ssb_pcie_mdio_write(struct ssb_pcicore *pc, u8 device,
-				u8 address, u16 data)
+static void ssb_pcie_mdio_set_phy(struct ssb_pcicore *pc, u8 phy)
 {
 	const u16 mdio_control = 0x128;
 	const u16 mdio_data = 0x12C;
 	u32 v;
 	int i;
 
+	v = (1 << 30); /* Start of Transaction */
+	v |= (1 << 28); /* Write Transaction */
+	v |= (1 << 17); /* Turnaround */
+	v |= (0x1F << 18);
+	v |= (phy << 4);
+	pcicore_write32(pc, mdio_data, v);
+
+	udelay(10);
+	for (i = 0; i < 200; i++) {
+		v = pcicore_read32(pc, mdio_control);
+		if (v & 0x100 /* Trans complete */)
+			break;
+		msleep(1);
+	}
+}
+
+static u16 ssb_pcie_mdio_read(struct ssb_pcicore *pc, u8 device, u8 address)
+{
+	const u16 mdio_control = 0x128;
+	const u16 mdio_data = 0x12C;
+	int max_retries = 10;
+	u16 ret = 0;
+	u32 v;
+	int i;
+
 	v = 0x80; /* Enable Preamble Sequence */
 	v |= 0x2; /* MDIO Clock Divisor */
 	pcicore_write32(pc, mdio_control, v);
 
+	if (pc->dev->id.revision >= 10) {
+		max_retries = 200;
+		ssb_pcie_mdio_set_phy(pc, device);
+	}
+
 	v = (1 << 30); /* Start of Transaction */
-	v |= (1 << 28); /* Write Transaction */
+	v |= (1 << 29); /* Read Transaction */
 	v |= (1 << 17); /* Turnaround */
-	v |= (u32)device << 22;
+	if (pc->dev->id.revision < 10)
+		v |= (u32)device << 22;
 	v |= (u32)address << 18;
-	v |= data;
 	pcicore_write32(pc, mdio_data, v);
 	/* Wait for the device to complete the transaction */
 	udelay(10);
-	for (i = 0; i < 10; i++) {
+	for (i = 0; i < max_retries; i++) {
 		v = pcicore_read32(pc, mdio_control);
-		if (v & 0x100 /* Trans complete */)
+		if (v & 0x100 /* Trans complete */) {
+			udelay(10);
+			ret = pcicore_read32(pc, mdio_data);
 			break;
+		}
 		msleep(1);
 	}
 	pcicore_write32(pc, mdio_control, 0);
+	return ret;
 }
 
-static void ssb_broadcast_value(struct ssb_device *dev,
-				u32 address, u32 data)
+static void ssb_pcie_mdio_write(struct ssb_pcicore *pc, u8 device,
+				u8 address, u16 data)
 {
-	/* This is used for both, PCI and ChipCommon core, so be careful. */
-	BUILD_BUG_ON(SSB_PCICORE_BCAST_ADDR != SSB_CHIPCO_BCAST_ADDR);
-	BUILD_BUG_ON(SSB_PCICORE_BCAST_DATA != SSB_CHIPCO_BCAST_DATA);
+	const u16 mdio_control = 0x128;
+	const u16 mdio_data = 0x12C;
+	int max_retries = 10;
+	u32 v;
+	int i;
 
-	ssb_write32(dev, SSB_PCICORE_BCAST_ADDR, address);
-	ssb_read32(dev, SSB_PCICORE_BCAST_ADDR); /* flush */
-	ssb_write32(dev, SSB_PCICORE_BCAST_DATA, data);
-	ssb_read32(dev, SSB_PCICORE_BCAST_DATA); /* flush */
-}
+	v = 0x80; /* Enable Preamble Sequence */
+	v |= 0x2; /* MDIO Clock Divisor */
+	pcicore_write32(pc, mdio_control, v);
 
-static void ssb_commit_settings(struct ssb_bus *bus)
-{
-	struct ssb_device *dev;
+	if (pc->dev->id.revision >= 10) {
+		max_retries = 200;
+		ssb_pcie_mdio_set_phy(pc, device);
+	}
 
-	dev = bus->chipco.dev ? bus->chipco.dev : bus->pcicore.dev;
-	if (WARN_ON(!dev))
-		return;
-	/* This forces an update of the cached registers. */
-	ssb_broadcast_value(dev, 0xFD8, 0);
+	v = (1 << 30); /* Start of Transaction */
+	v |= (1 << 28); /* Write Transaction */
+	v |= (1 << 17); /* Turnaround */
+	if (pc->dev->id.revision < 10)
+		v |= (u32)device << 22;
+	v |= (u32)address << 18;
+	v |= data;
+	pcicore_write32(pc, mdio_data, v);
+	/* Wait for the device to complete the transaction */
+	udelay(10);
+	for (i = 0; i < max_retries; i++) {
+		v = pcicore_read32(pc, mdio_control);
+		if (v & 0x100 /* Trans complete */)
+			break;
+		msleep(1);
+	}
+	pcicore_write32(pc, mdio_control, 0);
 }
 
 int ssb_pcicore_dev_irqvecs_enable(struct ssb_pcicore *pc,
@@ -551,13 +685,13 @@ int ssb_pcicore_dev_irqvecs_enable(struc
 	might_sleep_if(pdev->id.coreid != SSB_DEV_PCI);
 
 	/* Enable interrupts for this device. */
-	if (bus->host_pci &&
-	    ((pdev->id.revision >= 6) || (pdev->id.coreid == SSB_DEV_PCIE))) {
+	if ((pdev->id.revision >= 6) || (pdev->id.coreid == SSB_DEV_PCIE)) {
 		u32 coremask;
 
 		/* Calculate the "coremask" for the device. */
 		coremask = (1 << dev->core_index);
 
+		SSB_WARN_ON(bus->bustype != SSB_BUSTYPE_PCI);
 		err = pci_read_config_dword(bus->host_pci, SSB_PCI_IRQMASK, &tmp);
 		if (err)
 			goto out;
@@ -579,48 +713,10 @@ int ssb_pcicore_dev_irqvecs_enable(struc
 	if (pc->setup_done)
 		goto out;
 	if (pdev->id.coreid == SSB_DEV_PCI) {
-		tmp = pcicore_read32(pc, SSB_PCICORE_SBTOPCI2);
-		tmp |= SSB_PCICORE_SBTOPCI_PREF;
-		tmp |= SSB_PCICORE_SBTOPCI_BURST;
-		pcicore_write32(pc, SSB_PCICORE_SBTOPCI2, tmp);
-
-		if (pdev->id.revision < 5) {
-			tmp = ssb_read32(pdev, SSB_IMCFGLO);
-			tmp &= ~SSB_IMCFGLO_SERTO;
-			tmp |= 2;
-			tmp &= ~SSB_IMCFGLO_REQTO;
-			tmp |= 3 << SSB_IMCFGLO_REQTO_SHIFT;
-			ssb_write32(pdev, SSB_IMCFGLO, tmp);
-			ssb_commit_settings(bus);
-		} else if (pdev->id.revision >= 11) {
-			tmp = pcicore_read32(pc, SSB_PCICORE_SBTOPCI2);
-			tmp |= SSB_PCICORE_SBTOPCI_MRM;
-			pcicore_write32(pc, SSB_PCICORE_SBTOPCI2, tmp);
-		}
+		ssb_pcicore_pci_setup_workarounds(pc);
 	} else {
 		WARN_ON(pdev->id.coreid != SSB_DEV_PCIE);
-		//TODO: Better make defines for all these magic PCIE values.
-		if ((pdev->id.revision == 0) || (pdev->id.revision == 1)) {
-			/* TLP Workaround register. */
-			tmp = ssb_pcie_read(pc, 0x4);
-			tmp |= 0x8;
-			ssb_pcie_write(pc, 0x4, tmp);
-		}
-		if (pdev->id.revision == 0) {
-			const u8 serdes_rx_device = 0x1F;
-
-			ssb_pcie_mdio_write(pc, serdes_rx_device,
-					    2 /* Timer */, 0x8128);
-			ssb_pcie_mdio_write(pc, serdes_rx_device,
-					    6 /* CDR */, 0x0100);
-			ssb_pcie_mdio_write(pc, serdes_rx_device,
-					    7 /* CDR BW */, 0x1466);
-		} else if (pdev->id.revision == 1) {
-			/* DLLP Link Control register. */
-			tmp = ssb_pcie_read(pc, 0x100);
-			tmp |= 0x40;
-			ssb_pcie_write(pc, 0x100, tmp);
-		}
+		ssb_pcicore_pcie_setup_workarounds(pc);
 	}
 	pc->setup_done = 1;
 out:
--- a/drivers/ssb/main.c
+++ b/drivers/ssb/main.c
@@ -3,7 +3,7 @@
  * Subsystem core
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -12,12 +12,14 @@
 
 #include <linux/delay.h>
 #include <linux/io.h>
+#include <linux/module.h>
 #include <linux/ssb/ssb.h>
 #include <linux/ssb/ssb_regs.h>
 #include <linux/ssb/ssb_driver_gige.h>
 #include <linux/dma-mapping.h>
 #include <linux/pci.h>
 #include <linux/mmc/sdio_func.h>
+#include <linux/slab.h>
 
 #include <pcmcia/cs_types.h>
 #include <pcmcia/cs.h>
@@ -210,90 +212,78 @@ int ssb_bus_suspend(struct ssb_bus *bus)
 EXPORT_SYMBOL(ssb_bus_suspend);
 
 #ifdef CONFIG_SSB_SPROM
-int ssb_devices_freeze(struct ssb_bus *bus)
+/** ssb_devices_freeze - Freeze all devices on the bus.
+ *
+ * After freezing no device driver will be handling a device
+ * on this bus anymore. ssb_devices_thaw() must be called after
+ * a successful freeze to reactivate the devices.
+ *
+ * @bus: The bus.
+ * @ctx: Context structure. Pass this to ssb_devices_thaw().
+ */
+int ssb_devices_freeze(struct ssb_bus *bus, struct ssb_freeze_context *ctx)
 {
-	struct ssb_device *dev;
-	struct ssb_driver *drv;
-	int err = 0;
-	int i;
-	pm_message_t state = PMSG_FREEZE;
+	struct ssb_device *sdev;
+	struct ssb_driver *sdrv;
+	unsigned int i;
+
+	memset(ctx, 0, sizeof(*ctx));
+	ctx->bus = bus;
+	SSB_WARN_ON(bus->nr_devices > ARRAY_SIZE(ctx->device_frozen));
 
-	/* First check that we are capable to freeze all devices. */
 	for (i = 0; i < bus->nr_devices; i++) {
-		dev = &(bus->devices[i]);
-		if (!dev->dev ||
-		    !dev->dev->driver ||
-		    !device_is_registered(dev->dev))
-			continue;
-		drv = drv_to_ssb_drv(dev->dev->driver);
-		if (!drv)
+		sdev = ssb_device_get(&bus->devices[i]);
+
+		if (!sdev->dev || !sdev->dev->driver ||
+		    !device_is_registered(sdev->dev)) {
+			ssb_device_put(sdev);
 			continue;
-		if (!drv->suspend) {
-			/* Nope, can't suspend this one. */
-			return -EOPNOTSUPP;
 		}
-	}
-	/* Now suspend all devices */
-	for (i = 0; i < bus->nr_devices; i++) {
-		dev = &(bus->devices[i]);
-		if (!dev->dev ||
-		    !dev->dev->driver ||
-		    !device_is_registered(dev->dev))
-			continue;
-		drv = drv_to_ssb_drv(dev->dev->driver);
-		if (!drv)
+		sdrv = drv_to_ssb_drv(sdev->dev->driver);
+		if (SSB_WARN_ON(!sdrv->remove))
 			continue;
-		err = drv->suspend(dev, state);
-		if (err) {
-			ssb_printk(KERN_ERR PFX "Failed to freeze device %s\n",
-				   dev_name(dev->dev));
-			goto err_unwind;
-		}
+		sdrv->remove(sdev);
+		ctx->device_frozen[i] = 1;
 	}
 
 	return 0;
-err_unwind:
-	for (i--; i >= 0; i--) {
-		dev = &(bus->devices[i]);
-		if (!dev->dev ||
-		    !dev->dev->driver ||
-		    !device_is_registered(dev->dev))
-			continue;
-		drv = drv_to_ssb_drv(dev->dev->driver);
-		if (!drv)
-			continue;
-		if (drv->resume)
-			drv->resume(dev);
-	}
-	return err;
 }
 
-int ssb_devices_thaw(struct ssb_bus *bus)
+/** ssb_devices_thaw - Unfreeze all devices on the bus.
+ *
+ * This will re-attach the device drivers and re-init the devices.
+ *
+ * @ctx: The context structure from ssb_devices_freeze()
+ */
+int ssb_devices_thaw(struct ssb_freeze_context *ctx)
 {
-	struct ssb_device *dev;
-	struct ssb_driver *drv;
-	int err;
-	int i;
+	struct ssb_bus *bus = ctx->bus;
+	struct ssb_device *sdev;
+	struct ssb_driver *sdrv;
+	unsigned int i;
+	int err, result = 0;
 
 	for (i = 0; i < bus->nr_devices; i++) {
-		dev = &(bus->devices[i]);
-		if (!dev->dev ||
-		    !dev->dev->driver ||
-		    !device_is_registered(dev->dev))
+		if (!ctx->device_frozen[i])
 			continue;
-		drv = drv_to_ssb_drv(dev->dev->driver);
-		if (!drv)
+		sdev = &bus->devices[i];
+
+		if (SSB_WARN_ON(!sdev->dev || !sdev->dev->driver))
 			continue;
-		if (SSB_WARN_ON(!drv->resume))
+		sdrv = drv_to_ssb_drv(sdev->dev->driver);
+		if (SSB_WARN_ON(!sdrv || !sdrv->probe))
 			continue;
-		err = drv->resume(dev);
+
+		err = sdrv->probe(sdev, &sdev->id);
 		if (err) {
 			ssb_printk(KERN_ERR PFX "Failed to thaw device %s\n",
-				   dev_name(dev->dev));
+				   dev_name(sdev->dev));
+			result = err;
 		}
+		ssb_device_put(sdev);
 	}
 
-	return 0;
+	return result;
 }
 #endif /* CONFIG_SSB_SPROM */
 
@@ -380,6 +370,35 @@ static int ssb_device_uevent(struct devi
 			     ssb_dev->id.revision);
 }
 
+#define ssb_config_attr(attrib, field, format_string) \
+static ssize_t \
+attrib##_show(struct device *dev, struct device_attribute *attr, char *buf) \
+{ \
+	return sprintf(buf, format_string, dev_to_ssb_dev(dev)->field); \
+}
+
+ssb_config_attr(core_num, core_index, "%u\n")
+ssb_config_attr(coreid, id.coreid, "0x%04x\n")
+ssb_config_attr(vendor, id.vendor, "0x%04x\n")
+ssb_config_attr(revision, id.revision, "%u\n")
+ssb_config_attr(irq, irq, "%u\n")
+static ssize_t
+name_show(struct device *dev, struct device_attribute *attr, char *buf)
+{
+	return sprintf(buf, "%s\n",
+		       ssb_core_name(dev_to_ssb_dev(dev)->id.coreid));
+}
+
+static struct device_attribute ssb_device_attrs[] = {
+	__ATTR_RO(name),
+	__ATTR_RO(core_num),
+	__ATTR_RO(coreid),
+	__ATTR_RO(vendor),
+	__ATTR_RO(revision),
+	__ATTR_RO(irq),
+	__ATTR_NULL,
+};
+
 static struct bus_type ssb_bustype = {
 	.name		= "ssb",
 	.match		= ssb_bus_match,
@@ -389,6 +408,7 @@ static struct bus_type ssb_bustype = {
 	.suspend	= ssb_device_suspend,
 	.resume		= ssb_device_resume,
 	.uevent		= ssb_device_uevent,
+	.dev_attrs	= ssb_device_attrs,
 };
 
 static void ssb_buses_lock(void)
@@ -481,6 +501,7 @@ static int ssb_devices_register(struct s
 #ifdef CONFIG_SSB_PCIHOST
 			sdev->irq = bus->host_pci->irq;
 			dev->parent = &bus->host_pci->dev;
+			sdev->dma_dev = dev->parent;
 #endif
 			break;
 		case SSB_BUSTYPE_PCMCIA:
@@ -490,13 +511,13 @@ static int ssb_devices_register(struct s
 #endif
 			break;
 		case SSB_BUSTYPE_SDIO:
-#ifdef CONFIG_SSB_SDIO
-			sdev->irq = bus->host_sdio->dev.irq;
+#ifdef CONFIG_SSB_SDIOHOST
 			dev->parent = &bus->host_sdio->dev;
 #endif
 			break;
 		case SSB_BUSTYPE_SSB:
 			dev->dma_mask = &dev->coherent_dma_mask;
+			sdev->dma_dev = dev;
 			break;
 		}
 
@@ -523,7 +544,7 @@ error:
 }
 
 /* Needs ssb_buses_lock() */
-static int ssb_attach_queued_buses(void)
+static int __devinit ssb_attach_queued_buses(void)
 {
 	struct ssb_bus *bus, *n;
 	int err = 0;
@@ -734,9 +755,9 @@ out:
 	return err;
 }
 
-static int ssb_bus_register(struct ssb_bus *bus,
-			    ssb_invariants_func_t get_invariants,
-			    unsigned long baseaddr)
+static int __devinit ssb_bus_register(struct ssb_bus *bus,
+				      ssb_invariants_func_t get_invariants,
+				      unsigned long baseaddr)
 {
 	int err;
 
@@ -817,8 +838,8 @@ err_disable_xtal:
 }
 
 #ifdef CONFIG_SSB_PCIHOST
-int ssb_bus_pcibus_register(struct ssb_bus *bus,
-			    struct pci_dev *host_pci)
+int __devinit ssb_bus_pcibus_register(struct ssb_bus *bus,
+				      struct pci_dev *host_pci)
 {
 	int err;
 
@@ -830,6 +851,9 @@ int ssb_bus_pcibus_register(struct ssb_b
 	if (!err) {
 		ssb_printk(KERN_INFO PFX "Sonics Silicon Backplane found on "
 			   "PCI device %s\n", dev_name(&host_pci->dev));
+	} else {
+		ssb_printk(KERN_ERR PFX "Failed to register PCI version"
+			   " of SSB with error %d\n", err);
 	}
 
 	return err;
@@ -838,9 +862,9 @@ EXPORT_SYMBOL(ssb_bus_pcibus_register);
 #endif /* CONFIG_SSB_PCIHOST */
 
 #ifdef CONFIG_SSB_PCMCIAHOST
-int ssb_bus_pcmciabus_register(struct ssb_bus *bus,
-			       struct pcmcia_device *pcmcia_dev,
-			       unsigned long baseaddr)
+int __devinit ssb_bus_pcmciabus_register(struct ssb_bus *bus,
+					 struct pcmcia_device *pcmcia_dev,
+					 unsigned long baseaddr)
 {
 	int err;
 
@@ -860,8 +884,9 @@ EXPORT_SYMBOL(ssb_bus_pcmciabus_register
 #endif /* CONFIG_SSB_PCMCIAHOST */
 
 #ifdef CONFIG_SSB_SDIOHOST
-int ssb_bus_sdiobus_register(struct ssb_bus *bus, struct sdio_func *func,
-			     unsigned int quirks)
+int __devinit ssb_bus_sdiobus_register(struct ssb_bus *bus,
+				       struct sdio_func *func,
+				       unsigned int quirks)
 {
 	int err;
 
@@ -881,9 +906,9 @@ int ssb_bus_sdiobus_register(struct ssb_
 EXPORT_SYMBOL(ssb_bus_sdiobus_register);
 #endif /* CONFIG_SSB_PCMCIAHOST */
 
-int ssb_bus_ssbbus_register(struct ssb_bus *bus,
-			    unsigned long baseaddr,
-			    ssb_invariants_func_t get_invariants)
+int __devinit ssb_bus_ssbbus_register(struct ssb_bus *bus,
+				      unsigned long baseaddr,
+				      ssb_invariants_func_t get_invariants)
 {
 	int err;
 
@@ -964,8 +989,8 @@ u32 ssb_calc_clock_rate(u32 plltype, u32
 	switch (plltype) {
 	case SSB_PLLTYPE_6: /* 100/200 or 120/240 only */
 		if (m & SSB_CHIPCO_CLK_T6_MMASK)
-			return SSB_CHIPCO_CLK_T6_M0;
-		return SSB_CHIPCO_CLK_T6_M1;
+			return SSB_CHIPCO_CLK_T6_M1;
+		return SSB_CHIPCO_CLK_T6_M0;
 	case SSB_PLLTYPE_1: /* 48Mhz base, 3 dividers */
 	case SSB_PLLTYPE_3: /* 25Mhz, 2 dividers */
 	case SSB_PLLTYPE_4: /* 48Mhz, 4 dividers */
@@ -1055,6 +1080,9 @@ u32 ssb_clockspeed(struct ssb_bus *bus)
 	u32 plltype;
 	u32 clkctl_n, clkctl_m;
 
+	if (bus->chipco.capabilities & SSB_CHIPCO_CAP_PMU)
+		return ssb_pmu_get_controlclock(&bus->chipco);
+
 	if (ssb_extif_available(&bus->extif))
 		ssb_extif_get_clockcontrol(&bus->extif, &plltype,
 					   &clkctl_n, &clkctl_m);
@@ -1080,23 +1108,22 @@ static u32 ssb_tmslow_reject_bitmask(str
 {
 	u32 rev = ssb_read32(dev, SSB_IDLOW) & SSB_IDLOW_SSBREV;
 
-	/* The REJECT bit changed position in TMSLOW between
-	 * Backplane revisions. */
+	/* The REJECT bit seems to be different for Backplane rev 2.3 */
 	switch (rev) {
 	case SSB_IDLOW_SSBREV_22:
-		return SSB_TMSLOW_REJECT_22;
+	case SSB_IDLOW_SSBREV_24:
+	case SSB_IDLOW_SSBREV_26:
+		return SSB_TMSLOW_REJECT;
 	case SSB_IDLOW_SSBREV_23:
 		return SSB_TMSLOW_REJECT_23;
-	case SSB_IDLOW_SSBREV_24:     /* TODO - find the proper REJECT bits */
-	case SSB_IDLOW_SSBREV_25:     /* same here */
-	case SSB_IDLOW_SSBREV_26:     /* same here */
+	case SSB_IDLOW_SSBREV_25:     /* TODO - find the proper REJECT bit */
 	case SSB_IDLOW_SSBREV_27:     /* same here */
-		return SSB_TMSLOW_REJECT_23;	/* this is a guess */
+		return SSB_TMSLOW_REJECT;	/* this is a guess */
 	default:
 		printk(KERN_INFO "ssb: Backplane Revision 0x%.8X\n", rev);
 		WARN_ON(1);
 	}
-	return (SSB_TMSLOW_REJECT_22 | SSB_TMSLOW_REJECT_23);
+	return (SSB_TMSLOW_REJECT | SSB_TMSLOW_REJECT_23);
 }
 
 int ssb_device_is_enabled(struct ssb_device *dev)
@@ -1155,10 +1182,10 @@ void ssb_device_enable(struct ssb_device
 }
 EXPORT_SYMBOL(ssb_device_enable);
 
-/* Wait for a bit in a register to get set or unset.
+/* Wait for bitmask in a register to get set or cleared.
  * timeout is in units of ten-microseconds */
-static int ssb_wait_bit(struct ssb_device *dev, u16 reg, u32 bitmask,
-			int timeout, int set)
+static int ssb_wait_bits(struct ssb_device *dev, u16 reg, u32 bitmask,
+			 int timeout, int set)
 {
 	int i;
 	u32 val;
@@ -1166,7 +1193,7 @@ static int ssb_wait_bit(struct ssb_devic
 	for (i = 0; i < timeout; i++) {
 		val = ssb_read32(dev, reg);
 		if (set) {
-			if (val & bitmask)
+			if ((val & bitmask) == bitmask)
 				return 0;
 		} else {
 			if (!(val & bitmask))
@@ -1183,20 +1210,38 @@ static int ssb_wait_bit(struct ssb_devic
 
 void ssb_device_disable(struct ssb_device *dev, u32 core_specific_flags)
 {
-	u32 reject;
+	u32 reject, val;
 
 	if (ssb_read32(dev, SSB_TMSLOW) & SSB_TMSLOW_RESET)
 		return;
 
 	reject = ssb_tmslow_reject_bitmask(dev);
-	ssb_write32(dev, SSB_TMSLOW, reject | SSB_TMSLOW_CLOCK);
-	ssb_wait_bit(dev, SSB_TMSLOW, reject, 1000, 1);
-	ssb_wait_bit(dev, SSB_TMSHIGH, SSB_TMSHIGH_BUSY, 1000, 0);
-	ssb_write32(dev, SSB_TMSLOW,
-		    SSB_TMSLOW_FGC | SSB_TMSLOW_CLOCK |
-		    reject | SSB_TMSLOW_RESET |
-		    core_specific_flags);
-	ssb_flush_tmslow(dev);
+
+	if (ssb_read32(dev, SSB_TMSLOW) & SSB_TMSLOW_CLOCK) {
+		ssb_write32(dev, SSB_TMSLOW, reject | SSB_TMSLOW_CLOCK);
+		ssb_wait_bits(dev, SSB_TMSLOW, reject, 1000, 1);
+		ssb_wait_bits(dev, SSB_TMSHIGH, SSB_TMSHIGH_BUSY, 1000, 0);
+
+		if (ssb_read32(dev, SSB_IDLOW) & SSB_IDLOW_INITIATOR) {
+			val = ssb_read32(dev, SSB_IMSTATE);
+			val |= SSB_IMSTATE_REJECT;
+			ssb_write32(dev, SSB_IMSTATE, val);
+			ssb_wait_bits(dev, SSB_IMSTATE, SSB_IMSTATE_BUSY, 1000,
+				      0);
+		}
+
+		ssb_write32(dev, SSB_TMSLOW,
+			SSB_TMSLOW_FGC | SSB_TMSLOW_CLOCK |
+			reject | SSB_TMSLOW_RESET |
+			core_specific_flags);
+		ssb_flush_tmslow(dev);
+
+		if (ssb_read32(dev, SSB_IDLOW) & SSB_IDLOW_INITIATOR) {
+			val = ssb_read32(dev, SSB_IMSTATE);
+			val &= ~SSB_IMSTATE_REJECT;
+			ssb_write32(dev, SSB_IMSTATE, val);
+		}
+	}
 
 	ssb_write32(dev, SSB_TMSLOW,
 		    reject | SSB_TMSLOW_RESET |
@@ -1205,13 +1250,34 @@ void ssb_device_disable(struct ssb_devic
 }
 EXPORT_SYMBOL(ssb_device_disable);
 
+/* Some chipsets need routing known for PCIe and 64-bit DMA */
+static bool ssb_dma_translation_special_bit(struct ssb_device *dev)
+{
+	u16 chip_id = dev->bus->chip_id;
+
+	if (dev->id.coreid == SSB_DEV_80211) {
+		return (chip_id == 0x4322 || chip_id == 43221 ||
+			chip_id == 43231 || chip_id == 43222);
+	}
+
+	return 0;
+}
+
 u32 ssb_dma_translation(struct ssb_device *dev)
 {
 	switch (dev->bus->bustype) {
 	case SSB_BUSTYPE_SSB:
 		return 0;
 	case SSB_BUSTYPE_PCI:
-		return SSB_PCI_DMA;
+		if (dev->bus->host_pci->is_pcie &&
+		    ssb_read32(dev, SSB_TMSHIGH) & SSB_TMSHIGH_DMA64) {
+			return SSB_PCIE_DMA_H32;
+		} else {
+			if (ssb_dma_translation_special_bit(dev))
+				return SSB_PCIE_DMA_H32;
+			else
+				return SSB_PCI_DMA;
+		}
 	default:
 		__ssb_dma_not_implemented(dev);
 	}
@@ -1328,20 +1394,20 @@ EXPORT_SYMBOL(ssb_bus_may_powerdown);
 
 int ssb_bus_powerup(struct ssb_bus *bus, bool dynamic_pctl)
 {
-	struct ssb_chipcommon *cc;
 	int err;
 	enum ssb_clkmode mode;
 
 	err = ssb_pci_xtal(bus, SSB_GPIO_XTAL | SSB_GPIO_PLL, 1);
 	if (err)
 		goto error;
-	cc = &bus->chipco;
-	mode = dynamic_pctl ? SSB_CLKMODE_DYNAMIC : SSB_CLKMODE_FAST;
-	ssb_chipco_set_clockmode(cc, mode);
 
 #ifdef CONFIG_SSB_DEBUG
 	bus->powered_up = 1;
 #endif
+
+	mode = dynamic_pctl ? SSB_CLKMODE_DYNAMIC : SSB_CLKMODE_FAST;
+	ssb_chipco_set_clockmode(&bus->chipco, mode);
+
 	return 0;
 error:
 	ssb_printk(KERN_ERR PFX "Bus powerup failed\n");
@@ -1349,6 +1415,37 @@ error:
 }
 EXPORT_SYMBOL(ssb_bus_powerup);
 
+static void ssb_broadcast_value(struct ssb_device *dev,
+				u32 address, u32 data)
+{
+#ifdef CONFIG_SSB_DRIVER_PCICORE
+	/* This is used for both, PCI and ChipCommon core, so be careful. */
+	BUILD_BUG_ON(SSB_PCICORE_BCAST_ADDR != SSB_CHIPCO_BCAST_ADDR);
+	BUILD_BUG_ON(SSB_PCICORE_BCAST_DATA != SSB_CHIPCO_BCAST_DATA);
+#endif
+
+	ssb_write32(dev, SSB_CHIPCO_BCAST_ADDR, address);
+	ssb_read32(dev, SSB_CHIPCO_BCAST_ADDR); /* flush */
+	ssb_write32(dev, SSB_CHIPCO_BCAST_DATA, data);
+	ssb_read32(dev, SSB_CHIPCO_BCAST_DATA); /* flush */
+}
+
+void ssb_commit_settings(struct ssb_bus *bus)
+{
+	struct ssb_device *dev;
+
+#ifdef CONFIG_SSB_DRIVER_PCICORE
+	dev = bus->chipco.dev ? bus->chipco.dev : bus->pcicore.dev;
+#else
+	dev = bus->chipco.dev;
+#endif
+	if (WARN_ON(!dev))
+		return;
+	/* This forces an update of the cached registers. */
+	ssb_broadcast_value(dev, 0xFD8, 0);
+}
+EXPORT_SYMBOL(ssb_commit_settings);
+
 u32 ssb_admatch_base(u32 adm)
 {
 	u32 base = 0;
--- a/drivers/ssb/pci.c
+++ b/drivers/ssb/pci.c
@@ -1,7 +1,7 @@
 /*
  * Sonics Silicon Backplane PCI-Hostbus related functions.
  *
- * Copyright (C) 2005-2006 Michael Buesch <mb@bu3sch.de>
+ * Copyright (C) 2005-2006 Michael Buesch <m@bues.ch>
  * Copyright (C) 2005 Martin Langer <martin-langer@gmx.de>
  * Copyright (C) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (C) 2005 Danny van Dyk <kugelfang@gentoo.org>
@@ -17,6 +17,7 @@
 
 #include <linux/ssb/ssb.h>
 #include <linux/ssb/ssb_regs.h>
+#include <linux/slab.h>
 #include <linux/pci.h>
 #include <linux/delay.h>
 
@@ -167,7 +168,7 @@ err_pci:
 }
 
 /* Get the word-offset for a SSB_SPROM_XXX define. */
-#define SPOFF(offset)	(((offset) - SSB_SPROM_BASE1) / sizeof(u16))
+#define SPOFF(offset)	((offset) / sizeof(u16))
 /* Helper to extract some _offset, which is one of the SSB_SPROM_XXX defines. */
 #define SPEX16(_outvar, _offset, _mask, _shift)	\
 	out->_outvar = ((in[SPOFF(_offset)] & (_mask)) >> (_shift))
@@ -330,7 +331,6 @@ static void sprom_extract_r123(struct ss
 {
 	int i;
 	u16 v;
-	s8 gain;
 	u16 loc[3];
 
 	if (out->revision == 3)			/* rev 3 moved MAC */
@@ -389,20 +389,52 @@ static void sprom_extract_r123(struct ss
 		SPEX(boardflags_hi, SSB_SPROM2_BFLHI, 0xFFFF, 0);
 
 	/* Extract the antenna gain values. */
-	gain = r123_extract_antgain(out->revision, in,
-				    SSB_SPROM1_AGAIN_BG,
-				    SSB_SPROM1_AGAIN_BG_SHIFT);
-	out->antenna_gain.ghz24.a0 = gain;
-	out->antenna_gain.ghz24.a1 = gain;
-	out->antenna_gain.ghz24.a2 = gain;
-	out->antenna_gain.ghz24.a3 = gain;
-	gain = r123_extract_antgain(out->revision, in,
-				    SSB_SPROM1_AGAIN_A,
-				    SSB_SPROM1_AGAIN_A_SHIFT);
-	out->antenna_gain.ghz5.a0 = gain;
-	out->antenna_gain.ghz5.a1 = gain;
-	out->antenna_gain.ghz5.a2 = gain;
-	out->antenna_gain.ghz5.a3 = gain;
+	out->antenna_gain.a0 = r123_extract_antgain(out->revision, in,
+						    SSB_SPROM1_AGAIN_BG,
+						    SSB_SPROM1_AGAIN_BG_SHIFT);
+	out->antenna_gain.a1 = r123_extract_antgain(out->revision, in,
+						    SSB_SPROM1_AGAIN_A,
+						    SSB_SPROM1_AGAIN_A_SHIFT);
+}
+
+/* Revs 4 5 and 8 have partially shared layout */
+static void sprom_extract_r458(struct ssb_sprom *out, const u16 *in)
+{
+	SPEX(txpid2g[0], SSB_SPROM4_TXPID2G01,
+	     SSB_SPROM4_TXPID2G0, SSB_SPROM4_TXPID2G0_SHIFT);
+	SPEX(txpid2g[1], SSB_SPROM4_TXPID2G01,
+	     SSB_SPROM4_TXPID2G1, SSB_SPROM4_TXPID2G1_SHIFT);
+	SPEX(txpid2g[2], SSB_SPROM4_TXPID2G23,
+	     SSB_SPROM4_TXPID2G2, SSB_SPROM4_TXPID2G2_SHIFT);
+	SPEX(txpid2g[3], SSB_SPROM4_TXPID2G23,
+	     SSB_SPROM4_TXPID2G3, SSB_SPROM4_TXPID2G3_SHIFT);
+
+	SPEX(txpid5gl[0], SSB_SPROM4_TXPID5GL01,
+	     SSB_SPROM4_TXPID5GL0, SSB_SPROM4_TXPID5GL0_SHIFT);
+	SPEX(txpid5gl[1], SSB_SPROM4_TXPID5GL01,
+	     SSB_SPROM4_TXPID5GL1, SSB_SPROM4_TXPID5GL1_SHIFT);
+	SPEX(txpid5gl[2], SSB_SPROM4_TXPID5GL23,
+	     SSB_SPROM4_TXPID5GL2, SSB_SPROM4_TXPID5GL2_SHIFT);
+	SPEX(txpid5gl[3], SSB_SPROM4_TXPID5GL23,
+	     SSB_SPROM4_TXPID5GL3, SSB_SPROM4_TXPID5GL3_SHIFT);
+
+	SPEX(txpid5g[0], SSB_SPROM4_TXPID5G01,
+	     SSB_SPROM4_TXPID5G0, SSB_SPROM4_TXPID5G0_SHIFT);
+	SPEX(txpid5g[1], SSB_SPROM4_TXPID5G01,
+	     SSB_SPROM4_TXPID5G1, SSB_SPROM4_TXPID5G1_SHIFT);
+	SPEX(txpid5g[2], SSB_SPROM4_TXPID5G23,
+	     SSB_SPROM4_TXPID5G2, SSB_SPROM4_TXPID5G2_SHIFT);
+	SPEX(txpid5g[3], SSB_SPROM4_TXPID5G23,
+	     SSB_SPROM4_TXPID5G3, SSB_SPROM4_TXPID5G3_SHIFT);
+
+	SPEX(txpid5gh[0], SSB_SPROM4_TXPID5GH01,
+	     SSB_SPROM4_TXPID5GH0, SSB_SPROM4_TXPID5GH0_SHIFT);
+	SPEX(txpid5gh[1], SSB_SPROM4_TXPID5GH01,
+	     SSB_SPROM4_TXPID5GH1, SSB_SPROM4_TXPID5GH1_SHIFT);
+	SPEX(txpid5gh[2], SSB_SPROM4_TXPID5GH23,
+	     SSB_SPROM4_TXPID5GH2, SSB_SPROM4_TXPID5GH2_SHIFT);
+	SPEX(txpid5gh[3], SSB_SPROM4_TXPID5GH23,
+	     SSB_SPROM4_TXPID5GH3, SSB_SPROM4_TXPID5GH3_SHIFT);
 }
 
 static void sprom_extract_r45(struct ssb_sprom *out, const u16 *in)
@@ -427,10 +459,14 @@ static void sprom_extract_r45(struct ssb
 		SPEX(country_code, SSB_SPROM4_CCODE, 0xFFFF, 0);
 		SPEX(boardflags_lo, SSB_SPROM4_BFLLO, 0xFFFF, 0);
 		SPEX(boardflags_hi, SSB_SPROM4_BFLHI, 0xFFFF, 0);
+		SPEX(boardflags2_lo, SSB_SPROM4_BFL2LO, 0xFFFF, 0);
+		SPEX(boardflags2_hi, SSB_SPROM4_BFL2HI, 0xFFFF, 0);
 	} else {
 		SPEX(country_code, SSB_SPROM5_CCODE, 0xFFFF, 0);
 		SPEX(boardflags_lo, SSB_SPROM5_BFLLO, 0xFFFF, 0);
 		SPEX(boardflags_hi, SSB_SPROM5_BFLHI, 0xFFFF, 0);
+		SPEX(boardflags2_lo, SSB_SPROM5_BFL2LO, 0xFFFF, 0);
+		SPEX(boardflags2_hi, SSB_SPROM5_BFL2HI, 0xFFFF, 0);
 	}
 	SPEX(ant_available_a, SSB_SPROM4_ANTAVAIL, SSB_SPROM4_ANTAVAIL_A,
 	     SSB_SPROM4_ANTAVAIL_A_SHIFT);
@@ -459,16 +495,16 @@ static void sprom_extract_r45(struct ssb
 	}
 
 	/* Extract the antenna gain values. */
-	SPEX(antenna_gain.ghz24.a0, SSB_SPROM4_AGAIN01,
+	SPEX(antenna_gain.a0, SSB_SPROM4_AGAIN01,
 	     SSB_SPROM4_AGAIN0, SSB_SPROM4_AGAIN0_SHIFT);
-	SPEX(antenna_gain.ghz24.a1, SSB_SPROM4_AGAIN01,
+	SPEX(antenna_gain.a1, SSB_SPROM4_AGAIN01,
 	     SSB_SPROM4_AGAIN1, SSB_SPROM4_AGAIN1_SHIFT);
-	SPEX(antenna_gain.ghz24.a2, SSB_SPROM4_AGAIN23,
+	SPEX(antenna_gain.a2, SSB_SPROM4_AGAIN23,
 	     SSB_SPROM4_AGAIN2, SSB_SPROM4_AGAIN2_SHIFT);
-	SPEX(antenna_gain.ghz24.a3, SSB_SPROM4_AGAIN23,
+	SPEX(antenna_gain.a3, SSB_SPROM4_AGAIN23,
 	     SSB_SPROM4_AGAIN3, SSB_SPROM4_AGAIN3_SHIFT);
-	memcpy(&out->antenna_gain.ghz5, &out->antenna_gain.ghz24,
-	       sizeof(out->antenna_gain.ghz5));
+
+	sprom_extract_r458(out, in);
 
 	/* TODO - get remaining rev 4 stuff needed */
 }
@@ -476,7 +512,13 @@ static void sprom_extract_r45(struct ssb
 static void sprom_extract_r8(struct ssb_sprom *out, const u16 *in)
 {
 	int i;
-	u16 v;
+	u16 v, o;
+	u16 pwr_info_offset[] = {
+		SSB_SROM8_PWR_INFO_CORE0, SSB_SROM8_PWR_INFO_CORE1,
+		SSB_SROM8_PWR_INFO_CORE2, SSB_SROM8_PWR_INFO_CORE3
+	};
+	BUILD_BUG_ON(ARRAY_SIZE(pwr_info_offset) !=
+			ARRAY_SIZE(out->core_pwr_info));
 
 	/* extract the MAC address */
 	for (i = 0; i < 3; i++) {
@@ -549,16 +591,71 @@ static void sprom_extract_r8(struct ssb_
 	SPEX32(ofdm5ghpo, SSB_SPROM8_OFDM5GHPO, 0xFFFFFFFF, 0);
 
 	/* Extract the antenna gain values. */
-	SPEX(antenna_gain.ghz24.a0, SSB_SPROM8_AGAIN01,
+	SPEX(antenna_gain.a0, SSB_SPROM8_AGAIN01,
 	     SSB_SPROM8_AGAIN0, SSB_SPROM8_AGAIN0_SHIFT);
-	SPEX(antenna_gain.ghz24.a1, SSB_SPROM8_AGAIN01,
+	SPEX(antenna_gain.a1, SSB_SPROM8_AGAIN01,
 	     SSB_SPROM8_AGAIN1, SSB_SPROM8_AGAIN1_SHIFT);
-	SPEX(antenna_gain.ghz24.a2, SSB_SPROM8_AGAIN23,
+	SPEX(antenna_gain.a2, SSB_SPROM8_AGAIN23,
 	     SSB_SPROM8_AGAIN2, SSB_SPROM8_AGAIN2_SHIFT);
-	SPEX(antenna_gain.ghz24.a3, SSB_SPROM8_AGAIN23,
+	SPEX(antenna_gain.a3, SSB_SPROM8_AGAIN23,
 	     SSB_SPROM8_AGAIN3, SSB_SPROM8_AGAIN3_SHIFT);
-	memcpy(&out->antenna_gain.ghz5, &out->antenna_gain.ghz24,
-	       sizeof(out->antenna_gain.ghz5));
+
+	/* Extract cores power info info */
+	for (i = 0; i < ARRAY_SIZE(pwr_info_offset); i++) {
+		o = pwr_info_offset[i];
+		SPEX(core_pwr_info[i].itssi_2g, o + SSB_SROM8_2G_MAXP_ITSSI,
+			SSB_SPROM8_2G_ITSSI, SSB_SPROM8_2G_ITSSI_SHIFT);
+		SPEX(core_pwr_info[i].maxpwr_2g, o + SSB_SROM8_2G_MAXP_ITSSI,
+			SSB_SPROM8_2G_MAXP, 0);
+
+		SPEX(core_pwr_info[i].pa_2g[0], o + SSB_SROM8_2G_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_2g[1], o + SSB_SROM8_2G_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_2g[2], o + SSB_SROM8_2G_PA_2, ~0, 0);
+
+		SPEX(core_pwr_info[i].itssi_5g, o + SSB_SROM8_5G_MAXP_ITSSI,
+			SSB_SPROM8_5G_ITSSI, SSB_SPROM8_5G_ITSSI_SHIFT);
+		SPEX(core_pwr_info[i].maxpwr_5g, o + SSB_SROM8_5G_MAXP_ITSSI,
+			SSB_SPROM8_5G_MAXP, 0);
+		SPEX(core_pwr_info[i].maxpwr_5gh, o + SSB_SPROM8_5GHL_MAXP,
+			SSB_SPROM8_5GH_MAXP, 0);
+		SPEX(core_pwr_info[i].maxpwr_5gl, o + SSB_SPROM8_5GHL_MAXP,
+			SSB_SPROM8_5GL_MAXP, SSB_SPROM8_5GL_MAXP_SHIFT);
+
+		SPEX(core_pwr_info[i].pa_5gl[0], o + SSB_SROM8_5GL_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gl[1], o + SSB_SROM8_5GL_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gl[2], o + SSB_SROM8_5GL_PA_2, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[0], o + SSB_SROM8_5G_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[1], o + SSB_SROM8_5G_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5g[2], o + SSB_SROM8_5G_PA_2, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[0], o + SSB_SROM8_5GH_PA_0, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[1], o + SSB_SROM8_5GH_PA_1, ~0, 0);
+		SPEX(core_pwr_info[i].pa_5gh[2], o + SSB_SROM8_5GH_PA_2, ~0, 0);
+	}
+
+	/* Extract FEM info */
+	SPEX(fem.ghz2.tssipos, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_TSSIPOS, SSB_SROM8_FEM_TSSIPOS_SHIFT);
+	SPEX(fem.ghz2.extpa_gain, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_EXTPA_GAIN, SSB_SROM8_FEM_EXTPA_GAIN_SHIFT);
+	SPEX(fem.ghz2.pdet_range, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_PDET_RANGE, SSB_SROM8_FEM_PDET_RANGE_SHIFT);
+	SPEX(fem.ghz2.tr_iso, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_TR_ISO, SSB_SROM8_FEM_TR_ISO_SHIFT);
+	SPEX(fem.ghz2.antswlut, SSB_SPROM8_FEM2G,
+		SSB_SROM8_FEM_ANTSWLUT, SSB_SROM8_FEM_ANTSWLUT_SHIFT);
+
+	SPEX(fem.ghz5.tssipos, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_TSSIPOS, SSB_SROM8_FEM_TSSIPOS_SHIFT);
+	SPEX(fem.ghz5.extpa_gain, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_EXTPA_GAIN, SSB_SROM8_FEM_EXTPA_GAIN_SHIFT);
+	SPEX(fem.ghz5.pdet_range, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_PDET_RANGE, SSB_SROM8_FEM_PDET_RANGE_SHIFT);
+	SPEX(fem.ghz5.tr_iso, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_TR_ISO, SSB_SROM8_FEM_TR_ISO_SHIFT);
+	SPEX(fem.ghz5.antswlut, SSB_SPROM8_FEM5G,
+		SSB_SROM8_FEM_ANTSWLUT, SSB_SROM8_FEM_ANTSWLUT_SHIFT);
+
+	sprom_extract_r458(out, in);
 
 	/* TODO - get remaining rev 8 stuff needed */
 }
@@ -572,37 +669,34 @@ static int sprom_extract(struct ssb_bus
 	ssb_dprintk(KERN_DEBUG PFX "SPROM revision %d detected.\n", out->revision);
 	memset(out->et0mac, 0xFF, 6);		/* preset et0 and et1 mac */
 	memset(out->et1mac, 0xFF, 6);
+
 	if ((bus->chip_id & 0xFF00) == 0x4400) {
 		/* Workaround: The BCM44XX chip has a stupid revision
 		 * number stored in the SPROM.
 		 * Always extract r1. */
 		out->revision = 1;
+		ssb_dprintk(KERN_DEBUG PFX "SPROM treated as revision %d\n", out->revision);
+	}
+
+	switch (out->revision) {
+	case 1:
+	case 2:
+	case 3:
 		sprom_extract_r123(out, in);
-	} else if (bus->chip_id == 0x4321) {
-		/* the BCM4328 has a chipid == 0x4321 and a rev 4 SPROM */
-		out->revision = 4;
+		break;
+	case 4:
+	case 5:
 		sprom_extract_r45(out, in);
-	} else {
-		switch (out->revision) {
-		case 1:
-		case 2:
-		case 3:
-			sprom_extract_r123(out, in);
-			break;
-		case 4:
-		case 5:
-			sprom_extract_r45(out, in);
-			break;
-		case 8:
-			sprom_extract_r8(out, in);
-			break;
-		default:
-			ssb_printk(KERN_WARNING PFX "Unsupported SPROM"
-				   "  revision %d detected. Will extract"
-				   " v1\n", out->revision);
-			out->revision = 1;
-			sprom_extract_r123(out, in);
-		}
+		break;
+	case 8:
+		sprom_extract_r8(out, in);
+		break;
+	default:
+		ssb_printk(KERN_WARNING PFX "Unsupported SPROM"
+			   " revision %d detected. Will extract"
+			   " v1\n", out->revision);
+		out->revision = 1;
+		sprom_extract_r123(out, in);
 	}
 
 	if (out->boardflags_lo == 0xFFFF)
@@ -616,15 +710,14 @@ static int sprom_extract(struct ssb_bus
 static int ssb_pci_sprom_get(struct ssb_bus *bus,
 			     struct ssb_sprom *sprom)
 {
-	const struct ssb_sprom *fallback;
-	int err = -ENOMEM;
+	int err;
 	u16 *buf;
 
 	if (!ssb_is_sprom_available(bus)) {
 		ssb_printk(KERN_ERR PFX "No SPROM available!\n");
 		return -ENODEV;
 	}
-	if (bus->chipco.dev) {	/* can be unavailible! */
+	if (bus->chipco.dev) {	/* can be unavailable! */
 		/*
 		 * get SPROM offset: SSB_SPROM_BASE1 except for
 		 * chipcommon rev >= 31 or chip ID is 0x4312 and
@@ -644,7 +737,7 @@ static int ssb_pci_sprom_get(struct ssb_
 
 	buf = kcalloc(SSB_SPROMSIZE_WORDS_R123, sizeof(u16), GFP_KERNEL);
 	if (!buf)
-		goto out;
+		return -ENOMEM;
 	bus->sprom_size = SSB_SPROMSIZE_WORDS_R123;
 	sprom_do_read(bus, buf);
 	err = sprom_check_crc(buf, bus->sprom_size);
@@ -654,17 +747,24 @@ static int ssb_pci_sprom_get(struct ssb_
 		buf = kcalloc(SSB_SPROMSIZE_WORDS_R4, sizeof(u16),
 			      GFP_KERNEL);
 		if (!buf)
-			goto out;
+			return -ENOMEM;
 		bus->sprom_size = SSB_SPROMSIZE_WORDS_R4;
 		sprom_do_read(bus, buf);
 		err = sprom_check_crc(buf, bus->sprom_size);
 		if (err) {
 			/* All CRC attempts failed.
 			 * Maybe there is no SPROM on the device?
-			 * If we have a fallback, use that. */
-			fallback = ssb_get_fallback_sprom();
-			if (fallback) {
-				memcpy(sprom, fallback, sizeof(*sprom));
+			 * Now we ask the arch code if there is some sprom
+			 * available for this device in some other storage */
+			err = ssb_fill_sprom_with_fallback(bus, sprom);
+			if (err) {
+				ssb_printk(KERN_WARNING PFX "WARNING: Using"
+					   " fallback SPROM failed (err %d)\n",
+					   err);
+			} else {
+				ssb_dprintk(KERN_DEBUG PFX "Using SPROM"
+					    " revision %d provided by"
+					    " platform.\n", sprom->revision);
 				err = 0;
 				goto out_free;
 			}
@@ -676,19 +776,15 @@ static int ssb_pci_sprom_get(struct ssb_
 
 out_free:
 	kfree(buf);
-out:
 	return err;
 }
 
 static void ssb_pci_get_boardinfo(struct ssb_bus *bus,
 				  struct ssb_boardinfo *bi)
 {
-	pci_read_config_word(bus->host_pci, PCI_SUBSYSTEM_VENDOR_ID,
-			     &bi->vendor);
-	pci_read_config_word(bus->host_pci, PCI_SUBSYSTEM_ID,
-			     &bi->type);
-	pci_read_config_word(bus->host_pci, PCI_REVISION_ID,
-			     &bi->rev);
+	bi->vendor = bus->host_pci->subsystem_vendor;
+	bi->type = bus->host_pci->subsystem_device;
+	bi->rev = bus->host_pci->revision;
 }
 
 int ssb_pci_get_invariants(struct ssb_bus *bus,
--- a/drivers/ssb/pcihost_wrapper.c
+++ b/drivers/ssb/pcihost_wrapper.c
@@ -6,12 +6,13 @@
  * Copyright (c) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (c) 2005 Danny van Dyk <kugelfang@gentoo.org>
  * Copyright (c) 2005 Andreas Jaggi <andreas.jaggi@waterwave.ch>
- * Copyright (c) 2005-2007 Michael Buesch <mbuesch@freenet.de>
+ * Copyright (c) 2005-2007 Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
 
 #include <linux/pci.h>
+#include <linux/slab.h>
 #include <linux/ssb/ssb.h>
 
 
@@ -52,12 +53,13 @@ static int ssb_pcihost_resume(struct pci
 # define ssb_pcihost_resume	NULL
 #endif /* CONFIG_PM */
 
-static int ssb_pcihost_probe(struct pci_dev *dev,
-			     const struct pci_device_id *id)
+static int __devinit ssb_pcihost_probe(struct pci_dev *dev,
+				       const struct pci_device_id *id)
 {
 	struct ssb_bus *ssb;
 	int err = -ENOMEM;
 	const char *name;
+	u32 val;
 
 	ssb = kzalloc(sizeof(*ssb), GFP_KERNEL);
 	if (!ssb)
@@ -73,6 +75,12 @@ static int ssb_pcihost_probe(struct pci_
 		goto err_pci_disable;
 	pci_set_master(dev);
 
+	/* Disable the RETRY_TIMEOUT register (0x41) to keep
+	 * PCI Tx retries from interfering with C3 CPU state */
+	pci_read_config_dword(dev, 0x40, &val);
+	if ((val & 0x0000ff00) != 0)
+		pci_write_config_dword(dev, 0x40, val & 0xffff00ff);
+
 	err = ssb_bus_pcibus_register(ssb, dev);
 	if (err)
 		goto err_pci_release_regions;
@@ -102,7 +110,7 @@ static void ssb_pcihost_remove(struct pc
 	pci_set_drvdata(dev, NULL);
 }
 
-int ssb_pcihost_register(struct pci_driver *driver)
+int __devinit ssb_pcihost_register(struct pci_driver *driver)
 {
 	driver->probe = ssb_pcihost_probe;
 	driver->remove = ssb_pcihost_remove;
--- a/drivers/ssb/pcmcia.c
+++ b/drivers/ssb/pcmcia.c
@@ -3,7 +3,7 @@
  * PCMCIA-Hostbus related functions
  *
  * Copyright 2006 Johannes Berg <johannes@sipsolutions.net>
- * Copyright 2007-2008 Michael Buesch <mb@bu3sch.de>
+ * Copyright 2007-2008 Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
@@ -617,136 +617,136 @@ static int ssb_pcmcia_sprom_check_crc(co
 	}						\
   } while (0)
 
-int ssb_pcmcia_get_invariants(struct ssb_bus *bus,
-			      struct ssb_init_invariants *iv)
+static int ssb_pcmcia_get_mac(struct pcmcia_device *p_dev,
+			tuple_t *tuple,
+			void *priv)
+{
+	struct ssb_sprom *sprom = priv;
+
+	if (tuple->TupleData[0] != CISTPL_FUNCE_LAN_NODE_ID)
+		return -EINVAL;
+	if (tuple->TupleDataLen != ETH_ALEN + 2)
+		return -EINVAL;
+	if (tuple->TupleData[1] != ETH_ALEN)
+		return -EINVAL;
+	memcpy(sprom->il0mac, &tuple->TupleData[2], ETH_ALEN);
+	return 0;
+};
+
+static int ssb_pcmcia_do_get_invariants(struct pcmcia_device *p_dev,
+					tuple_t *tuple,
+					void *priv)
 {
-	tuple_t tuple;
-	int res;
-	unsigned char buf[32];
+	struct ssb_init_invariants *iv = priv;
 	struct ssb_sprom *sprom = &iv->sprom;
 	struct ssb_boardinfo *bi = &iv->boardinfo;
 	const char *error_description;
 
+	GOTO_ERROR_ON(tuple->TupleDataLen < 1, "VEN tpl < 1");
+	switch (tuple->TupleData[0]) {
+	case SSB_PCMCIA_CIS_ID:
+		GOTO_ERROR_ON((tuple->TupleDataLen != 5) &&
+			      (tuple->TupleDataLen != 7),
+			      "id tpl size");
+		bi->vendor = tuple->TupleData[1] |
+			((u16)tuple->TupleData[2] << 8);
+		break;
+	case SSB_PCMCIA_CIS_BOARDREV:
+		GOTO_ERROR_ON(tuple->TupleDataLen != 2,
+			"boardrev tpl size");
+		sprom->board_rev = tuple->TupleData[1];
+		break;
+	case SSB_PCMCIA_CIS_PA:
+		GOTO_ERROR_ON((tuple->TupleDataLen != 9) &&
+			(tuple->TupleDataLen != 10),
+			"pa tpl size");
+		sprom->pa0b0 = tuple->TupleData[1] |
+			((u16)tuple->TupleData[2] << 8);
+		sprom->pa0b1 = tuple->TupleData[3] |
+			((u16)tuple->TupleData[4] << 8);
+		sprom->pa0b2 = tuple->TupleData[5] |
+			((u16)tuple->TupleData[6] << 8);
+		sprom->itssi_a = tuple->TupleData[7];
+		sprom->itssi_bg = tuple->TupleData[7];
+		sprom->maxpwr_a = tuple->TupleData[8];
+		sprom->maxpwr_bg = tuple->TupleData[8];
+		break;
+	case SSB_PCMCIA_CIS_OEMNAME:
+		/* We ignore this. */
+		break;
+	case SSB_PCMCIA_CIS_CCODE:
+		GOTO_ERROR_ON(tuple->TupleDataLen != 2,
+			"ccode tpl size");
+		sprom->country_code = tuple->TupleData[1];
+		break;
+	case SSB_PCMCIA_CIS_ANTENNA:
+		GOTO_ERROR_ON(tuple->TupleDataLen != 2,
+			"ant tpl size");
+		sprom->ant_available_a = tuple->TupleData[1];
+		sprom->ant_available_bg = tuple->TupleData[1];
+		break;
+	case SSB_PCMCIA_CIS_ANTGAIN:
+		GOTO_ERROR_ON(tuple->TupleDataLen != 2,
+			"antg tpl size");
+		sprom->antenna_gain.a0 = tuple->TupleData[1];
+		sprom->antenna_gain.a1 = tuple->TupleData[1];
+		sprom->antenna_gain.a2 = tuple->TupleData[1];
+		sprom->antenna_gain.a3 = tuple->TupleData[1];
+		break;
+	case SSB_PCMCIA_CIS_BFLAGS:
+		GOTO_ERROR_ON((tuple->TupleDataLen != 3) &&
+			(tuple->TupleDataLen != 5),
+			"bfl tpl size");
+		sprom->boardflags_lo = tuple->TupleData[1] |
+			((u16)tuple->TupleData[2] << 8);
+		break;
+	case SSB_PCMCIA_CIS_LEDS:
+		GOTO_ERROR_ON(tuple->TupleDataLen != 5,
+			"leds tpl size");
+		sprom->gpio0 = tuple->TupleData[1];
+		sprom->gpio1 = tuple->TupleData[2];
+		sprom->gpio2 = tuple->TupleData[3];
+		sprom->gpio3 = tuple->TupleData[4];
+		break;
+	}
+	return -ENOSPC; /* continue with next entry */
+
+error:
+	ssb_printk(KERN_ERR PFX
+		   "PCMCIA: Failed to fetch device invariants: %s\n",
+		   error_description);
+	return -ENODEV;
+}
+
+
+int ssb_pcmcia_get_invariants(struct ssb_bus *bus,
+			      struct ssb_init_invariants *iv)
+{
+	struct ssb_sprom *sprom = &iv->sprom;
+	int res;
+
 	memset(sprom, 0xFF, sizeof(*sprom));
 	sprom->revision = 1;
 	sprom->boardflags_lo = 0;
 	sprom->boardflags_hi = 0;
 
 	/* First fetch the MAC address. */
-	memset(&tuple, 0, sizeof(tuple));
-	tuple.DesiredTuple = CISTPL_FUNCE;
-	tuple.TupleData = buf;
-	tuple.TupleDataMax = sizeof(buf);
-	res = pcmcia_get_first_tuple(bus->host_pcmcia, &tuple);
-	GOTO_ERROR_ON(res != 0, "MAC first tpl");
-	res = pcmcia_get_tuple_data(bus->host_pcmcia, &tuple);
-	GOTO_ERROR_ON(res != 0, "MAC first tpl data");
-	while (1) {
-		GOTO_ERROR_ON(tuple.TupleDataLen < 1, "MAC tpl < 1");
-		if (tuple.TupleData[0] == CISTPL_FUNCE_LAN_NODE_ID)
-			break;
-		res = pcmcia_get_next_tuple(bus->host_pcmcia, &tuple);
-		GOTO_ERROR_ON(res != 0, "MAC next tpl");
-		res = pcmcia_get_tuple_data(bus->host_pcmcia, &tuple);
-		GOTO_ERROR_ON(res != 0, "MAC next tpl data");
+	res = pcmcia_loop_tuple(bus->host_pcmcia, CISTPL_FUNCE,
+				ssb_pcmcia_get_mac, sprom);
+	if (res != 0) {
+		ssb_printk(KERN_ERR PFX
+			"PCMCIA: Failed to fetch MAC address\n");
+		return -ENODEV;
 	}
-	GOTO_ERROR_ON(tuple.TupleDataLen != ETH_ALEN + 2, "MAC tpl size");
-	memcpy(sprom->il0mac, &tuple.TupleData[2], ETH_ALEN);
 
 	/* Fetch the vendor specific tuples. */
-	memset(&tuple, 0, sizeof(tuple));
-	tuple.DesiredTuple = SSB_PCMCIA_CIS;
-	tuple.TupleData = buf;
-	tuple.TupleDataMax = sizeof(buf);
-	res = pcmcia_get_first_tuple(bus->host_pcmcia, &tuple);
-	GOTO_ERROR_ON(res != 0, "VEN first tpl");
-	res = pcmcia_get_tuple_data(bus->host_pcmcia, &tuple);
-	GOTO_ERROR_ON(res != 0, "VEN first tpl data");
-	while (1) {
-		GOTO_ERROR_ON(tuple.TupleDataLen < 1, "VEN tpl < 1");
-		switch (tuple.TupleData[0]) {
-		case SSB_PCMCIA_CIS_ID:
-			GOTO_ERROR_ON((tuple.TupleDataLen != 5) &&
-				      (tuple.TupleDataLen != 7),
-				      "id tpl size");
-			bi->vendor = tuple.TupleData[1] |
-			       ((u16)tuple.TupleData[2] << 8);
-			break;
-		case SSB_PCMCIA_CIS_BOARDREV:
-			GOTO_ERROR_ON(tuple.TupleDataLen != 2,
-				      "boardrev tpl size");
-			sprom->board_rev = tuple.TupleData[1];
-			break;
-		case SSB_PCMCIA_CIS_PA:
-			GOTO_ERROR_ON((tuple.TupleDataLen != 9) &&
-				      (tuple.TupleDataLen != 10),
-				      "pa tpl size");
-			sprom->pa0b0 = tuple.TupleData[1] |
-				 ((u16)tuple.TupleData[2] << 8);
-			sprom->pa0b1 = tuple.TupleData[3] |
-				 ((u16)tuple.TupleData[4] << 8);
-			sprom->pa0b2 = tuple.TupleData[5] |
-				 ((u16)tuple.TupleData[6] << 8);
-			sprom->itssi_a = tuple.TupleData[7];
-			sprom->itssi_bg = tuple.TupleData[7];
-			sprom->maxpwr_a = tuple.TupleData[8];
-			sprom->maxpwr_bg = tuple.TupleData[8];
-			break;
-		case SSB_PCMCIA_CIS_OEMNAME:
-			/* We ignore this. */
-			break;
-		case SSB_PCMCIA_CIS_CCODE:
-			GOTO_ERROR_ON(tuple.TupleDataLen != 2,
-				      "ccode tpl size");
-			sprom->country_code = tuple.TupleData[1];
-			break;
-		case SSB_PCMCIA_CIS_ANTENNA:
-			GOTO_ERROR_ON(tuple.TupleDataLen != 2,
-				      "ant tpl size");
-			sprom->ant_available_a = tuple.TupleData[1];
-			sprom->ant_available_bg = tuple.TupleData[1];
-			break;
-		case SSB_PCMCIA_CIS_ANTGAIN:
-			GOTO_ERROR_ON(tuple.TupleDataLen != 2,
-				      "antg tpl size");
-			sprom->antenna_gain.ghz24.a0 = tuple.TupleData[1];
-			sprom->antenna_gain.ghz24.a1 = tuple.TupleData[1];
-			sprom->antenna_gain.ghz24.a2 = tuple.TupleData[1];
-			sprom->antenna_gain.ghz24.a3 = tuple.TupleData[1];
-			sprom->antenna_gain.ghz5.a0 = tuple.TupleData[1];
-			sprom->antenna_gain.ghz5.a1 = tuple.TupleData[1];
-			sprom->antenna_gain.ghz5.a2 = tuple.TupleData[1];
-			sprom->antenna_gain.ghz5.a3 = tuple.TupleData[1];
-			break;
-		case SSB_PCMCIA_CIS_BFLAGS:
-			GOTO_ERROR_ON((tuple.TupleDataLen != 3) &&
-				      (tuple.TupleDataLen != 5),
-				      "bfl tpl size");
-			sprom->boardflags_lo = tuple.TupleData[1] |
-					 ((u16)tuple.TupleData[2] << 8);
-			break;
-		case SSB_PCMCIA_CIS_LEDS:
-			GOTO_ERROR_ON(tuple.TupleDataLen != 5,
-				      "leds tpl size");
-			sprom->gpio0 = tuple.TupleData[1];
-			sprom->gpio1 = tuple.TupleData[2];
-			sprom->gpio2 = tuple.TupleData[3];
-			sprom->gpio3 = tuple.TupleData[4];
-			break;
-		}
-		res = pcmcia_get_next_tuple(bus->host_pcmcia, &tuple);
-		if (res == -ENOSPC)
-			break;
-		GOTO_ERROR_ON(res != 0, "VEN next tpl");
-		res = pcmcia_get_tuple_data(bus->host_pcmcia, &tuple);
-		GOTO_ERROR_ON(res != 0, "VEN next tpl data");
-	}
+	res = pcmcia_loop_tuple(bus->host_pcmcia, SSB_PCMCIA_CIS,
+				ssb_pcmcia_do_get_invariants, iv);
+	if ((res == 0) || (res == -ENOSPC))
+		return 0;
 
-	return 0;
-error:
 	ssb_printk(KERN_ERR PFX
-		   "PCMCIA: Failed to fetch device invariants: %s\n",
-		   error_description);
+			"PCMCIA: Failed to fetch device invariants\n");
 	return -ENODEV;
 }
 
--- a/drivers/ssb/scan.c
+++ b/drivers/ssb/scan.c
@@ -2,7 +2,7 @@
  * Sonics Silicon Backplane
  * Bus scanning
  *
- * Copyright (C) 2005-2007 Michael Buesch <mb@bu3sch.de>
+ * Copyright (C) 2005-2007 Michael Buesch <m@bues.ch>
  * Copyright (C) 2005 Martin Langer <martin-langer@gmx.de>
  * Copyright (C) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (C) 2005 Danny van Dyk <kugelfang@gentoo.org>
@@ -260,7 +260,10 @@ static int we_support_multiple_80211_cor
 #ifdef CONFIG_SSB_PCIHOST
 	if (bus->bustype == SSB_BUSTYPE_PCI) {
 		if (bus->host_pci->vendor == PCI_VENDOR_ID_BROADCOM &&
-		    bus->host_pci->device == 0x4324)
+		    ((bus->host_pci->device == 0x4313) ||
+		     (bus->host_pci->device == 0x431A) ||
+		     (bus->host_pci->device == 0x4321) ||
+		     (bus->host_pci->device == 0x4324)))
 			return 1;
 	}
 #endif /* CONFIG_SSB_PCIHOST */
@@ -309,8 +312,7 @@ int ssb_bus_scan(struct ssb_bus *bus,
 	} else {
 		if (bus->bustype == SSB_BUSTYPE_PCI) {
 			bus->chip_id = pcidev_to_chipid(bus->host_pci);
-			pci_read_config_word(bus->host_pci, PCI_REVISION_ID,
-					     &bus->chip_rev);
+			bus->chip_rev = bus->host_pci->revision;
 			bus->chip_package = 0;
 		} else {
 			bus->chip_id = 0x4710;
@@ -318,6 +320,9 @@ int ssb_bus_scan(struct ssb_bus *bus,
 			bus->chip_package = 0;
 		}
 	}
+	ssb_printk(KERN_INFO PFX "Found chip with id 0x%04X, rev 0x%02X and "
+		   "package 0x%02X\n", bus->chip_id, bus->chip_rev,
+		   bus->chip_package);
 	if (!bus->nr_devices)
 		bus->nr_devices = chipid_to_nrcores(bus->chip_id);
 	if (bus->nr_devices > ARRAY_SIZE(bus->devices)) {
@@ -354,7 +359,7 @@ int ssb_bus_scan(struct ssb_bus *bus,
 		dev->bus = bus;
 		dev->ops = bus->ops;
 
-		ssb_dprintk(KERN_INFO PFX
+		printk(KERN_DEBUG PFX
 			    "Core %d found: %s "
 			    "(cc 0x%03X, rev 0x%02X, vendor 0x%04X)\n",
 			    i, ssb_core_name(dev->id.coreid),
@@ -422,6 +427,16 @@ int ssb_bus_scan(struct ssb_bus *bus,
 			bus->pcicore.dev = dev;
 #endif /* CONFIG_SSB_DRIVER_PCICORE */
 			break;
+		case SSB_DEV_ETHERNET:
+			if (bus->bustype == SSB_BUSTYPE_PCI) {
+				if (bus->host_pci->vendor == PCI_VENDOR_ID_BROADCOM &&
+				    (bus->host_pci->device & 0xFF00) == 0x4300) {
+					/* This is a dangling ethernet core on a
+					 * wireless device. Ignore it. */
+					continue;
+				}
+			}
+			break;
 		default:
 			break;
 		}
--- a/drivers/ssb/sprom.c
+++ b/drivers/ssb/sprom.c
@@ -2,7 +2,7 @@
  * Sonics Silicon Backplane
  * Common SPROM support routines
  *
- * Copyright (C) 2005-2008 Michael Buesch <mb@bu3sch.de>
+ * Copyright (C) 2005-2008 Michael Buesch <m@bues.ch>
  * Copyright (C) 2005 Martin Langer <martin-langer@gmx.de>
  * Copyright (C) 2005 Stefano Brivio <st3@riseup.net>
  * Copyright (C) 2005 Danny van Dyk <kugelfang@gentoo.org>
@@ -14,9 +14,10 @@
 #include "ssb_private.h"
 
 #include <linux/ctype.h>
+#include <linux/slab.h>
 
 
-static const struct ssb_sprom *fallback_sprom;
+static int(*get_fallback_sprom)(struct ssb_bus *dev, struct ssb_sprom *out);
 
 
 static int sprom2hex(const u16 *sprom, char *buf, size_t buf_len,
@@ -102,6 +103,7 @@ ssize_t ssb_attr_sprom_store(struct ssb_
 	u16 *sprom;
 	int res = 0, err = -ENOMEM;
 	size_t sprom_size_words = bus->sprom_size;
+	struct ssb_freeze_context freeze;
 
 	sprom = kcalloc(bus->sprom_size, sizeof(u16), GFP_KERNEL);
 	if (!sprom)
@@ -123,18 +125,13 @@ ssize_t ssb_attr_sprom_store(struct ssb_
 	err = -ERESTARTSYS;
 	if (mutex_lock_interruptible(&bus->sprom_mutex))
 		goto out_kfree;
-	err = ssb_devices_freeze(bus);
-	if (err == -EOPNOTSUPP) {
-		ssb_printk(KERN_ERR PFX "SPROM write: Could not freeze devices. "
-			   "No suspend support. Is CONFIG_PM enabled?\n");
-		goto out_unlock;
-	}
+	err = ssb_devices_freeze(bus, &freeze);
 	if (err) {
 		ssb_printk(KERN_ERR PFX "SPROM write: Could not freeze all devices\n");
 		goto out_unlock;
 	}
 	res = sprom_write(bus, sprom);
-	err = ssb_devices_thaw(bus);
+	err = ssb_devices_thaw(&freeze);
 	if (err)
 		ssb_printk(KERN_ERR PFX "SPROM write: Could not thaw all devices\n");
 out_unlock:
@@ -148,36 +145,43 @@ out:
 }
 
 /**
- * ssb_arch_set_fallback_sprom - Set a fallback SPROM for use if no SPROM is found.
- *
- * @sprom: The SPROM data structure to register.
+ * ssb_arch_register_fallback_sprom - Registers a method providing a
+ * fallback SPROM if no SPROM is found.
  *
- * With this function the architecture implementation may register a fallback
- * SPROM data structure. The fallback is only used for PCI based SSB devices,
- * where no valid SPROM can be found in the shadow registers.
+ * @sprom_callback: The callback function.
  *
- * This function is useful for weird architectures that have a half-assed SSB device
- * hardwired to their PCI bus.
+ * With this function the architecture implementation may register a
+ * callback handler which fills the SPROM data structure. The fallback is
+ * only used for PCI based SSB devices, where no valid SPROM can be found
+ * in the shadow registers.
+ *
+ * This function is useful for weird architectures that have a half-assed
+ * SSB device hardwired to their PCI bus.
+ *
+ * Note that it does only work with PCI attached SSB devices. PCMCIA
+ * devices currently don't use this fallback.
+ * Architectures must provide the SPROM for native SSB devices anyway, so
+ * the fallback also isn't used for native devices.
  *
- * Note that it does only work with PCI attached SSB devices. PCMCIA devices currently
- * don't use this fallback.
- * Architectures must provide the SPROM for native SSB devices anyway,
- * so the fallback also isn't used for native devices.
- *
- * This function is available for architecture code, only. So it is not exported.
+ * This function is available for architecture code, only. So it is not
+ * exported.
  */
-int ssb_arch_set_fallback_sprom(const struct ssb_sprom *sprom)
+int ssb_arch_register_fallback_sprom(int (*sprom_callback)(struct ssb_bus *bus,
+				     struct ssb_sprom *out))
 {
-	if (fallback_sprom)
+	if (get_fallback_sprom)
 		return -EEXIST;
-	fallback_sprom = sprom;
+	get_fallback_sprom = sprom_callback;
 
 	return 0;
 }
 
-const struct ssb_sprom *ssb_get_fallback_sprom(void)
+int ssb_fill_sprom_with_fallback(struct ssb_bus *bus, struct ssb_sprom *out)
 {
-	return fallback_sprom;
+	if (!get_fallback_sprom)
+		return -ENOENT;
+
+	return get_fallback_sprom(bus, out);
 }
 
 /* http://bcm-v4.sipsolutions.net/802.11/IsSpromAvailable */
@@ -188,7 +192,7 @@ bool ssb_is_sprom_available(struct ssb_b
 	/* this routine differs from specs as we do not access SPROM directly
 	   on PCMCIA */
 	if (bus->bustype == SSB_BUSTYPE_PCI &&
-	    bus->chipco.dev &&	/* can be unavailible! */
+	    bus->chipco.dev &&	/* can be unavailable! */
 	    bus->chipco.dev->id.revision >= 31)
 		return bus->chipco.capabilities & SSB_CHIPCO_CAP_SPROM;
 
--- a/drivers/ssb/ssb_private.h
+++ b/drivers/ssb/ssb_private.h
@@ -171,24 +171,33 @@ ssize_t ssb_attr_sprom_store(struct ssb_
 			     const char *buf, size_t count,
 			     int (*sprom_check_crc)(const u16 *sprom, size_t size),
 			     int (*sprom_write)(struct ssb_bus *bus, const u16 *sprom));
-extern const struct ssb_sprom *ssb_get_fallback_sprom(void);
+extern int ssb_fill_sprom_with_fallback(struct ssb_bus *bus,
+					struct ssb_sprom *out);
 
 
 /* core.c */
 extern u32 ssb_calc_clock_rate(u32 plltype, u32 n, u32 m);
-extern int ssb_devices_freeze(struct ssb_bus *bus);
-extern int ssb_devices_thaw(struct ssb_bus *bus);
 extern struct ssb_bus *ssb_pci_dev_to_bus(struct pci_dev *pdev);
 int ssb_for_each_bus_call(unsigned long data,
 			  int (*func)(struct ssb_bus *bus, unsigned long data));
 extern struct ssb_bus *ssb_pcmcia_dev_to_bus(struct pcmcia_device *pdev);
 
+struct ssb_freeze_context {
+	/* Pointer to the bus */
+	struct ssb_bus *bus;
+	/* Boolean list to indicate whether a device is frozen on this bus. */
+	bool device_frozen[SSB_MAX_NR_CORES];
+};
+extern int ssb_devices_freeze(struct ssb_bus *bus, struct ssb_freeze_context *ctx);
+extern int ssb_devices_thaw(struct ssb_freeze_context *ctx);
+
+
 
 /* b43_pci_bridge.c */
 #ifdef CONFIG_SSB_B43_PCI_BRIDGE
 extern int __init b43_pci_ssb_bridge_init(void);
 extern void __exit b43_pci_ssb_bridge_exit(void);
-#else /* CONFIG_SSB_B43_PCI_BRIDGR */
+#else /* CONFIG_SSB_B43_PCI_BRIDGE */
 static inline int b43_pci_ssb_bridge_init(void)
 {
 	return 0;
@@ -196,6 +205,10 @@ static inline int b43_pci_ssb_bridge_ini
 static inline void b43_pci_ssb_bridge_exit(void)
 {
 }
-#endif /* CONFIG_SSB_PCIHOST */
+#endif /* CONFIG_SSB_B43_PCI_BRIDGE */
+
+/* driver_chipcommon_pmu.c */
+extern u32 ssb_pmu_get_cpu_clock(struct ssb_chipcommon *cc);
+extern u32 ssb_pmu_get_controlclock(struct ssb_chipcommon *cc);
 
 #endif /* LINUX_SSB_PRIVATE_H_ */
--- a/include/linux/ssb/ssb.h
+++ b/include/linux/ssb/ssb.h
@@ -16,6 +16,12 @@ struct pcmcia_device;
 struct ssb_bus;
 struct ssb_driver;
 
+struct ssb_sprom_core_pwr_info {
+	u8 itssi_2g, itssi_5g;
+	u8 maxpwr_2g, maxpwr_5gl, maxpwr_5g, maxpwr_5gh;
+	u16 pa_2g[4], pa_5gl[4], pa_5g[4], pa_5gh[4];
+};
+
 struct ssb_sprom {
 	u8 revision;
 	u8 il0mac[6];		/* MAC address for 802.11b/g */
@@ -25,8 +31,13 @@ struct ssb_sprom {
 	u8 et1phyaddr;		/* MII address for enet1 */
 	u8 et0mdcport;		/* MDIO for enet0 */
 	u8 et1mdcport;		/* MDIO for enet1 */
-	u8 board_rev;		/* Board revision number from SPROM. */
+	u16 board_rev;		/* Board revision number from SPROM. */
+	u16 board_num;		/* Board number from SPROM. */
+	u16 board_type;		/* Board type from SPROM. */
 	u8 country_code;	/* Country Code */
+	char alpha2[2];		/* Country Code as two chars like EU or US */
+	u8 leddc_on_time;	/* LED Powersave Duty Cycle On Count */
+	u8 leddc_off_time;	/* LED Powersave Duty Cycle Off Count */
 	u8 ant_available_a;	/* 2GHz antenna available bits (up to 4) */
 	u8 ant_available_bg;	/* 5GHz antenna available bits (up to 4) */
 	u16 pa0b0;
@@ -45,18 +56,22 @@ struct ssb_sprom {
 	u8 gpio1;		/* GPIO pin 1 */
 	u8 gpio2;		/* GPIO pin 2 */
 	u8 gpio3;		/* GPIO pin 3 */
-	u16 maxpwr_bg;		/* 2.4GHz Amplifier Max Power (in dBm Q5.2) */
-	u16 maxpwr_al;		/* 5.2GHz Amplifier Max Power (in dBm Q5.2) */
-	u16 maxpwr_a;		/* 5.3GHz Amplifier Max Power (in dBm Q5.2) */
-	u16 maxpwr_ah;		/* 5.8GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_bg;		/* 2.4GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_al;		/* 5.2GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_a;		/* 5.3GHz Amplifier Max Power (in dBm Q5.2) */
+	u8 maxpwr_ah;		/* 5.8GHz Amplifier Max Power (in dBm Q5.2) */
 	u8 itssi_a;		/* Idle TSSI Target for A-PHY */
 	u8 itssi_bg;		/* Idle TSSI Target for B/G-PHY */
 	u8 tri2g;		/* 2.4GHz TX isolation */
 	u8 tri5gl;		/* 5.2GHz TX isolation */
 	u8 tri5g;		/* 5.3GHz TX isolation */
 	u8 tri5gh;		/* 5.8GHz TX isolation */
-	u8 rxpo2g;		/* 2GHz RX power offset */
-	u8 rxpo5g;		/* 5GHz RX power offset */
+	u8 txpid2g[4];		/* 2GHz TX power index */
+	u8 txpid5gl[4];		/* 4.9 - 5.1GHz TX power index */
+	u8 txpid5g[4];		/* 5.1 - 5.5GHz TX power index */
+	u8 txpid5gh[4];		/* 5.5 - ...GHz TX power index */
+	s8 rxpo2g;		/* 2GHz RX power offset */
+	s8 rxpo5g;		/* 5GHz RX power offset */
 	u8 rssisav2g;		/* 2GHz RSSI params */
 	u8 rssismc2g;
 	u8 rssismf2g;
@@ -76,26 +91,104 @@ struct ssb_sprom {
 	u16 boardflags2_hi;	/* Board flags (bits 48-63) */
 	/* TODO store board flags in a single u64 */
 
+	struct ssb_sprom_core_pwr_info core_pwr_info[4];
+
 	/* Antenna gain values for up to 4 antennas
 	 * on each band. Values in dBm/4 (Q5.2). Negative gain means the
 	 * loss in the connectors is bigger than the gain. */
 	struct {
-		struct {
-			s8 a0, a1, a2, a3;
-		} ghz24;	/* 2.4GHz band */
-		struct {
-			s8 a0, a1, a2, a3;
-		} ghz5;		/* 5GHz band */
+		s8 a0, a1, a2, a3;
 	} antenna_gain;
 
-	/* TODO - add any parameters needed from rev 2, 3, 4, 5 or 8 SPROMs */
+	struct {
+		struct {
+			u8 tssipos, extpa_gain, pdet_range, tr_iso, antswlut;
+		} ghz2;
+		struct {
+			u8 tssipos, extpa_gain, pdet_range, tr_iso, antswlut;
+		} ghz5;
+	} fem;
+
+	u16 mcs2gpo[8];
+	u16 mcs5gpo[8];
+	u16 mcs5glpo[8];
+	u16 mcs5ghpo[8];
+	u8 opo;
+
+	u8 rxgainerr2ga[3];
+	u8 rxgainerr5gla[3];
+	u8 rxgainerr5gma[3];
+	u8 rxgainerr5gha[3];
+	u8 rxgainerr5gua[3];
+
+	u8 noiselvl2ga[3];
+	u8 noiselvl5gla[3];
+	u8 noiselvl5gma[3];
+	u8 noiselvl5gha[3];
+	u8 noiselvl5gua[3];
+
+	u8 regrev;
+	u8 txchain;
+	u8 rxchain;
+	u8 antswitch;
+	u16 cddpo;
+	u16 stbcpo;
+	u16 bw40po;
+	u16 bwduppo;
+
+	u8 tempthresh;
+	u8 tempoffset;
+	u16 rawtempsense;
+	u8 measpower;
+	u8 tempsense_slope;
+	u8 tempcorrx;
+	u8 tempsense_option;
+	u8 freqoffset_corr;
+	u8 iqcal_swp_dis;
+	u8 hw_iqcal_en;
+	u8 elna2g;
+	u8 elna5g;
+	u8 phycal_tempdelta;
+	u8 temps_period;
+	u8 temps_hysteresis;
+	u8 measpower1;
+	u8 measpower2;
+	u8 pcieingress_war;
+
+	/* power per rate from sromrev 9 */
+	u16 cckbw202gpo;
+	u16 cckbw20ul2gpo;
+	u32 legofdmbw202gpo;
+	u32 legofdmbw20ul2gpo;
+	u32 legofdmbw205glpo;
+	u32 legofdmbw20ul5glpo;
+	u32 legofdmbw205gmpo;
+	u32 legofdmbw20ul5gmpo;
+	u32 legofdmbw205ghpo;
+	u32 legofdmbw20ul5ghpo;
+	u32 mcsbw202gpo;
+	u32 mcsbw20ul2gpo;
+	u32 mcsbw402gpo;
+	u32 mcsbw205glpo;
+	u32 mcsbw20ul5glpo;
+	u32 mcsbw405glpo;
+	u32 mcsbw205gmpo;
+	u32 mcsbw20ul5gmpo;
+	u32 mcsbw405gmpo;
+	u32 mcsbw205ghpo;
+	u32 mcsbw20ul5ghpo;
+	u32 mcsbw405ghpo;
+	u16 mcs32po;
+	u16 legofdm40duppo;
+	u8 sar2g;
+	u8 sar5g;
 };
 
 /* Information about the PCB the circuitry is soldered on. */
 struct ssb_boardinfo {
 	u16 vendor;
 	u16 type;
-	u16 rev;
+	u8  rev;
 };
 
 
@@ -167,7 +260,7 @@ struct ssb_device {
 	 * is an optimization. */
 	const struct ssb_bus_ops *ops;
 
-	struct device *dev;
+	struct device *dev, *dma_dev;
 
 	struct ssb_bus *bus;
 	struct ssb_device_id id;
@@ -225,10 +318,9 @@ struct ssb_driver {
 #define drv_to_ssb_drv(_drv) container_of(_drv, struct ssb_driver, drv)
 
 extern int __ssb_driver_register(struct ssb_driver *drv, struct module *owner);
-static inline int ssb_driver_register(struct ssb_driver *drv)
-{
-	return __ssb_driver_register(drv, THIS_MODULE);
-}
+#define ssb_driver_register(drv) \
+	__ssb_driver_register(drv, THIS_MODULE)
+
 extern void ssb_driver_unregister(struct ssb_driver *drv);
 
 
@@ -269,7 +361,8 @@ struct ssb_bus {
 
 	const struct ssb_bus_ops *ops;
 
-	/* The core in the basic address register window. (PCI bus only) */
+	/* The core currently mapped into the MMIO window.
+	 * Not valid on all host-buses. So don't use outside of SSB. */
 	struct ssb_device *mapped_device;
 	union {
 		/* Currently mapped PCMCIA segment. (bustype == SSB_BUSTYPE_PCMCIA only) */
@@ -281,14 +374,17 @@ struct ssb_bus {
 	 * On PCMCIA-host busses this is used to protect the whole MMIO access. */
 	spinlock_t bar_lock;
 
-	/* The bus this backplane is running on. */
+	/* The host-bus this backplane is running on. */
 	enum ssb_bustype bustype;
-	/* Pointer to the PCI bus (only valid if bustype == SSB_BUSTYPE_PCI). */
-	struct pci_dev *host_pci;
-	/* Pointer to the PCMCIA device (only if bustype == SSB_BUSTYPE_PCMCIA). */
-	struct pcmcia_device *host_pcmcia;
-	/* Pointer to the SDIO device (only if bustype == SSB_BUSTYPE_SDIO). */
-	struct sdio_func *host_sdio;
+	/* Pointers to the host-bus. Check bustype before using any of these pointers. */
+	union {
+		/* Pointer to the PCI bus (only valid if bustype == SSB_BUSTYPE_PCI). */
+		struct pci_dev *host_pci;
+		/* Pointer to the PCMCIA device (only if bustype == SSB_BUSTYPE_PCMCIA). */
+		struct pcmcia_device *host_pcmcia;
+		/* Pointer to the SDIO device (only if bustype == SSB_BUSTYPE_SDIO). */
+		struct sdio_func *host_sdio;
+	};
 
 	/* See enum ssb_quirks */
 	unsigned int quirks;
@@ -300,7 +396,7 @@ struct ssb_bus {
 
 	/* ID information about the Chip. */
 	u16 chip_id;
-	u16 chip_rev;
+	u8 chip_rev;
 	u16 sprom_offset;
 	u16 sprom_size;		/* number of words in sprom */
 	u8 chip_package;
@@ -396,7 +492,9 @@ extern bool ssb_is_sprom_available(struc
 
 /* Set a fallback SPROM.
  * See kdoc at the function definition for complete documentation. */
-extern int ssb_arch_set_fallback_sprom(const struct ssb_sprom *sprom);
+extern int ssb_arch_register_fallback_sprom(
+		int (*sprom_callback)(struct ssb_bus *bus,
+		struct ssb_sprom *out));
 
 /* Suspend a SSB bus.
  * Call this from the parent bus suspend routine. */
@@ -667,6 +765,7 @@ extern int ssb_bus_may_powerdown(struct
  * Otherwise static always-on powercontrol will be used. */
 extern int ssb_bus_powerup(struct ssb_bus *bus, bool dynamic_pctl);
 
+extern void ssb_commit_settings(struct ssb_bus *bus);
 
 /* Various helper functions */
 extern u32 ssb_admatch_base(u32 adm);
--- a/include/linux/ssb/ssb_regs.h
+++ b/include/linux/ssb/ssb_regs.h
@@ -85,6 +85,8 @@
 #define  SSB_IMSTATE_AP_RSV	0x00000030 /* Reserved */
 #define  SSB_IMSTATE_IBE	0x00020000 /* In Band Error */
 #define  SSB_IMSTATE_TO		0x00040000 /* Timeout */
+#define  SSB_IMSTATE_BUSY	0x01800000 /* Busy (Backplane rev >= 2.3 only) */
+#define  SSB_IMSTATE_REJECT	0x02000000 /* Reject (Backplane rev >= 2.3 only) */
 #define SSB_INTVEC		0x0F94     /* SB Interrupt Mask */
 #define  SSB_INTVEC_PCI		0x00000001 /* Enable interrupts for PCI */
 #define  SSB_INTVEC_ENET0	0x00000002 /* Enable interrupts for enet 0 */
@@ -95,7 +97,7 @@
 #define  SSB_INTVEC_ENET1	0x00000040 /* Enable interrupts for enet 1 */
 #define SSB_TMSLOW		0x0F98     /* SB Target State Low */
 #define  SSB_TMSLOW_RESET	0x00000001 /* Reset */
-#define  SSB_TMSLOW_REJECT_22	0x00000002 /* Reject (Backplane rev 2.2) */
+#define  SSB_TMSLOW_REJECT	0x00000002 /* Reject (Standard Backplane) */
 #define  SSB_TMSLOW_REJECT_23	0x00000004 /* Reject (Backplane rev 2.3) */
 #define  SSB_TMSLOW_CLOCK	0x00010000 /* Clock Enable */
 #define  SSB_TMSLOW_FGC		0x00020000 /* Force Gated Clocks On */
@@ -172,25 +174,25 @@
 #define SSB_SPROMSIZE_BYTES_R4		(SSB_SPROMSIZE_WORDS_R4 * sizeof(u16))
 #define SSB_SPROM_BASE1			0x1000
 #define SSB_SPROM_BASE31		0x0800
-#define SSB_SPROM_REVISION		0x107E
+#define SSB_SPROM_REVISION		0x007E
 #define  SSB_SPROM_REVISION_REV		0x00FF	/* SPROM Revision number */
 #define  SSB_SPROM_REVISION_CRC		0xFF00	/* SPROM CRC8 value */
 #define  SSB_SPROM_REVISION_CRC_SHIFT	8
 
 /* SPROM Revision 1 */
-#define SSB_SPROM1_SPID			0x1004	/* Subsystem Product ID for PCI */
-#define SSB_SPROM1_SVID			0x1006	/* Subsystem Vendor ID for PCI */
-#define SSB_SPROM1_PID			0x1008	/* Product ID for PCI */
-#define SSB_SPROM1_IL0MAC		0x1048	/* 6 bytes MAC address for 802.11b/g */
-#define SSB_SPROM1_ET0MAC		0x104E	/* 6 bytes MAC address for Ethernet */
-#define SSB_SPROM1_ET1MAC		0x1054	/* 6 bytes MAC address for 802.11a */
-#define SSB_SPROM1_ETHPHY		0x105A	/* Ethernet PHY settings */
+#define SSB_SPROM1_SPID			0x0004	/* Subsystem Product ID for PCI */
+#define SSB_SPROM1_SVID			0x0006	/* Subsystem Vendor ID for PCI */
+#define SSB_SPROM1_PID			0x0008	/* Product ID for PCI */
+#define SSB_SPROM1_IL0MAC		0x0048	/* 6 bytes MAC address for 802.11b/g */
+#define SSB_SPROM1_ET0MAC		0x004E	/* 6 bytes MAC address for Ethernet */
+#define SSB_SPROM1_ET1MAC		0x0054	/* 6 bytes MAC address for 802.11a */
+#define SSB_SPROM1_ETHPHY		0x005A	/* Ethernet PHY settings */
 #define  SSB_SPROM1_ETHPHY_ET0A		0x001F	/* MII Address for enet0 */
 #define  SSB_SPROM1_ETHPHY_ET1A		0x03E0	/* MII Address for enet1 */
 #define  SSB_SPROM1_ETHPHY_ET1A_SHIFT	5
 #define  SSB_SPROM1_ETHPHY_ET0M		(1<<14)	/* MDIO for enet0 */
 #define  SSB_SPROM1_ETHPHY_ET1M		(1<<15)	/* MDIO for enet1 */
-#define SSB_SPROM1_BINF			0x105C	/* Board info */
+#define SSB_SPROM1_BINF			0x005C	/* Board info */
 #define  SSB_SPROM1_BINF_BREV		0x00FF	/* Board Revision */
 #define  SSB_SPROM1_BINF_CCODE		0x0F00	/* Country Code */
 #define  SSB_SPROM1_BINF_CCODE_SHIFT	8
@@ -198,63 +200,63 @@
 #define  SSB_SPROM1_BINF_ANTBG_SHIFT	12
 #define  SSB_SPROM1_BINF_ANTA		0xC000	/* Available A-PHY antennas */
 #define  SSB_SPROM1_BINF_ANTA_SHIFT	14
-#define SSB_SPROM1_PA0B0		0x105E
-#define SSB_SPROM1_PA0B1		0x1060
-#define SSB_SPROM1_PA0B2		0x1062
-#define SSB_SPROM1_GPIOA		0x1064	/* General Purpose IO pins 0 and 1 */
+#define SSB_SPROM1_PA0B0		0x005E
+#define SSB_SPROM1_PA0B1		0x0060
+#define SSB_SPROM1_PA0B2		0x0062
+#define SSB_SPROM1_GPIOA		0x0064	/* General Purpose IO pins 0 and 1 */
 #define  SSB_SPROM1_GPIOA_P0		0x00FF	/* Pin 0 */
 #define  SSB_SPROM1_GPIOA_P1		0xFF00	/* Pin 1 */
 #define  SSB_SPROM1_GPIOA_P1_SHIFT	8
-#define SSB_SPROM1_GPIOB		0x1066	/* General Purpuse IO pins 2 and 3 */
+#define SSB_SPROM1_GPIOB		0x0066	/* General Purpuse IO pins 2 and 3 */
 #define  SSB_SPROM1_GPIOB_P2		0x00FF	/* Pin 2 */
 #define  SSB_SPROM1_GPIOB_P3		0xFF00	/* Pin 3 */
 #define  SSB_SPROM1_GPIOB_P3_SHIFT	8
-#define SSB_SPROM1_MAXPWR		0x1068	/* Power Amplifier Max Power */
+#define SSB_SPROM1_MAXPWR		0x0068	/* Power Amplifier Max Power */
 #define  SSB_SPROM1_MAXPWR_BG		0x00FF	/* B-PHY and G-PHY (in dBm Q5.2) */
 #define  SSB_SPROM1_MAXPWR_A		0xFF00	/* A-PHY (in dBm Q5.2) */
 #define  SSB_SPROM1_MAXPWR_A_SHIFT	8
-#define SSB_SPROM1_PA1B0		0x106A
-#define SSB_SPROM1_PA1B1		0x106C
-#define SSB_SPROM1_PA1B2		0x106E
-#define SSB_SPROM1_ITSSI		0x1070	/* Idle TSSI Target */
+#define SSB_SPROM1_PA1B0		0x006A
+#define SSB_SPROM1_PA1B1		0x006C
+#define SSB_SPROM1_PA1B2		0x006E
+#define SSB_SPROM1_ITSSI		0x0070	/* Idle TSSI Target */
 #define  SSB_SPROM1_ITSSI_BG		0x00FF	/* B-PHY and G-PHY*/
 #define  SSB_SPROM1_ITSSI_A		0xFF00	/* A-PHY */
 #define  SSB_SPROM1_ITSSI_A_SHIFT	8
-#define SSB_SPROM1_BFLLO		0x1072	/* Boardflags (low 16 bits) */
-#define SSB_SPROM1_AGAIN		0x1074	/* Antenna Gain (in dBm Q5.2) */
+#define SSB_SPROM1_BFLLO		0x0072	/* Boardflags (low 16 bits) */
+#define SSB_SPROM1_AGAIN		0x0074	/* Antenna Gain (in dBm Q5.2) */
 #define  SSB_SPROM1_AGAIN_BG		0x00FF	/* B-PHY and G-PHY */
 #define  SSB_SPROM1_AGAIN_BG_SHIFT	0
 #define  SSB_SPROM1_AGAIN_A		0xFF00	/* A-PHY */
 #define  SSB_SPROM1_AGAIN_A_SHIFT	8
 
 /* SPROM Revision 2 (inherits from rev 1) */
-#define SSB_SPROM2_BFLHI		0x1038	/* Boardflags (high 16 bits) */
-#define SSB_SPROM2_MAXP_A		0x103A	/* A-PHY Max Power */
+#define SSB_SPROM2_BFLHI		0x0038	/* Boardflags (high 16 bits) */
+#define SSB_SPROM2_MAXP_A		0x003A	/* A-PHY Max Power */
 #define  SSB_SPROM2_MAXP_A_HI		0x00FF	/* Max Power High */
 #define  SSB_SPROM2_MAXP_A_LO		0xFF00	/* Max Power Low */
 #define  SSB_SPROM2_MAXP_A_LO_SHIFT	8
-#define SSB_SPROM2_PA1LOB0		0x103C	/* A-PHY PowerAmplifier Low Settings */
-#define SSB_SPROM2_PA1LOB1		0x103E	/* A-PHY PowerAmplifier Low Settings */
-#define SSB_SPROM2_PA1LOB2		0x1040	/* A-PHY PowerAmplifier Low Settings */
-#define SSB_SPROM2_PA1HIB0		0x1042	/* A-PHY PowerAmplifier High Settings */
-#define SSB_SPROM2_PA1HIB1		0x1044	/* A-PHY PowerAmplifier High Settings */
-#define SSB_SPROM2_PA1HIB2		0x1046	/* A-PHY PowerAmplifier High Settings */
-#define SSB_SPROM2_OPO			0x1078	/* OFDM Power Offset from CCK Level */
+#define SSB_SPROM2_PA1LOB0		0x003C	/* A-PHY PowerAmplifier Low Settings */
+#define SSB_SPROM2_PA1LOB1		0x003E	/* A-PHY PowerAmplifier Low Settings */
+#define SSB_SPROM2_PA1LOB2		0x0040	/* A-PHY PowerAmplifier Low Settings */
+#define SSB_SPROM2_PA1HIB0		0x0042	/* A-PHY PowerAmplifier High Settings */
+#define SSB_SPROM2_PA1HIB1		0x0044	/* A-PHY PowerAmplifier High Settings */
+#define SSB_SPROM2_PA1HIB2		0x0046	/* A-PHY PowerAmplifier High Settings */
+#define SSB_SPROM2_OPO			0x0078	/* OFDM Power Offset from CCK Level */
 #define  SSB_SPROM2_OPO_VALUE		0x00FF
 #define  SSB_SPROM2_OPO_UNUSED		0xFF00
-#define SSB_SPROM2_CCODE		0x107C	/* Two char Country Code */
+#define SSB_SPROM2_CCODE		0x007C	/* Two char Country Code */
 
 /* SPROM Revision 3 (inherits most data from rev 2) */
-#define SSB_SPROM3_IL0MAC		0x104A	/* 6 bytes MAC address for 802.11b/g */
-#define SSB_SPROM3_OFDMAPO		0x102C	/* A-PHY OFDM Mid Power Offset (4 bytes, BigEndian) */
-#define SSB_SPROM3_OFDMALPO		0x1030	/* A-PHY OFDM Low Power Offset (4 bytes, BigEndian) */
-#define SSB_SPROM3_OFDMAHPO		0x1034	/* A-PHY OFDM High Power Offset (4 bytes, BigEndian) */
-#define SSB_SPROM3_GPIOLDC		0x1042	/* GPIO LED Powersave Duty Cycle (4 bytes, BigEndian) */
+#define SSB_SPROM3_OFDMAPO		0x002C	/* A-PHY OFDM Mid Power Offset (4 bytes, BigEndian) */
+#define SSB_SPROM3_OFDMALPO		0x0030	/* A-PHY OFDM Low Power Offset (4 bytes, BigEndian) */
+#define SSB_SPROM3_OFDMAHPO		0x0034	/* A-PHY OFDM High Power Offset (4 bytes, BigEndian) */
+#define SSB_SPROM3_GPIOLDC		0x0042	/* GPIO LED Powersave Duty Cycle (4 bytes, BigEndian) */
 #define  SSB_SPROM3_GPIOLDC_OFF		0x0000FF00	/* Off Count */
 #define  SSB_SPROM3_GPIOLDC_OFF_SHIFT	8
 #define  SSB_SPROM3_GPIOLDC_ON		0x00FF0000	/* On Count */
 #define  SSB_SPROM3_GPIOLDC_ON_SHIFT	16
-#define SSB_SPROM3_CCKPO		0x1078	/* CCK Power Offset */
+#define SSB_SPROM3_IL0MAC		0x004A	/* 6 bytes MAC address for 802.11b/g */
+#define SSB_SPROM3_CCKPO		0x0078	/* CCK Power Offset */
 #define  SSB_SPROM3_CCKPO_1M		0x000F	/* 1M Rate PO */
 #define  SSB_SPROM3_CCKPO_2M		0x00F0	/* 2M Rate PO */
 #define  SSB_SPROM3_CCKPO_2M_SHIFT	4
@@ -265,100 +267,144 @@
 #define  SSB_SPROM3_OFDMGPO		0x107A	/* G-PHY OFDM Power Offset (4 bytes, BigEndian) */
 
 /* SPROM Revision 4 */
-#define SSB_SPROM4_IL0MAC		0x104C	/* 6 byte MAC address for a/b/g/n */
-#define SSB_SPROM4_ETHPHY		0x105A	/* Ethernet PHY settings ?? */
+#define SSB_SPROM4_BFLLO		0x0044	/* Boardflags (low 16 bits) */
+#define SSB_SPROM4_BFLHI		0x0046  /* Board Flags Hi */
+#define SSB_SPROM4_BFL2LO		0x0048	/* Board flags 2 (low 16 bits) */
+#define SSB_SPROM4_BFL2HI		0x004A	/* Board flags 2 Hi */
+#define SSB_SPROM4_IL0MAC		0x004C	/* 6 byte MAC address for a/b/g/n */
+#define SSB_SPROM4_CCODE		0x0052	/* Country Code (2 bytes) */
+#define SSB_SPROM4_GPIOA		0x0056	/* Gen. Purpose IO # 0 and 1 */
+#define  SSB_SPROM4_GPIOA_P0		0x00FF	/* Pin 0 */
+#define  SSB_SPROM4_GPIOA_P1		0xFF00	/* Pin 1 */
+#define  SSB_SPROM4_GPIOA_P1_SHIFT	8
+#define SSB_SPROM4_GPIOB		0x0058	/* Gen. Purpose IO # 2 and 3 */
+#define  SSB_SPROM4_GPIOB_P2		0x00FF	/* Pin 2 */
+#define  SSB_SPROM4_GPIOB_P3		0xFF00	/* Pin 3 */
+#define  SSB_SPROM4_GPIOB_P3_SHIFT	8
+#define SSB_SPROM4_ETHPHY		0x005A	/* Ethernet PHY settings ?? */
 #define  SSB_SPROM4_ETHPHY_ET0A		0x001F	/* MII Address for enet0 */
 #define  SSB_SPROM4_ETHPHY_ET1A		0x03E0	/* MII Address for enet1 */
 #define  SSB_SPROM4_ETHPHY_ET1A_SHIFT	5
 #define  SSB_SPROM4_ETHPHY_ET0M		(1<<14)	/* MDIO for enet0 */
 #define  SSB_SPROM4_ETHPHY_ET1M		(1<<15)	/* MDIO for enet1 */
-#define SSB_SPROM4_CCODE		0x1052	/* Country Code (2 bytes) */
-#define SSB_SPROM4_ANTAVAIL		0x105D  /* Antenna available bitfields */
-#define SSB_SPROM4_ANTAVAIL_A		0x00FF	/* A-PHY bitfield */
-#define SSB_SPROM4_ANTAVAIL_A_SHIFT	0
-#define SSB_SPROM4_ANTAVAIL_BG		0xFF00	/* B-PHY and G-PHY bitfield */
-#define SSB_SPROM4_ANTAVAIL_BG_SHIFT	8
-#define SSB_SPROM4_BFLLO		0x1044	/* Boardflags (low 16 bits) */
-#define SSB_SPROM4_AGAIN01		0x105E	/* Antenna Gain (in dBm Q5.2) */
+#define SSB_SPROM4_ANTAVAIL		0x005D  /* Antenna available bitfields */
+#define  SSB_SPROM4_ANTAVAIL_A		0x00FF	/* A-PHY bitfield */
+#define  SSB_SPROM4_ANTAVAIL_A_SHIFT	0
+#define  SSB_SPROM4_ANTAVAIL_BG		0xFF00	/* B-PHY and G-PHY bitfield */
+#define  SSB_SPROM4_ANTAVAIL_BG_SHIFT	8
+#define SSB_SPROM4_AGAIN01		0x005E	/* Antenna Gain (in dBm Q5.2) */
 #define  SSB_SPROM4_AGAIN0		0x00FF	/* Antenna 0 */
 #define  SSB_SPROM4_AGAIN0_SHIFT	0
 #define  SSB_SPROM4_AGAIN1		0xFF00	/* Antenna 1 */
 #define  SSB_SPROM4_AGAIN1_SHIFT	8
-#define SSB_SPROM4_AGAIN23		0x1060
+#define SSB_SPROM4_AGAIN23		0x0060
 #define  SSB_SPROM4_AGAIN2		0x00FF	/* Antenna 2 */
 #define  SSB_SPROM4_AGAIN2_SHIFT	0
 #define  SSB_SPROM4_AGAIN3		0xFF00	/* Antenna 3 */
 #define  SSB_SPROM4_AGAIN3_SHIFT	8
-#define SSB_SPROM4_BFLHI		0x1046  /* Board Flags Hi */
-#define SSB_SPROM4_MAXP_BG		0x1080  /* Max Power BG in path 1 */
+#define SSB_SPROM4_TXPID2G01		0x0062 	/* TX Power Index 2GHz */
+#define  SSB_SPROM4_TXPID2G0		0x00FF
+#define  SSB_SPROM4_TXPID2G0_SHIFT	0
+#define  SSB_SPROM4_TXPID2G1		0xFF00
+#define  SSB_SPROM4_TXPID2G1_SHIFT	8
+#define SSB_SPROM4_TXPID2G23		0x0064 	/* TX Power Index 2GHz */
+#define  SSB_SPROM4_TXPID2G2		0x00FF
+#define  SSB_SPROM4_TXPID2G2_SHIFT	0
+#define  SSB_SPROM4_TXPID2G3		0xFF00
+#define  SSB_SPROM4_TXPID2G3_SHIFT	8
+#define SSB_SPROM4_TXPID5G01		0x0066 	/* TX Power Index 5GHz middle subband */
+#define  SSB_SPROM4_TXPID5G0		0x00FF
+#define  SSB_SPROM4_TXPID5G0_SHIFT	0
+#define  SSB_SPROM4_TXPID5G1		0xFF00
+#define  SSB_SPROM4_TXPID5G1_SHIFT	8
+#define SSB_SPROM4_TXPID5G23		0x0068 	/* TX Power Index 5GHz middle subband */
+#define  SSB_SPROM4_TXPID5G2		0x00FF
+#define  SSB_SPROM4_TXPID5G2_SHIFT	0
+#define  SSB_SPROM4_TXPID5G3		0xFF00
+#define  SSB_SPROM4_TXPID5G3_SHIFT	8
+#define SSB_SPROM4_TXPID5GL01		0x006A 	/* TX Power Index 5GHz low subband */
+#define  SSB_SPROM4_TXPID5GL0		0x00FF
+#define  SSB_SPROM4_TXPID5GL0_SHIFT	0
+#define  SSB_SPROM4_TXPID5GL1		0xFF00
+#define  SSB_SPROM4_TXPID5GL1_SHIFT	8
+#define SSB_SPROM4_TXPID5GL23		0x006C 	/* TX Power Index 5GHz low subband */
+#define  SSB_SPROM4_TXPID5GL2		0x00FF
+#define  SSB_SPROM4_TXPID5GL2_SHIFT	0
+#define  SSB_SPROM4_TXPID5GL3		0xFF00
+#define  SSB_SPROM4_TXPID5GL3_SHIFT	8
+#define SSB_SPROM4_TXPID5GH01		0x006E 	/* TX Power Index 5GHz high subband */
+#define  SSB_SPROM4_TXPID5GH0		0x00FF
+#define  SSB_SPROM4_TXPID5GH0_SHIFT	0
+#define  SSB_SPROM4_TXPID5GH1		0xFF00
+#define  SSB_SPROM4_TXPID5GH1_SHIFT	8
+#define SSB_SPROM4_TXPID5GH23		0x0070 	/* TX Power Index 5GHz high subband */
+#define  SSB_SPROM4_TXPID5GH2		0x00FF
+#define  SSB_SPROM4_TXPID5GH2_SHIFT	0
+#define  SSB_SPROM4_TXPID5GH3		0xFF00
+#define  SSB_SPROM4_TXPID5GH3_SHIFT	8
+#define SSB_SPROM4_MAXP_BG		0x0080  /* Max Power BG in path 1 */
 #define  SSB_SPROM4_MAXP_BG_MASK	0x00FF  /* Mask for Max Power BG */
 #define  SSB_SPROM4_ITSSI_BG		0xFF00	/* Mask for path 1 itssi_bg */
 #define  SSB_SPROM4_ITSSI_BG_SHIFT	8
-#define SSB_SPROM4_MAXP_A		0x108A  /* Max Power A in path 1 */
+#define SSB_SPROM4_MAXP_A		0x008A  /* Max Power A in path 1 */
 #define  SSB_SPROM4_MAXP_A_MASK		0x00FF  /* Mask for Max Power A */
 #define  SSB_SPROM4_ITSSI_A		0xFF00	/* Mask for path 1 itssi_a */
 #define  SSB_SPROM4_ITSSI_A_SHIFT	8
-#define SSB_SPROM4_GPIOA		0x1056	/* Gen. Purpose IO # 0 and 1 */
-#define  SSB_SPROM4_GPIOA_P0		0x00FF	/* Pin 0 */
-#define  SSB_SPROM4_GPIOA_P1		0xFF00	/* Pin 1 */
-#define  SSB_SPROM4_GPIOA_P1_SHIFT	8
-#define SSB_SPROM4_GPIOB		0x1058	/* Gen. Purpose IO # 2 and 3 */
-#define  SSB_SPROM4_GPIOB_P2		0x00FF	/* Pin 2 */
-#define  SSB_SPROM4_GPIOB_P3		0xFF00	/* Pin 3 */
-#define  SSB_SPROM4_GPIOB_P3_SHIFT	8
-#define SSB_SPROM4_PA0B0		0x1082	/* The paXbY locations are */
-#define SSB_SPROM4_PA0B1		0x1084	/*   only guesses */
-#define SSB_SPROM4_PA0B2		0x1086
-#define SSB_SPROM4_PA1B0		0x108E
-#define SSB_SPROM4_PA1B1		0x1090
-#define SSB_SPROM4_PA1B2		0x1092
+#define SSB_SPROM4_PA0B0		0x0082	/* The paXbY locations are */
+#define SSB_SPROM4_PA0B1		0x0084	/*   only guesses */
+#define SSB_SPROM4_PA0B2		0x0086
+#define SSB_SPROM4_PA1B0		0x008E
+#define SSB_SPROM4_PA1B1		0x0090
+#define SSB_SPROM4_PA1B2		0x0092
 
 /* SPROM Revision 5 (inherits most data from rev 4) */
-#define SSB_SPROM5_BFLLO		0x104A	/* Boardflags (low 16 bits) */
-#define SSB_SPROM5_BFLHI		0x104C  /* Board Flags Hi */
-#define SSB_SPROM5_IL0MAC		0x1052	/* 6 byte MAC address for a/b/g/n */
-#define SSB_SPROM5_CCODE		0x1044	/* Country Code (2 bytes) */
-#define SSB_SPROM5_GPIOA		0x1076	/* Gen. Purpose IO # 0 and 1 */
+#define SSB_SPROM5_CCODE		0x0044	/* Country Code (2 bytes) */
+#define SSB_SPROM5_BFLLO		0x004A	/* Boardflags (low 16 bits) */
+#define SSB_SPROM5_BFLHI		0x004C  /* Board Flags Hi */
+#define SSB_SPROM5_BFL2LO		0x004E	/* Board flags 2 (low 16 bits) */
+#define SSB_SPROM5_BFL2HI		0x0050	/* Board flags 2 Hi */
+#define SSB_SPROM5_IL0MAC		0x0052	/* 6 byte MAC address for a/b/g/n */
+#define SSB_SPROM5_GPIOA		0x0076	/* Gen. Purpose IO # 0 and 1 */
 #define  SSB_SPROM5_GPIOA_P0		0x00FF	/* Pin 0 */
 #define  SSB_SPROM5_GPIOA_P1		0xFF00	/* Pin 1 */
 #define  SSB_SPROM5_GPIOA_P1_SHIFT	8
-#define SSB_SPROM5_GPIOB		0x1078	/* Gen. Purpose IO # 2 and 3 */
+#define SSB_SPROM5_GPIOB		0x0078	/* Gen. Purpose IO # 2 and 3 */
 #define  SSB_SPROM5_GPIOB_P2		0x00FF	/* Pin 2 */
 #define  SSB_SPROM5_GPIOB_P3		0xFF00	/* Pin 3 */
 #define  SSB_SPROM5_GPIOB_P3_SHIFT	8
 
 /* SPROM Revision 8 */
-#define SSB_SPROM8_BOARDREV		0x1082	/* Board revision */
-#define SSB_SPROM8_BFLLO		0x1084	/* Board flags (bits 0-15) */
-#define SSB_SPROM8_BFLHI		0x1086	/* Board flags (bits 16-31) */
-#define SSB_SPROM8_BFL2LO		0x1088	/* Board flags (bits 32-47) */
-#define SSB_SPROM8_BFL2HI		0x108A	/* Board flags (bits 48-63) */
-#define SSB_SPROM8_IL0MAC		0x108C	/* 6 byte MAC address */
-#define SSB_SPROM8_CCODE		0x1092	/* 2 byte country code */
-#define SSB_SPROM8_ANTAVAIL		0x109C  /* Antenna available bitfields*/
-#define SSB_SPROM8_ANTAVAIL_A		0xFF00	/* A-PHY bitfield */
-#define SSB_SPROM8_ANTAVAIL_A_SHIFT	8
-#define SSB_SPROM8_ANTAVAIL_BG		0x00FF	/* B-PHY and G-PHY bitfield */
-#define SSB_SPROM8_ANTAVAIL_BG_SHIFT	0
-#define SSB_SPROM8_AGAIN01		0x109E	/* Antenna Gain (in dBm Q5.2) */
+#define SSB_SPROM8_BOARDREV		0x0082	/* Board revision */
+#define SSB_SPROM8_BFLLO		0x0084	/* Board flags (bits 0-15) */
+#define SSB_SPROM8_BFLHI		0x0086	/* Board flags (bits 16-31) */
+#define SSB_SPROM8_BFL2LO		0x0088	/* Board flags (bits 32-47) */
+#define SSB_SPROM8_BFL2HI		0x008A	/* Board flags (bits 48-63) */
+#define SSB_SPROM8_IL0MAC		0x008C	/* 6 byte MAC address */
+#define SSB_SPROM8_CCODE		0x0092	/* 2 byte country code */
+#define SSB_SPROM8_GPIOA		0x0096	/*Gen. Purpose IO # 0 and 1 */
+#define  SSB_SPROM8_GPIOA_P0		0x00FF	/* Pin 0 */
+#define  SSB_SPROM8_GPIOA_P1		0xFF00	/* Pin 1 */
+#define  SSB_SPROM8_GPIOA_P1_SHIFT	8
+#define SSB_SPROM8_GPIOB		0x0098	/* Gen. Purpose IO # 2 and 3 */
+#define  SSB_SPROM8_GPIOB_P2		0x00FF	/* Pin 2 */
+#define  SSB_SPROM8_GPIOB_P3		0xFF00	/* Pin 3 */
+#define  SSB_SPROM8_GPIOB_P3_SHIFT	8
+#define SSB_SPROM8_ANTAVAIL		0x009C  /* Antenna available bitfields*/
+#define  SSB_SPROM8_ANTAVAIL_A		0xFF00	/* A-PHY bitfield */
+#define  SSB_SPROM8_ANTAVAIL_A_SHIFT	8
+#define  SSB_SPROM8_ANTAVAIL_BG		0x00FF	/* B-PHY and G-PHY bitfield */
+#define  SSB_SPROM8_ANTAVAIL_BG_SHIFT	0
+#define SSB_SPROM8_AGAIN01		0x009E	/* Antenna Gain (in dBm Q5.2) */
 #define  SSB_SPROM8_AGAIN0		0x00FF	/* Antenna 0 */
 #define  SSB_SPROM8_AGAIN0_SHIFT	0
 #define  SSB_SPROM8_AGAIN1		0xFF00	/* Antenna 1 */
 #define  SSB_SPROM8_AGAIN1_SHIFT	8
-#define SSB_SPROM8_AGAIN23		0x10A0
+#define SSB_SPROM8_AGAIN23		0x00A0
 #define  SSB_SPROM8_AGAIN2		0x00FF	/* Antenna 2 */
 #define  SSB_SPROM8_AGAIN2_SHIFT	0
 #define  SSB_SPROM8_AGAIN3		0xFF00	/* Antenna 3 */
 #define  SSB_SPROM8_AGAIN3_SHIFT	8
-#define SSB_SPROM8_GPIOA		0x1096	/*Gen. Purpose IO # 0 and 1 */
-#define  SSB_SPROM8_GPIOA_P0		0x00FF	/* Pin 0 */
-#define  SSB_SPROM8_GPIOA_P1		0xFF00	/* Pin 1 */
-#define  SSB_SPROM8_GPIOA_P1_SHIFT	8
-#define SSB_SPROM8_GPIOB		0x1098	/* Gen. Purpose IO # 2 and 3 */
-#define  SSB_SPROM8_GPIOB_P2		0x00FF	/* Pin 2 */
-#define  SSB_SPROM8_GPIOB_P3		0xFF00	/* Pin 3 */
-#define  SSB_SPROM8_GPIOB_P3_SHIFT	8
-#define SSB_SPROM8_RSSIPARM2G		0x10A4	/* RSSI params for 2GHz */
+#define SSB_SPROM8_RSSIPARM2G		0x00A4	/* RSSI params for 2GHz */
 #define  SSB_SPROM8_RSSISMF2G		0x000F
 #define  SSB_SPROM8_RSSISMC2G		0x00F0
 #define  SSB_SPROM8_RSSISMC2G_SHIFT	4
@@ -366,7 +412,7 @@
 #define  SSB_SPROM8_RSSISAV2G_SHIFT	8
 #define  SSB_SPROM8_BXA2G		0x1800
 #define  SSB_SPROM8_BXA2G_SHIFT		11
-#define SSB_SPROM8_RSSIPARM5G		0x10A6	/* RSSI params for 5GHz */
+#define SSB_SPROM8_RSSIPARM5G		0x00A6	/* RSSI params for 5GHz */
 #define  SSB_SPROM8_RSSISMF5G		0x000F
 #define  SSB_SPROM8_RSSISMC5G		0x00F0
 #define  SSB_SPROM8_RSSISMC5G_SHIFT	4
@@ -374,47 +420,138 @@
 #define  SSB_SPROM8_RSSISAV5G_SHIFT	8
 #define  SSB_SPROM8_BXA5G		0x1800
 #define  SSB_SPROM8_BXA5G_SHIFT		11
-#define SSB_SPROM8_TRI25G		0x10A8	/* TX isolation 2.4&5.3GHz */
+#define SSB_SPROM8_TRI25G		0x00A8	/* TX isolation 2.4&5.3GHz */
 #define  SSB_SPROM8_TRI2G		0x00FF	/* TX isolation 2.4GHz */
 #define  SSB_SPROM8_TRI5G		0xFF00	/* TX isolation 5.3GHz */
 #define  SSB_SPROM8_TRI5G_SHIFT		8
-#define SSB_SPROM8_TRI5GHL		0x10AA	/* TX isolation 5.2/5.8GHz */
+#define SSB_SPROM8_TRI5GHL		0x00AA	/* TX isolation 5.2/5.8GHz */
 #define  SSB_SPROM8_TRI5GL		0x00FF	/* TX isolation 5.2GHz */
 #define  SSB_SPROM8_TRI5GH		0xFF00	/* TX isolation 5.8GHz */
 #define  SSB_SPROM8_TRI5GH_SHIFT	8
-#define SSB_SPROM8_RXPO			0x10AC  /* RX power offsets */
+#define SSB_SPROM8_RXPO			0x00AC  /* RX power offsets */
 #define  SSB_SPROM8_RXPO2G		0x00FF	/* 2GHz RX power offset */
 #define  SSB_SPROM8_RXPO5G		0xFF00	/* 5GHz RX power offset */
 #define  SSB_SPROM8_RXPO5G_SHIFT	8
-#define SSB_SPROM8_MAXP_BG		0x10C0  /* Max Power 2GHz in path 1 */
+#define SSB_SPROM8_FEM2G		0x00AE
+#define SSB_SPROM8_FEM5G		0x00B0
+#define  SSB_SROM8_FEM_TSSIPOS		0x0001
+#define  SSB_SROM8_FEM_TSSIPOS_SHIFT	0
+#define  SSB_SROM8_FEM_EXTPA_GAIN	0x0006
+#define  SSB_SROM8_FEM_EXTPA_GAIN_SHIFT	1
+#define  SSB_SROM8_FEM_PDET_RANGE	0x00F8
+#define  SSB_SROM8_FEM_PDET_RANGE_SHIFT	3
+#define  SSB_SROM8_FEM_TR_ISO		0x0700
+#define  SSB_SROM8_FEM_TR_ISO_SHIFT	8
+#define  SSB_SROM8_FEM_ANTSWLUT		0xF800
+#define  SSB_SROM8_FEM_ANTSWLUT_SHIFT	11
+#define SSB_SPROM8_THERMAL		0x00B2
+#define SSB_SPROM8_MPWR_RAWTS		0x00B4
+#define SSB_SPROM8_TS_SLP_OPT_CORRX	0x00B6
+#define SSB_SPROM8_FOC_HWIQ_IQSWP	0x00B8
+#define SSB_SPROM8_PHYCAL_TEMPDELTA	0x00BA
+
+/* There are 4 blocks with power info sharing the same layout */
+#define SSB_SROM8_PWR_INFO_CORE0	0x00C0
+#define SSB_SROM8_PWR_INFO_CORE1	0x00E0
+#define SSB_SROM8_PWR_INFO_CORE2	0x0100
+#define SSB_SROM8_PWR_INFO_CORE3	0x0120
+
+#define SSB_SROM8_2G_MAXP_ITSSI		0x00
+#define  SSB_SPROM8_2G_MAXP		0x00FF
+#define  SSB_SPROM8_2G_ITSSI		0xFF00
+#define  SSB_SPROM8_2G_ITSSI_SHIFT	8
+#define SSB_SROM8_2G_PA_0		0x02	/* 2GHz power amp settings */
+#define SSB_SROM8_2G_PA_1		0x04
+#define SSB_SROM8_2G_PA_2		0x06
+#define SSB_SROM8_5G_MAXP_ITSSI		0x08	/* 5GHz ITSSI and 5.3GHz Max Power */
+#define  SSB_SPROM8_5G_MAXP		0x00FF
+#define  SSB_SPROM8_5G_ITSSI		0xFF00
+#define  SSB_SPROM8_5G_ITSSI_SHIFT	8
+#define SSB_SPROM8_5GHL_MAXP		0x0A	/* 5.2GHz and 5.8GHz Max Power */
+#define  SSB_SPROM8_5GH_MAXP		0x00FF
+#define  SSB_SPROM8_5GL_MAXP		0xFF00
+#define  SSB_SPROM8_5GL_MAXP_SHIFT	8
+#define SSB_SROM8_5G_PA_0		0x0C	/* 5.3GHz power amp settings */
+#define SSB_SROM8_5G_PA_1		0x0E
+#define SSB_SROM8_5G_PA_2		0x10
+#define SSB_SROM8_5GL_PA_0		0x12	/* 5.2GHz power amp settings */
+#define SSB_SROM8_5GL_PA_1		0x14
+#define SSB_SROM8_5GL_PA_2		0x16
+#define SSB_SROM8_5GH_PA_0		0x18	/* 5.8GHz power amp settings */
+#define SSB_SROM8_5GH_PA_1		0x1A
+#define SSB_SROM8_5GH_PA_2		0x1C
+
+/* TODO: Make it deprecated */
+#define SSB_SPROM8_MAXP_BG		0x00C0  /* Max Power 2GHz in path 1 */
 #define  SSB_SPROM8_MAXP_BG_MASK	0x00FF  /* Mask for Max Power 2GHz */
 #define  SSB_SPROM8_ITSSI_BG		0xFF00	/* Mask for path 1 itssi_bg */
 #define  SSB_SPROM8_ITSSI_BG_SHIFT	8
-#define SSB_SPROM8_PA0B0		0x10C2	/* 2GHz power amp settings */
-#define SSB_SPROM8_PA0B1		0x10C4
-#define SSB_SPROM8_PA0B2		0x10C6
-#define SSB_SPROM8_MAXP_A		0x10C8  /* Max Power 5.3GHz */
+#define SSB_SPROM8_PA0B0		0x00C2	/* 2GHz power amp settings */
+#define SSB_SPROM8_PA0B1		0x00C4
+#define SSB_SPROM8_PA0B2		0x00C6
+#define SSB_SPROM8_MAXP_A		0x00C8  /* Max Power 5.3GHz */
 #define  SSB_SPROM8_MAXP_A_MASK		0x00FF  /* Mask for Max Power 5.3GHz */
 #define  SSB_SPROM8_ITSSI_A		0xFF00	/* Mask for path 1 itssi_a */
 #define  SSB_SPROM8_ITSSI_A_SHIFT	8
-#define SSB_SPROM8_MAXP_AHL		0x10CA  /* Max Power 5.2/5.8GHz */
+#define SSB_SPROM8_MAXP_AHL		0x00CA  /* Max Power 5.2/5.8GHz */
 #define  SSB_SPROM8_MAXP_AH_MASK	0x00FF  /* Mask for Max Power 5.8GHz */
 #define  SSB_SPROM8_MAXP_AL_MASK	0xFF00  /* Mask for Max Power 5.2GHz */
 #define  SSB_SPROM8_MAXP_AL_SHIFT	8
-#define SSB_SPROM8_PA1B0		0x10CC	/* 5.3GHz power amp settings */
-#define SSB_SPROM8_PA1B1		0x10CE
-#define SSB_SPROM8_PA1B2		0x10D0
-#define SSB_SPROM8_PA1LOB0		0x10D2	/* 5.2GHz power amp settings */
-#define SSB_SPROM8_PA1LOB1		0x10D4
-#define SSB_SPROM8_PA1LOB2		0x10D6
-#define SSB_SPROM8_PA1HIB0		0x10D8	/* 5.8GHz power amp settings */
-#define SSB_SPROM8_PA1HIB1		0x10DA
-#define SSB_SPROM8_PA1HIB2		0x10DC
-#define SSB_SPROM8_CCK2GPO		0x1140	/* CCK power offset */
-#define SSB_SPROM8_OFDM2GPO		0x1142	/* 2.4GHz OFDM power offset */
-#define SSB_SPROM8_OFDM5GPO		0x1146	/* 5.3GHz OFDM power offset */
-#define SSB_SPROM8_OFDM5GLPO		0x114A	/* 5.2GHz OFDM power offset */
-#define SSB_SPROM8_OFDM5GHPO		0x114E	/* 5.8GHz OFDM power offset */
+#define SSB_SPROM8_PA1B0		0x00CC	/* 5.3GHz power amp settings */
+#define SSB_SPROM8_PA1B1		0x00CE
+#define SSB_SPROM8_PA1B2		0x00D0
+#define SSB_SPROM8_PA1LOB0		0x00D2	/* 5.2GHz power amp settings */
+#define SSB_SPROM8_PA1LOB1		0x00D4
+#define SSB_SPROM8_PA1LOB2		0x00D6
+#define SSB_SPROM8_PA1HIB0		0x00D8	/* 5.8GHz power amp settings */
+#define SSB_SPROM8_PA1HIB1		0x00DA
+#define SSB_SPROM8_PA1HIB2		0x00DC
+
+#define SSB_SPROM8_CCK2GPO		0x0140	/* CCK power offset */
+#define SSB_SPROM8_OFDM2GPO		0x0142	/* 2.4GHz OFDM power offset */
+#define SSB_SPROM8_OFDM5GPO		0x0146	/* 5.3GHz OFDM power offset */
+#define SSB_SPROM8_OFDM5GLPO		0x014A	/* 5.2GHz OFDM power offset */
+#define SSB_SPROM8_OFDM5GHPO		0x014E	/* 5.8GHz OFDM power offset */
+
+/* Values for boardflags_lo read from SPROM */
+#define SSB_BFL_BTCOEXIST		0x0001	/* implements Bluetooth coexistance */
+#define SSB_BFL_PACTRL			0x0002	/* GPIO 9 controlling the PA */
+#define SSB_BFL_AIRLINEMODE		0x0004	/* implements GPIO 13 radio disable indication */
+#define SSB_BFL_RSSI			0x0008	/* software calculates nrssi slope. */
+#define SSB_BFL_ENETSPI			0x0010	/* has ephy roboswitch spi */
+#define SSB_BFL_XTAL_NOSLOW		0x0020	/* no slow clock available */
+#define SSB_BFL_CCKHIPWR		0x0040	/* can do high power CCK transmission */
+#define SSB_BFL_ENETADM			0x0080	/* has ADMtek switch */
+#define SSB_BFL_ENETVLAN		0x0100	/* can do vlan */
+#define SSB_BFL_AFTERBURNER		0x0200	/* supports Afterburner mode */
+#define SSB_BFL_NOPCI			0x0400	/* board leaves PCI floating */
+#define SSB_BFL_FEM			0x0800	/* supports the Front End Module */
+#define SSB_BFL_EXTLNA			0x1000	/* has an external LNA */
+#define SSB_BFL_HGPA			0x2000	/* had high gain PA */
+#define SSB_BFL_BTCMOD			0x4000	/* BFL_BTCOEXIST is given in alternate GPIOs */
+#define SSB_BFL_ALTIQ			0x8000	/* alternate I/Q settings */
+
+/* Values for boardflags_hi read from SPROM */
+#define SSB_BFH_NOPA			0x0001	/* has no PA */
+#define SSB_BFH_RSSIINV			0x0002	/* RSSI uses positive slope (not TSSI) */
+#define SSB_BFH_PAREF			0x0004	/* uses the PARef LDO */
+#define SSB_BFH_3TSWITCH		0x0008	/* uses a triple throw switch shared with bluetooth */
+#define SSB_BFH_PHASESHIFT		0x0010	/* can support phase shifter */
+#define SSB_BFH_BUCKBOOST		0x0020	/* has buck/booster */
+#define SSB_BFH_FEM_BT			0x0040	/* has FEM and switch to share antenna with bluetooth */
+
+/* Values for boardflags2_lo read from SPROM */
+#define SSB_BFL2_RXBB_INT_REG_DIS	0x0001	/* external RX BB regulator present */
+#define SSB_BFL2_APLL_WAR		0x0002	/* alternative A-band PLL settings implemented */
+#define SSB_BFL2_TXPWRCTRL_EN 		0x0004	/* permits enabling TX Power Control */
+#define SSB_BFL2_2X4_DIV		0x0008	/* 2x4 diversity switch */
+#define SSB_BFL2_5G_PWRGAIN		0x0010	/* supports 5G band power gain */
+#define SSB_BFL2_PCIEWAR_OVR		0x0020	/* overrides ASPM and Clkreq settings */
+#define SSB_BFL2_CAESERS_BRD		0x0040	/* is Caesers board (unused) */
+#define SSB_BFL2_BTC3WIRE		0x0080	/* used 3-wire bluetooth coexist */
+#define SSB_BFL2_SKWRKFEM_BRD		0x0100	/* 4321mcm93 uses Skyworks FEM */
+#define SSB_BFL2_SPUR_WAR		0x0200	/* has a workaround for clock-harmonic spurs */
+#define SSB_BFL2_GPLL_WAR		0x0400	/* altenative G-band PLL settings implemented */
 
 /* Values for SSB_SPROM1_BINF_CCODE */
 enum {
--- a/include/linux/ssb/ssb_driver_chipcommon.h
+++ b/include/linux/ssb/ssb_driver_chipcommon.h
@@ -8,7 +8,7 @@
  * gpio interface, extbus, and support for serial and parallel flashes.
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GPL version 2. See COPYING for details.
  */
@@ -123,6 +123,8 @@
 #define SSB_CHIPCO_FLASHDATA		0x0048
 #define SSB_CHIPCO_BCAST_ADDR		0x0050
 #define SSB_CHIPCO_BCAST_DATA		0x0054
+#define SSB_CHIPCO_GPIOPULLUP		0x0058		/* Rev >= 20 only */
+#define SSB_CHIPCO_GPIOPULLDOWN		0x005C		/* Rev >= 20 only */
 #define SSB_CHIPCO_GPIOIN		0x0060
 #define SSB_CHIPCO_GPIOOUT		0x0064
 #define SSB_CHIPCO_GPIOOUTEN		0x0068
@@ -131,6 +133,9 @@
 #define SSB_CHIPCO_GPIOIRQ		0x0074
 #define SSB_CHIPCO_WATCHDOG		0x0080
 #define SSB_CHIPCO_GPIOTIMER		0x0088		/* LED powersave (corerev >= 16) */
+#define  SSB_CHIPCO_GPIOTIMER_OFFTIME	0x0000FFFF
+#define  SSB_CHIPCO_GPIOTIMER_OFFTIME_SHIFT	0
+#define  SSB_CHIPCO_GPIOTIMER_ONTIME	0xFFFF0000
 #define  SSB_CHIPCO_GPIOTIMER_ONTIME_SHIFT	16
 #define SSB_CHIPCO_GPIOTOUTM		0x008C		/* LED powersave (corerev >= 16) */
 #define SSB_CHIPCO_CLOCK_N		0x0090
@@ -189,8 +194,10 @@
 #define  SSB_CHIPCO_CLKCTLST_HAVEALPREQ	0x00000008 /* ALP available request */
 #define  SSB_CHIPCO_CLKCTLST_HAVEHTREQ	0x00000010 /* HT available request */
 #define  SSB_CHIPCO_CLKCTLST_HWCROFF	0x00000020 /* Force HW clock request off */
-#define  SSB_CHIPCO_CLKCTLST_HAVEHT	0x00010000 /* HT available */
-#define  SSB_CHIPCO_CLKCTLST_HAVEALP	0x00020000 /* APL available */
+#define  SSB_CHIPCO_CLKCTLST_HAVEALP	0x00010000 /* ALP available */
+#define  SSB_CHIPCO_CLKCTLST_HAVEHT	0x00020000 /* HT available */
+#define  SSB_CHIPCO_CLKCTLST_4328A0_HAVEHT	0x00010000 /* 4328a0 has reversed bits */
+#define  SSB_CHIPCO_CLKCTLST_4328A0_HAVEALP	0x00020000 /* 4328a0 has reversed bits */
 #define SSB_CHIPCO_HW_WORKAROUND	0x01E4 /* Hardware workaround (rev >= 20) */
 #define SSB_CHIPCO_UART0_DATA		0x0300
 #define SSB_CHIPCO_UART0_IMR		0x0304
--- a/drivers/ssb/b43_pci_bridge.c
+++ b/drivers/ssb/b43_pci_bridge.c
@@ -5,12 +5,13 @@
  * because of its small size we include it in the SSB core
  * instead of creating a standalone module.
  *
- * Copyright 2007  Michael Buesch <mb@bu3sch.de>
+ * Copyright 2007  Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
 
 #include <linux/pci.h>
+#include <linux/module.h>
 #include <linux/ssb/ssb.h>
 
 #include "ssb_private.h"
--- a/drivers/ssb/driver_extif.c
+++ b/drivers/ssb/driver_extif.c
@@ -3,7 +3,7 @@
  * Broadcom EXTIF core driver
  *
  * Copyright 2005, Broadcom Corporation
- * Copyright 2006, 2007, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006, 2007, Michael Buesch <m@bues.ch>
  * Copyright 2006, 2007, Felix Fietkau <nbd@openwrt.org>
  * Copyright 2007, Aurelien Jarno <aurelien@aurel32.net>
  *
--- a/drivers/ssb/embedded.c
+++ b/drivers/ssb/embedded.c
@@ -3,7 +3,7 @@
  * Embedded systems support code
  *
  * Copyright 2005-2008, Broadcom Corporation
- * Copyright 2006-2008, Michael Buesch <mb@bu3sch.de>
+ * Copyright 2006-2008, Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  */
--- a/drivers/ssb/sdio.c
+++ b/drivers/ssb/sdio.c
@@ -6,7 +6,7 @@
  *
  * Based on drivers/ssb/pcmcia.c
  * Copyright 2006 Johannes Berg <johannes@sipsolutions.net>
- * Copyright 2007-2008 Michael Buesch <mb@bu3sch.de>
+ * Copyright 2007-2008 Michael Buesch <m@bues.ch>
  *
  * Licensed under the GNU/GPL. See COPYING for details.
  *
@@ -551,14 +551,10 @@ int ssb_sdio_get_invariants(struct ssb_b
 			case SSB_SDIO_CIS_ANTGAIN:
 				GOTO_ERROR_ON(tuple->size != 2,
 					      "antg tpl size");
-				sprom->antenna_gain.ghz24.a0 = tuple->data[1];
-				sprom->antenna_gain.ghz24.a1 = tuple->data[1];
-				sprom->antenna_gain.ghz24.a2 = tuple->data[1];
-				sprom->antenna_gain.ghz24.a3 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a0 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a1 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a2 = tuple->data[1];
-				sprom->antenna_gain.ghz5.a3 = tuple->data[1];
+				sprom->antenna_gain.a0 = tuple->data[1];
+				sprom->antenna_gain.a1 = tuple->data[1];
+				sprom->antenna_gain.a2 = tuple->data[1];
+				sprom->antenna_gain.a3 = tuple->data[1];
 				break;
 			case SSB_SDIO_CIS_BFLAGS:
 				GOTO_ERROR_ON((tuple->size != 3) &&
--- a/include/linux/ssb/ssb_driver_gige.h
+++ b/include/linux/ssb/ssb_driver_gige.h
@@ -2,6 +2,7 @@
 #define LINUX_SSB_DRIVER_GIGE_H_
 
 #include <linux/ssb/ssb.h>
+#include <linux/bug.h>
 #include <linux/pci.h>
 #include <linux/spinlock.h>
 
