#!/bin/sh

. /lib/ramips.sh

set_usb_led() {
	local sysfs="$1"

	uci batch <<EOF
set system.usb_led=led
set system.usb_led.name='usb'
set system.usb_led.sysfs='$sysfs'
set system.usb_led.trigger='usbdev'
set system.usb_led.dev='1-1'
set system.usb_led.interval='50'
commit system
EOF
}

set_wifi_led() {
	local sysfs="$1"

	uci batch <<EOF
set system.wifi_led=led
set system.wifi_led.name='wifi'
set system.wifi_led.sysfs='$sysfs'
set system.wifi_led.trigger='netdev'
set system.wifi_led.dev='wlan0'
set system.wifi_led.mode='link rx tx'
commit system
EOF
}

board=$(ramips_board_name)

case $board in
	all0256n)
		set_wifi_led "rt2800pci-phy0::radio"
		;;
	bc2)
		set_usb_led "bc2:blue:usb"
		;;
	esr-9753)
		set_wifi_led "rt2800pci-phy0::radio"
		;;
	f5d8235-v1)
		set_usb_led "f5d8235-v1:blue:storage"
		;;
	f5d8235-v2)
		set_usb_led "f5d8235v2:blue:storage"
		;;
	fonera20n)
		set_usb_led "fonera20n:amber:usb"
		;;
	hw550-3g)
		set_usb_led "hw550-3g:green:usb"
		;;
	mofi3500-3gn)
		set_usb_led "mofi3500-3gn:green:usb"
		;;
	nw718)
		set_usb_led "nw718:amber:usb"
		;;
	sl-r7205)
		set_wifi_led "rt2800pci-phy0::radio"
		;;
	v11st-fe)
		set_wifi_led "rt2800pci-phy0::radio"
		;;
	w306r-v20)
		set_wifi_led "rt2800pci-phy0::radio"
		;;
	w502u)
		set_usb_led "alfa:blue:usb"
		set_wifi_led "rt2800pci-phy0::radio"
		;;
	wcr-150gn)
		set_usb_led "wcr150gn:amber:user"
		;;
esac
