From 9c19e86a7eccf8efd159ba213290830164f33a71 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Sun, 11 Dec 2011 17:36:42 +0100
Subject: [PATCH 23/35] MIPS: ath79: add SoC detection code for AR934X

Also add 'soc_is_ar934[124x]' helper functions and a Kconfig
symbol for the AR934X SoCs.

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
Acked-by: Luis R. Rodriguez <mcgrof@qca.qualcomm.com>
---
 arch/mips/ath79/Kconfig                        |    4 ++++
 arch/mips/ath79/setup.c                        |   21 ++++++++++++++++++++-
 arch/mips/include/asm/mach-ath79/ar71xx_regs.h |    2 ++
 arch/mips/include/asm/mach-ath79/ath79.h       |   23 +++++++++++++++++++++++
 4 files changed, 49 insertions(+), 1 deletions(-)

--- a/arch/mips/ath79/Kconfig
+++ b/arch/mips/ath79/Kconfig
@@ -69,6 +69,10 @@ config SOC_AR933X
 	select USB_ARCH_HAS_EHCI
 	def_bool n
 
+config SOC_AR934X
+	select USB_ARCH_HAS_EHCI
+	def_bool n
+
 config ATH79_DEV_GPIO_BUTTONS
 	def_bool n
 
--- a/arch/mips/ath79/setup.c
+++ b/arch/mips/ath79/setup.c
@@ -1,10 +1,11 @@
 /*
  *  Atheros AR71XX/AR724X/AR913X specific setup
  *
+ *  Copyright (C) 2010-2011 Jaiganesh Narayanan <jnarayanan@atheros.com>
  *  Copyright (C) 2008-2011 Gabor Juhos <juhosg@openwrt.org>
  *  Copyright (C) 2008 Imre Kaloz <kaloz@openwrt.org>
  *
- *  Parts of this file are based on Atheros' 2.6.15 BSP
+ *  Parts of this file are based on Atheros' 2.6.15/2.6.31 BSP
  *
  *  This program is free software; you can redistribute it and/or modify it
  *  under the terms of the GNU General Public License version 2 as published
@@ -145,6 +146,24 @@ static void __init ath79_detect_sys_type
 		rev = id & AR933X_REV_ID_REVISION_MASK;
 		break;
 
+	case REV_ID_MAJOR_AR9341:
+		ath79_soc = ATH79_SOC_AR9341;
+		chip = "9341";
+		rev = id & AR934X_REV_ID_REVISION_MASK;
+		break;
+
+	case REV_ID_MAJOR_AR9342:
+		ath79_soc = ATH79_SOC_AR9342;
+		chip = "9342";
+		rev = id & AR934X_REV_ID_REVISION_MASK;
+		break;
+
+	case REV_ID_MAJOR_AR9344:
+		ath79_soc = ATH79_SOC_AR9344;
+		chip = "9344";
+		rev = id & AR934X_REV_ID_REVISION_MASK;
+		break;
+
 	default:
 		panic("ath79: unknown SoC, id:0x%08x", id);
 	}
--- a/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
+++ b/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
@@ -271,6 +271,8 @@
 
 #define AR724X_REV_ID_REVISION_MASK	0x3
 
+#define AR934X_REV_ID_REVISION_MASK     0xf
+
 /*
  * SPI block
  */
--- a/arch/mips/include/asm/mach-ath79/ath79.h
+++ b/arch/mips/include/asm/mach-ath79/ath79.h
@@ -29,6 +29,9 @@ enum ath79_soc_type {
 	ATH79_SOC_AR9132,
 	ATH79_SOC_AR9330,
 	ATH79_SOC_AR9331,
+	ATH79_SOC_AR9341,
+	ATH79_SOC_AR9342,
+	ATH79_SOC_AR9344,
 };
 
 extern enum ath79_soc_type ath79_soc;
@@ -75,6 +78,26 @@ static inline int soc_is_ar933x(void)
 		ath79_soc == ATH79_SOC_AR9331);
 }
 
+static inline int soc_is_ar9341(void)
+{
+	return (ath79_soc == ATH79_SOC_AR9341);
+}
+
+static inline int soc_is_ar9342(void)
+{
+	return (ath79_soc == ATH79_SOC_AR9342);
+}
+
+static inline int soc_is_ar9344(void)
+{
+	return (ath79_soc == ATH79_SOC_AR9344);
+}
+
+static inline int soc_is_ar934x(void)
+{
+	return soc_is_ar9341() || soc_is_ar9342() || soc_is_ar9344();
+}
+
 extern void __iomem *ath79_ddr_base;
 extern void __iomem *ath79_pll_base;
 extern void __iomem *ath79_reset_base;
