--- a/Documentation/feature-removal-schedule.txt
+++ b/Documentation/feature-removal-schedule.txt
@@ -551,3 +551,15 @@ When:	3.5
 Why:	The iwlagn module has been renamed iwlwifi.  The alias will be around
 	for backward compatibility for several cycles and then dropped.
 Who:	Don Fry <donald.h.fry@intel.com>
+
+----------------------------
+
+What:	pci_scan_bus_parented()
+When:	3.5
+Why:	The pci_scan_bus_parented() interface creates a new root bus.  The
+	bus is created with default resources (ioport_resource and
+	iomem_resource) that are always wrong, so we rely on arch code to
+	correct them later.  Callers of pci_scan_bus_parented() should
+	convert to using pci_scan_root_bus() so they can supply a list of
+	bus resources when the bus is created.
+Who:	Bjorn Helgaas <bhelgaas@google.com>
--- a/arch/alpha/kernel/pci.c
+++ b/arch/alpha/kernel/pci.c
@@ -281,27 +281,9 @@ pcibios_fixup_device_resources(struct pc
 void __devinit
 pcibios_fixup_bus(struct pci_bus *bus)
 {
-	/* Propagate hose info into the subordinate devices.  */
-
-	struct pci_controller *hose = bus->sysdata;
 	struct pci_dev *dev = bus->self;
 
-	if (!dev) {
-		/* Root bus. */
-		u32 pci_mem_end;
-		u32 sg_base = hose->sg_pci ? hose->sg_pci->dma_base : ~0;
-		unsigned long end;
-
-		bus->resource[0] = hose->io_space;
-		bus->resource[1] = hose->mem_space;
-
-		/* Adjust hose mem_space limit to prevent PCI allocations
-		   in the iommu windows. */
-		pci_mem_end = min((u32)__direct_map_base, sg_base) - 1;
-		end = hose->mem_space->start + pci_mem_end;
-		if (hose->mem_space->end > end)
-			hose->mem_space->end = end;
- 	} else if (pci_probe_only &&
+	if (pci_probe_only && dev &&
  		   (dev->class >> 8) == PCI_CLASS_BRIDGE_PCI) {
  		pci_read_bridge_bases(bus);
  		pcibios_fixup_device_resources(dev, bus);
@@ -414,13 +396,31 @@ void __init
 common_init_pci(void)
 {
 	struct pci_controller *hose;
+	struct list_head resources;
 	struct pci_bus *bus;
 	int next_busno;
 	int need_domain_info = 0;
+	u32 pci_mem_end;
+	u32 sg_base;
+	unsigned long end;
 
 	/* Scan all of the recorded PCI controllers.  */
 	for (next_busno = 0, hose = hose_head; hose; hose = hose->next) {
-		bus = pci_scan_bus(next_busno, alpha_mv.pci_ops, hose);
+		sg_base = hose->sg_pci ? hose->sg_pci->dma_base : ~0;
+
+		/* Adjust hose mem_space limit to prevent PCI allocations
+		   in the iommu windows. */
+		pci_mem_end = min((u32)__direct_map_base, sg_base) - 1;
+		end = hose->mem_space->start + pci_mem_end;
+		if (hose->mem_space->end > end)
+			hose->mem_space->end = end;
+
+		INIT_LIST_HEAD(&resources);
+		pci_add_resource(&resources, hose->io_space);
+		pci_add_resource(&resources, hose->mem_space);
+
+		bus = pci_scan_root_bus(NULL, next_busno, alpha_mv.pci_ops,
+					hose, &resources);
 		hose->bus = bus;
 		hose->need_domain_info = need_domain_info;
 		next_busno = bus->subordinate + 1;
--- a/arch/arm/common/it8152.c
+++ b/arch/arm/common/it8152.c
@@ -299,8 +299,8 @@ int __init it8152_pci_setup(int nr, stru
 		goto err1;
 	}
 
-	sys->resource[0] = &it8152_io;
-	sys->resource[1] = &it8152_mem;
+	pci_add_resource(&sys->resources, &it8152_io);
+	pci_add_resource(&sys->resources, &it8152_mem);
 
 	if (platform_notify || platform_notify_remove) {
 		printk(KERN_ERR "PCI: Can't use platform_notify\n");
@@ -352,7 +352,7 @@ void pcibios_set_master(struct pci_dev *
 
 struct pci_bus * __init it8152_pci_scan_bus(int nr, struct pci_sys_data *sys)
 {
-	return pci_scan_bus(nr, &it8152_ops, sys);
+	return pci_scan_root_bus(NULL, nr, &it8152_ops, sys, &sys->resources);
 }
 
 EXPORT_SYMBOL(dma_set_coherent_mask);
--- a/arch/arm/common/via82c505.c
+++ b/arch/arm/common/via82c505.c
@@ -86,7 +86,8 @@ int __init via82c505_setup(int nr, struc
 struct pci_bus * __init via82c505_scan_bus(int nr, struct pci_sys_data *sysdata)
 {
 	if (nr == 0)
-		return pci_scan_bus(0, &via82c505_ops, sysdata);
+		return pci_scan_root_bus(NULL, 0, &via82c505_ops, sysdata,
+					 &sysdata->resources);
 
 	return NULL;
 }
--- a/arch/arm/include/asm/mach/pci.h
+++ b/arch/arm/include/asm/mach/pci.h
@@ -40,7 +40,7 @@ struct pci_sys_data {
 	u64		mem_offset;	/* bus->cpu memory mapping offset	*/
 	unsigned long	io_offset;	/* bus->cpu IO mapping offset		*/
 	struct pci_bus	*bus;		/* PCI bus				*/
-	struct resource *resource[3];	/* Primary PCI bus resources		*/
+	struct list_head resources;	/* root bus resources (apertures)       */
 					/* Bridge swizzling			*/
 	u8		(*swizzle)(struct pci_dev *, u8 *);
 					/* IRQ mapping				*/
--- a/arch/arm/kernel/bios32.c
+++ b/arch/arm/kernel/bios32.c
@@ -316,21 +316,6 @@ pdev_fixup_device_resources(struct pci_s
 	}
 }
 
-static void __devinit
-pbus_assign_bus_resources(struct pci_bus *bus, struct pci_sys_data *root)
-{
-	struct pci_dev *dev = bus->self;
-	int i;
-
-	if (!dev) {
-		/*
-		 * Assign root bus resources.
-		 */
-		for (i = 0; i < 3; i++)
-			bus->resource[i] = root->resource[i];
-	}
-}
-
 /*
  * pcibios_fixup_bus - Called after each bus is probed,
  * but before its children are examined.
@@ -341,8 +326,6 @@ void pcibios_fixup_bus(struct pci_bus *b
 	struct pci_dev *dev;
 	u16 features = PCI_COMMAND_SERR | PCI_COMMAND_PARITY | PCI_COMMAND_FAST_BACK;
 
-	pbus_assign_bus_resources(bus, root);
-
 	/*
 	 * Walk the devices on this bus, working out what we can
 	 * and can't support.
@@ -508,12 +491,18 @@ static void __init pcibios_init_hw(struc
 		sys->busnr   = busnr;
 		sys->swizzle = hw->swizzle;
 		sys->map_irq = hw->map_irq;
-		sys->resource[0] = &ioport_resource;
-		sys->resource[1] = &iomem_resource;
+		INIT_LIST_HEAD(&sys->resources);
 
 		ret = hw->setup(nr, sys);
 
 		if (ret > 0) {
+			if (list_empty(&sys->resources)) {
+				pci_add_resource(&sys->resources,
+						 &ioport_resource);
+				pci_add_resource(&sys->resources,
+						 &iomem_resource);
+			}
+
 			sys->bus = hw->scan(nr, sys);
 
 			if (!sys->bus)
--- a/arch/arm/mach-cns3xxx/pcie.c
+++ b/arch/arm/mach-cns3xxx/pcie.c
@@ -151,13 +151,12 @@ static int cns3xxx_pci_setup(int nr, str
 	struct cns3xxx_pcie *cnspci = sysdata_to_cnspci(sys);
 	struct resource *res_io = &cnspci->res_io;
 	struct resource *res_mem = &cnspci->res_mem;
-	struct resource **sysres = sys->resource;
 
 	BUG_ON(request_resource(&iomem_resource, res_io) ||
 	       request_resource(&iomem_resource, res_mem));
 
-	sysres[0] = res_io;
-	sysres[1] = res_mem;
+	pci_add_resource(&sys->resources, res_io);
+	pci_add_resource(&sys->resources, res_mem);
 
 	return 1;
 }
@@ -169,7 +168,8 @@ static struct pci_ops cns3xxx_pcie_ops =
 
 static struct pci_bus *cns3xxx_pci_scan_bus(int nr, struct pci_sys_data *sys)
 {
-	return pci_scan_bus(sys->busnr, &cns3xxx_pcie_ops, sys);
+	return pci_scan_root_bus(NULL, sys->busnr, &cns3xxx_pcie_ops, sys,
+				 &sys->resources);
 }
 
 static int cns3xxx_pcie_map_irq(const struct pci_dev *dev, u8 slot, u8 pin)
--- a/arch/arm/mach-dove/pcie.c
+++ b/arch/arm/mach-dove/pcie.c
@@ -69,7 +69,7 @@ static int __init dove_pcie_setup(int nr
 	pp->res[0].flags = IORESOURCE_IO;
 	if (request_resource(&ioport_resource, &pp->res[0]))
 		panic("Request PCIe IO resource failed\n");
-	sys->resource[0] = &pp->res[0];
+	pci_add_resource(&sys->resources, &pp->res[0]);
 
 	/*
 	 * IORESOURCE_MEM
@@ -88,9 +88,7 @@ static int __init dove_pcie_setup(int nr
 	pp->res[1].flags = IORESOURCE_MEM;
 	if (request_resource(&iomem_resource, &pp->res[1]))
 		panic("Request PCIe Memory resource failed\n");
-	sys->resource[1] = &pp->res[1];
-
-	sys->resource[2] = NULL;
+	pci_add_resource(&sys->resources, &pp->res[1]);
 
 	return 1;
 }
@@ -184,7 +182,8 @@ dove_pcie_scan_bus(int nr, struct pci_sy
 	struct pci_bus *bus;
 
 	if (nr < num_pcie_ports) {
-		bus = pci_scan_bus(sys->busnr, &pcie_ops, sys);
+		bus = pci_scan_root_bus(NULL, sys->busnr, &pcie_ops, sys,
+					&sys->resources);
 	} else {
 		bus = NULL;
 		BUG();
--- a/arch/arm/mach-footbridge/dc21285.c
+++ b/arch/arm/mach-footbridge/dc21285.c
@@ -275,9 +275,9 @@ int __init dc21285_setup(int nr, struct
 	allocate_resource(&iomem_resource, &res[0], 0x40000000,
 			  0x80000000, 0xffffffff, 0x40000000, NULL, NULL);
 
-	sys->resource[0] = &ioport_resource;
-	sys->resource[1] = &res[0];
-	sys->resource[2] = &res[1];
+	pci_add_resource(&sys->resources, &ioport_resource);
+	pci_add_resource(&sys->resources, &res[0]);
+	pci_add_resource(&sys->resources, &res[1]);
 	sys->mem_offset  = DC21285_PCI_MEM;
 
 	return 1;
@@ -285,7 +285,7 @@ int __init dc21285_setup(int nr, struct
 
 struct pci_bus * __init dc21285_scan_bus(int nr, struct pci_sys_data *sys)
 {
-	return pci_scan_bus(0, &dc21285_ops, sys);
+	return pci_scan_root_bus(NULL, 0, &dc21285_ops, sys, &sys->resources);
 }
 
 #define dc21285_request_irq(_a, _b, _c, _d, _e) \
--- a/arch/arm/mach-integrator/pci_v3.c
+++ b/arch/arm/mach-integrator/pci_v3.c
@@ -359,7 +359,7 @@ static struct resource pre_mem = {
 	.flags	= IORESOURCE_MEM | IORESOURCE_PREFETCH,
 };
 
-static int __init pci_v3_setup_resources(struct resource **resource)
+static int __init pci_v3_setup_resources(struct pci_sys_data *sys)
 {
 	if (request_resource(&iomem_resource, &non_mem)) {
 		printk(KERN_ERR "PCI: unable to allocate non-prefetchable "
@@ -374,13 +374,13 @@ static int __init pci_v3_setup_resources
 	}
 
 	/*
-	 * bus->resource[0] is the IO resource for this bus
-	 * bus->resource[1] is the mem resource for this bus
-	 * bus->resource[2] is the prefetch mem resource for this bus
+	 * the IO resource for this bus
+	 * the mem resource for this bus
+	 * the prefetch mem resource for this bus
 	 */
-	resource[0] = &ioport_resource;
-	resource[1] = &non_mem;
-	resource[2] = &pre_mem;
+	pci_add_resource(&sys->resources, &ioport_resource);
+	pci_add_resource(&sys->resources, &non_mem);
+	pci_add_resource(&sys->resources, &pre_mem);
 
 	return 1;
 }
@@ -481,7 +481,7 @@ int __init pci_v3_setup(int nr, struct p
 
 	if (nr == 0) {
 		sys->mem_offset = PHYS_PCI_MEM_BASE;
-		ret = pci_v3_setup_resources(sys->resource);
+		ret = pci_v3_setup_resources(sys);
 	}
 
 	return ret;
@@ -489,7 +489,8 @@ int __init pci_v3_setup(int nr, struct p
 
 struct pci_bus * __init pci_v3_scan_bus(int nr, struct pci_sys_data *sys)
 {
-	return pci_scan_bus(sys->busnr, &pci_v3_ops, sys);
+	return pci_scan_root_bus(NULL, sys->busnr, &pci_v3_ops, sys,
+				 &sys->resources);
 }
 
 /*
--- a/arch/arm/mach-iop13xx/pci.c
+++ b/arch/arm/mach-iop13xx/pci.c
@@ -537,14 +537,14 @@ struct pci_bus *iop13xx_scan_bus(int nr,
 			while(time_before(jiffies, atux_trhfa_timeout))
 				udelay(100);
 
-		bus = pci_bus_atux = pci_scan_bus(sys->busnr,
-						  &iop13xx_atux_ops,
-						  sys);
+		bus = pci_bus_atux = pci_scan_root_bus(NULL, sys->busnr,
+						       &iop13xx_atux_ops,
+						       sys, &sys->resources);
 		break;
 	case IOP13XX_INIT_ATU_ATUE:
-		bus = pci_bus_atue = pci_scan_bus(sys->busnr,
-						  &iop13xx_atue_ops,
-						  sys);
+		bus = pci_bus_atue = pci_scan_root_bus(NULL, sys->busnr,
+						       &iop13xx_atue_ops,
+						       sys, &sys->resources);
 		break;
 	}
 
@@ -1084,9 +1084,8 @@ int iop13xx_pci_setup(int nr, struct pci
 	request_resource(&ioport_resource, &res[0]);
 	request_resource(&iomem_resource, &res[1]);
 
-	sys->resource[0] = &res[0];
-	sys->resource[1] = &res[1];
-	sys->resource[2] = NULL;
+	pci_add_resource(&sys->resources, &res[0]);
+	pci_add_resource(&sys->resources, &res[1]);
 
 	return 1;
 }
--- a/arch/arm/mach-ixp2000/enp2611.c
+++ b/arch/arm/mach-ixp2000/enp2611.c
@@ -145,7 +145,8 @@ static struct pci_ops enp2611_pci_ops =
 static struct pci_bus * __init enp2611_pci_scan_bus(int nr,
 						struct pci_sys_data *sys)
 {
-	return pci_scan_bus(sys->busnr, &enp2611_pci_ops, sys);
+	return pci_scan_root_bus(NULL, sys->busnr, &enp2611_pci_ops, sys,
+				 &sys->resources);
 }
 
 static int __init enp2611_pci_map_irq(const struct pci_dev *dev, u8 slot,
--- a/arch/arm/mach-ixp2000/pci.c
+++ b/arch/arm/mach-ixp2000/pci.c
@@ -132,7 +132,8 @@ static struct pci_ops ixp2000_pci_ops =
 
 struct pci_bus *ixp2000_pci_scan_bus(int nr, struct pci_sys_data *sysdata)
 {
-	return pci_scan_bus(sysdata->busnr, &ixp2000_pci_ops, sysdata);
+	return pci_scan_root_bus(NULL, sysdata->busnr, &ixp2000_pci_ops,
+				 sysdata, &sysdata->resources);
 }
 
 
@@ -242,9 +243,8 @@ int ixp2000_pci_setup(int nr, struct pci
 	if (nr >= 1)
 		return 0;
 
-	sys->resource[0] = &ixp2000_pci_io_space;
-	sys->resource[1] = &ixp2000_pci_mem_space;
-	sys->resource[2] = NULL;
+	pci_add_resource(&sys->resources, &ixp2000_pci_io_space);
+	pci_add_resource(&sys->resources, &ixp2000_pci_mem_space);
 
 	return 1;
 }
--- a/arch/arm/mach-ixp23xx/pci.c
+++ b/arch/arm/mach-ixp23xx/pci.c
@@ -143,7 +143,8 @@ struct pci_ops ixp23xx_pci_ops = {
 
 struct pci_bus *ixp23xx_pci_scan_bus(int nr, struct pci_sys_data *sysdata)
 {
-	return pci_scan_bus(sysdata->busnr, &ixp23xx_pci_ops, sysdata);
+	return pci_scan_root_bus(NULL, sysdata->busnr, &ixp23xx_pci_ops,
+				 sysdata, &sysdata->resources);
 }
 
 int ixp23xx_pci_abort_handler(unsigned long addr, unsigned int fsr, struct pt_regs *regs)
@@ -280,9 +281,8 @@ int ixp23xx_pci_setup(int nr, struct pci
 	if (nr >= 1)
 		return 0;
 
-	sys->resource[0] = &ixp23xx_pci_io_space;
-	sys->resource[1] = &ixp23xx_pci_mem_space;
-	sys->resource[2] = NULL;
+	pci_add_resource(&sys->resources, &ixp23xx_pci_io_space);
+	pci_add_resource(&sys->resources, &ixp23xx_pci_mem_space);
 
 	return 1;
 }
--- a/arch/arm/mach-ixp4xx/common-pci.c
+++ b/arch/arm/mach-ixp4xx/common-pci.c
@@ -472,9 +472,8 @@ int ixp4xx_setup(int nr, struct pci_sys_
 	request_resource(&ioport_resource, &res[0]);
 	request_resource(&iomem_resource, &res[1]);
 
-	sys->resource[0] = &res[0];
-	sys->resource[1] = &res[1];
-	sys->resource[2] = NULL;
+	pci_add_resource(&sys->resources, &res[0]);
+	pci_add_resource(&sys->resources, &res[1]);
 
 	platform_notify = ixp4xx_pci_platform_notify;
 	platform_notify_remove = ixp4xx_pci_platform_notify_remove;
@@ -484,7 +483,8 @@ int ixp4xx_setup(int nr, struct pci_sys_
 
 struct pci_bus * __devinit ixp4xx_scan_bus(int nr, struct pci_sys_data *sys)
 {
-	return pci_scan_bus(sys->busnr, &ixp4xx_ops, sys);
+	return pci_scan_root_bus(NULL, sys->busnr, &ixp4xx_ops, sys,
+				 &sys->resources);
 }
 
 int dma_set_coherent_mask(struct device *dev, u64 mask)
--- a/arch/arm/mach-kirkwood/pcie.c
+++ b/arch/arm/mach-kirkwood/pcie.c
@@ -198,9 +198,8 @@ static int __init kirkwood_pcie_setup(in
 	if (request_resource(&iomem_resource, &pp->res[1]))
 		panic("Request PCIe%d Memory resource failed\n", index);
 
-	sys->resource[0] = &pp->res[0];
-	sys->resource[1] = &pp->res[1];
-	sys->resource[2] = NULL;
+	pci_add_resource(&sys->resources, &pp->res[0]);
+	pci_add_resource(&sys->resources, &pp->res[1]);
 	sys->io_offset = 0;
 
 	/*
@@ -236,7 +235,8 @@ kirkwood_pcie_scan_bus(int nr, struct pc
 	struct pci_bus *bus;
 
 	if (nr < num_pcie_ports) {
-		bus = pci_scan_bus(sys->busnr, &pcie_ops, sys);
+		bus = pci_scan_root_bus(NULL, sys->busnr, &pcie_ops, sys,
+					&sys->resources);
 	} else {
 		bus = NULL;
 		BUG();
--- a/arch/arm/mach-ks8695/pci.c
+++ b/arch/arm/mach-ks8695/pci.c
@@ -143,7 +143,8 @@ static struct pci_ops ks8695_pci_ops = {
 
 static struct pci_bus* __init ks8695_pci_scan_bus(int nr, struct pci_sys_data *sys)
 {
-	return pci_scan_bus(sys->busnr, &ks8695_pci_ops, sys);
+	return pci_scan_root_bus(NULL, sys->busnr, &ks8695_pci_ops, sys,
+				 &sys->resources);
 }
 
 static struct resource pci_mem = {
@@ -168,9 +169,8 @@ static int __init ks8695_pci_setup(int n
 	request_resource(&iomem_resource, &pci_mem);
 	request_resource(&ioport_resource, &pci_io);
 
-	sys->resource[0] = &pci_io;
-	sys->resource[1] = &pci_mem;
-	sys->resource[2] = NULL;
+	pci_add_resource(&sys->resources, &pci_io);
+	pci_add_resource(&sys->resources, &pci_mem);
 
 	/* Assign and enable processor bridge */
 	ks8695_local_writeconfig(PCI_BASE_ADDRESS_0, KS8695_PCIMEM_PA);
--- a/arch/arm/mach-mv78xx0/pcie.c
+++ b/arch/arm/mach-mv78xx0/pcie.c
@@ -155,9 +155,8 @@ static int __init mv78xx0_pcie_setup(int
 	orion_pcie_set_local_bus_nr(pp->base, sys->busnr);
 	orion_pcie_setup(pp->base, &mv78xx0_mbus_dram_info);
 
-	sys->resource[0] = &pp->res[0];
-	sys->resource[1] = &pp->res[1];
-	sys->resource[2] = NULL;
+	pci_add_resource(&sys->resources, &pp->res[0]);
+	pci_add_resource(&sys->resources, &pp->res[1]);
 
 	return 1;
 }
@@ -251,7 +250,8 @@ mv78xx0_pcie_scan_bus(int nr, struct pci
 	struct pci_bus *bus;
 
 	if (nr < num_pcie_ports) {
-		bus = pci_scan_bus(sys->busnr, &pcie_ops, sys);
+		bus = pci_scan_root_bus(NULL, sys->busnr, &pcie_ops, sys,
+					&sys->resources);
 	} else {
 		bus = NULL;
 		BUG();
--- a/arch/arm/mach-orion5x/pci.c
+++ b/arch/arm/mach-orion5x/pci.c
@@ -176,7 +176,7 @@ static int __init pcie_setup(struct pci_
 	res[0].end = res[0].start + ORION5X_PCIE_IO_SIZE - 1;
 	if (request_resource(&ioport_resource, &res[0]))
 		panic("Request PCIe IO resource failed\n");
-	sys->resource[0] = &res[0];
+	pci_add_resource(&sys->resources, &res[0]);
 
 	/*
 	 * IORESOURCE_MEM
@@ -187,9 +187,8 @@ static int __init pcie_setup(struct pci_
 	res[1].end = res[1].start + ORION5X_PCIE_MEM_SIZE - 1;
 	if (request_resource(&iomem_resource, &res[1]))
 		panic("Request PCIe Memory resource failed\n");
-	sys->resource[1] = &res[1];
+	pci_add_resource(&sys->resources, &res[1]);
 
-	sys->resource[2] = NULL;
 	sys->io_offset = 0;
 
 	return 1;
@@ -505,7 +504,7 @@ static int __init pci_setup(struct pci_s
 	res[0].end = res[0].start + ORION5X_PCI_IO_SIZE - 1;
 	if (request_resource(&ioport_resource, &res[0]))
 		panic("Request PCI IO resource failed\n");
-	sys->resource[0] = &res[0];
+	pci_add_resource(&sys->resources, &res[0]);
 
 	/*
 	 * IORESOURCE_MEM
@@ -516,9 +515,8 @@ static int __init pci_setup(struct pci_s
 	res[1].end = res[1].start + ORION5X_PCI_MEM_SIZE - 1;
 	if (request_resource(&iomem_resource, &res[1]))
 		panic("Request PCI Memory resource failed\n");
-	sys->resource[1] = &res[1];
+	pci_add_resource(&sys->resources, &res[1]);
 
-	sys->resource[2] = NULL;
 	sys->io_offset = 0;
 
 	return 1;
@@ -579,9 +577,11 @@ struct pci_bus __init *orion5x_pci_sys_s
 	struct pci_bus *bus;
 
 	if (nr == 0) {
-		bus = pci_scan_bus(sys->busnr, &pcie_ops, sys);
+		bus = pci_scan_root_bus(NULL, sys->busnr, &pcie_ops, sys,
+					&sys->resources);
 	} else if (nr == 1 && !orion5x_pci_disabled) {
-		bus = pci_scan_bus(sys->busnr, &pci_ops, sys);
+		bus = pci_scan_root_bus(NULL, sys->busnr, &pci_ops, sys,
+					&sys->resources);
 	} else {
 		bus = NULL;
 		BUG();
--- a/arch/arm/mach-sa1100/pci-nanoengine.c
+++ b/arch/arm/mach-sa1100/pci-nanoengine.c
@@ -131,7 +131,8 @@ static int __init pci_nanoengine_map_irq
 
 struct pci_bus * __init pci_nanoengine_scan_bus(int nr, struct pci_sys_data *sys)
 {
-	return pci_scan_bus(sys->busnr, &pci_nano_ops, sys);
+	return pci_scan_root_bus(NULL, sys->busnr, &pci_nano_ops, sys,
+				 &sys->resources);
 }
 
 static struct resource pci_io_ports = {
@@ -226,7 +227,7 @@ static struct resource pci_prefetchable_
 	.flags	= IORESOURCE_MEM  | IORESOURCE_PREFETCH,
 };
 
-static int __init pci_nanoengine_setup_resources(struct resource **resource)
+static int __init pci_nanoengine_setup_resources(struct pci_sys_data *sys)
 {
 	if (request_resource(&ioport_resource, &pci_io_ports)) {
 		printk(KERN_ERR "PCI: unable to allocate io port region\n");
@@ -243,9 +244,9 @@ static int __init pci_nanoengine_setup_r
 		printk(KERN_ERR "PCI: unable to allocate prefetchable\n");
 		return -EBUSY;
 	}
-	resource[0] = &pci_io_ports;
-	resource[1] = &pci_non_prefetchable_memory;
-	resource[2] = &pci_prefetchable_memory;
+	pci_add_resource(&sys->resources, &pci_io_ports);
+	pci_add_resource(&sys->resources, &pci_non_prefetchable_memory);
+	pci_add_resource(&sys->resources, &pci_prefetchable_memory);
 
 	return 1;
 }
@@ -260,7 +261,7 @@ int __init pci_nanoengine_setup(int nr,
 	if (nr == 0) {
 		sys->mem_offset = NANO_PCI_MEM_RW_PHYS;
 		sys->io_offset = 0x400;
-		ret = pci_nanoengine_setup_resources(sys->resource);
+		ret = pci_nanoengine_setup_resources(sys);
 		/* Enable alternate memory bus master mode, see
 		 * "Intel StrongARM SA1110 Developer's Manual",
 		 * section 10.8, "Alternate Memory Bus Master Mode". */
--- a/arch/arm/mach-tegra/pcie.c
+++ b/arch/arm/mach-tegra/pcie.c
@@ -409,7 +409,7 @@ static int tegra_pcie_setup(int nr, stru
 	pp->res[0].flags = IORESOURCE_IO;
 	if (request_resource(&ioport_resource, &pp->res[0]))
 		panic("Request PCIe IO resource failed\n");
-	sys->resource[0] = &pp->res[0];
+	pci_add_resource(&sys->resources, &pp->res[0]);
 
 	/*
 	 * IORESOURCE_MEM
@@ -428,7 +428,7 @@ static int tegra_pcie_setup(int nr, stru
 	pp->res[1].flags = IORESOURCE_MEM;
 	if (request_resource(&iomem_resource, &pp->res[1]))
 		panic("Request PCIe Memory resource failed\n");
-	sys->resource[1] = &pp->res[1];
+	pci_add_resource(&sys->resources, &pp->res[1]);
 
 	/*
 	 * IORESOURCE_MEM | IORESOURCE_PREFETCH
@@ -447,7 +447,7 @@ static int tegra_pcie_setup(int nr, stru
 	pp->res[2].flags = IORESOURCE_MEM | IORESOURCE_PREFETCH;
 	if (request_resource(&iomem_resource, &pp->res[2]))
 		panic("Request PCIe Prefetch Memory resource failed\n");
-	sys->resource[2] = &pp->res[2];
+	pci_add_resource(&sys->resources, &pp->res[2]);
 
 	return 1;
 }
@@ -468,7 +468,8 @@ static struct pci_bus __init *tegra_pcie
 	pp = tegra_pcie.port + nr;
 	pp->root_bus_nr = sys->busnr;
 
-	return pci_scan_bus(sys->busnr, &tegra_pcie_ops, sys);
+	return pci_scan_root_bus(NULL, sys->busnr, &tegra_pcie_ops, sys,
+				 &sys->resources);
 }
 
 static struct hw_pci tegra_pcie_hw __initdata = {
--- a/arch/arm/mach-versatile/pci.c
+++ b/arch/arm/mach-versatile/pci.c
@@ -191,7 +191,7 @@ static struct resource pre_mem = {
 	.flags	= IORESOURCE_MEM | IORESOURCE_PREFETCH,
 };
 
-static int __init pci_versatile_setup_resources(struct resource **resource)
+static int __init pci_versatile_setup_resources(struct list_head *resources)
 {
 	int ret = 0;
 
@@ -215,13 +215,13 @@ static int __init pci_versatile_setup_re
 	}
 
 	/*
-	 * bus->resource[0] is the IO resource for this bus
-	 * bus->resource[1] is the mem resource for this bus
-	 * bus->resource[2] is the prefetch mem resource for this bus
+	 * the IO resource for this bus
+	 * the mem resource for this bus
+	 * the prefetch mem resource for this bus
 	 */
-	resource[0] = &io_mem;
-	resource[1] = &non_mem;
-	resource[2] = &pre_mem;
+	pci_add_resource(resources, &io_mem);
+	pci_add_resource(resources, &non_mem);
+	pci_add_resource(resources, &pre_mem);
 
 	goto out;
 
@@ -250,7 +250,7 @@ int __init pci_versatile_setup(int nr, s
 
 	if (nr == 0) {
 		sys->mem_offset = 0;
-		ret = pci_versatile_setup_resources(sys->resource);
+		ret = pci_versatile_setup_resources(&sys->resources);
 		if (ret < 0) {
 			printk("pci_versatile_setup: resources... oops?\n");
 			goto out;
@@ -306,7 +306,8 @@ int __init pci_versatile_setup(int nr, s
 
 struct pci_bus * __init pci_versatile_scan_bus(int nr, struct pci_sys_data *sys)
 {
-	return pci_scan_bus(sys->busnr, &pci_versatile_ops, sys);
+	return pci_scan_root_bus(NULL, sys->busnr, &pci_versatile_ops, sys,
+				 &sys->resources);
 }
 
 void __init pci_versatile_preinit(void)
--- a/arch/arm/plat-iop/pci.c
+++ b/arch/arm/plat-iop/pci.c
@@ -215,16 +215,16 @@ int iop3xx_pci_setup(int nr, struct pci_
 	sys->mem_offset = IOP3XX_PCI_LOWER_MEM_PA - *IOP3XX_OMWTVR0;
 	sys->io_offset  = IOP3XX_PCI_LOWER_IO_PA - *IOP3XX_OIOWTVR;
 
-	sys->resource[0] = &res[0];
-	sys->resource[1] = &res[1];
-	sys->resource[2] = NULL;
+	pci_add_resource(&sys->resources, &res[0]);
+	pci_add_resource(&sys->resources, &res[1]);
 
 	return 1;
 }
 
 struct pci_bus *iop3xx_pci_scan_bus(int nr, struct pci_sys_data *sys)
 {
-	return pci_scan_bus(sys->busnr, &iop3xx_ops, sys);
+	return pci_scan_root_bus(NULL, sys->busnr, &iop3xx_ops, sys,
+				 &sys->resources);
 }
 
 void __init iop3xx_atu_setup(void)
--- a/arch/frv/mb93090-mb00/pci-vdk.c
+++ b/arch/frv/mb93090-mb00/pci-vdk.c
@@ -327,11 +327,6 @@ void __init pcibios_fixup_bus(struct pci
 	printk("### PCIBIOS_FIXUP_BUS(%d)\n",bus->number);
 #endif
 
-	if (bus->number == 0) {
-		bus->resource[0] = &pci_ioport_resource;
-		bus->resource[1] = &pci_iomem_resource;
-	}
-
 	pci_read_bridge_bases(bus);
 
 	if (bus->number == 0) {
@@ -357,6 +352,7 @@ void __init pcibios_fixup_bus(struct pci
 int __init pcibios_init(void)
 {
 	struct pci_ops *dir = NULL;
+	LIST_HEAD(resources);
 
 	if (!mb93090_mb00_detected)
 		return -ENXIO;
@@ -420,7 +416,10 @@ int __init pcibios_init(void)
 	}
 
 	printk("PCI: Probing PCI hardware\n");
-	pci_root_bus = pci_scan_bus(0, pci_root_ops, NULL);
+	pci_add_resource(&resources, &pci_ioport_resource);
+	pci_add_resource(&resources, &pci_iomem_resource);
+	pci_root_bus = pci_scan_root_bus(NULL, 0, pci_root_ops, NULL,
+					 &resources);
 
 	pcibios_irq_init();
 	pcibios_fixup_peer_bridges();
--- a/arch/ia64/pci/pci.c
+++ b/arch/ia64/pci/pci.c
@@ -134,6 +134,7 @@ alloc_pci_controller (int seg)
 struct pci_root_info {
 	struct acpi_device *bridge;
 	struct pci_controller *controller;
+	struct list_head resources;
 	char *name;
 };
 
@@ -315,24 +316,13 @@ static __devinit acpi_status add_window(
 				 &window->resource);
 	}
 
-	return AE_OK;
-}
+	/* HP's firmware has a hack to work around a Windows bug.
+	 * Ignore these tiny memory ranges */
+	if (!((window->resource.flags & IORESOURCE_MEM) &&
+	      (window->resource.end - window->resource.start < 16)))
+		pci_add_resource(&info->resources, &window->resource);
 
-static void __devinit
-pcibios_setup_root_windows(struct pci_bus *bus, struct pci_controller *ctrl)
-{
-	int i;
-
-	pci_bus_remove_resources(bus);
-	for (i = 0; i < ctrl->windows; i++) {
-		struct resource *res = &ctrl->window[i].resource;
-		/* HP's firmware has a hack to work around a Windows bug.
-		 * Ignore these tiny memory ranges */
-		if ((res->flags & IORESOURCE_MEM) &&
-		    (res->end - res->start < 16))
-			continue;
-		pci_bus_add_resource(bus, res, 0);
-	}
+	return AE_OK;
 }
 
 struct pci_bus * __devinit
@@ -343,6 +333,7 @@ pci_acpi_scan_root(struct acpi_pci_root
 	int bus = root->secondary.start;
 	struct pci_controller *controller;
 	unsigned int windows = 0;
+	struct pci_root_info info;
 	struct pci_bus *pbus;
 	char *name;
 	int pxm;
@@ -359,11 +350,10 @@ pci_acpi_scan_root(struct acpi_pci_root
 		controller->node = pxm_to_node(pxm);
 #endif
 
+	INIT_LIST_HEAD(&info.resources);
 	acpi_walk_resources(device->handle, METHOD_NAME__CRS, count_window,
 			&windows);
 	if (windows) {
-		struct pci_root_info info;
-
 		controller->window =
 			kmalloc_node(sizeof(*controller->window) * windows,
 				     GFP_KERNEL, controller->node);
@@ -387,8 +377,14 @@ pci_acpi_scan_root(struct acpi_pci_root
 	 * should handle the case here, but it appears that IA64 hasn't
 	 * such quirk. So we just ignore the case now.
 	 */
-	pbus = pci_scan_bus_parented(NULL, bus, &pci_root_ops, controller);
+	pbus = pci_create_root_bus(NULL, bus, &pci_root_ops, controller,
+				   &info.resources);
+	if (!pbus) {
+		pci_free_resource_list(&info.resources);
+		return NULL;
+	}
 
+	pbus->subordinate = pci_scan_child_bus(pbus);
 	return pbus;
 
 out3:
@@ -504,14 +500,10 @@ pcibios_fixup_bus (struct pci_bus *b)
 	if (b->self) {
 		pci_read_bridge_bases(b);
 		pcibios_fixup_bridge_resources(b->self);
-	} else {
-		pcibios_setup_root_windows(b, b->sysdata);
 	}
 	list_for_each_entry(dev, &b->devices, bus_list)
 		pcibios_fixup_device_resources(dev);
 	platform_pci_fixup_bus(b);
-
-	return;
 }
 
 void __devinit
--- a/arch/microblaze/include/asm/pci-bridge.h
+++ b/arch/microblaze/include/asm/pci-bridge.h
@@ -140,7 +140,6 @@ extern void pci_process_bridge_OF_ranges
 /* Allocate & free a PCI host bridge structure */
 extern struct pci_controller *pcibios_alloc_controller(struct device_node *dev);
 extern void pcibios_free_controller(struct pci_controller *phb);
-extern void pcibios_setup_phb_resources(struct pci_controller *hose);
 
 #endif	/* __KERNEL__ */
 #endif	/* _ASM_MICROBLAZE_PCI_BRIDGE_H */
--- a/arch/microblaze/pci/pci-common.c
+++ b/arch/microblaze/pci/pci-common.c
@@ -1019,7 +1019,6 @@ static void __devinit pcibios_fixup_brid
 	struct pci_dev *dev = bus->self;
 
 	pci_bus_for_each_resource(bus, res, i) {
-		res = bus->resource[i];
 		if (!res)
 			continue;
 		if (!res->flags)
@@ -1219,7 +1218,6 @@ void pcibios_allocate_bus_resources(stru
 		 pci_domain_nr(bus), bus->number);
 
 	pci_bus_for_each_resource(bus, res, i) {
-		res = bus->resource[i];
 		if (!res || !res->flags
 		    || res->start > res->end || res->parent)
 			continue;
@@ -1510,14 +1508,18 @@ int pcibios_enable_device(struct pci_dev
 	return pci_enable_resources(dev, mask);
 }
 
-void __devinit pcibios_setup_phb_resources(struct pci_controller *hose)
+static void __devinit pcibios_setup_phb_resources(struct pci_controller *hose, struct list_head *resources)
 {
-	struct pci_bus *bus = hose->bus;
 	struct resource *res;
 	int i;
 
 	/* Hookup PHB IO resource */
-	bus->resource[0] = res = &hose->io_resource;
+	res = &hose->io_resource;
+
+	/* Fixup IO space offset */
+	io_offset = (unsigned long)hose->io_base_virt - isa_io_base;
+	res->start = (res->start + io_offset) & 0xffffffffu;
+	res->end = (res->end + io_offset) & 0xffffffffu;
 
 	if (!res->flags) {
 		printk(KERN_WARNING "PCI: I/O resource not set for host"
@@ -1528,6 +1530,7 @@ void __devinit pcibios_setup_phb_resourc
 		res->end = res->start + IO_SPACE_LIMIT;
 		res->flags = IORESOURCE_IO;
 	}
+	pci_add_resource(resources, res);
 
 	pr_debug("PCI: PHB IO resource    = %016llx-%016llx [%lx]\n",
 		 (unsigned long long)res->start,
@@ -1550,7 +1553,7 @@ void __devinit pcibios_setup_phb_resourc
 			res->flags = IORESOURCE_MEM;
 
 		}
-		bus->resource[i+1] = res;
+		pci_add_resource(resources, res);
 
 		pr_debug("PCI: PHB MEM resource %d = %016llx-%016llx [%lx]\n",
 			i, (unsigned long long)res->start,
@@ -1573,34 +1576,27 @@ struct device_node *pcibios_get_phb_of_n
 
 static void __devinit pcibios_scan_phb(struct pci_controller *hose)
 {
+	LIST_HEAD(resources);
 	struct pci_bus *bus;
 	struct device_node *node = hose->dn;
-	unsigned long io_offset;
-	struct resource *res = &hose->io_resource;
 
 	pr_debug("PCI: Scanning PHB %s\n",
 		 node ? node->full_name : "<NO NAME>");
 
-	/* Create an empty bus for the toplevel */
-	bus = pci_create_bus(hose->parent, hose->first_busno, hose->ops, hose);
+	pcibios_setup_phb_resources(hose, &resources);
+
+	bus = pci_scan_root_bus(hose->parent, hose->first_busno,
+				hose->ops, hose, &resources);
 	if (bus == NULL) {
 		printk(KERN_ERR "Failed to create bus for PCI domain %04x\n",
 		       hose->global_number);
+		pci_free_resource_list(&resources);
 		return;
 	}
 	bus->secondary = hose->first_busno;
 	hose->bus = bus;
 
-	/* Fixup IO space offset */
-	io_offset = (unsigned long)hose->io_base_virt - isa_io_base;
-	res->start = (res->start + io_offset) & 0xffffffffu;
-	res->end = (res->end + io_offset) & 0xffffffffu;
-
-	/* Wire up PHB bus resources */
-	pcibios_setup_phb_resources(hose);
-
-	/* Scan children */
-	hose->last_busno = bus->subordinate = pci_scan_child_bus(bus);
+	hose->last_busno = bus->subordinate;
 }
 
 static int __init pcibios_init(void)
@@ -1614,8 +1610,6 @@ static int __init pcibios_init(void)
 	list_for_each_entry_safe(hose, tmp, &hose_list, list_node) {
 		hose->last_busno = 0xff;
 		pcibios_scan_phb(hose);
-		printk(KERN_INFO "calling pci_bus_add_devices()\n");
-		pci_bus_add_devices(hose->bus);
 		if (next_busno <= hose->last_busno)
 			next_busno = hose->last_busno + 1;
 	}
--- a/arch/mips/pci/pci.c
+++ b/arch/mips/pci/pci.c
@@ -81,6 +81,7 @@ static void __devinit pcibios_scanbus(st
 {
 	static int next_busno;
 	static int need_domain_info;
+	LIST_HEAD(resources);
 	struct pci_bus *bus;
 
 	if (!hose->iommu)
@@ -89,7 +90,13 @@ static void __devinit pcibios_scanbus(st
 	if (hose->get_busno && pci_probe_only)
 		next_busno = (*hose->get_busno)();
 
-	bus = pci_scan_bus(next_busno, hose->pci_ops, hose);
+	pci_add_resource(&resources, hose->mem_resource);
+	pci_add_resource(&resources, hose->io_resource);
+	bus = pci_scan_root_bus(NULL, next_busno, hose->pci_ops, hose,
+				&resources);
+	if (!bus)
+		pci_free_resource_list(&resources);
+
 	hose->bus = bus;
 
 	need_domain_info = need_domain_info || hose->index;
@@ -266,15 +273,11 @@ void __devinit pcibios_fixup_bus(struct
 {
 	/* Propagate hose info into the subordinate devices.  */
 
-	struct pci_controller *hose = bus->sysdata;
 	struct list_head *ln;
 	struct pci_dev *dev = bus->self;
 
-	if (!dev) {
-		bus->resource[0] = hose->io_resource;
-		bus->resource[1] = hose->mem_resource;
-	} else if (pci_probe_only &&
-		   (dev->class >> 8) == PCI_CLASS_BRIDGE_PCI) {
+	if (pci_probe_only && dev &&
+	    (dev->class >> 8) == PCI_CLASS_BRIDGE_PCI) {
 		pci_read_bridge_bases(bus);
 		pcibios_fixup_device_resources(dev, bus);
 	}
--- a/arch/mn10300/unit-asb2305/pci.c
+++ b/arch/mn10300/unit-asb2305/pci.c
@@ -380,11 +380,6 @@ void __devinit pcibios_fixup_bus(struct
 {
 	struct pci_dev *dev;
 
-	if (bus->number == 0) {
-		bus->resource[0] = &pci_ioport_resource;
-		bus->resource[1] = &pci_iomem_resource;
-	}
-
 	if (bus->self) {
 		pci_read_bridge_bases(bus);
 		pcibios_fixup_device_resources(bus->self);
@@ -402,6 +397,8 @@ void __devinit pcibios_fixup_bus(struct
  */
 static int __init pcibios_init(void)
 {
+	LIST_HEAD(resources);
+
 	ioport_resource.start	= 0xA0000000;
 	ioport_resource.end	= 0xDFFFFFFF;
 	iomem_resource.start	= 0xA0000000;
@@ -423,7 +420,10 @@ static int __init pcibios_init(void)
 	printk(KERN_INFO "PCI: Probing PCI hardware [mempage %08x]\n",
 	       MEM_PAGING_REG);
 
-	pci_root_bus = pci_scan_bus(0, &pci_direct_ampci, NULL);
+	pci_add_resource(&resources, &pci_ioport_resource);
+	pci_add_resource(&resources, &pci_iomem_resource);
+	pci_root_bus = pci_scan_root_bus(NULL, 0, &pci_direct_ampci, NULL,
+					 &resources);
 
 	pcibios_irq_init();
 	pcibios_fixup_irqs();
--- a/arch/powerpc/include/asm/pci-bridge.h
+++ b/arch/powerpc/include/asm/pci-bridge.h
@@ -222,7 +222,6 @@ extern void pci_process_bridge_OF_ranges
 /* Allocate & free a PCI host bridge structure */
 extern struct pci_controller *pcibios_alloc_controller(struct device_node *dev);
 extern void pcibios_free_controller(struct pci_controller *phb);
-extern void pcibios_setup_phb_resources(struct pci_controller *hose);
 
 #ifdef CONFIG_PCI
 extern int pcibios_vaddr_is_ioport(void __iomem *address);
--- a/arch/powerpc/kernel/pci-common.c
+++ b/arch/powerpc/kernel/pci-common.c
@@ -1555,14 +1555,13 @@ int pcibios_enable_device(struct pci_dev
 	return pci_enable_resources(dev, mask);
 }
 
-void __devinit pcibios_setup_phb_resources(struct pci_controller *hose)
+static void __devinit pcibios_setup_phb_resources(struct pci_controller *hose, struct list_head *resources)
 {
-	struct pci_bus *bus = hose->bus;
 	struct resource *res;
 	int i;
 
 	/* Hookup PHB IO resource */
-	bus->resource[0] = res = &hose->io_resource;
+	res = &hose->io_resource;
 
 	if (!res->flags) {
 		printk(KERN_WARNING "PCI: I/O resource not set for host"
@@ -1580,6 +1579,7 @@ void __devinit pcibios_setup_phb_resourc
 		 (unsigned long long)res->start,
 		 (unsigned long long)res->end,
 		 (unsigned long)res->flags);
+	pci_add_resource(resources, res);
 
 	/* Hookup PHB Memory resources */
 	for (i = 0; i < 3; ++i) {
@@ -1597,12 +1597,12 @@ void __devinit pcibios_setup_phb_resourc
 			res->flags = IORESOURCE_MEM;
 #endif /* CONFIG_PPC32 */
 		}
-		bus->resource[i+1] = res;
 
 		pr_debug("PCI: PHB MEM resource %d = %016llx-%016llx [%lx]\n", i,
 			 (unsigned long long)res->start,
 			 (unsigned long long)res->end,
 			 (unsigned long)res->flags);
+		pci_add_resource(resources, res);
 	}
 
 	pr_debug("PCI: PHB MEM offset     = %016llx\n",
@@ -1696,6 +1696,7 @@ struct device_node *pcibios_get_phb_of_n
  */
 void __devinit pcibios_scan_phb(struct pci_controller *hose)
 {
+	LIST_HEAD(resources);
 	struct pci_bus *bus;
 	struct device_node *node = hose->dn;
 	int mode;
@@ -1703,22 +1704,24 @@ void __devinit pcibios_scan_phb(struct p
 	pr_debug("PCI: Scanning PHB %s\n",
 		 node ? node->full_name : "<NO NAME>");
 
+	/* Get some IO space for the new PHB */
+	pcibios_setup_phb_io_space(hose);
+
+	/* Wire up PHB bus resources */
+	pcibios_setup_phb_resources(hose, &resources);
+
 	/* Create an empty bus for the toplevel */
-	bus = pci_create_bus(hose->parent, hose->first_busno, hose->ops, hose);
+	bus = pci_create_root_bus(hose->parent, hose->first_busno,
+				  hose->ops, hose, &resources);
 	if (bus == NULL) {
 		pr_err("Failed to create bus for PCI domain %04x\n",
 			hose->global_number);
+		pci_free_resource_list(&resources);
 		return;
 	}
 	bus->secondary = hose->first_busno;
 	hose->bus = bus;
 
-	/* Get some IO space for the new PHB */
-	pcibios_setup_phb_io_space(hose);
-
-	/* Wire up PHB bus resources */
-	pcibios_setup_phb_resources(hose);
-
 	/* Get probe mode and perform scan */
 	mode = PCI_PROBE_NORMAL;
 	if (node && ppc_md.pci_probe_mode)
--- a/arch/powerpc/kernel/pci_64.c
+++ b/arch/powerpc/kernel/pci_64.c
@@ -131,30 +131,13 @@ EXPORT_SYMBOL_GPL(pcibios_unmap_io_space
 
 #endif /* CONFIG_HOTPLUG */
 
-int __devinit pcibios_map_io_space(struct pci_bus *bus)
+static int __devinit pcibios_map_phb_io_space(struct pci_controller *hose)
 {
 	struct vm_struct *area;
 	unsigned long phys_page;
 	unsigned long size_page;
 	unsigned long io_virt_offset;
-	struct pci_controller *hose;
-
-	WARN_ON(bus == NULL);
 
-	/* If this not a PHB, nothing to do, page tables still exist and
-	 * thus HPTEs will be faulted in when needed
-	 */
-	if (bus->self) {
-		pr_debug("IO mapping for PCI-PCI bridge %s\n",
-			 pci_name(bus->self));
-		pr_debug("  virt=0x%016llx...0x%016llx\n",
-			 bus->resource[0]->start + _IO_BASE,
-			 bus->resource[0]->end + _IO_BASE);
-		return 0;
-	}
-
-	/* Get the host bridge */
-	hose = pci_bus_to_host(bus);
 	phys_page = _ALIGN_DOWN(hose->io_base_phys, PAGE_SIZE);
 	size_page = _ALIGN_UP(hose->pci_io_size, PAGE_SIZE);
 
@@ -198,11 +181,30 @@ int __devinit pcibios_map_io_space(struc
 
 	return 0;
 }
+
+int __devinit pcibios_map_io_space(struct pci_bus *bus)
+{
+	WARN_ON(bus == NULL);
+
+	/* If this not a PHB, nothing to do, page tables still exist and
+	 * thus HPTEs will be faulted in when needed
+	 */
+	if (bus->self) {
+		pr_debug("IO mapping for PCI-PCI bridge %s\n",
+			 pci_name(bus->self));
+		pr_debug("  virt=0x%016llx...0x%016llx\n",
+			 bus->resource[0]->start + _IO_BASE,
+			 bus->resource[0]->end + _IO_BASE);
+		return 0;
+	}
+
+	return pcibios_map_phb_io_space(pci_bus_to_host(bus));
+}
 EXPORT_SYMBOL_GPL(pcibios_map_io_space);
 
 void __devinit pcibios_setup_phb_io_space(struct pci_controller *hose)
 {
-	pcibios_map_io_space(hose->bus);
+	pcibios_map_phb_io_space(hose);
 }
 
 #define IOBASE_BRIDGE_NUMBER	0
--- a/arch/sh/drivers/pci/pci.c
+++ b/arch/sh/drivers/pci/pci.c
@@ -36,9 +36,15 @@ static void __devinit pcibios_scanbus(st
 {
 	static int next_busno;
 	static int need_domain_info;
+	LIST_HEAD(resources);
+	int i;
 	struct pci_bus *bus;
 
-	bus = pci_scan_bus(next_busno, hose->pci_ops, hose);
+	for (i = 0; i < hose->nr_resources; i++)
+		pci_add_resource(&resources, hose->resources + i);
+
+	bus = pci_scan_root_bus(NULL, next_busno, hose->pci_ops, hose,
+				&resources);
 	hose->bus = bus;
 
 	need_domain_info = need_domain_info || hose->index;
@@ -55,6 +61,8 @@ static void __devinit pcibios_scanbus(st
 		pci_bus_size_bridges(bus);
 		pci_bus_assign_resources(bus);
 		pci_enable_bridges(bus);
+	} else {
+		pci_free_resource_list(&resources);
 	}
 }
 
@@ -162,16 +170,8 @@ static void pcibios_fixup_device_resourc
  */
 void __devinit pcibios_fixup_bus(struct pci_bus *bus)
 {
-	struct pci_dev *dev = bus->self;
+	struct pci_dev *dev;
 	struct list_head *ln;
-	struct pci_channel *hose = bus->sysdata;
-
-	if (!dev) {
-		int i;
-
-		for (i = 0; i < hose->nr_resources; i++)
-			bus->resource[i] = hose->resources + i;
-	}
 
 	for (ln = bus->devices.next; ln != &bus->devices; ln = ln->next) {
 		dev = pci_dev_b(ln);
--- a/arch/sparc/kernel/leon_pci.c
+++ b/arch/sparc/kernel/leon_pci.c
@@ -19,22 +19,22 @@
  */
 void leon_pci_init(struct platform_device *ofdev, struct leon_pci_info *info)
 {
+	LIST_HEAD(resources);
 	struct pci_bus *root_bus;
 
-	root_bus = pci_scan_bus_parented(&ofdev->dev, 0, info->ops, info);
-	if (root_bus) {
-		root_bus->resource[0] = &info->io_space;
-		root_bus->resource[1] = &info->mem_space;
-		root_bus->resource[2] = NULL;
-
-		/* Init all PCI devices into PCI tree */
-		pci_bus_add_devices(root_bus);
+	pci_add_resource(&resources, &info->io_space);
+	pci_add_resource(&resources, &info->mem_space);
 
+	root_bus = pci_scan_root_bus(&ofdev->dev, 0, info->ops, info,
+				     &resources);
+	if (root_bus) {
 		/* Setup IRQs of all devices using custom routines */
 		pci_fixup_irqs(pci_common_swizzle, info->map_irq);
 
 		/* Assign devices with resources */
 		pci_assign_unassigned_resources();
+	} else {
+		pci_free_resource_list(&resources);
 	}
 }
 
@@ -83,15 +83,6 @@ void __devinit pcibios_fixup_bus(struct
 	int i, has_io, has_mem;
 	u16 cmd;
 
-	/* Generic PCI bus probing sets these to point at
-	 * &io{port,mem}_resouce which is wrong for us.
-	 */
-	if (pbus->self == NULL) {
-		pbus->resource[0] = &info->io_space;
-		pbus->resource[1] = &info->mem_space;
-		pbus->resource[2] = NULL;
-	}
-
 	list_for_each_entry(dev, &pbus->devices, bus_list) {
 		/*
 		 * We can not rely on that the bootloader has enabled I/O
--- a/arch/sparc/kernel/pci.c
+++ b/arch/sparc/kernel/pci.c
@@ -685,23 +685,25 @@ static void __devinit pci_bus_register_o
 struct pci_bus * __devinit pci_scan_one_pbm(struct pci_pbm_info *pbm,
 					    struct device *parent)
 {
+	LIST_HEAD(resources);
 	struct device_node *node = pbm->op->dev.of_node;
 	struct pci_bus *bus;
 
 	printk("PCI: Scanning PBM %s\n", node->full_name);
 
-	bus = pci_create_bus(parent, pbm->pci_first_busno, pbm->pci_ops, pbm);
+	pci_add_resource(&resources, &pbm->io_space);
+	pci_add_resource(&resources, &pbm->mem_space);
+	bus = pci_create_root_bus(parent, pbm->pci_first_busno, pbm->pci_ops,
+				  pbm, &resources);
 	if (!bus) {
 		printk(KERN_ERR "Failed to create bus for %s\n",
 		       node->full_name);
+		pci_free_resource_list(&resources);
 		return NULL;
 	}
 	bus->secondary = pbm->pci_first_busno;
 	bus->subordinate = pbm->pci_last_busno;
 
-	bus->resource[0] = &pbm->io_space;
-	bus->resource[1] = &pbm->mem_space;
-
 	pci_of_scan_bus(pbm, node, bus);
 	pci_bus_add_devices(bus);
 	pci_bus_register_of_sysfs(bus);
@@ -711,13 +713,6 @@ struct pci_bus * __devinit pci_scan_one_
 
 void __devinit pcibios_fixup_bus(struct pci_bus *pbus)
 {
-	struct pci_pbm_info *pbm = pbus->sysdata;
-
-	/* Generic PCI bus probing sets these to point at
-	 * &io{port,mem}_resouce which is wrong for us.
-	 */
-	pbus->resource[0] = &pbm->io_space;
-	pbus->resource[1] = &pbm->mem_space;
 }
 
 void pcibios_update_irq(struct pci_dev *pdev, int irq)
--- a/arch/x86/include/asm/topology.h
+++ b/arch/x86/include/asm/topology.h
@@ -174,7 +174,7 @@ static inline void arch_fix_phys_package
 }
 
 struct pci_bus;
-void x86_pci_root_bus_res_quirks(struct pci_bus *b);
+void x86_pci_root_bus_resources(int bus, struct list_head *resources);
 
 #ifdef CONFIG_SMP
 #define mc_capable()	((boot_cpu_data.x86_max_cores > 1) && \
--- a/arch/x86/pci/acpi.c
+++ b/arch/x86/pci/acpi.c
@@ -12,7 +12,7 @@ struct pci_root_info {
 	char *name;
 	unsigned int res_num;
 	struct resource *res;
-	struct pci_bus *bus;
+	struct list_head *resources;
 	int busnum;
 };
 
@@ -285,23 +285,20 @@ static void add_resources(struct pci_roo
 				 "ignoring host bridge window %pR (conflicts with %s %pR)\n",
 				 res, conflict->name, conflict);
 		else
-			pci_bus_add_resource(info->bus, res, 0);
+			pci_add_resource(info->resources, res);
 	}
 }
 
 static void
 get_current_resources(struct acpi_device *device, int busnum,
-			int domain, struct pci_bus *bus)
+		      int domain, struct list_head *resources)
 {
 	struct pci_root_info info;
 	size_t size;
 
-	if (pci_use_crs)
-		pci_bus_remove_resources(bus);
-
 	info.bridge = device;
-	info.bus = bus;
 	info.res_num = 0;
+	info.resources = resources;
 	acpi_walk_resources(device->handle, METHOD_NAME__CRS, count_resource,
 				&info);
 	if (!info.res_num)
@@ -310,7 +307,7 @@ get_current_resources(struct acpi_device
 	size = sizeof(*info.res) * info.res_num;
 	info.res = kmalloc(size, GFP_KERNEL);
 	if (!info.res)
-		goto res_alloc_fail;
+		return;
 
 	info.name = kasprintf(GFP_KERNEL, "PCI Bus %04x:%02x", domain, busnum);
 	if (!info.name)
@@ -325,8 +322,6 @@ get_current_resources(struct acpi_device
 
 name_alloc_fail:
 	kfree(info.res);
-res_alloc_fail:
-	return;
 }
 
 struct pci_bus * __devinit pci_acpi_scan_root(struct acpi_pci_root *root)
@@ -334,6 +329,7 @@ struct pci_bus * __devinit pci_acpi_scan
 	struct acpi_device *device = root->device;
 	int domain = root->segment;
 	int busnum = root->secondary.start;
+	LIST_HEAD(resources);
 	struct pci_bus *bus;
 	struct pci_sysdata *sd;
 	int node;
@@ -388,11 +384,15 @@ struct pci_bus * __devinit pci_acpi_scan
 		memcpy(bus->sysdata, sd, sizeof(*sd));
 		kfree(sd);
 	} else {
-		bus = pci_create_bus(NULL, busnum, &pci_root_ops, sd);
-		if (bus) {
-			get_current_resources(device, busnum, domain, bus);
+		get_current_resources(device, busnum, domain, &resources);
+		if (list_empty(&resources))
+			x86_pci_root_bus_resources(busnum, &resources);
+		bus = pci_create_root_bus(NULL, busnum, &pci_root_ops, sd,
+					  &resources);
+		if (bus)
 			bus->subordinate = pci_scan_child_bus(bus);
-		}
+		else
+			pci_free_resource_list(&resources);
 	}
 
 	/* After the PCI-E bus has been walked and all devices discovered,
--- a/arch/x86/pci/broadcom_bus.c
+++ b/arch/x86/pci/broadcom_bus.c
@@ -15,10 +15,11 @@
 #include <linux/pci.h>
 #include <linux/init.h>
 #include <asm/pci_x86.h>
+#include <asm/pci-direct.h>
 
 #include "bus_numa.h"
 
-static void __devinit cnb20le_res(struct pci_dev *dev)
+static void __init cnb20le_res(u8 bus, u8 slot, u8 func)
 {
 	struct pci_root_info *info;
 	struct resource res;
@@ -26,21 +27,12 @@ static void __devinit cnb20le_res(struct
 	u8 fbus, lbus;
 	int i;
 
-#ifdef CONFIG_ACPI
-	/*
-	 * We should get host bridge information from ACPI unless the BIOS
-	 * doesn't support it.
-	 */
-	if (acpi_os_get_root_pointer())
-		return;
-#endif
-
 	info = &pci_root_info[pci_root_num];
 	pci_root_num++;
 
 	/* read the PCI bus numbers */
-	pci_read_config_byte(dev, 0x44, &fbus);
-	pci_read_config_byte(dev, 0x45, &lbus);
+	fbus = read_pci_config_byte(bus, slot, func, 0x44);
+	lbus = read_pci_config_byte(bus, slot, func, 0x45);
 	info->bus_min = fbus;
 	info->bus_max = lbus;
 
@@ -59,8 +51,8 @@ static void __devinit cnb20le_res(struct
 	}
 
 	/* read the non-prefetchable memory window */
-	pci_read_config_word(dev, 0xc0, &word1);
-	pci_read_config_word(dev, 0xc2, &word2);
+	word1 = read_pci_config_16(bus, slot, func, 0xc0);
+	word2 = read_pci_config_16(bus, slot, func, 0xc2);
 	if (word1 != word2) {
 		res.start = (word1 << 16) | 0x0000;
 		res.end   = (word2 << 16) | 0xffff;
@@ -69,8 +61,8 @@ static void __devinit cnb20le_res(struct
 	}
 
 	/* read the prefetchable memory window */
-	pci_read_config_word(dev, 0xc4, &word1);
-	pci_read_config_word(dev, 0xc6, &word2);
+	word1 = read_pci_config_16(bus, slot, func, 0xc4);
+	word2 = read_pci_config_16(bus, slot, func, 0xc6);
 	if (word1 != word2) {
 		res.start = (word1 << 16) | 0x0000;
 		res.end   = (word2 << 16) | 0xffff;
@@ -79,8 +71,8 @@ static void __devinit cnb20le_res(struct
 	}
 
 	/* read the IO port window */
-	pci_read_config_word(dev, 0xd0, &word1);
-	pci_read_config_word(dev, 0xd2, &word2);
+	word1 = read_pci_config_16(bus, slot, func, 0xd0);
+	word2 = read_pci_config_16(bus, slot, func, 0xd2);
 	if (word1 != word2) {
 		res.start = word1;
 		res.end   = word2;
@@ -92,13 +84,37 @@ static void __devinit cnb20le_res(struct
 	res.start = fbus;
 	res.end   = lbus;
 	res.flags = IORESOURCE_BUS;
-	dev_info(&dev->dev, "CNB20LE PCI Host Bridge (domain %04x %pR)\n",
-			    pci_domain_nr(dev->bus), &res);
+	printk(KERN_INFO "CNB20LE PCI Host Bridge (domain 0000 %pR)\n", &res);
 
 	for (i = 0; i < info->res_num; i++)
-		dev_info(&dev->dev, "host bridge window %pR\n", &info->res[i]);
+		printk(KERN_INFO "host bridge window %pR\n", &info->res[i]);
 }
 
-DECLARE_PCI_FIXUP_EARLY(PCI_VENDOR_ID_SERVERWORKS, PCI_DEVICE_ID_SERVERWORKS_LE,
-			cnb20le_res);
+static int __init broadcom_postcore_init(void)
+{
+	u8 bus = 0, slot = 0;
+	u32 id;
+	u16 vendor, device;
+
+#ifdef CONFIG_ACPI
+	/*
+	 * We should get host bridge information from ACPI unless the BIOS
+	 * doesn't support it.
+	 */
+	if (acpi_os_get_root_pointer())
+		return 0;
+#endif
+
+	id = read_pci_config(bus, slot, 0, PCI_VENDOR_ID);
+	vendor = id & 0xffff;
+	device = (id >> 16) & 0xffff;
+
+	if (vendor == PCI_VENDOR_ID_SERVERWORKS &&
+	    device == PCI_DEVICE_ID_SERVERWORKS_LE) {
+		cnb20le_res(bus, slot, 0);
+		cnb20le_res(bus, slot, 1);
+	}
+	return 0;
+}
 
+postcore_initcall(broadcom_postcore_init);
--- a/arch/x86/pci/bus_numa.c
+++ b/arch/x86/pci/bus_numa.c
@@ -7,45 +7,50 @@
 int pci_root_num;
 struct pci_root_info pci_root_info[PCI_ROOT_NR];
 
-void x86_pci_root_bus_res_quirks(struct pci_bus *b)
+void x86_pci_root_bus_resources(int bus, struct list_head *resources)
 {
 	int i;
 	int j;
 	struct pci_root_info *info;
 
-	/* don't go for it if _CRS is used already */
-	if (b->resource[0] != &ioport_resource ||
-	    b->resource[1] != &iomem_resource)
-		return;
-
 	if (!pci_root_num)
-		return;
+		goto default_resources;
 
 	for (i = 0; i < pci_root_num; i++) {
-		if (pci_root_info[i].bus_min == b->number)
+		if (pci_root_info[i].bus_min == bus)
 			break;
 	}
 
 	if (i == pci_root_num)
-		return;
+		goto default_resources;
 
-	printk(KERN_DEBUG "PCI: peer root bus %02x res updated from pci conf\n",
-			b->number);
+	printk(KERN_DEBUG "PCI: root bus %02x: hardware-probed resources\n",
+	       bus);
 
-	pci_bus_remove_resources(b);
 	info = &pci_root_info[i];
 	for (j = 0; j < info->res_num; j++) {
 		struct resource *res;
 		struct resource *root;
 
 		res = &info->res[j];
-		pci_bus_add_resource(b, res, 0);
+		pci_add_resource(resources, res);
 		if (res->flags & IORESOURCE_IO)
 			root = &ioport_resource;
 		else
 			root = &iomem_resource;
 		insert_resource(root, res);
 	}
+	return;
+
+default_resources:
+	/*
+	 * We don't have any host bridge aperture information from the
+	 * "native host bridge drivers," e.g., amd_bus or broadcom_bus,
+	 * so fall back to the defaults historically used by pci_create_bus().
+	 */
+	printk(KERN_DEBUG "PCI: root bus %02x: using default resources\n", bus);
+	pci_add_resource(resources, &ioport_resource);
+	pci_add_resource(resources, &iomem_resource);
 }
 
 void __devinit update_res(struct pci_root_info *info, resource_size_t start,
--- a/arch/x86/pci/common.c
+++ b/arch/x86/pci/common.c
@@ -164,9 +164,6 @@ void __devinit pcibios_fixup_bus(struct
 {
 	struct pci_dev *dev;
 
-	/* root bus? */
-	if (!b->parent)
-		x86_pci_root_bus_res_quirks(b);
 	pci_read_bridge_bases(b);
 	list_for_each_entry(dev, &b->devices, bus_list)
 		pcibios_fixup_device_resources(dev);
@@ -433,6 +430,7 @@ void __init dmi_check_pciprobe(void)
 
 struct pci_bus * __devinit pcibios_scan_root(int busnum)
 {
+	LIST_HEAD(resources);
 	struct pci_bus *bus = NULL;
 	struct pci_sysdata *sd;
 
@@ -456,9 +454,12 @@ struct pci_bus * __devinit pcibios_scan_
 	sd->node = get_mp_bus_to_node(busnum);
 
 	printk(KERN_DEBUG "PCI: Probing PCI hardware (bus %02x)\n", busnum);
-	bus = pci_scan_bus_parented(NULL, busnum, &pci_root_ops, sd);
-	if (!bus)
+	x86_pci_root_bus_resources(busnum, &resources);
+	bus = pci_scan_root_bus(NULL, busnum, &pci_root_ops, sd, &resources);
+	if (!bus) {
+		pci_free_resource_list(&resources);
 		kfree(sd);
+	}
 
 	return bus;
 }
@@ -639,6 +640,7 @@ int pci_ext_cfg_avail(struct pci_dev *de
 
 struct pci_bus * __devinit pci_scan_bus_on_node(int busno, struct pci_ops *ops, int node)
 {
+	LIST_HEAD(resources);
 	struct pci_bus *bus = NULL;
 	struct pci_sysdata *sd;
 
@@ -653,9 +655,12 @@ struct pci_bus * __devinit pci_scan_bus_
 		return NULL;
 	}
 	sd->node = node;
-	bus = pci_scan_bus(busno, ops, sd);
-	if (!bus)
+	x86_pci_root_bus_resources(busno, &resources);
+	bus = pci_scan_root_bus(NULL, busno, ops, sd, &resources);
+	if (!bus) {
+		pci_free_resource_list(&resources);
 		kfree(sd);
+	}
 
 	return bus;
 }
--- a/arch/x86/pci/legacy.c
+++ b/arch/x86/pci/legacy.c
@@ -31,9 +31,6 @@ int __init pci_legacy_init(void)
 
 	printk("PCI: Probing PCI hardware\n");
 	pci_root_bus = pcibios_scan_root(0);
-	if (pci_root_bus)
-		pci_bus_add_devices(pci_root_bus);
-
 	return 0;
 }
 
--- a/arch/x86/pci/numaq_32.c
+++ b/arch/x86/pci/numaq_32.c
@@ -153,8 +153,6 @@ int __init pci_numaq_init(void)
 	raw_pci_ops = &pci_direct_conf1_mq;
 
 	pci_root_bus = pcibios_scan_root(0);
-	if (pci_root_bus)
-		pci_bus_add_devices(pci_root_bus);
 	if (num_online_nodes() > 1)
 		for_each_online_node(quad) {
 			if (quad == 0)
--- a/arch/xtensa/kernel/pci.c
+++ b/arch/xtensa/kernel/pci.c
@@ -134,9 +134,46 @@ struct pci_controller * __init pcibios_a
 	return pci_ctrl;
 }
 
+static void __init pci_controller_apertures(struct pci_controller *pci_ctrl,
+					    struct list_head *resources)
+{
+	struct resource *res;
+	unsigned long io_offset;
+	int i;
+
+	io_offset = (unsigned long)pci_ctrl->io_space.base;
+	res = &pci_ctrl->io_resource;
+	if (!res->flags) {
+		if (io_offset)
+			printk (KERN_ERR "I/O resource not set for host"
+				" bridge %d\n", pci_ctrl->index);
+		res->start = 0;
+		res->end = IO_SPACE_LIMIT;
+		res->flags = IORESOURCE_IO;
+	}
+	res->start += io_offset;
+	res->end += io_offset;
+	pci_add_resource(resources, res);
+
+	for (i = 0; i < 3; i++) {
+		res = &pci_ctrl->mem_resources[i];
+		if (!res->flags) {
+			if (i > 0)
+				continue;
+			printk(KERN_ERR "Memory resource not set for "
+			       "host bridge %d\n", pci_ctrl->index);
+			res->start = 0;
+			res->end = ~0U;
+			res->flags = IORESOURCE_MEM;
+		}
+		pci_add_resource(resources, res);
+	}
+}
+
 static int __init pcibios_init(void)
 {
 	struct pci_controller *pci_ctrl;
+	struct list_head resources;
 	struct pci_bus *bus;
 	int next_busno = 0, i;
 
@@ -145,19 +182,10 @@ static int __init pcibios_init(void)
 	/* Scan all of the recorded PCI controllers.  */
 	for (pci_ctrl = pci_ctrl_head; pci_ctrl; pci_ctrl = pci_ctrl->next) {
 		pci_ctrl->last_busno = 0xff;
-		bus = pci_scan_bus(pci_ctrl->first_busno, pci_ctrl->ops,
-				   pci_ctrl);
-		if (pci_ctrl->io_resource.flags) {
-			unsigned long offs;
-
-			offs = (unsigned long)pci_ctrl->io_space.base;
-			pci_ctrl->io_resource.start += offs;
-			pci_ctrl->io_resource.end += offs;
-			bus->resource[0] = &pci_ctrl->io_resource;
-		}
-		for (i = 0; i < 3; ++i)
-			if (pci_ctrl->mem_resources[i].flags)
-				bus->resource[i+1] =&pci_ctrl->mem_resources[i];
+		INIT_LIST_HEAD(&resources);
+		pci_controller_apertures(pci_ctrl, &resources);
+		bus = pci_scan_root_bus(NULL, pci_ctrl->first_busno,
+					pci_ctrl->ops, pci_ctrl, &resources);
 		pci_ctrl->bus = bus;
 		pci_ctrl->last_busno = bus->subordinate;
 		if (next_busno <= pci_ctrl->last_busno)
@@ -178,36 +206,7 @@ void __init pcibios_fixup_bus(struct pci
 	int i;
 
 	io_offset = (unsigned long)pci_ctrl->io_space.base;
-	if (bus->parent == NULL) {
-		/* this is a host bridge - fill in its resources */
-		pci_ctrl->bus = bus;
-
-		bus->resource[0] = res = &pci_ctrl->io_resource;
-		if (!res->flags) {
-			if (io_offset)
-				printk (KERN_ERR "I/O resource not set for host"
-					" bridge %d\n", pci_ctrl->index);
-			res->start = 0;
-			res->end = IO_SPACE_LIMIT;
-			res->flags = IORESOURCE_IO;
-		}
-		res->start += io_offset;
-		res->end += io_offset;
-
-		for (i = 0; i < 3; i++) {
-			res = &pci_ctrl->mem_resources[i];
-			if (!res->flags) {
-				if (i > 0)
-					continue;
-				printk(KERN_ERR "Memory resource not set for "
-				       "host bridge %d\n", pci_ctrl->index);
-				res->start = 0;
-				res->end = ~0U;
-				res->flags = IORESOURCE_MEM;
-			}
-			bus->resource[i+1] = res;
-		}
-	} else {
+	if (bus->parent) {
 		/* This is a subordinate bridge */
 		pci_read_bridge_bases(bus);
 
--- a/drivers/parisc/dino.c
+++ b/drivers/parisc/dino.c
@@ -562,19 +562,6 @@ dino_fixup_bus(struct pci_bus *bus)
 	/* Firmware doesn't set up card-mode dino, so we have to */
 	if (is_card_dino(&dino_dev->hba.dev->id)) {
 		dino_card_setup(bus, dino_dev->hba.base_addr);
-	} else if(bus->parent == NULL) {
-		/* must have a dino above it, reparent the resources
-		 * into the dino window */
-		int i;
-		struct resource *res = &dino_dev->hba.lmmio_space;
-
-		bus->resource[0] = &(dino_dev->hba.io_space);
-		for(i = 0; i < DINO_MAX_LMMIO_RESOURCES; i++) {
-			if(res[i].flags == 0)
-				break;
-			bus->resource[i+1] = &res[i];
-		}
-
 	} else if (bus->parent) {
 		int i;
 
@@ -927,6 +914,7 @@ static int __init dino_probe(struct pari
 	const char *version = "unknown";
 	char *name;
 	int is_cujo = 0;
+	LIST_HEAD(resources);
 	struct pci_bus *bus;
 	unsigned long hpa = dev->hpa.start;
 
@@ -1003,26 +991,37 @@ static int __init dino_probe(struct pari
 
 	dev->dev.platform_data = dino_dev;
 
+	pci_add_resource(&resources, &dino_dev->hba.io_space);
+	if (dino_dev->hba.lmmio_space.flags)
+		pci_add_resource(&resources, &dino_dev->hba.lmmio_space);
+	if (dino_dev->hba.elmmio_space.flags)
+		pci_add_resource(&resources, &dino_dev->hba.elmmio_space);
+	if (dino_dev->hba.gmmio_space.flags)
+		pci_add_resource(&resources, &dino_dev->hba.gmmio_space);
+
 	/*
 	** It's not used to avoid chicken/egg problems
 	** with configuration accessor functions.
 	*/
-	dino_dev->hba.hba_bus = bus = pci_scan_bus_parented(&dev->dev,
-			 dino_current_bus, &dino_cfg_ops, NULL);
-
-	if(bus) {
-		/* This code *depends* on scanning being single threaded
-		 * if it isn't, this global bus number count will fail
-		 */
-		dino_current_bus = bus->subordinate + 1;
-		pci_bus_assign_resources(bus);
-		pci_bus_add_devices(bus);
-	} else {
+	dino_dev->hba.hba_bus = bus = pci_create_root_bus(&dev->dev,
+			 dino_current_bus, &dino_cfg_ops, NULL, &resources);
+	if (!bus) {
 		printk(KERN_ERR "ERROR: failed to scan PCI bus on %s (duplicate bus number %d?)\n",
 		       dev_name(&dev->dev), dino_current_bus);
+		pci_free_resource_list(&resources);
 		/* increment the bus number in case of duplicates */
 		dino_current_bus++;
+		return 0;
 	}
+
+	bus->subordinate = pci_scan_child_bus(bus);
+
+	/* This code *depends* on scanning being single threaded
+	 * if it isn't, this global bus number count will fail
+	 */
+	dino_current_bus = bus->subordinate + 1;
+	pci_bus_assign_resources(bus);
+	pci_bus_add_devices(bus);
 	return 0;
 }
 
--- a/drivers/parisc/lba_pci.c
+++ b/drivers/parisc/lba_pci.c
@@ -653,7 +653,7 @@ lba_fixup_bus(struct pci_bus *bus)
 		}
 	} else {
 		/* Host-PCI Bridge */
-		int err, i;
+		int err;
 
 		DBG("lba_fixup_bus() %s [%lx/%lx]/%lx\n",
 			ldev->hba.io_space.name,
@@ -669,9 +669,6 @@ lba_fixup_bus(struct pci_bus *bus)
 			lba_dump_res(&ioport_resource, 2);
 			BUG();
 		}
-		/* advertize Host bridge resources to PCI bus */
-		bus->resource[0] = &(ldev->hba.io_space);
-		i = 1;
 
 		if (ldev->hba.elmmio_space.start) {
 			err = request_resource(&iomem_resource,
@@ -685,35 +682,17 @@ lba_fixup_bus(struct pci_bus *bus)
 
 				/* lba_dump_res(&iomem_resource, 2); */
 				/* BUG(); */
-			} else
-				bus->resource[i++] = &(ldev->hba.elmmio_space);
+			}
 		}
 
-
-		/*   Overlaps with elmmio can (and should) fail here.
-		 *   We will prune (or ignore) the distributed range.
-		 *
-		 *   FIXME: SBA code should register all elmmio ranges first.
-		 *      that would take care of elmmio ranges routed
-		 *	to a different rope (already discovered) from
-		 *	getting registered *after* LBA code has already
-		 *	registered it's distributed lmmio range.
-		 */
-		if (truncate_pat_collision(&iomem_resource,
-				       	&(ldev->hba.lmmio_space))) {
-
-			printk(KERN_WARNING "LBA: lmmio_space [%lx/%lx] duplicate!\n",
-					(long)ldev->hba.lmmio_space.start,
-					(long)ldev->hba.lmmio_space.end);
-		} else {
+		if (ldev->hba.lmmio_space.flags) {
 			err = request_resource(&iomem_resource, &(ldev->hba.lmmio_space));
 			if (err < 0) {
 				printk(KERN_ERR "FAILED: lba_fixup_bus() request for "
 					"lmmio_space [%lx/%lx]\n",
 					(long)ldev->hba.lmmio_space.start,
 					(long)ldev->hba.lmmio_space.end);
-			} else
-				bus->resource[i++] = &(ldev->hba.lmmio_space);
+			}
 		}
 
 #ifdef CONFIG_64BIT
@@ -728,7 +707,6 @@ lba_fixup_bus(struct pci_bus *bus)
 				lba_dump_res(&iomem_resource, 2);
 				BUG();
 			}
-			bus->resource[i++] = &(ldev->hba.gmmio_space);
 		}
 #endif
 
@@ -1404,6 +1382,7 @@ static int __init
 lba_driver_probe(struct parisc_device *dev)
 {
 	struct lba_device *lba_dev;
+	LIST_HEAD(resources);
 	struct pci_bus *lba_bus;
 	struct pci_ops *cfg_ops;
 	u32 func_class;
@@ -1518,10 +1497,41 @@ lba_driver_probe(struct parisc_device *d
 	if (lba_dev->hba.bus_num.start < lba_next_bus)
 		lba_dev->hba.bus_num.start = lba_next_bus;
 
+	/*   Overlaps with elmmio can (and should) fail here.
+	 *   We will prune (or ignore) the distributed range.
+	 *
+	 *   FIXME: SBA code should register all elmmio ranges first.
+	 *      that would take care of elmmio ranges routed
+	 *	to a different rope (already discovered) from
+	 *	getting registered *after* LBA code has already
+	 *	registered it's distributed lmmio range.
+	 */
+	if (truncate_pat_collision(&iomem_resource,
+				   &(lba_dev->hba.lmmio_space))) {
+		printk(KERN_WARNING "LBA: lmmio_space [%lx/%lx] duplicate!\n",
+				(long)lba_dev->hba.lmmio_space.start,
+				(long)lba_dev->hba.lmmio_space.end);
+		lba_dev->hba.lmmio_space.flags = 0;
+	}
+
+	pci_add_resource(&resources, &lba_dev->hba.io_space);
+	if (lba_dev->hba.elmmio_space.start)
+		pci_add_resource(&resources, &lba_dev->hba.elmmio_space);
+	if (lba_dev->hba.lmmio_space.flags)
+		pci_add_resource(&resources, &lba_dev->hba.lmmio_space);
+	if (lba_dev->hba.gmmio_space.flags)
+		pci_add_resource(&resources, &lba_dev->hba.gmmio_space);
+
 	dev->dev.platform_data = lba_dev;
 	lba_bus = lba_dev->hba.hba_bus =
-		pci_scan_bus_parented(&dev->dev, lba_dev->hba.bus_num.start,
-				cfg_ops, NULL);
+		pci_create_root_bus(&dev->dev, lba_dev->hba.bus_num.start,
+				    cfg_ops, NULL, &resources);
+	if (!lba_bus) {
+		pci_free_resource_list(&resources);
+		return 0;
+	}
+
+	lba_bus->subordinate = pci_scan_child_bus(lba_bus);
 
 	/* This is in lieu of calling pci_assign_unassigned_resources() */
 	if (is_pdc_pat()) {
@@ -1551,10 +1561,8 @@ lba_driver_probe(struct parisc_device *d
 		lba_dev->flags |= LBA_FLAG_SKIP_PROBE;
 	}
 
-	if (lba_bus) {
-		lba_next_bus = lba_bus->subordinate + 1;
-		pci_bus_add_devices(lba_bus);
-	}
+	lba_next_bus = lba_bus->subordinate + 1;
+	pci_bus_add_devices(lba_bus);
 
 	/* Whew! Finally done! Tell services we got this one covered. */
 	return 0;
--- a/drivers/pci/bus.c
+++ b/drivers/pci/bus.c
@@ -18,6 +18,32 @@
 
 #include "pci.h"
 
+void pci_add_resource(struct list_head *resources, struct resource *res)
+{
+	struct pci_bus_resource *bus_res;
+
+	bus_res = kzalloc(sizeof(struct pci_bus_resource), GFP_KERNEL);
+	if (!bus_res) {
+		printk(KERN_ERR "PCI: can't add bus resource %pR\n", res);
+		return;
+	}
+
+	bus_res->res = res;
+	list_add_tail(&bus_res->list, resources);
+}
+EXPORT_SYMBOL(pci_add_resource);
+
+void pci_free_resource_list(struct list_head *resources)
+{
+	struct pci_bus_resource *bus_res, *tmp;
+
+	list_for_each_entry_safe(bus_res, tmp, resources, list) {
+		list_del(&bus_res->list);
+		kfree(bus_res);
+	}
+}
+EXPORT_SYMBOL(pci_free_resource_list);
+
 void pci_bus_add_resource(struct pci_bus *bus, struct resource *res,
 			  unsigned int flags)
 {
@@ -52,16 +78,12 @@ EXPORT_SYMBOL_GPL(pci_bus_resource_n);
 
 void pci_bus_remove_resources(struct pci_bus *bus)
 {
-	struct pci_bus_resource *bus_res, *tmp;
 	int i;
 
 	for (i = 0; i < PCI_BRIDGE_RESOURCE_NUM; i++)
 		bus->resource[i] = NULL;
 
-	list_for_each_entry_safe(bus_res, tmp, &bus->resources, list) {
-		list_del(&bus_res->list);
-		kfree(bus_res);
-	}
+	pci_free_resource_list(&bus->resources);
 }
 
 /**
--- a/drivers/pci/probe.c
+++ b/drivers/pci/probe.c
@@ -1527,12 +1527,14 @@ unsigned int __devinit pci_scan_child_bu
 	return max;
 }
 
-struct pci_bus * pci_create_bus(struct device *parent,
-		int bus, struct pci_ops *ops, void *sysdata)
+struct pci_bus *pci_create_root_bus(struct device *parent, int bus,
+		struct pci_ops *ops, void *sysdata, struct list_head *resources)
 {
-	int error;
+	int error, i;
 	struct pci_bus *b, *b2;
 	struct device *dev;
+	struct pci_bus_resource *bus_res, *n;
+	struct resource *res;
 
 	b = pci_alloc_bus();
 	if (!b)
@@ -1582,8 +1584,20 @@ struct pci_bus * pci_create_bus(struct d
 	pci_create_legacy_files(b);
 
 	b->number = b->secondary = bus;
-	b->resource[0] = &ioport_resource;
-	b->resource[1] = &iomem_resource;
+
+	/* Add initial resources to the bus */
+	list_for_each_entry_safe(bus_res, n, resources, list)
+		list_move_tail(&bus_res->list, &b->resources);
+
+	if (parent)
+		dev_info(parent, "PCI host bridge to bus %s\n", dev_name(&b->dev));
+	else
+		printk(KERN_INFO "PCI host bridge to bus %s\n", dev_name(&b->dev));
+
+	pci_bus_for_each_resource(b, res, i) {
+		if (res)
+			dev_info(&b->dev, "root bus resource %pR\n", res);
+	}
 
 	return b;
 
@@ -1599,18 +1613,58 @@ err_out:
 	return NULL;
 }
 
+struct pci_bus * __devinit pci_scan_root_bus(struct device *parent, int bus,
+		struct pci_ops *ops, void *sysdata, struct list_head *resources)
+{
+	struct pci_bus *b;
+
+	b = pci_create_root_bus(parent, bus, ops, sysdata, resources);
+	if (!b)
+		return NULL;
+
+	b->subordinate = pci_scan_child_bus(b);
+	pci_bus_add_devices(b);
+	return b;
+}
+EXPORT_SYMBOL(pci_scan_root_bus);
+
+/* Deprecated; use pci_scan_root_bus() instead */
 struct pci_bus * __devinit pci_scan_bus_parented(struct device *parent,
 		int bus, struct pci_ops *ops, void *sysdata)
 {
+	LIST_HEAD(resources);
 	struct pci_bus *b;
 
-	b = pci_create_bus(parent, bus, ops, sysdata);
+	pci_add_resource(&resources, &ioport_resource);
+	pci_add_resource(&resources, &iomem_resource);
+	b = pci_create_root_bus(parent, bus, ops, sysdata, &resources);
 	if (b)
 		b->subordinate = pci_scan_child_bus(b);
+	else
+		pci_free_resource_list(&resources);
 	return b;
 }
 EXPORT_SYMBOL(pci_scan_bus_parented);
 
+struct pci_bus * __devinit pci_scan_bus(int bus, struct pci_ops *ops,
+					void *sysdata)
+{
+	LIST_HEAD(resources);
+	struct pci_bus *b;
+
+	pci_add_resource(&resources, &ioport_resource);
+	pci_add_resource(&resources, &iomem_resource);
+	b = pci_create_root_bus(NULL, bus, ops, sysdata, &resources);
+	if (b) {
+		b->subordinate = pci_scan_child_bus(b);
+		pci_bus_add_devices(b);
+	} else {
+		pci_free_resource_list(&resources);
+	}
+	return b;
+}
+EXPORT_SYMBOL(pci_scan_bus);
+
 #ifdef CONFIG_HOTPLUG
 /**
  * pci_rescan_bus - scan a PCI bus for devices.
--- a/include/linux/pci.h
+++ b/include/linux/pci.h
@@ -660,17 +660,13 @@ extern struct pci_bus *pci_find_bus(int
 void pci_bus_add_devices(const struct pci_bus *bus);
 struct pci_bus *pci_scan_bus_parented(struct device *parent, int bus,
 				      struct pci_ops *ops, void *sysdata);
-static inline struct pci_bus * __devinit pci_scan_bus(int bus, struct pci_ops *ops,
-					   void *sysdata)
-{
-	struct pci_bus *root_bus;
-	root_bus = pci_scan_bus_parented(NULL, bus, ops, sysdata);
-	if (root_bus)
-		pci_bus_add_devices(root_bus);
-	return root_bus;
-}
-struct pci_bus *pci_create_bus(struct device *parent, int bus,
-			       struct pci_ops *ops, void *sysdata);
+struct pci_bus *pci_scan_bus(int bus, struct pci_ops *ops, void *sysdata);
+struct pci_bus *pci_create_root_bus(struct device *parent, int bus,
+				    struct pci_ops *ops, void *sysdata,
+				    struct list_head *resources);
+struct pci_bus * __devinit pci_scan_root_bus(struct device *parent, int bus,
+					     struct pci_ops *ops, void *sysdata,
+					     struct list_head *resources);
 struct pci_bus *pci_add_new_bus(struct pci_bus *parent, struct pci_dev *dev,
 				int busnr);
 void pcie_update_link_speed(struct pci_bus *bus, u16 link_status);
@@ -910,6 +906,8 @@ int pci_request_selected_regions_exclusi
 void pci_release_selected_regions(struct pci_dev *, int);
 
 /* drivers/pci/bus.c */
+void pci_add_resource(struct list_head *resources, struct resource *res);
+void pci_free_resource_list(struct list_head *resources);
 void pci_bus_add_resource(struct pci_bus *bus, struct resource *res, unsigned int flags);
 struct resource *pci_bus_resource_n(const struct pci_bus *bus, int n);
 void pci_bus_remove_resources(struct pci_bus *bus);
