--- a/drivers/bcma/host_pci.c
+++ b/drivers/bcma/host_pci.c
@@ -222,7 +222,7 @@ err_kfree_bus:
 	return err;
 }
 
-static void bcma_host_pci_remove(struct pci_dev *dev)
+static void __devexit bcma_host_pci_remove(struct pci_dev *dev)
 {
 	struct bcma_bus *bus = pci_get_drvdata(dev);
 
@@ -278,7 +278,7 @@ static struct pci_driver bcma_pci_bridge
 	.name = "bcma-pci-bridge",
 	.id_table = bcma_pci_bridge_tbl,
 	.probe = bcma_host_pci_probe,
-	.remove = bcma_host_pci_remove,
+	.remove = __devexit_p(bcma_host_pci_remove),
 	.driver.pm = BCMA_PM_OPS,
 };
 
