--- a/arch/mips/ath79/mach-ubnt-xm.c
+++ b/arch/mips/ath79/mach-ubnt-xm.c
@@ -13,15 +13,17 @@
 #include <linux/init.h>
 #include <linux/pci.h>
 #include <linux/ath9k_platform.h>
+#include <linux/etherdevice.h>
 
 #include <asm/mach-ath79/irq.h>
 
 #include "dev-ap9x-pci.h"
+#include "dev-eth.h"
 #include "dev-gpio-buttons.h"
 #include "dev-leds-gpio.h"
 #include "dev-m25p80.h"
+#include "dev-usb.h"
 #include "machtypes.h"
-#include "pci.h"
 
 #define UBNT_XM_GPIO_LED_L1		0
 #define UBNT_XM_GPIO_LED_L2		1
@@ -37,19 +39,19 @@
 
 static struct gpio_led ubnt_xm_leds_gpio[] __initdata = {
 	{
-		.name		= "ubnt-xm:red:link1",
+		.name		= "ubnt:red:link1",
 		.gpio		= UBNT_XM_GPIO_LED_L1,
 		.active_low	= 0,
 	}, {
-		.name		= "ubnt-xm:orange:link2",
+		.name		= "ubnt:orange:link2",
 		.gpio		= UBNT_XM_GPIO_LED_L2,
 		.active_low	= 0,
 	}, {
-		.name		= "ubnt-xm:green:link3",
+		.name		= "ubnt:green:link3",
 		.gpio		= UBNT_XM_GPIO_LED_L3,
 		.active_low	= 0,
 	}, {
-		.name		= "ubnt-xm:green:link4",
+		.name		= "ubnt:green:link4",
 		.gpio		= UBNT_XM_GPIO_LED_L4,
 		.active_low	= 0,
 	},
@@ -66,9 +68,13 @@ static struct gpio_keys_button ubnt_xm_g
 	}
 };
 
+#define UBNT_M_WAN_PHYMASK	BIT(4)
+
 static void __init ubnt_xm_init(void)
 {
 	u8 *eeprom = (u8 *) KSEG1ADDR(UBNT_XM_EEPROM_ADDR);
+	u8 *mac1 = (u8 *) KSEG1ADDR(0x1fff0000);
+	u8 *mac2 = (u8 *) KSEG1ADDR(0x1fff0000 + ETH_ALEN);
 
 	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_xm_leds_gpio),
 				 ubnt_xm_leds_gpio);
@@ -79,9 +85,99 @@ static void __init ubnt_xm_init(void)
 
 	ath79_register_m25p80(NULL);
 	ap91_pci_init(eeprom, NULL);
+
+	ath79_register_mdio(0, ~UBNT_M_WAN_PHYMASK);
+	ath79_init_mac(ath79_eth0_data.mac_addr, mac1, 0);
+	ath79_init_mac(ath79_eth1_data.mac_addr, mac2, 0);
+	ath79_register_eth(0);
 }
 
 MIPS_MACHINE(ATH79_MACH_UBNT_XM,
 	     "UBNT-XM",
 	     "Ubiquiti Networks XM (rev 1.0) board",
 	     ubnt_xm_init);
+
+MIPS_MACHINE(ATH79_MACH_UBNT_BULLET_M, "UBNT-BM", "Ubiquiti Bullet M",
+	     ubnt_xm_init);
+
+static void __init ubnt_rocket_m_setup(void)
+{
+	ubnt_xm_init();
+	ath79_register_usb();
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_ROCKET_M, "UBNT-RM", "Ubiquiti Rocket M",
+	     ubnt_rocket_m_setup);
+
+static void __init ubnt_nano_m_setup(void)
+{
+	ubnt_xm_init();
+	ath79_register_eth(1);
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_NANO_M, "UBNT-NM", "Ubiquiti Nanostation M",
+	     ubnt_nano_m_setup);
+
+static struct gpio_led ubnt_airrouter_leds_gpio[] __initdata = {
+	{
+		.name		= "ubnt:green:globe",
+		.gpio		= 0,
+		.active_low	= 1,
+	}
+};
+
+static void __init ubnt_airrouter_setup(void)
+{
+	u8 *mac1 = (u8 *) KSEG1ADDR(0x1fff0000);
+	u8 *ee = (u8 *) KSEG1ADDR(0x1fff1000);
+
+	ath79_register_m25p80(NULL);
+	ath79_register_mdio(0, ~UBNT_M_WAN_PHYMASK);
+
+	ath79_init_mac(ath79_eth0_data.mac_addr, mac1, 0);
+	ath79_init_local_mac(ath79_eth1_data.mac_addr, mac1);
+
+	ath79_register_eth(1);
+	ath79_register_eth(0);
+	ath79_register_usb();
+
+	ap91_pci_init(ee, NULL);
+	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_airrouter_leds_gpio),
+				 ubnt_airrouter_leds_gpio);
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_AIRROUTER, "UBNT-AR", "Ubiquiti AirRouter",
+	     ubnt_airrouter_setup);
+
+static struct gpio_led ubnt_unifi_leds_gpio[] __initdata = {
+	{
+		.name		= "ubnt:orange:dome",
+		.gpio		= 1,
+		.active_low	= 0,
+	}, {
+		.name		= "ubnt:green:dome",
+		.gpio		= 0,
+		.active_low	= 0,
+	}
+};
+
+static void __init ubnt_unifi_setup(void)
+{
+	u8 *mac = (u8 *) KSEG1ADDR(0x1fff0000);
+	u8 *ee = (u8 *) KSEG1ADDR(0x1fff1000);
+
+	ath79_register_m25p80(NULL);
+
+	ath79_register_mdio(0, ~UBNT_M_WAN_PHYMASK);
+
+	ath79_init_mac(ath79_eth0_data.mac_addr, mac, 0);
+	ath79_register_eth(0);
+
+	ap91_pci_init(ee, NULL);
+
+	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_unifi_leds_gpio),
+				 ubnt_unifi_leds_gpio);
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_UNIFI, "UBNT-UF", "Ubiquiti UniFi",
+	     ubnt_unifi_setup);
--- a/arch/mips/ath79/Kconfig
+++ b/arch/mips/ath79/Kconfig
@@ -58,9 +58,11 @@ config ATH79_MACH_UBNT_XM
 	bool "Ubiquiti Networks XM (rev 1.0) board"
 	select SOC_AR724X
 	select ATH79_DEV_AP9X_PCI if PCI
+	select ATH79_DEV_ETH
 	select ATH79_DEV_GPIO_BUTTONS
 	select ATH79_DEV_LEDS_GPIO
 	select ATH79_DEV_M25P80
+	select ATH79_DEV_USB
 	help
 	  Say 'Y' here if you want your kernel to support the
 	  Ubiquiti Networks XM (rev 1.0) board.
--- a/arch/mips/ath79/machtypes.h
+++ b/arch/mips/ath79/machtypes.h
@@ -21,6 +21,11 @@ enum ath79_mach_type {
 	ATH79_MACH_AP81,		/* Atheros AP81 reference board */
 	ATH79_MACH_DB120,		/* Atheros DB120 reference board */
 	ATH79_MACH_PB44,		/* Atheros PB44 reference board */
+	ATH79_MACH_UBNT_AIRROUTER,	/* Ubiquiti AirRouter */
+	ATH79_MACH_UBNT_BULLET_M,	/* Ubiquiti Bullet M */
+	ATH79_MACH_UBNT_NANO_M, 	/* Ubiquiti NanoStation M */
+	ATH79_MACH_UBNT_ROCKET_M,	/* Ubiquiti Rocket M */
+	ATH79_MACH_UBNT_UNIFI, 		/* Ubiquiti Unifi */
 	ATH79_MACH_UBNT_XM,		/* Ubiquiti Networks XM board rev 1.0 */
 };
 
