--- a/arch/mips/ath79/gpio.c
+++ b/arch/mips/ath79/gpio.c
@@ -188,8 +188,10 @@ void __init ath79_gpio_init(void)
 
 	if (soc_is_ar71xx())
 		ath79_gpio_count = AR71XX_GPIO_COUNT;
-	else if (soc_is_ar724x())
-		ath79_gpio_count = AR724X_GPIO_COUNT;
+	else if (soc_is_ar7240())
+		ath79_gpio_count = AR7240_GPIO_COUNT;
+	else if (soc_is_ar7241() || soc_is_ar7242())
+		ath79_gpio_count = AR7241_GPIO_COUNT;
 	else if (soc_is_ar913x())
 		ath79_gpio_count = AR913X_GPIO_COUNT;
 	else if (soc_is_ar933x())
--- a/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
+++ b/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
@@ -428,7 +428,8 @@
 #define AR71XX_GPIO_REG_FUNC		0x28
 
 #define AR71XX_GPIO_COUNT		16
-#define AR724X_GPIO_COUNT		18
+#define AR7240_GPIO_COUNT		18
+#define AR7241_GPIO_COUNT		20
 #define AR913X_GPIO_COUNT		22
 #define AR933X_GPIO_COUNT		30
 #define AR934X_GPIO_COUNT		23
