--- /dev/null
+++ b/arch/powerpc/boot/dts/rb600.dts
@@ -0,0 +1,242 @@
+/*
+ * RouterBOARD 600 series Device Tree Source
+ *
+ * Copyright 2009 Michael Guntsche <mike@it-loops.com>
+ *
+ * This program is free software; you can redistribute  it and/or modify it
+ * under  the terms of  the GNU General  Public License as published by the
+ * Free Software Foundation;  either version 2 of the  License, or (at your
+ * option) any later version.
+ */
+
+/dts-v1/;
+
+/ {
+	model = "RB600";
+	compatible = "MPC83xx";
+	#address-cells = <1>;
+	#size-cells = <1>;
+
+	aliases {
+		ethernet0 = &enet0;
+		ethernet1 = &enet1;
+	};
+
+	chosen {
+		linux,stdout-path = "/soc8343@e0000000/serial@4500";
+	};
+
+	cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		PowerPC,8343E@0 {
+			device_type = "cpu";
+			reg = <0x0>;
+			d-cache-line-size = <0x20>;
+			i-cache-line-size = <0x20>;
+			d-cache-size = <0x8000>;
+			i-cache-size = <0x8000>;
+			timebase-frequency = <0x0000000>; // filled by the bootwrapper from the firmware blob
+			clock-frequency = <0x00000000>; // filled by the bootwrapper from the firmware blob
+		};
+	};
+
+	memory {
+		device_type = "memory";
+		reg = <0x0 0x0000000>; // filled by the bootwrapper from the firmware blob
+	};
+
+	cf@f9200000 {
+		lb-timings = <0x5dc 0x3e8 0x1194 0x5dc 0x2af8>;
+		interrupt-at-level = <0x0>;
+		interrupt-parent = <&ipic>;
+		interrupts = <0x16 0x8>;
+		lbc_extra_divider = <0x1>;
+		reg = <0xf9200000 0x200000>;
+		device_type = "rb,cf";
+	};
+
+	cf@f9000000 {
+		lb-timings = <0x5dc 0x3e8 0x1194 0x5dc 0x2af8>;
+		interrupt-at-level = <0x0>;
+		interrupt-parent = <&ipic>;
+		interrupts = <0x14 0x8>;
+		lbc_extra_divider = <0x1>;
+		reg = <0xf9000000 0x200000>;
+		device_type = "rb,cf";
+	};
+
+	flash {
+		reg = <0xff800000 0x20000>;
+	};
+
+	nnand {
+		reg = <0xf0000000 0x1000>;
+	};
+
+	nand {
+		ale = <&gpio 0x6>;
+		cle = <&gpio 0x5>;
+		nce = <&gpio 0x4>;
+		rdy = <&gpio 0x3>;
+		reg = <0xf8000000 0x1000>;
+		device_type = "rb,nand";
+	};
+
+	fancon {
+		interrupt-parent = <&ipic>;
+		interrupts = <0x17 0x8>;
+		sense = <&gpio 0x7>;
+		fan_on = <&gpio 0x9>;
+	};
+
+	pci0: pci@e0008500 {
+		device_type = "pci";
+		compatible = "fsl,mpc8349-pci";
+		reg = <0xe0008500 0x100 0xe0008300 0x8>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+		#interrupt-cells = <1>;
+		ranges = <0x2000000 0x0 0x80000000 0x80000000 0x0 0x20000000 0x1000000 0x0 0x0 0xd0000000 0x0 0x4000000>;
+		bus-range = <0x0 0x0>;
+		interrupt-map = <
+			0x5800 0x0 0x0 0x1 &ipic 0x15 0x8
+			0x6000 0x0 0x0 0x1 &ipic 0x30 0x8
+			0x6000 0x0 0x0 0x2 &ipic 0x11 0x8
+			0x6800 0x0 0x0 0x1 &ipic 0x11 0x8
+			0x6800 0x0 0x0 0x2 &ipic 0x12 0x8
+			0x7000 0x0 0x0 0x1 &ipic 0x12 0x8
+			0x7000 0x0 0x0 0x2 &ipic 0x13 0x8
+			0x7800 0x0 0x0 0x1 &ipic 0x13 0x8
+			0x7800 0x0 0x0 0x2 &ipic 0x30 0x8
+			0x8000 0x0 0x0 0x1 &ipic 0x30 0x8
+			0x8000 0x0 0x0 0x2 &ipic 0x12 0x8
+			0x8000 0x0 0x0 0x3 &ipic 0x11 0x8
+			0x8000 0x0 0x0 0x4 &ipic 0x13 0x8
+			0xa000 0x0 0x0 0x1 &ipic 0x30 0x8
+			0xa000 0x0 0x0 0x2 &ipic 0x11 0x8
+			0xa000 0x0 0x0 0x3 &ipic 0x12 0x8
+			0xa000 0x0 0x0 0x4 &ipic 0x13 0x8
+			0xa800 0x0 0x0 0x1 &ipic 0x11 0x8
+			0xa800 0x0 0x0 0x2 &ipic 0x12 0x8
+			0xa800 0x0 0x0 0x3 &ipic 0x13 0x8
+			0xa800 0x0 0x0 0x4 &ipic 0x30 0x8>;
+		interrupt-map-mask = <0xf800 0x0 0x0 0x7>;
+		interrupt-parent = <&ipic>;
+	};
+
+	soc8343@e0000000 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		device_type = "soc";
+		compatible = "simple-bus";
+		ranges = <0x0 0xe0000000 0x100000>;
+		reg = <0xe0000000 0x200>;
+		bus-frequency = <0x1>;
+
+		led {
+			user_led = <0x400 0x8>;
+		};
+
+		beeper {
+			reg = <0x500 0x100>;
+		};
+
+		gpio: gpio@0 {
+			reg = <0xc08 0x4>;
+			device-id = <0x0>;
+			compatible = "gpio";
+			device_type = "gpio";
+		};
+
+		enet0: ethernet@25000 {
+			#address-cells = <1>;
+			#size-cells = <1>;
+			cell-index = <0>;
+			phy-handle = <&phy0>;
+			tbi-handle = <&tbi0>;
+			interrupt-parent = <&ipic>;
+			interrupts = <0x23 0x8 0x24 0x8 0x25 0x8>;
+			local-mac-address = [00 00 00 00 00 00];
+			reg = <0x25000 0x1000>;
+			ranges = <0x0 0x25000 0x1000>;
+			compatible = "gianfar";
+			model = "TSEC";
+			device_type = "network";
+
+			mdio@520 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,gianfar-tbi";
+				reg = <0x520 0x20>;
+
+				tbi0: tbi-phy@11 {
+					reg = <0x11>;
+					device_type = "tbi-phy";
+				};
+			};
+		};
+
+		enet1: ethernet@24000 {
+			#address-cells = <1>;
+			#size-cells = <1>;
+			cell-index = <1>;
+			phy-handle = <&phy1>;
+			tbi-handle = <&tbi1>;
+			interrupt-parent = <&ipic>;
+			interrupts = <0x20 0x8 0x21 0x8 0x22 0x8>;
+			local-mac-address = [00 00 00 00 00 00];
+			reg = <0x24000 0x1000>;
+			ranges = <0x0 0x24000 0x1000>;
+			compatible = "gianfar";
+			model = "TSEC";
+			device_type = "network";
+
+			mdio@520 {
+				#size-cells = <0x0>;
+				#address-cells = <0x1>;
+				reg = <0x520 0x20>;
+				compatible = "fsl,gianfar-mdio";
+
+				phy0: ethernet-phy@0 {
+					device_type = "ethernet-phy";
+					reg = <0x0>;
+				};
+
+				phy1: ethernet-phy@1 {
+					device_type = "ethernet-phy";
+					reg = <0x1>;
+				};
+
+				tbi1: tbi-phy@11 {
+					reg = <0x11>;
+					device_type = "tbi-phy";
+				};
+			};
+		};
+
+		ipic: pic@700 {
+			interrupt-controller;
+			#address-cells = <0>;
+			#interrupt-cells = <2>;
+			reg = <0x700 0x100>;
+			device_type = "ipic";
+		};
+
+		serial@4500 {
+			interrupt-parent = <&ipic>;
+			interrupts = <0x9 0x8>;
+			clock-frequency = <0xfe4f840>;
+			reg = <0x4500 0x100>;
+			compatible = "ns16550";
+			device_type = "serial";
+		};
+
+		wdt@200 {
+			reg = <0x200 0x100>;
+			compatible = "mpc83xx_wdt";
+			device_type = "watchdog";
+		};
+	};
+};
