From 1759a5bc87d0eb8dbb0d8a9794b336813057eb88 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Thu, 25 Nov 2010 17:59:28 +0100
Subject: [PATCH 19/35] MIPS: ath79: register PCI controller on the PB44 board

The PB44 reference board has two miniPCI slots. Register
the PCI controller to make those usable.

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>

v2: - no changes
---
 arch/mips/ath79/mach-pb44.c |    2 ++
 1 files changed, 2 insertions(+), 0 deletions(-)

--- a/arch/mips/ath79/mach-pb44.c
+++ b/arch/mips/ath79/mach-pb44.c
@@ -19,6 +19,7 @@
 #include "dev-leds-gpio.h"
 #include "dev-spi.h"
 #include "dev-usb.h"
+#include "pci.h"
 
 #define PB44_GPIO_I2C_SCL	0
 #define PB44_GPIO_I2C_SDA	1
@@ -114,6 +115,7 @@ static void __init pb44_init(void)
 	ath79_register_spi(&pb44_spi_data, pb44_spi_info,
 			   ARRAY_SIZE(pb44_spi_info));
 	ath79_register_usb();
+	ath79_register_pci();
 }
 
 MIPS_MACHINE(ATH79_MACH_PB44, "PB44", "Atheros PB44 reference board",
