The pwr_in_suspend flag depends on the MMC settings which can be
retrieved from the SDIO subsystem, so it doesn't need to be part of
the platform data structure.  Move it to the platform device data that
is passed from SDIO to wlcore.

Signed-off-by: Luciano Coelho <coelho@ti.com>
Reviewed-by: Felipe Balbi <balbi@ti.com>

---
 drivers/net/wireless/ti/wlcore/main.c     | 3 +--
 drivers/net/wireless/ti/wlcore/sdio.c     | 2 +-
 drivers/net/wireless/ti/wlcore/wlcore_i.h | 1 +
 include/linux/wl12xx.h                    | 1 -
 4 files changed, 3 insertions(+), 4 deletions(-)

--- a/drivers/net/wireless/ti/wlcore/main.c
+++ b/drivers/net/wireless/ti/wlcore/main.c
@@ -5901,7 +5901,6 @@ static void wlcore_nvs_cb(const struct f
 	struct wl1271 *wl = context;
 	struct platform_device *pdev = wl->pdev;
 	struct wlcore_platdev_data *pdev_data = pdev->dev.platform_data;
-	struct wl12xx_platform_data *pdata = pdev_data->pdata;
 
 	int ret;
 
@@ -5948,7 +5947,7 @@ static void wlcore_nvs_cb(const struct f
 	if (!ret) {
 		wl->irq_wake_enabled = true;
 		device_init_wakeup(wl->dev, 1);
-		if (pdata->pwr_in_suspend)
+		if (pdev_data->pwr_in_suspend)
 			wl->hw->wiphy->wowlan = &wlcore_wowlan_support;
 	}
 #endif
--- a/drivers/net/wireless/ti/wlcore/sdio.c
+++ b/drivers/net/wireless/ti/wlcore/sdio.c
@@ -260,7 +260,7 @@ static int wl1271_probe(struct sdio_func
 	dev_dbg(glue->dev, "sdio PM caps = 0x%x\n", mmcflags);
 
 	if (mmcflags & MMC_PM_KEEP_POWER)
-		pdev_data->pdata->pwr_in_suspend = true;
+		pdev_data->pwr_in_suspend = true;
 
 	sdio_set_drvdata(func, glue);
 
--- a/drivers/net/wireless/ti/wlcore/wlcore_i.h
+++ b/drivers/net/wireless/ti/wlcore/wlcore_i.h
@@ -209,6 +209,7 @@ struct wl1271_if_operations {
 struct wlcore_platdev_data {
 	struct wl12xx_platform_data *pdata;
 	struct wl1271_if_operations *if_ops;
+	bool pwr_in_suspend;
 };
 
 #define MAX_NUM_KEYS 14
--- a/include/linux/wl12xx.h
+++ b/include/linux/wl12xx.h
@@ -59,7 +59,6 @@ struct wl12xx_platform_data {
 	int irq;
 	int board_ref_clock;
 	int board_tcxo_clock;
-	bool pwr_in_suspend;
 };
 
 #ifdef CONFIG_WILINK_PLATFORM_DATA
